(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6002)
    (drawings 10)
    (tracks 81)
    (zones 0)
    (modules 7)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.127)
    (segment_width 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.25)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 /HV6)
  (net 6 /HV5)
  (net 7 /HV10)
  (net 8 /HV4)
  (net 9 /HV9)
  (net 10 /HV3)
  (net 11 /HV8)
  (net 12 /HV2)
  (net 13 /HV7)
  (net 14 /HV1)
  (net 15 "Net-(J1-Pad15)")
  (net 16 /HV11)
  (net 17 "Net-(NX1-Pad12)")
  (net 18 "Net-(D1-Pad1)")
  (net 19 "Net-(J2-Pad1)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV11)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(NX1-Pad12)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module SparkFun-LED:SparkFun-LED-LED-RGB-THRU (layer B.Cu) (tedit 200000)
    (at 139.02 124.88 180)
    (descr "LED - RGB PTH")
    (tags "LED - RGB PTH")
    (attr virtual)
    (fp_text reference D1 (at -3.4105 -0.0245) (layer Dwgs.User))
    (fp_text value LED (at 0 -1.739) (layer B.SilkS))
    (pad 1 thru_hole oval (at 1.905 0) (size 0.889 1.778) (drill 0.762) (layers *.Cu *.Paste *.Mask)
      (net 18 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 0.635 0) (size 0.889 1.778) (drill 0.762) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at -0.635 0) (size 0.889 1.778) (drill 0.762) (layers *.Cu *.Paste *.Mask)
      (net 1 +5V))
    (pad 4 thru_hole oval (at -1.905 0) (size 0.889 1.778) (drill 0.762) (layers *.Cu *.Paste *.Mask)
      (net 4 /Din))
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 151.892 133.6675 270)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.128 270) (layer Dwgs.User))
    (fp_text value DP (at 1.2125 2.372 270) (layer B.SilkS))
    (fp_text user %R (at 1.27 0) (layer B.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /HV11))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mynixies:mynixies-TSB-12P-MILL-MAX (layer F.Cu) (tedit 200000)
    (at 160.02 119.38)
    (attr virtual)
    (fp_text reference NX1 (at 21.30298 0) (layer F.SilkS))
    (fp_text value TSB12P (at -20.14474 0) (layer F.SilkS))
    (fp_text user TOP (at -0.26924 -22.31898) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 7.99846) (size 5.99948 5.99948) (drill 5.99948) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 16.49984 16.49984) (drill 16.49984) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -3.4925 13.03782) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 17 "Net-(NX1-Pad12)"))
    (pad 11 thru_hole circle (at -9.54532 9.54532) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad1)"))
    (pad 10 thru_hole circle (at -13.03782 3.4925) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 7 /HV10))
    (pad 9 thru_hole circle (at -13.03782 -3.4925) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 9 /HV9))
    (pad 8 thru_hole circle (at -9.54532 -9.54532) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 11 /HV8))
    (pad 7 thru_hole circle (at -3.4925 -13.03782) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 13 /HV7))
    (pad 6 thru_hole circle (at 3.4925 -13.03782) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 5 /HV6))
    (pad 5 thru_hole circle (at 9.54532 -9.54532) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 6 /HV5))
    (pad 4 thru_hole circle (at 13.03782 -3.4925) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 8 /HV4))
    (pad 3 thru_hole circle (at 13.03782 3.4925) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 10 /HV3))
    (pad 2 thru_hole circle (at 9.54532 9.54532) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 12 /HV2))
    (pad 1 thru_hole circle (at 3.4925 13.03782) (size 4.6736 4.6736) (drill 3.6576) (layers *.Cu *.Mask)
      (net 14 /HV1))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 167.1695 100.33 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5C664162)
    (at 139.02 127.38 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 -1.905) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer B.Cu) (tedit 5C664122)
    (at 157.4165 138.43)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 6.35 2.66 180) (layer B.SilkS) hide)
    (fp_text value Anode (at 6.286179 0 180) (layer B.SilkS))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(NX1-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x09_Pitch2.54mm (layer B.Cu) (tedit 5C66468F)
    (at 149.86 143.764 270)
    (descr "Through hole angled pin header, 2x09, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 5.655 2.27 270) (layer B.SilkS) hide)
    (fp_text value Nixie (at 5.655 -22.59 270) (layer B.Fab))
    (fp_text user %R (at 5.31 -10.16 180) (layer B.Fab))
    (pad 18 thru_hole oval (at 2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 16 thru_hole oval (at 2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV6))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV5))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /HV11))
    (pad 12 thru_hole oval (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV4))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV10))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV3))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV9))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV2))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV8))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV1))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV7))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text DO (at 137.16 123.825 90) (layer B.SilkS))
  (gr_text GND (at 138.3665 123.825 90) (layer B.SilkS))
  (gr_text 5V (at 139.6365 123.825 90) (layer B.SilkS))
  (gr_text DIN (at 140.9065 123.825 90) (layer B.SilkS))
  (gr_arc (start 160.02 119.38) (end 172.084999 141.604999) (angle -303.0087237) (layer Edge.Cuts) (width 0.127))
  (dimension 8.5 (width 0.127) (layer Dwgs.User)
    (gr_text "8.500 mm" (at 161.874 154.63 90) (layer Dwgs.User))
    (feature1 (pts (xy 160.52 150.38) (xy 161.606421 150.38)))
    (feature2 (pts (xy 160.52 158.88) (xy 161.606421 158.88)))
    (crossbar (pts (xy 161.02 158.88) (xy 161.02 150.38)))
    (arrow1a (pts (xy 161.02 150.38) (xy 161.606421 151.506504)))
    (arrow1b (pts (xy 161.02 150.38) (xy 160.433579 151.506504)))
    (arrow2a (pts (xy 161.02 158.88) (xy 161.606421 157.753496)))
    (arrow2b (pts (xy 161.02 158.88) (xy 160.433579 157.753496)))
  )
  (gr_text "nixies.us\nCD27 CD12, CD16, GN1 GN5" (at 166.1795 100.965) (layer B.Mask))
  (gr_line (start 147.955 158.88) (end 147.955001 141.604999) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 172.085 158.88) (end 172.084999 141.604999) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 147.955 158.88) (end 172.085 158.88) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 186.055 93.6625) (xy 133.35 93.6625) (xy 133.6675 159.88) (xy 186.3725 159.88)
      )
    )
  )
)
