(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 134)
    (no_connects 0)
    (area 82.774999 25.154999 148.052001 53.403001)
    (thickness 1.6)
    (drawings 33)
    (tracks 855)
    (zones 0)
    (modules 61)
    (nets 106)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.027)
    (via_min_drill 0.3302)
    (uvia_size 0.0762)
    (uvia_drill 0.0254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 91.4 27.3)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /D0)
  (net 2 "Net-(D1-Pad1)")
  (net 3 /D1)
  (net 4 "Net-(D2-Pad1)")
  (net 5 /D2)
  (net 6 "Net-(D3-Pad1)")
  (net 7 /D3)
  (net 8 "Net-(D4-Pad1)")
  (net 9 /D4)
  (net 10 "Net-(D5-Pad1)")
  (net 11 /D5)
  (net 12 "Net-(D6-Pad1)")
  (net 13 /D6)
  (net 14 "Net-(D7-Pad1)")
  (net 15 /D7)
  (net 16 "Net-(D8-Pad1)")
  (net 17 /A0)
  (net 18 "Net-(D9-Pad1)")
  (net 19 /A1)
  (net 20 "Net-(D10-Pad1)")
  (net 21 /A2)
  (net 22 "Net-(D11-Pad1)")
  (net 23 /A3)
  (net 24 "Net-(D12-Pad1)")
  (net 25 /A4)
  (net 26 "Net-(D13-Pad1)")
  (net 27 /A5)
  (net 28 "Net-(D14-Pad1)")
  (net 29 /A6)
  (net 30 "Net-(D15-Pad1)")
  (net 31 /A7)
  (net 32 "Net-(D16-Pad1)")
  (net 33 /A8)
  (net 34 "Net-(D17-Pad1)")
  (net 35 /A9)
  (net 36 "Net-(D18-Pad1)")
  (net 37 /A10)
  (net 38 "Net-(D19-Pad1)")
  (net 39 /A11)
  (net 40 "Net-(D20-Pad1)")
  (net 41 /A12)
  (net 42 "Net-(D21-Pad1)")
  (net 43 /A13)
  (net 44 "Net-(D22-Pad1)")
  (net 45 /A14)
  (net 46 "Net-(D23-Pad1)")
  (net 47 /A15)
  (net 48 "Net-(D24-Pad1)")
  (net 49 /WR)
  (net 50 "Net-(D25-Pad1)")
  (net 51 /RD)
  (net 52 "Net-(D26-Pad1)")
  (net 53 /CS)
  (net 54 "Net-(D27-Pad1)")
  (net 55 Vsc)
  (net 56 ext_detect)
  (net 57 "Net-(JP2-Pad31)")
  (net 58 GND)
  (net 59 +3V3)
  (net 60 +5V)
  (net 61 SDA)
  (net 62 SCL)
  (net 63 "Net-(P1-Pad7)")
  (net 64 "Net-(P1-Pad8)")
  (net 65 "Net-(P1-Pad9)")
  (net 66 "Net-(P1-Pad10)")
  (net 67 "Net-(P1-Pad11)")
  (net 68 "Net-(P1-Pad12)")
  (net 69 "Net-(P1-Pad13)")
  (net 70 "Net-(P1-Pad14)")
  (net 71 "Net-(P1-Pad15)")
  (net 72 "Net-(P1-Pad16)")
  (net 73 "Net-(P1-Pad17)")
  (net 74 "Net-(P1-Pad18)")
  (net 75 "Net-(P1-Pad19)")
  (net 76 "Net-(P1-Pad20)")
  (net 77 "Net-(P1-Pad21)")
  (net 78 "Net-(P1-Pad22)")
  (net 79 "Net-(P1-Pad23)")
  (net 80 "Net-(P1-Pad24)")
  (net 81 "Net-(P1-Pad25)")
  (net 82 "Net-(P1-Pad26)")
  (net 83 "Net-(P1-Pad27)")
  (net 84 "Net-(P1-Pad28)")
  (net 85 "Net-(P1-Pad29)")
  (net 86 "Net-(P1-Pad30)")
  (net 87 "Net-(P1-Pad31)")
  (net 88 "Net-(P1-Pad32)")
  (net 89 "Net-(P1-Pad33)")
  (net 90 "Net-(P1-Pad34)")
  (net 91 "Net-(P1-Pad35)")
  (net 92 "Net-(P1-Pad36)")
  (net 93 "Net-(P1-Pad37)")
  (net 94 "Net-(P1-Pad38)")
  (net 95 "Net-(P1-Pad39)")
  (net 96 "Net-(P1-Pad40)")
  (net 97 "Net-(U1-Pad19)")
  (net 98 "Net-(U1-Pad20)")
  (net 99 "Net-(U2-Pad4)")
  (net 100 "Net-(U2-Pad5)")
  (net 101 "Net-(U2-Pad6)")
  (net 102 "Net-(U2-Pad7)")
  (net 103 "Net-(U2-Pad8)")
  (net 104 "Net-(U2-Pad19)")
  (net 105 "Net-(U2-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.0762)
    (uvia_drill 0.0254)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /RD)
    (add_net /WR)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D18-Pad1)")
    (add_net "Net-(D19-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D20-Pad1)")
    (add_net "Net-(D21-Pad1)")
    (add_net "Net-(D22-Pad1)")
    (add_net "Net-(D23-Pad1)")
    (add_net "Net-(D24-Pad1)")
    (add_net "Net-(D25-Pad1)")
    (add_net "Net-(D26-Pad1)")
    (add_net "Net-(D27-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(JP2-Pad31)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad17)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad20)")
    (add_net "Net-(P1-Pad21)")
    (add_net "Net-(P1-Pad22)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad25)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad27)")
    (add_net "Net-(P1-Pad28)")
    (add_net "Net-(P1-Pad29)")
    (add_net "Net-(P1-Pad30)")
    (add_net "Net-(P1-Pad31)")
    (add_net "Net-(P1-Pad32)")
    (add_net "Net-(P1-Pad33)")
    (add_net "Net-(P1-Pad34)")
    (add_net "Net-(P1-Pad35)")
    (add_net "Net-(P1-Pad36)")
    (add_net "Net-(P1-Pad37)")
    (add_net "Net-(P1-Pad38)")
    (add_net "Net-(P1-Pad39)")
    (add_net "Net-(P1-Pad40)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net SCL)
    (add_net SDA)
    (add_net ext_detect)
  )
  (net_class power ""
    (clearance 0.1524)
    (trace_width 0.4)
    (via_dia 0.6858)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net Vsc)
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58705AE3)
    (at 107.061 42.164 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value or_Led (at 0 1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /D0))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58705AD8)
    (at 105.029 42.164 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value or_Led (at 0 1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /D1))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58705AD3)
    (at 102.997 42.164 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value or_Led (at 0 1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /D2))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58705AC7)
    (at 100.965 42.164 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value or_Led (at 0 1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /D3))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58705AB8)
    (at 98.933 42.164 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value or_Led (at 0 1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 /D4))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58705AB2)
    (at 96.901 42.164 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value or_Led (at 0 1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /D5))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D6-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58705AA1)
    (at 94.869 42.164 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value or_Led (at 0 1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 /D6))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D7-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58705A9B)
    (at 92.837 42.164 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value or_Led (at 0 1.55 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 /D7))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D8-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58700E3C)
    (at 139.7 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 /A0))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D9-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5876BAFC)
    (at 137.668 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D10 (at 3.435 0.098 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 /A1))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5876BAF3)
    (at 135.636 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D11 (at 3.435 -0.064 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /A2))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D11-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58756900)
    (at 133.604 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D12 (at 3.465 0.304 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /A3))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D12-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58756904)
    (at 131.572 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D13 (at 3.465 -0.028 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 /A4))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58700E57)
    (at 129.54 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D14 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 /A5))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D14-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58700E5C)
    (at 127.508 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D15 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 /A6))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D15-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5875692E)
    (at 125.476 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D16 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.905 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /A7))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D16-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 587019D2)
    (at 123.571 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D17 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 /A8))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D17-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 587019D9)
    (at 121.412 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D18 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /A9))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D18-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 587019E1)
    (at 119.38 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D19 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 /A10))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D19-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 587019E8)
    (at 117.348 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D20 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 /A11))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D20-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 587019F4)
    (at 115.316 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D21 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 /A12))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D21-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 587019F9)
    (at 113.284 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D22 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 /A13))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D22-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 587019FE)
    (at 111.252 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D23 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /A14))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D23-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5875682A)
    (at 109.22 38.735 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D24 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value gn_Led (at 6.365 -1.18 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 /A15))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D24-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5878063C)
    (at 143.475 43.55 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D25 (at -0.035 -1.408 180) (layer F.SilkS))
    (fp_text value rd_Led (at 2.54 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 49 /WR))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D25-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58780630)
    (at 143.5 41.16 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D26 (at -0.137 1.282 180) (layer F.SilkS))
    (fp_text value rd_Led (at 2.54 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 51 /RD))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D26-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58780615)
    (at 143.4 38.5 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D27 (at 0.017 1.416 180) (layer F.SilkS))
    (fp_text value rd_Led (at 1.37 -2.387 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 53 /CS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D27-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x20 (layer B.Cu) (tedit 58741841)
    (at 91.44 29.845)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -2.286 -2.286) (layer F.SilkS))
    (fp_text value CONN_02X20 (at 0 3.1) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 +3V3))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 +5V))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 SDA))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 +5V))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 SCL))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 GND))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at 12.7 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at 17.78 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "Net-(P1-Pad17)"))
    (pad 18 thru_hole oval (at 20.32 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "Net-(P1-Pad18)"))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "Net-(P1-Pad19)"))
    (pad 20 thru_hole oval (at 22.86 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "Net-(P1-Pad20)"))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "Net-(P1-Pad21)"))
    (pad 22 thru_hole oval (at 25.4 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 "Net-(P1-Pad22)"))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 "Net-(P1-Pad23)"))
    (pad 24 thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(P1-Pad24)"))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 "Net-(P1-Pad25)"))
    (pad 26 thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 "Net-(P1-Pad26)"))
    (pad 27 thru_hole oval (at 33.02 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 "Net-(P1-Pad27)"))
    (pad 28 thru_hole oval (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 "Net-(P1-Pad28)"))
    (pad 29 thru_hole oval (at 35.56 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 85 "Net-(P1-Pad29)"))
    (pad 30 thru_hole oval (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 86 "Net-(P1-Pad30)"))
    (pad 31 thru_hole oval (at 38.1 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 "Net-(P1-Pad31)"))
    (pad 32 thru_hole oval (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 88 "Net-(P1-Pad32)"))
    (pad 33 thru_hole oval (at 40.64 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 "Net-(P1-Pad33)"))
    (pad 34 thru_hole oval (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 90 "Net-(P1-Pad34)"))
    (pad 35 thru_hole oval (at 43.18 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 91 "Net-(P1-Pad35)"))
    (pad 36 thru_hole oval (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 92 "Net-(P1-Pad36)"))
    (pad 37 thru_hole oval (at 45.72 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 93 "Net-(P1-Pad37)"))
    (pad 38 thru_hole oval (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 94 "Net-(P1-Pad38)"))
    (pad 39 thru_hole oval (at 48.26 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 95 "Net-(P1-Pad39)"))
    (pad 40 thru_hole oval (at 48.26 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 96 "Net-(P1-Pad40)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x20.wrl
      (at (xyz 0.95 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 58755CDD)
    (at 86.36 32.766)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at -1.76 -2.166 180) (layer F.SilkS))
    (fp_text value "" (at 13.97 -0.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 Vsc))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 587568A1)
    (at 97.7 34.475 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.654 0.061 90) (layer B.SilkS))
    (fp_text value R (at 6.35 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5875689D)
    (at 94.825 34.475 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.554 0.029 90) (layer B.SilkS))
    (fp_text value R (at 6.35 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756899)
    (at 90.425 36.925 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.554 -0.003 180) (layer B.SilkS))
    (fp_text value R (at 6.35 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756893)
    (at 90.45 39.075 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.654 -0.035 180) (layer B.SilkS))
    (fp_text value R (at 6.35 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5875688D)
    (at 86.55 44.15 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.654 -0.067 270) (layer B.SilkS))
    (fp_text value R (at 6.35 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5875688A)
    (at 88.45 44.125 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 2.654 0.001 270) (layer B.SilkS))
    (fp_text value R (at 6.35 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756876)
    (at 90.325 44.15 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 2.554 -0.131 270) (layer B.SilkS))
    (fp_text value R (at -3.446 4.469 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756874)
    (at 92.225 44.15 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 2.654 -0.463 270) (layer B.SilkS))
    (fp_text value R (at -3.646 3.937 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 587566D9)
    (at 142.025 46.1 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 2.425 0 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756785)
    (at 140.275 46.1 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 2.825 -0.232 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 587566EB)
    (at 138.5 46.1 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 2.925 -0.064 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756780)
    (at 136.675 46.025 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 2.825 0.204 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756778)
    (at 132.225 38.75 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 2.825 0.172 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5875676E)
    (at 130.4 38.2 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 2.825 -0.56 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756769)
    (at 136.4 40.15 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 2.825 -0.492 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756937)
    (at 138.3 40.15 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 2.925 -0.024 270) (layer B.SilkS))
    (fp_text value R (at 0 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756708)
    (at 140.175 40.175 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 2.925 -0.056 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 587804A1)
    (at 141.35 36.2 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0.122 1.65 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58756759)
    (at 140.475 32.7)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 2.825 0.28) (layer B.SilkS))
    (fp_text value R (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(D19-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58780577)
    (at 137.9 33.2 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 2.741 -0.022 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D20-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 587804F4)
    (at 135.325 34.775)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at -0.07 1.674) (layer B.SilkS))
    (fp_text value R (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(D21-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5878053C)
    (at 135.325 32.8)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at -2.61 0.093) (layer B.SilkS))
    (fp_text value R (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D22-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5878054F)
    (at 132.125 34.75 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 2.712 -0.175 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(D23-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58780555)
    (at 130.175 32.8 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 2.667 -0.22 180) (layer B.SilkS))
    (fp_text value R (at 2.225 3.32 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(D24-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 587805AD)
    (at 144.7 45.3 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 0.039 -1.477 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 587567D5)
    (at 144.675 40.425 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at -0.217 1.602 270) (layer B.SilkS))
    (fp_text value R (at 0.635 4.445 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(D26-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5878058A)
    (at 144.5 35.675 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at -0.266 -1.371 90) (layer B.SilkS))
    (fp_text value R (at 1.905 1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(D27-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 119.888 38.354)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 6.25) (layer B.SilkS))
    (fp_text value MCP_23017 (at 0 -6.25) (layer B.Fab))
    (pad 1 smd rect (at -3.6 4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 /A8))
    (pad 2 smd rect (at -3.6 3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 35 /A9))
    (pad 3 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 37 /A10))
    (pad 4 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 39 /A11))
    (pad 5 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 41 /A12))
    (pad 6 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 43 /A13))
    (pad 7 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 45 /A14))
    (pad 8 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 47 /A15))
    (pad 9 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 55 Vsc))
    (pad 10 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (pad 11 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 62 SCL))
    (pad 13 smd rect (at -3.6 -3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 61 SDA))
    (pad 14 smd rect (at -3.6 -4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 3.6 -4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (pad 16 smd rect (at 3.6 -3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (pad 17 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (pad 18 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 55 Vsc))
    (pad 19 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 17 /A0))
    (pad 22 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 19 /A1))
    (pad 23 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 21 /A2))
    (pad 24 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 23 /A3))
    (pad 25 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 25 /A4))
    (pad 26 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 27 /A5))
    (pad 27 smd rect (at 3.6 3.575) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 29 /A6))
    (pad 28 smd rect (at 3.6 4.225) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 31 /A7))
    (model Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 104.648 38.354 270)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 6.25 270) (layer B.SilkS))
    (fp_text value MCP_23017 (at 0 -6.25 270) (layer B.Fab))
    (pad 1 smd rect (at -3.6 4.225 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 49 /WR))
    (pad 2 smd rect (at -3.6 3.575 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 51 /RD))
    (pad 3 smd rect (at -3.6 2.925 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 53 /CS))
    (pad 4 smd rect (at -3.6 2.275 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 99 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -3.6 1.625 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 100 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -3.6 0.975 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 101 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -3.6 0.325 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 102 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -3.6 -0.325 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at -3.6 -0.975 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 55 Vsc))
    (pad 10 smd rect (at -3.6 -1.625 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (pad 11 smd rect (at -3.6 -2.275 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -3.6 -2.925 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 62 SCL))
    (pad 13 smd rect (at -3.6 -3.575 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 61 SDA))
    (pad 14 smd rect (at -3.6 -4.225 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 3.6 -4.225 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 55 Vsc))
    (pad 16 smd rect (at 3.6 -3.575 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (pad 17 smd rect (at 3.6 -2.925 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (pad 18 smd rect (at 3.6 -2.275 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 55 Vsc))
    (pad 19 smd rect (at 3.6 -1.625 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 104 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 3.6 -0.975 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 105 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 3.6 -0.325 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 /D0))
    (pad 22 smd rect (at 3.6 0.325 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 /D1))
    (pad 23 smd rect (at 3.6 0.975 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 /D2))
    (pad 24 smd rect (at 3.6 1.625 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 /D3))
    (pad 25 smd rect (at 3.6 2.275 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 9 /D4))
    (pad 26 smd rect (at 3.6 2.925 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 /D5))
    (pad 27 smd rect (at 3.6 3.575 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 /D6))
    (pad 28 smd rect (at 3.6 4.225 270) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 15 /D7))
    (model Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:GB_DS_Cart_Socket (layer F.Cu) (tedit 5875687F)
    (at 115.316 48.006 180)
    (fp_text reference JP2 (at 25.316 2.206 180) (layer F.SilkS))
    (fp_text value GB_CONN (at -22.384 -2.494 180) (layer F.Fab))
    (fp_text user 1 (at -24.5 0.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -23.25 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 55 Vsc))
    (pad 4 smd rect (at -18.75 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 51 /RD))
    (pad 3 smd rect (at -20.25 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 49 /WR))
    (pad 2 smd rect (at -21.75 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 56 ext_detect))
    (pad 7 smd rect (at -14.25 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 19 /A1))
    (pad 6 smd rect (at -15.75 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 17 /A0))
    (pad 5 smd rect (at -17.25 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 53 /CS))
    (pad 10 smd rect (at -9.75 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 25 /A4))
    (pad 9 smd rect (at -11.25 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 23 /A3))
    (pad 8 smd rect (at -12.75 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 21 /A2))
    (pad 13 smd rect (at -5.25 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /A7))
    (pad 12 smd rect (at -6.75 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 29 /A6))
    (pad 11 smd rect (at -8.25 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 27 /A5))
    (pad 15 smd rect (at -2.25 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 35 /A9))
    (pad 14 smd rect (at -3.75 0) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 33 /A8))
    (pad 16 smd rect (at -0.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 37 /A10))
    (pad 17 smd rect (at 0.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 39 /A11))
    (pad 18 smd rect (at 2.25 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 41 /A12))
    (pad 19 smd rect (at 3.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 43 /A13))
    (pad 20 smd rect (at 5.25 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 45 /A14))
    (pad 21 smd rect (at 6.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 47 /A15))
    (pad 22 smd rect (at 8.25 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 1 /D0))
    (pad 23 smd rect (at 9.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /D1))
    (pad 24 smd rect (at 11.25 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 5 /D2))
    (pad 25 smd rect (at 12.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 7 /D3))
    (pad 26 smd rect (at 14.25 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /D4))
    (pad 27 smd rect (at 15.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /D5))
    (pad 28 smd rect (at 17.25 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 13 /D6))
    (pad 29 smd rect (at 18.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 15 /D7))
    (pad 30 smd rect (at 20.25 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 55 Vsc))
    (pad 31 smd rect (at 21.75 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(JP2-Pad31)"))
    (pad 32 smd rect (at 23.25 0 180) (size 0.75 2) (layers F.Cu F.Paste F.Mask)
      (net 58 GND))
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 587803DE)
    (at 112.59 37.26 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.589 0.186 90) (layer B.SilkS))
    (fp_text value C_Small (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 55 Vsc))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 58 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 105.78 37.36 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 58 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 55 Vsc))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GBCartSlurp (at 119.126 49.403) (layer B.Cu))
  (gr_text "D1-D8 Data bus" (at 97.917 39.243) (layer F.SilkS))
  (gr_text "RPi 1 header" (at 118.11 32.004) (layer F.SilkS))
  (gr_text "GBCartSlurp V0.1\nABrugsch" (at 93.472 35.687) (layer F.SilkS))
  (gr_line (start 85.35 53.325) (end 84.75 53.325) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.072 51.423) (end 147.977 51.423) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.35 53.325) (end 85.35 51.525) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.2 53.325) (end 145.2 51.525) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.072 53.325) (end 145.2 53.325) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 144.7 28.6) (end 146.2 28.7) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 86.4 28.6) (end 87.9 28.7) (layer Edge.Cuts) (width 0.15))
  (gr_text "D9-D24\nAddress Bus" (at 136.51 33.41) (layer F.SilkS))
  (gr_text "R1-R8\n150R" (at 94.83 38.29) (layer B.SilkS))
  (gr_line (start 82.85 27.135) (end 82.85 51.423) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.2 51.528) (end 85.355 51.528) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 84.755 51.423) (end 84.755 53.328) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 84.755 27.135) (end 82.85 27.135) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.072 25.23) (end 84.755 25.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.977 51.423) (end 147.977 27.135) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.072 27.135) (end 146.072 25.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 1 (at 89.789 29.845) (layer F.SilkS))
  (gr_text 3.3 (at 90.678 35.179) (layer F.SilkS))
  (gr_text "5\n" (at 87.122 35.306) (layer F.SilkS))
  (zone (net 58) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.98 53.26) (xy 83.1 53.26) (xy 83.1 25.68) (xy 147.98 25.68) (xy 147.98 53.26)
      )
    )
  )
  (zone (net 58) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.98 53.28) (xy 83.1 53.28) (xy 83.1 25.68) (xy 147.98 25.68) (xy 147.98 53.28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.857 51.054) (xy 112.268 51.054) (xy 112.268 48.006) (xy 125.857 48.006) (xy 125.857 51.054)
      )
    )
  )
)
