(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 58)
    (zones 0)
    (modules 15)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad25)")
  (net 2 "Net-(J1-Pad22)")
  (net 3 "Net-(J1-Pad19)")
  (net 4 "Net-(J1-Pad16)")
  (net 5 "Net-(J1-Pad14)")
  (net 6 "Net-(J1-Pad13)")
  (net 7 "Net-(J1-Pad12)")
  (net 8 "Net-(J1-Pad9)")
  (net 9 "Net-(J1-Pad6)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(J6-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J6-Pad2)")
  )
  (module digikey_resistor_RMCF0603ZT0R00:digikey_resistor_RMCF0603ZT0R00 (layer B.Cu) (tedit 0)
    (at 181.6 90.5)
    (fp_text reference R6 (at 0 0) (layer B.SilkS))
    (fp_text value R (at 0 0) (layer B.SilkS))
    (fp_text user 0.027in/0.686mm (at 0 -3.5179) (layer Cmts.User))
    (fp_text user 0.083in/2.108mm (at 0 3.5179) (layer Cmts.User))
    (fp_text user 0.037in/0.94mm (at 3.8989 0) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 0.6985 0) (size 0.7112 0.9398) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad13)"))
    (pad 1 smd rect (at -0.6985 0) (size 0.7112 0.9398) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad12)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 182.3 98)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J8 (at 0 2.25) (layer Cmts.User))
    (fp_text value "Fischer Shield" (at 0.1 -2) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer Cmts.User))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad13)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey_resistor_RMCF0603ZT0R00:digikey_resistor_RMCF0603ZT0R00 (layer F.Cu) (tedit 0)
    (at 145 98 180)
    (fp_text reference R5 (at 0 0) (layer F.SilkS))
    (fp_text value R (at 0 0) (layer F.SilkS))
    (fp_text user 0.027in/0.686mm (at 0 3.5179) (layer Cmts.User))
    (fp_text user 0.083in/2.108mm (at 0 -3.5179) (layer Cmts.User))
    (fp_text user 0.037in/0.94mm (at 3.8989 0) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 0.6985 0 180) (size 0.7112 0.9398) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -0.6985 0 180) (size 0.7112 0.9398) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J6-Pad2)"))
  )
  (module digikey_resistor_RMCF0603ZT0R00:digikey_resistor_RMCF0603ZT0R00 (layer F.Cu) (tedit 0)
    (at 145 101 180)
    (fp_text reference R4 (at 0 0) (layer F.SilkS))
    (fp_text value R (at 0 0) (layer F.SilkS))
    (fp_text user 0.027in/0.686mm (at 0 3.5179) (layer Cmts.User))
    (fp_text user 0.083in/2.108mm (at 0 -3.5179) (layer Cmts.User))
    (fp_text user 0.037in/0.94mm (at 3.8989 0) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 0.6985 0 180) (size 0.7112 0.9398) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad14)"))
    (pad 1 smd rect (at -0.6985 0 180) (size 0.7112 0.9398) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J6-Pad2)"))
  )
  (module digikey_resistor_RMCF0603ZT0R00:digikey_resistor_RMCF0603ZT0R00 (layer B.Cu) (tedit 0)
    (at 152.5 90.5 180)
    (fp_text reference R3 (at 0 0) (layer B.SilkS))
    (fp_text value R (at 0 0) (layer B.SilkS))
    (fp_text user 0.027in/0.686mm (at 0 -3.5179) (layer Cmts.User))
    (fp_text user 0.083in/2.108mm (at 0 3.5179) (layer Cmts.User))
    (fp_text user 0.037in/0.94mm (at 3.8989 0) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 0.6985 0 180) (size 0.7112 0.9398) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -0.6985 0 180) (size 0.7112 0.9398) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad6)"))
  )
  (module digikey_resistor_RMCF0603ZT0R00:digikey_resistor_RMCF0603ZT0R00 (layer B.Cu) (tedit 0)
    (at 162.5 90.5 180)
    (fp_text reference R2 (at 0 0) (layer B.SilkS))
    (fp_text value R (at 0 0) (layer B.SilkS))
    (fp_text user 0.027in/0.686mm (at 0 -3.5179) (layer Cmts.User))
    (fp_text user 0.083in/2.108mm (at 0 3.5179) (layer Cmts.User))
    (fp_text user 0.037in/0.94mm (at 3.8989 0) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 0.6985 0 180) (size 0.7112 0.9398) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad6)"))
    (pad 1 smd rect (at -0.6985 0 180) (size 0.7112 0.9398) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad9)"))
  )
  (module digikey_resistor_RMCF0603ZT0R00:digikey_resistor_RMCF0603ZT0R00 (layer B.Cu) (tedit 0)
    (at 172.1 90.5)
    (fp_text reference R1 (at 0 0) (layer B.SilkS))
    (fp_text value R (at 0 0) (layer B.SilkS))
    (fp_text user 0.027in/0.686mm (at 0 -3.5179) (layer Cmts.User))
    (fp_text user 0.083in/2.108mm (at 0 3.5179) (layer Cmts.User))
    (fp_text user 0.037in/0.94mm (at 3.8989 0) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 0.6985 0) (size 0.7112 0.9398) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad12)"))
    (pad 1 smd rect (at -0.6985 0) (size 0.7112 0.9398) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad9)"))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 172.5 98)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J7 (at 0 2.25) (layer Cmts.User))
    (fp_text value GND (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer Cmts.User))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J6-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey_10pin_1175-1627-ND:digikey_10pin_1175-1627-ND (layer F.Cu) (tedit 0)
    (at 160 99 180)
    (fp_text reference J6 (at 2.54 -0.635) (layer F.SilkS))
    (fp_text value 3220-10-0100-00 (at 2.54 -0.635) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad25)"))
    (pad 2 thru_hole circle (at 0 -1.27 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 11 "Net-(J6-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad22)"))
    (pad 4 thru_hole circle (at 1.27 -1.27 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 11 "Net-(J6-Pad2)"))
    (pad 5 thru_hole circle (at 2.54 0 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad19)"))
    (pad 6 thru_hole circle (at 2.54 -1.27 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 11 "Net-(J6-Pad2)"))
    (pad 7 thru_hole circle (at 3.81 0 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (pad 8 thru_hole circle (at 3.81 -1.27 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 11 "Net-(J6-Pad2)"))
    (pad 9 thru_hole circle (at 5.08 0 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 5.08 -1.27 180) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 148.8 94)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J5 (at 0 2.25) (layer Cmts.User))
    (fp_text value Y+ (at 0 -2.05) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 159 94)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J4 (at 0 2.25) (layer Cmts.User))
    (fp_text value Y- (at 0 -2.05) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer Cmts.User))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad19)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 169 94)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J3 (at 0 2.25) (layer Cmts.User))
    (fp_text value X- (at 0 -2.05) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer Cmts.User))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad22)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 177 94)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J2 (at 0 2.25) (layer Cmts.User))
    (fp_text value X+ (at 0 -2.05) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer Cmts.User))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad25)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey_DSub_NOR1137-ND:digikey_DSub_NOR1137-ND (layer F.Cu) (tedit 0)
    (at 158.44614 75.75)
    (fp_text reference J1 (at 0 0) (layer F.SilkS))
    (fp_text value DB25_Female_MountingHoles (at 0.1 0) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 27 thru_hole circle (at 23.5204 9.4996) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at -23.5204 9.4996) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 15.2273 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad25)"))
    (pad 24 thru_hole circle (at 12.4587 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 9.6901 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 6.9215 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad22)"))
    (pad 21 thru_hole circle (at 4.1529 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 1.3843 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at -1.3843 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad19)"))
    (pad 18 thru_hole circle (at -4.1529 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at -6.9215 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -9.6901 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (pad 15 thru_hole circle (at -12.4587 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -15.2273 8.0772) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad14)"))
    (pad 13 thru_hole circle (at 16.6116 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad13)"))
    (pad 12 thru_hole circle (at 13.843 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad12)"))
    (pad 11 thru_hole circle (at 11.0744 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 8.3058 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 5.5372 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad9)"))
    (pad 8 thru_hole circle (at 2.7686 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -2.7686 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at -5.5372 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -8.3058 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -11.0744 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -13.843 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -16.6116 10.922) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 137.5 95)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer Cmts.User))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 186 79.2) (end 186 82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131 79.2) (end 131 82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131 82) (end 131 103) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186 82) (end 186 103) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186 103) (end 131 103) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131 79.2) (end 186 79.2) (layer Edge.Cuts) (width 0.15))
  (gr_text "FNAL, June 2023" (at 137 102) (layer F.SilkS))
  (gr_text "\nMEMS DB25 to 10 pin\n" (at 185 101) (layer F.SilkS))
)
