(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6002)
    (drawings 60)
    (tracks 53)
    (zones 0)
    (modules 18)
    (nets 40)
  )
  (page A4)
  (title_block
    (date "lun. 30 mars 2015")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.127)
    (pcb_text_size 0.508 0.508)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 110.998 126.365)
    (grid_origin 110.998 126.365)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /IOREF)
  (net 2 /Reset)
  (net 3 +5V)
  (net 4 GND)
  (net 5 /Vin)
  (net 6 /A0)
  (net 7 /A1)
  (net 8 /A2)
  (net 9 /A3)
  (net 10 /AREF)
  (net 11 "/A4(SDA)")
  (net 12 "/A5(SCL)")
  (net 13 "/9(**)")
  (net 14 /8)
  (net 15 /7)
  (net 16 "/6(**)")
  (net 17 "/5(**)")
  (net 18 /4)
  (net 19 "/3(**)")
  (net 20 /2)
  (net 21 "/1(Tx)")
  (net 22 "/0(Rx)")
  (net 23 "Net-(P5-Pad1)")
  (net 24 "Net-(P6-Pad1)")
  (net 25 "Net-(P7-Pad1)")
  (net 26 "Net-(P8-Pad1)")
  (net 27 "/13(SCK)")
  (net 28 "/10(**/SS)")
  (net 29 "Net-(P1-Pad1)")
  (net 30 +3V3)
  (net 31 "/12(MISO)")
  (net 32 "/11(**/MOSI)")
  (net 33 +24V)
  (net 34 /B0_in)
  (net 35 /B1_in)
  (net 36 /B2_in)
  (net 37 /B3_in)
  (net 38 /A5)
  (net 39 /A4)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net "/0(Rx)")
    (add_net "/1(Tx)")
    (add_net "/10(**/SS)")
    (add_net "/11(**/MOSI)")
    (add_net "/12(MISO)")
    (add_net "/13(SCK)")
    (add_net /2)
    (add_net "/3(**)")
    (add_net /4)
    (add_net "/5(**)")
    (add_net "/6(**)")
    (add_net /7)
    (add_net /8)
    (add_net "/9(**)")
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net "/A4(SDA)")
    (add_net /A5)
    (add_net "/A5(SCL)")
    (add_net /AREF)
    (add_net /B0_in)
    (add_net /B1_in)
    (add_net /B2_in)
    (add_net /B3_in)
    (add_net /IOREF)
    (add_net /Reset)
    (add_net /Vin)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P8-Pad1)")
  )
  (net_class 24V ""
    (clearance 0.2)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 5BE25328)
    (at 138.938 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 8.89 -2.54) (layer F.SilkS) hide)
    (fp_text value Power (at 8.89 -4.064) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /IOREF))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Reset))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 +3V3))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /Vin))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x06 locked (layer F.Cu) (tedit 5BE25315)
    (at 161.798 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 6.604 -2.54) (layer F.SilkS) hide)
    (fp_text value Analog (at 6.604 -4.064) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A1))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A2))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A3))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "/A4(SDA)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "/A5(SCL)"))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x06.wrl
      (offset (xyz 6.349999904632568 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x10 locked (layer F.Cu) (tedit 5BE25304)
    (at 129.794 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 11.43 2.794) (layer F.SilkS) hide)
    (fp_text value Digital (at 11.43 4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /A5))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /A4))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /AREF))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "/13(SCK)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "/12(MISO)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "/11(**/MOSI)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "/10(**/SS)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "/9(**)"))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /8))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x10.wrl
      (offset (xyz 11.42999982833862 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 5BE252F1)
    (at 156.718 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 8.89 2.794) (layer F.SilkS) hide)
    (fp_text value Digital (at 8.89 4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /7))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "/6(**)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "/5(**)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /4))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "/3(**)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /2))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "/1(Tx)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "/0(Rx)"))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5524FC39)
    (at 124.968 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P5 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P5-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5524FC4A)
    (at 177.038 118.745)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P6-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5524FC2F)
    (at 126.238 75.565)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P7 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P7-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5524FC41)
    (at 177.038 90.805)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P8 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P8-Pad1)"))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 5BE2540F)
    (at 133.858 86.995)
    (descr "Through hole straight socket strip, 1x09, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x09 2.54mm single row")
    (fp_text reference J4 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value DSub_in_header (at 0 23.09) (layer F.Fab))
    (fp_text user %R (at 0 10.16 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /B0_in))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /B1_in))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /B2_in))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /B3_in))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A1))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A0))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5BE2540A)
    (at 154.178 86.995)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J5 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value Valve_header (at 0 15.47) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /B0_in))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /B1_in))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /B2_in))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /B3_in))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /7))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT (layer F.Cu) (tedit 5B741BB0)
    (at 151.638 112.395)
    (descr "DCDC-Converter, RECOM, RECOM_R-78E-0.5, SIP-3, pitch 2.54mm, package size 11.6x8.5x10.4mm^3, https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf")
    (tags "dc-dc recom buck sip-3 pitch 2.54mm")
    (fp_text reference U1 (at 2.54 -7.56) (layer F.SilkS))
    (fp_text value R-785.0-0.5 (at 2.54 3) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 33 +24V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Vin))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R-78E-0.5_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 117.348 97.155 90)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J1 (at 1.27 -4.37 90) (layer F.SilkS))
    (fp_text value 24V_in (at 1.27 4.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 +24V))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 117.348 117.165 90)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J2 (at 1.27 -4.37 90) (layer F.SilkS))
    (fp_text value motor_pwr (at 1.27 4.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 +24V))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 117.348 107.005 90)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J3 (at 1.27 -4.37 90) (layer F.SilkS))
    (fp_text value valve_pwr (at 1.27 4.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 +24V))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-2_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 170.688 89.535 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /B0_in))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 170.688 93.345 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /B1_in))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 170.688 97.155 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /B2_in))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 170.688 100.965 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /B3_in))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text AREF (at 135.128 78.105 180) (layer F.SilkS))
  (gr_text GND (at 137.668 78.105 180) (layer F.SilkS))
  (gr_text D13 (at 140.208 78.105 180) (layer F.SilkS))
  (gr_text D12 (at 142.748 78.105 180) (layer F.SilkS))
  (gr_text D11 (at 145.288 78.105 180) (layer F.SilkS))
  (gr_text D10 (at 147.828 78.105 180) (layer F.SilkS))
  (gr_text D9 (at 150.368 78.105 180) (layer F.SilkS))
  (gr_text D8 (at 152.908 78.105 180) (layer F.SilkS))
  (gr_text A3 (at 169.418 121.285) (layer F.SilkS))
  (gr_text "D7\nOK\n" (at 156.718 78.105 180) (layer F.SilkS))
  (gr_text "D6\nCS" (at 159.258 78.105 180) (layer F.SilkS))
  (gr_text "D5\nStep" (at 161.798 78.105 180) (layer F.SilkS))
  (gr_text "D4\nDir" (at 164.338 78.105 180) (layer F.SilkS))
  (gr_text D3 (at 166.878 78.105 180) (layer F.SilkS))
  (gr_text "D2\nMOT" (at 169.418 78.105 180) (layer F.SilkS))
  (gr_text "D1\nTX" (at 171.958 78.105 180) (layer F.SilkS))
  (gr_text "D0\nRX" (at 174.498 78.105 180) (layer F.SilkS))
  (gr_text A5 (at 174.498 121.285) (layer F.SilkS))
  (gr_text A4 (at 171.958 121.285) (layer F.SilkS))
  (gr_text A2 (at 166.878 121.285) (layer F.SilkS))
  (gr_text A1 (at 164.338 121.285) (layer F.SilkS))
  (gr_text A0 (at 161.798 121.285) (layer F.SilkS))
  (gr_text 5V (at 149.098 121.285) (layer F.SilkS))
  (gr_text Gnd (at 151.638 121.285) (layer F.SilkS))
  (gr_text Gnd (at 154.178 121.285) (layer F.SilkS))
  (gr_text Vin (at 156.718 121.285) (layer F.SilkS))
  (gr_text "InSituPrep v1\nKY" (at 116.078 81.915 90) (layer F.SilkS))
  (gr_text GND (at 154.178 116.205) (layer F.SilkS))
  (gr_text +24V (at 151.638 108.585) (layer F.SilkS))
  (gr_text +5V (at 156.718 108.585) (layer F.SilkS))
  (gr_text +5V (at 163.068 109.855) (layer F.SilkS))
  (gr_text B1 (at 150.368 92.075) (layer F.SilkS))
  (gr_text GND (at 150.368 86.995) (layer F.SilkS))
  (gr_text B3 (at 150.368 97.155) (layer F.SilkS))
  (gr_text "OK\n" (at 150.368 99.695) (layer F.SilkS))
  (gr_text B0 (at 150.368 89.535) (layer F.SilkS))
  (gr_text B2 (at 150.368 94.615) (layer F.SilkS))
  (gr_text Valve (at 154.178 83.185) (layer F.SilkS))
  (gr_text "Panel DSUB" (at 133.858 83.185) (layer F.SilkS))
  (gr_text A0 (at 130.048 107.315) (layer F.SilkS))
  (gr_text A1 (at 130.048 104.775) (layer F.SilkS))
  (gr_text A2 (at 130.048 102.235) (layer F.SilkS))
  (gr_text "MOT\n" (at 130.048 99.695) (layer F.SilkS))
  (gr_text B3 (at 130.048 97.155) (layer F.SilkS))
  (gr_text B2 (at 130.048 94.615) (layer F.SilkS))
  (gr_text B1 (at 130.048 92.075) (layer F.SilkS))
  (gr_text B0 (at 130.048 89.535) (layer F.SilkS))
  (gr_text GND (at 130.048 86.995) (layer F.SilkS))
  (gr_text + (at 112.268 93.345) (layer F.SilkS))
  (gr_text + (at 112.268 103.505) (layer F.SilkS))
  (gr_text + (at 112.268 113.665) (layer F.SilkS))
  (gr_line (start 177.038 74.549) (end 175.514 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 85.979) (end 177.038 74.549) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 88.519) (end 177.038 85.979) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 121.285) (end 179.578 88.519) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 123.825) (end 179.578 121.285) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 126.365) (end 177.038 123.825) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.998 126.365) (end 177.038 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.998 73.025) (end 110.998 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.514 73.025) (end 110.998 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.998 126.365) (xy 177.038 126.365) (xy 177.038 74.295) (xy 110.998 74.295)
      )
    )
  )
)
