(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 41.324999 30.124999 199.475001 162.275001)
    (thickness 1.6)
    (drawings 504)
    (tracks 11928)
    (zones 0)
    (modules 1056)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.15)
    (user_trace_width 0.15)
    (user_trace_width 0.15)
    (user_trace_width 0.15)
    (trace_clearance 0.15)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.15)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.125)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 41.43 30.22)
    (grid_origin 43.5 75.5)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory export/v1.1/gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C201-Pad2)")
  (net 3 "Net-(C202-Pad2)")
  (net 4 +3V3)
  (net 5 +5V)
  (net 6 "Net-(D601-Pad2)")
  (net 7 /LEDs/LED1)
  (net 8 "Net-(D602-Pad2)")
  (net 9 /LEDs/LED2)
  (net 10 "Net-(D603-Pad2)")
  (net 11 /Connectors/USB_DM)
  (net 12 /Connectors/USB_DP)
  (net 13 "Net-(R201-Pad2)")
  (net 14 "Net-(R202-Pad1)")
  (net 15 /CAN/CAN_S)
  (net 16 /CAN/CAN_H)
  (net 17 /CAN/CAN_L)
  (net 18 /Connectors/NRST)
  (net 19 "Net-(U201-Pad25)")
  (net 20 "Net-(U201-Pad26)")
  (net 21 "Net-(U201-Pad27)")
  (net 22 "Net-(U201-Pad28)")
  (net 23 "Net-(U201-Pad30)")
  (net 24 "Net-(U201-Pad31)")
  (net 25 /Connectors/SWDIO)
  (net 26 /Connectors/SWCLK)
  (net 27 /MCU/CAN_RX)
  (net 28 /MCU/CAN_TX)
  (net 29 /MCU/BOOT0)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /CAN/CAN_H)
    (add_net /CAN/CAN_L)
    (add_net /CAN/CAN_S)
    (add_net /Connectors/NRST)
    (add_net /Connectors/SWCLK)
    (add_net /Connectors/SWDIO)
    (add_net /Connectors/USB_DM)
    (add_net /Connectors/USB_DP)
    (add_net /LEDs/LED1)
    (add_net /LEDs/LED2)
    (add_net /MCU/BOOT0)
    (add_net /MCU/CAN_RX)
    (add_net /MCU/CAN_TX)
    (add_net GND)
    (add_net "Net-(C201-Pad2)")
    (add_net "Net-(C202-Pad2)")
    (add_net "Net-(D601-Pad2)")
    (add_net "Net-(D602-Pad2)")
    (add_net "Net-(D603-Pad2)")
    (add_net "Net-(R201-Pad2)")
    (add_net "Net-(R202-Pad1)")
    (add_net "Net-(U201-Pad25)")
    (add_net "Net-(U201-Pad26)")
    (add_net "Net-(U201-Pad27)")
    (add_net "Net-(U201-Pad28)")
    (add_net "Net-(U201-Pad30)")
    (add_net "Net-(U201-Pad31)")
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 132.7 159.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 131.7 153.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 135.2 159.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 134.2 153.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 134.2 150.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 135.2 136.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 132.7 136.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 134.2 130.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 134.2 125.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 131.7 125.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 131.7 130.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 134.2 127.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 131.7 127.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 124.5 100.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 131.7 102.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 128.35 100.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 134.2 102.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 128.35 123.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 124.5 123.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 135.2 114.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 132.7 114.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 124.5 145.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 134.2 147.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 131.7 150.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 128.35 145.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 131.7 147.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 131.7 108.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 134.2 108.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 134.2 105.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 131.7 105.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 51.5 147.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 48.15 145.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 54 147.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 44.3 145.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 51.5 150.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 51.5 125.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 54 125.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 44.3 123.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 54 127.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 51.5 127.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 48.15 123.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 51.5 102.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 48.15 100.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 44.3 100.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 54 102.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 51.5 130.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 52.5 136.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 54 130.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 55 136.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 55 114.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 54 108.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 51.5 108.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 51.5 105.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 52.5 114.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 54 105.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 55 159.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 54 153.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 52.5 159.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 51.5 153.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 54 150.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 172.8 159.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 174.3 153.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 175.3 159.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 171.8 153.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 174.3 150.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 168.45 145.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 164.6 145.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 171.8 150.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 171.8 147.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 174.3 147.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 174.3 108.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 171.8 108.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 174.3 105.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 171.8 105.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 168.45 123.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 164.6 123.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 175.3 114.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 172.8 114.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 164.6 100.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 168.45 100.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 174.3 102.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 171.8 102.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 175.3 136.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 172.8 136.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 174.3 130.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 171.8 130.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 171.8 125.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 174.3 127.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 174.3 125.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 171.8 127.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 94.1 147.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 91.6 147.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 88.25 145.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 84.4 145.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 91.6 150.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 92.6 136.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 95.1 136.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 91.6 130.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 94.1 130.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 94.1 127.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 84.4 100.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 88.25 100.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 91.6 105.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 91.6 102.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 94.1 102.9)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 94.1 105.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 91.6 153.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 92.6 159.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 95.1 159.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 94.1 150.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 94.1 153.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 91.6 108.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 95.1 114.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 92.6 114.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 94.1 108.4)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 91.6 125.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 88.25 123.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 84.4 123.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 94.1 125.3)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 91.6 127.8)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 177.45 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 185.2 150.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 177.65 152.4 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 185.2 151.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 196.8 160.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 199.3 152.2 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 191.95 152.7 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 194.3 160.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 192.7 160.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 191.95 149.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 182.25 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 196.3 143.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 196.8 138)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 191.95 145.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 187.35 146.2 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 194.3 138.05 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 177.9 160.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 176.1 160.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 174.5 160.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 181.4 159.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 179.65 160.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 185.2 154.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 188.85 152.45 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 183.15 160.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 188.1 159)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 185.2 153.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 145.1 151.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 145.1 154.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 145.1 150.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 145.1 153.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 142.15 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 147.25 146.2 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 148.75 152.45 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 163.8 144.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 171.25 157.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 172.9 138 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 172.7 145 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 151.85 152.7 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 152.6 160.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 148 159)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 151.85 149.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 151.85 145.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 167.3 152.2)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 156.7 160.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 172.9 160.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 154.2 160.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 159.2 152.2 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 165.5 160.2 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 134.15 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 140.55 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 135.8 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 137.35 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 138.95 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 132.6 145 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 139.55 160.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 141.3 159.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 143.05 160.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 137.8 160.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 137.55 152.4 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 131.15 157.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 132.8 160.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 136 160.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 134.4 160.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 139.55 137.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 141.3 137.5 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 137.8 137.7 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 143.05 137.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 151.85 100.8 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 151.85 104.45 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 147.25 101.4 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 151.85 107.9 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 137.55 107.6 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 138.95 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 142.15 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 140.55 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 135.8 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 137.35 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 132.6 100.2 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 134.15 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 145.1 109.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 145.1 105.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 145.1 108.4 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 145.1 106.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 148.75 107.65 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 148 114.2)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 143.05 115.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 137.8 115.3 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 141.3 115.1 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 139.55 115.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 132.8 115.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 131.15 112.45 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 134.4 115.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 136 115.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 180.65 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 179.05 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 175.9 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 174.25 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 183.15 137.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 179.65 137.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 176.1 138 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 174.5 138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 177.9 137.7 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 185.2 132.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 185.2 130.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 185.2 129.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 185.2 127.7)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 177.65 130 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 199.3 129.8 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 181.4 137.5 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 188.1 136.6)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 188.85 130.05 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 191.95 130.3 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 191.95 126.85 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 192.7 137.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 151.85 126.85 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 151.85 123.2 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 147.25 123.8 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 148.75 130.05 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 135.8 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 132.6 122.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 134.15 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 137.35 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 148 136.6)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 156.7 138)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 154.2 138.05 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 152.6 137.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 151.85 130.3 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 156.2 143.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 171.25 134.85 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 165.5 137.8 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 152.6 115.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 167.3 129.8)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 159.2 129.8 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 165.5 115.4 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 171.25 112.45 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 142.15 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 137.55 130 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 140.55 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 138.95 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 145.1 127.7)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 145.1 130.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 145.1 129.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 145.1 132.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 131.15 134.85 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 134.4 138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 136 138 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 132.8 138 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 196.3 121.3)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 199.3 107.4 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 194.3 115.65 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 191.95 107.9 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 196.8 115.6)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 196.3 98.9)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 191.95 100.8 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 187.35 101.4 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 191.95 104.45 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 185.2 109.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 185.2 108.4 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 185.2 106.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 185.2 105.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 188.85 107.65 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 191.95 123.2 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 188.1 114.2)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 187.35 123.8 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 192.7 115.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 182.25 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 179.05 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 174.25 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 172.7 122.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 175.9 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 177.45 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 180.65 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 182.25 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 180.65 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 181.4 115.1 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 177.65 107.6 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 177.9 115.3 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 179.05 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 175.9 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 172.7 100.2 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 177.45 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 174.25 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 167.3 107.4)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 163.8 99.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 159.2 107.4 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 156.2 98.9)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 174.5 115.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 176.1 115.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 172.9 115.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 179.65 115.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 183.15 115.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 156.2 121.3)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 163.8 121.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 154.2 115.65 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 156.7 115.6)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 72.4 160.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 71.65 152.7 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 67.8 159)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 74 160.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 71.65 149.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 64.9 153.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 64.9 154.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 68.55 152.45 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 64.9 150.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 64.9 151.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 53.95 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 50.95 157.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 52.4 145 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 45.2 160.2 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 47 152.2)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 52.6 160.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 59.35 160.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 55.8 160.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 62.85 160.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 61.1 159.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 57.6 160.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 57.35 152.4 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 54.2 160.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 60.35 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 57.15 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 61.1 137.5 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 62.85 137.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 71.65 145.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 74 138.05 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 72.4 137.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 67.05 146.2 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 67.8 136.6)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 95.7 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 94.05 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 98.85 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 102.05 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 100.45 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 97.25 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 94.3 138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 97.7 137.7 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 102.95 137.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 95.9 138 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 101.2 137.5 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 99.45 137.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 76 143.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 76.5 138)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 87.1 129.8)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 85.3 137.8 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 79 129.8 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 92.7 138 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 92.5 122.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 91.05 134.85 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 97.45 130 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 105 127.7)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 105 129.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 105 130.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 105 132.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 102.95 115.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 99.45 115.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 95.9 115.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 94.3 115.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 97.7 115.3 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 92.7 115.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 57.35 107.6 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 53.95 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 52.4 100.2 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 55.6 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 52.4 122.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 43.5 121.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 47 107.4)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 45.2 115.4 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 50.95 112.45 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 43.5 99.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 53.95 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 61.95 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 55.6 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 58.75 122.45 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 57.15 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 60.35 122.55 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 61.1 115.1 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 59.35 115.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 57.6 115.3 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 52.6 115.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 55.8 115.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 54.2 115.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 102.05 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 100.45 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 101.2 115.1 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 97.45 107.6 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 98.85 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 94.05 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 92.5 100.2 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 95.7 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 97.25 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 83.6 121.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 76 121.3)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 76.5 115.6)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 85.3 115.4 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 72.4 115.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 74 115.65 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 58.75 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 57.15 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 60.35 100.15 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 61.95 100.05 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 62.85 115.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 64.9 109.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 67.8 114.2)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 71.65 107.9 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 68.55 107.65 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 64.9 108.4 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 64.9 106.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 64.9 105.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 91.05 112.45 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 87.1 107.4)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 83.6 99.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 79 107.4 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 71.65 104.45 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 76 98.9)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 67.05 101.4 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 71.65 100.8 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 105 151.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 105 150.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 107.15 146.2 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 111.75 149.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 111.75 145.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 108.65 152.45 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 105 154.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 105 153.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 111.75 152.7 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 112.5 160.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 107.9 159)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 79 152.2 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 76.5 160.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 91.05 157.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 83.6 144.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 85.3 160.2 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 87.1 152.2)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 92.5 145 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 114.1 160.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 125.4 160.2 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 123.7 144.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 127.2 152.2)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 116.6 160.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 119.1 152.2 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 95.7 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 94.05 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 98.85 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 100.45 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 97.25 144.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 102.05 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 102.95 160.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 94.3 160.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 97.7 160.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 97.45 152.4 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 101.2 159.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 92.7 160.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 99.45 160.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 95.9 160.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 59.35 137.85 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 57.35 130 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 64.9 130.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 64.9 132.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 64.9 129.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 64.9 127.7)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 71.65 130.3 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 71.65 126.85 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 68.55 130.05 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 67.05 123.8 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 71.65 123.2 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 43.5 144.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 52.6 138 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 47 129.8)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 45.2 137.8 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 50.95 134.85 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 55.6 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 58.75 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 55.8 138 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 61.95 144.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 57.6 137.7 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 54.2 138 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 111.75 126.85 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 111.75 130.3 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 111.75 123.2 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 108.65 130.05 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 107.15 123.8 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 116.1 143.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 125.4 137.8 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 127.2 129.8)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 119.1 129.8 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 116.6 138)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 116.6 115.6)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 125.4 115.4 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 123.7 99.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 119.1 107.4 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 127.2 107.4)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 114.1 115.65 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 116.1 98.9)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 111.75 100.8 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 111.75 104.45 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 107.15 101.4 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 105 106.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 105 109.95 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 105 108.4 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 108.65 107.65 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 111.75 107.9 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 107.9 114.2)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 105 105.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 112.5 115.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 114.1 138.05 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 116.1 121.3)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 107.9 136.6)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 112.5 137.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 123.7 121.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 174.3 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 171.8 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 168.45 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 164.6 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 171.8 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 132.7 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 134.2 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 135.2 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 131.7 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 175.3 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 171.8 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 172.8 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 174.3 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 174.3 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 88.25 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 94.1 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 91.6 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 84.4 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 52.5 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 55 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 54 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 51.5 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 54 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 94.1 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 91.6 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 92.6 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 94.1 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 91.6 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 95.1 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 131.7 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 124.5 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 134.2 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 134.2 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 128.35 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 131.7 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 44.3 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 48.15 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 54 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 51.5 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 51.5 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 132.8 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 134.4 93.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 136 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 139.55 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 137.8 92.9 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 137.35 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 138.95 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 134.15 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 132.6 77.8 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 135.8 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 148.75 85.25 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 151.85 85.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 147.25 79 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 151.85 78.4 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 151.85 82.05 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 152.6 93.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 145.1 87.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 143.05 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 148 91.8)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 141.3 92.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 137.55 85.2 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 140.55 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 142.15 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 145.1 84.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 145.1 82.9)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 145.1 86 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 116.6 93.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 125.4 93 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 127.2 85)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 131.15 90.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 123.7 77)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 119.1 85 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 107.15 79 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 114.1 93.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 111.75 78.4 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 111.75 82.05 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 116.1 76.5)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 112.5 93.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 111.75 85.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 108.65 85.25 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 107.9 91.8)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 105 82.9)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 105 86 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 105 87.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 105 84.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 101.2 92.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 102.95 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 94.3 93.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 92.7 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 99.45 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 95.9 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 97.45 85.2 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 97.7 92.9 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 98.85 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 97.25 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 100.45 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 92.5 77.8 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 94.05 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 102.05 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 95.7 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 191.95 82.05 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 185.2 82.9)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 187.35 79 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 191.95 78.4 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 185.2 84.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 185.2 87.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 188.85 85.25 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 188.1 91.8)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 191.95 85.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 185.2 86 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 172.9 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 183.15 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 177.9 92.9 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 181.4 92.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 179.65 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 176.1 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 174.5 93.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 167.3 85)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 156.7 93.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 154.2 93.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 165.5 93 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 171.25 90.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 156.2 76.5)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 163.8 77)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 159.2 85 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 177.65 85.2 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 180.65 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 179.05 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 172.7 77.8 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 182.25 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 177.45 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 175.9 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 174.25 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 196.8 93.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 199.3 85 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 196.3 76.5)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 192.7 93.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 194.3 93.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 83.6 77)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 79 85 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 87.1 85)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 91.05 90.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 74 93.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 76.5 93.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 85.3 93 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 64.9 84.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 64.9 82.9)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 68.55 85.25 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 71.65 85.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 62.85 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 72.4 93.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 64.9 86 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 67.8 91.8)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 64.9 87.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 71.65 78.4 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 71.65 82.05 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 76 76.5)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 67.05 79 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 53.95 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 55.6 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 57.35 85.2 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 52.4 77.8 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 57.6 92.9 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 61.1 92.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 54.2 93.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 55.8 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 59.35 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 61.95 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 58.75 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 60.35 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 57.15 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 45.2 93 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 52.6 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 43.5 77)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 50.95 90.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 47 85)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 174.3 58.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 171.8 58.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 168.45 56.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 164.6 56.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 171.8 60.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 132.7 69.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 134.2 63.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 135.2 69.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 131.7 63.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 175.3 69.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 171.8 63.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 172.8 69.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 174.3 63.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 174.3 60.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 88.25 56.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 94.1 63.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 91.6 63.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 84.4 56.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 52.5 69.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 55 69.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 54 63.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 51.5 63.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 54 60.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 94.1 60.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 91.6 58.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 92.6 69.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 94.1 58.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 91.6 60.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 95.1 69.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 131.7 60.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 124.5 56.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 134.2 60.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 134.2 58.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 128.35 56.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 131.7 58.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 44.3 56.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 48.15 56.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 54 58.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 51.5 58.1)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 51.5 60.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 132.8 70.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 134.4 70.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 136 70.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 139.55 70.65 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 137.8 70.5 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 137.35 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 138.95 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 134.15 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 132.6 55.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 135.8 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 148.75 62.85 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 151.85 63.1 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 147.25 56.6 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 151.85 56 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 151.85 59.65 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 152.6 70.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 145.1 65.15 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 143.05 70.65 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 148 69.4)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 141.3 70.3 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 137.55 62.8 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 140.55 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 142.15 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 145.1 62.05)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 145.1 60.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 145.1 63.6 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 116.6 70.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 125.4 70.6 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 127.2 62.6)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 131.15 67.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 123.7 54.6)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 119.1 62.6 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 107.15 56.6 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 114.1 70.85 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 111.75 56 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 111.75 59.65 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 116.1 54.1)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 112.5 70.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 111.75 63.1 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 108.65 62.85 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 107.9 69.4)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 105 60.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 105 63.6 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 105 65.15 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 105 62.05)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 101.2 70.3 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 102.95 70.65 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 94.3 70.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 92.7 70.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 99.45 70.65 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 95.9 70.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 97.45 62.8 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 97.7 70.5 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 98.85 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 97.25 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 100.45 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 92.5 55.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 94.05 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 102.05 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 95.7 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 191.95 59.65 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 185.2 60.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 187.35 56.6 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 191.95 56 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 185.2 62.05)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 185.2 65.15 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 188.85 62.85 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 188.1 69.4)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 191.95 63.1 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 185.2 63.6 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 172.9 70.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 183.15 70.65 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 177.9 70.5 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 181.4 70.3 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 179.65 70.65 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 176.1 70.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 174.5 70.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 167.3 62.6)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 156.7 70.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 154.2 70.85 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 165.5 70.6 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 171.25 67.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 156.2 54.1)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 163.8 54.6)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 159.2 62.6 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 177.65 62.8 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 180.65 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 179.05 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 172.7 55.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 182.25 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 177.45 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 175.9 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 174.25 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 196.8 70.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 199.3 62.6 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 196.3 54.1)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 192.7 70.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 194.3 70.85 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 83.6 54.6)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 79 62.6 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 87.1 62.6)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 91.05 67.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 74 70.85 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 76.5 70.8)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 85.3 70.6 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 64.9 62.05)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 64.9 60.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 68.55 62.85 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 71.65 63.1 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 62.85 70.65 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 72.4 70.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 64.9 63.6 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 67.8 69.4)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 64.9 65.15 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 71.65 56 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 71.65 59.65 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 76 54.1)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 67.05 56.6 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 53.95 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 55.6 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 57.35 62.8 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 52.4 55.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 57.6 70.5 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 61.1 70.3 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 54.2 70.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 55.8 70.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 59.35 70.65 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 61.95 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 58.75 55.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 60.35 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 57.15 55.35 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 45.2 70.6 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 52.6 70.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 43.5 54.6)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 50.95 67.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 47 62.6)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 175.3 47.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 172.8 47.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 174.3 41.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 171.8 41.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 171.8 38.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 174.3 38.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 171.8 35.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 174.3 35.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 168.45 33.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 164.6 33.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 179.65 48.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 174.5 48.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 177.9 48.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 176.1 48.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 181.4 47.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 187.35 34.2 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 185.2 42.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 188.85 40.45 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 185.2 39.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 185.2 38.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 185.2 41.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 188.1 47)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 183.15 48.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 177.45 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 177.65 40.4 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 175.9 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 179.05 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 180.65 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 174.25 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 182.25 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 196.3 31.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 191.95 33.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 191.95 40.7 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 191.95 37.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 196.8 48.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 199.3 40.2 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 194.3 48.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 192.7 48.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 163.8 32.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 165.5 48.2 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 171.25 45.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 172.9 48.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 167.3 40.2)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 172.7 33 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 135.2 47.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 132.7 47.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 134.2 41.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 131.7 41.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 131.7 38.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 134.2 38.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 131.7 35.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 134.2 35.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 128.35 33.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 124.5 33.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 139.55 48.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 134.4 48.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 137.8 48.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 136 48.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 141.3 47.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 147.25 34.2 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 145.1 42.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 148.75 40.45 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 145.1 39.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 145.1 38.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 145.1 41.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 148 47)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 143.05 48.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 137.35 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 137.55 40.4 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 135.8 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 138.95 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 140.55 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 134.15 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 142.15 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 156.2 31.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 151.85 33.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 151.85 40.7 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 151.85 37.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 156.7 48.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 159.2 40.2 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 154.2 48.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 152.6 48.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 123.7 32.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 125.4 48.2 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 131.15 45.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 132.8 48.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 127.2 40.2)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 132.6 33 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 95.1 47.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 92.6 47.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 94.1 41.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 91.6 41.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 91.6 38.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 94.1 38.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 91.6 35.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 94.1 35.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 88.25 33.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 84.4 33.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 99.45 48.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 94.3 48.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 97.7 48.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 95.9 48.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 101.2 47.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 107.15 34.2 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 105 42.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 108.65 40.45 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 105 39.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 105 38.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 105 41.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 107.9 47)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 102.95 48.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 97.25 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 97.45 40.4 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 95.7 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 98.85 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 100.45 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 94.05 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 102.05 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 116.1 31.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 111.75 33.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 111.75 40.7 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 111.75 37.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 116.6 48.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 119.1 40.2 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 114.1 48.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 112.5 48.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 83.6 32.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 85.3 48.2 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 91.05 45.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 92.7 48.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 87.1 40.2)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 92.5 33 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57228F43)
    (at 68.55 40.45 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at -0.05 0.1 180) (layer F.SilkS) hide)
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57228F63)
    (at 57.35 40.4 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at -0.1 0.5 180) (layer F.SilkS) hide)
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F3A)
    (at 74 48.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at -0.1 1.15 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228ED7)
    (at 59.35 48.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F37)
    (at 72.4 48.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.85 -0.25 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228ED0)
    (at 57.6 48.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 -2.1 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 57228EEC)
    (at 47 40.2)
    (fp_text reference P501 (at -3.7 -6.6) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F55)
    (at 64.9 42.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 1.175 1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F58)
    (at 64.9 41.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0.55 -1.125 180) (layer F.SilkS) hide)
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4F)
    (at 64.9 38.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at -0.05 -1.05) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228EC7)
    (at 50.95 45.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 1.6 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F00)
    (at 52.4 33 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 2.425 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228EDB)
    (at 61.1 47.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0.7 1.2 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2F)
    (at 71.65 37.25 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0.05 -1.4 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -4 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57228F2C)
    (at 71.65 33.6 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 2 -0.05 360) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F5F)
    (at 62.85 48.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -1.8 0 360) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F10)
    (at 60.35 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at -1.75 0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F0A)
    (at 57.15 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at -1.75 0.025 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57228F05)
    (at 53.95 32.95 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at -1.75 -0.05 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECA)
    (at 52.6 48.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at -1.6 -0.05 180) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ECC)
    (at 54.2 48.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 1.6 0 360) (layer F.SilkS) hide)
    (fp_text value 4K7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228ED3)
    (at 55.8 48.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 1.65 -0.275 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F14)
    (at 61.95 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 1.65 0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F0D)
    (at 58.75 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 1.65 0 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57228F08)
    (at 55.6 32.85 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 1.65 -0.1 360) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 57228F23)
    (at 67.05 34.2 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 -3.1 90) (layer F.SilkS) hide)
    (fp_text value MCP1754ST-3302E/MB (at -0.20066 4.59994 90) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57228F5C)
    (at 67.8 47)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 45.2 48.2 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 51.5 41.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 54 41.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228EF4)
    (at 43.5 32.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F3D)
    (at 76.5 48.4)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 57228F70)
    (at 76 31.7)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57228F4C)
    (at 64.9 39.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 52.5 47.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 55 47.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 54 35.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 51.5 35.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 51.5 38.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 54 38.2)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 48.15 33.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 44.3 33.7)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57228F33)
    (at 71.65 40.7 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 -2.1 270) (layer F.SilkS) hide)
    (fp_text value dnp (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57232346)
    (at 79 40.2 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 -8.382 270) (layer F.SilkS) hide)
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab))
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (gr_text RX (at 100.45 120.7) (layer F.SilkS))
  (gr_text T (at 111.8 107.9 90) (layer F.SilkS))
  (gr_text TX (at 97.25 98.3) (layer F.SilkS))
  (gr_text RX (at 100.45 98.3) (layer F.SilkS))
  (gr_text PWR (at 94.1 98.3) (layer F.SilkS))
  (gr_text B (at 97.7 115.3 90) (layer F.SilkS))
  (gr_text TX (at 97.25 120.7) (layer F.SilkS))
  (gr_text PWR (at 94.1 120.7) (layer F.SilkS))
  (gr_text PWR (at 94.1 143.1) (layer F.SilkS))
  (gr_text B (at 97.7 137.7 90) (layer F.SilkS))
  (gr_text TX (at 97.25 143.1) (layer F.SilkS))
  (gr_text T (at 111.8 130.3 90) (layer F.SilkS))
  (gr_text T (at 111.8 152.7 90) (layer F.SilkS))
  (gr_text RX (at 100.45 143.1) (layer F.SilkS))
  (gr_text B (at 97.7 160.1 90) (layer F.SilkS))
  (gr_text T (at 151.9 107.9 90) (layer F.SilkS))
  (gr_text RX (at 140.55 98.3) (layer F.SilkS))
  (gr_text PWR (at 134.2 98.3) (layer F.SilkS))
  (gr_text TX (at 137.35 98.3) (layer F.SilkS))
  (gr_text B (at 137.8 115.3 90) (layer F.SilkS))
  (gr_text T (at 71.7 152.7 90) (layer F.SilkS))
  (gr_text RX (at 60.35 143.1) (layer F.SilkS))
  (gr_text PWR (at 54 143.1) (layer F.SilkS))
  (gr_text TX (at 57.15 143.1) (layer F.SilkS))
  (gr_text B (at 57.6 137.7 90) (layer F.SilkS))
  (gr_text T (at 71.7 130.3 90) (layer F.SilkS))
  (gr_text RX (at 60.35 120.7) (layer F.SilkS))
  (gr_text TX (at 57.15 120.7) (layer F.SilkS))
  (gr_text PWR (at 54 120.7) (layer F.SilkS))
  (gr_text B (at 57.6 160.1 90) (layer F.SilkS))
  (gr_text B (at 177.9 160.1 90) (layer F.SilkS))
  (gr_text RX (at 180.65 143.1) (layer F.SilkS))
  (gr_text T (at 192 152.7 90) (layer F.SilkS))
  (gr_text T (at 192 130.3 90) (layer F.SilkS))
  (gr_text PWR (at 174.3 143.1) (layer F.SilkS))
  (gr_text TX (at 177.45 143.1) (layer F.SilkS))
  (gr_text B (at 177.9 137.7 90) (layer F.SilkS))
  (gr_text T (at 192 107.9 90) (layer F.SilkS))
  (gr_text PWR (at 174.3 98.3) (layer F.SilkS))
  (gr_text RX (at 180.65 98.3) (layer F.SilkS))
  (gr_text TX (at 177.45 98.3) (layer F.SilkS))
  (gr_text B (at 177.9 115.3 90) (layer F.SilkS))
  (gr_text RX (at 180.65 120.7) (layer F.SilkS))
  (gr_text TX (at 177.45 120.7) (layer F.SilkS))
  (gr_text PWR (at 174.3 120.7) (layer F.SilkS))
  (gr_text PWR (at 54 98.3) (layer F.SilkS))
  (gr_text TX (at 57.15 98.3) (layer F.SilkS))
  (gr_text B (at 57.6 115.3 90) (layer F.SilkS))
  (gr_text T (at 71.7 107.9 90) (layer F.SilkS))
  (gr_text RX (at 60.35 98.3) (layer F.SilkS))
  (gr_text TX (at 137.35 143.1) (layer F.SilkS))
  (gr_text PWR (at 134.2 143.1) (layer F.SilkS))
  (gr_text RX (at 140.55 143.1) (layer F.SilkS))
  (gr_text TX (at 137.35 120.7) (layer F.SilkS))
  (gr_text PWR (at 134.2 120.7) (layer F.SilkS))
  (gr_text T (at 151.9 130.3 90) (layer F.SilkS))
  (gr_text B (at 137.8 160.1 90) (layer F.SilkS))
  (gr_text RX (at 140.55 120.7) (layer F.SilkS))
  (gr_text B (at 137.8 137.7 90) (layer F.SilkS))
  (gr_text T (at 151.9 152.7 90) (layer F.SilkS))
  (gr_arc (start 166.5 149.1) (end 166.5 148.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 148.3) (end 166.5 148.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 155.3) (end 167.3 155.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 156.1) (end 166.5 156.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.3 149.1) (end 167.3 155.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 162.2) (end 161.7 156.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 142.2) (end 161.7 148.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 162.2) (end 161.7 162.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 142.2) (end 199.4 162.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 142.2) (end 199.4 142.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 139.8) (end 161.7 139.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 119.8) (end 161.7 125.9) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 132.9) (end 167.3 132.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 126.7) (end 166.5 125.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 125.9) (end 166.5 125.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 119.8) (end 199.4 119.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 103.5) (end 166.5 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 104.3) (end 166.5 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 117.4) (end 161.7 117.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 97.4) (end 199.4 117.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 97.4) (end 161.7 103.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 97.4) (end 199.4 97.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 119.8) (end 199.4 139.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 133.7) (end 166.5 133.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 139.8) (end 161.7 133.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.3 126.7) (end 167.3 132.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.3 104.3) (end 167.3 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 111.3) (end 166.5 111.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 117.4) (end 161.7 111.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 110.5) (end 167.3 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 149.1) (end 46.2 148.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 155.3) (end 47 155.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 148.3) (end 46.2 148.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 142.2) (end 41.4 148.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 156.1) (end 46.2 156.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 142.2) (end 79.1 162.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47 149.1) (end 47 155.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 142.2) (end 79.1 142.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 162.2) (end 41.4 162.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 162.2) (end 41.4 156.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 133.7) (end 46.2 133.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 132.9) (end 47 132.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 139.8) (end 41.4 133.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 126.7) (end 46.2 125.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 119.8) (end 79.1 139.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 139.8) (end 41.4 139.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 119.8) (end 79.1 119.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47 126.7) (end 47 132.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47 104.3) (end 47 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 97.4) (end 41.4 103.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 104.3) (end 46.2 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 97.4) (end 79.1 117.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 103.5) (end 46.2 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 117.4) (end 41.4 117.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 97.4) (end 79.1 97.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 125.9) (end 46.2 125.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 119.8) (end 41.4 125.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 117.4) (end 41.4 111.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 110.5) (end 47 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 111.3) (end 46.2 111.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 156.1) (end 126.4 156.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 149.1) (end 126.4 148.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 148.3) (end 126.4 148.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 155.3) (end 127.2 155.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 162.2) (end 121.6 156.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 142.2) (end 121.6 148.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.2 149.1) (end 127.2 155.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 162.2) (end 121.6 162.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 119.8) (end 121.6 125.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 125.9) (end 126.4 125.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.2 126.7) (end 127.2 132.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 119.8) (end 159.3 119.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 142.2) (end 159.3 162.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 142.2) (end 159.3 142.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 119.8) (end 159.3 139.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 139.8) (end 121.6 139.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 97.4) (end 121.6 103.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 103.5) (end 126.4 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 104.3) (end 126.4 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 97.4) (end 159.3 97.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.2 104.3) (end 127.2 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 126.7) (end 126.4 125.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 139.8) (end 121.6 133.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 133.7) (end 126.4 133.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 132.9) (end 127.2 132.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 97.4) (end 159.3 117.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 117.4) (end 121.6 117.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 111.3) (end 126.4 111.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 110.5) (end 127.2 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 117.4) (end 121.6 111.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 103.5) (end 86.3 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 110.5) (end 87.1 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 104.3) (end 86.3 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.1 104.3) (end 87.1 110.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 97.4) (end 81.5 103.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 139.8) (end 81.5 133.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 133.7) (end 86.3 133.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 132.9) (end 87.1 132.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.1 126.7) (end 87.1 132.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 126.7) (end 86.3 125.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 142.2) (end 81.5 148.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 142.2) (end 119.2 142.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 139.8) (end 81.5 139.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 162.2) (end 81.5 162.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 162.2) (end 81.5 156.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 142.2) (end 119.2 162.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.1 149.1) (end 87.1 155.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 119.8) (end 119.2 139.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 119.8) (end 119.2 119.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 117.4) (end 81.5 117.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 97.4) (end 119.2 97.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 97.4) (end 119.2 117.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 125.9) (end 86.3 125.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 117.4) (end 81.5 111.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 119.8) (end 81.5 125.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 111.3) (end 86.3 111.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 155.3) (end 87.1 155.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 156.1) (end 86.3 156.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 148.3) (end 86.3 148.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 149.1) (end 86.3 148.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 44.25 143.3) (layer B.SilkS))
  (gr_text +5V (at 48.6 143.3) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 70.55 160.8) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 69.1 144.5) (layer B.SilkS))
  (gr_text CAN_H (at 71.2 131.3) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 70.55 138.4) (layer B.SilkS))
  (gr_text CAN_H (at 71.2 153.7) (layer B.SilkS))
  (gr_text GND (at 44.25 98.5) (layer B.SilkS))
  (gr_text +5V (at 48.6 98.5) (layer B.SilkS))
  (gr_text GND (at 44.25 120.9) (layer B.SilkS))
  (gr_text +5V (at 48.6 120.9) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 70.55 116) (layer B.SilkS))
  (gr_text CAN_H (at 71.2 108.9) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 69.1 122.1) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 69.1 99.7) (layer B.SilkS))
  (gr_text GND (at 124.45 143.3) (layer B.SilkS))
  (gr_text +5V (at 128.8 143.3) (layer B.SilkS))
  (gr_text GND (at 124.45 98.5) (layer B.SilkS))
  (gr_text +5V (at 128.8 98.5) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 150.75 160.8) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 149.3 122.1) (layer B.SilkS))
  (gr_text CAN_H (at 151.4 131.3) (layer B.SilkS))
  (gr_text CAN_H (at 151.4 153.7) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 150.75 138.4) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 149.3 144.5) (layer B.SilkS))
  (gr_text CAN_H (at 151.4 108.9) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 149.3 99.7) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 150.75 116) (layer B.SilkS))
  (gr_text GND (at 124.45 120.9) (layer B.SilkS))
  (gr_text +5V (at 128.8 120.9) (layer B.SilkS))
  (gr_text CAN_H (at 191.5 153.7) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 189.4 144.5) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 190.85 160.8) (layer B.SilkS))
  (gr_text CAN_H (at 191.5 131.3) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 190.85 138.4) (layer B.SilkS))
  (gr_text +5V (at 168.9 98.5) (layer B.SilkS))
  (gr_text GND (at 164.55 98.5) (layer B.SilkS))
  (gr_text GND (at 164.55 143.3) (layer B.SilkS))
  (gr_text +5V (at 168.9 143.3) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 190.85 116) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 189.4 99.7) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 189.4 122.1) (layer B.SilkS))
  (gr_text CAN_H (at 191.5 108.9) (layer B.SilkS))
  (gr_text GND (at 164.55 120.9) (layer B.SilkS))
  (gr_text +5V (at 168.9 120.9) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 109.2 122.1) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 109.2 99.7) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 110.65 116) (layer B.SilkS))
  (gr_text CAN_H (at 111.3 108.9) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 109.2 144.5) (layer B.SilkS))
  (gr_text CAN_H (at 111.3 153.7) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 110.65 160.8) (layer B.SilkS))
  (gr_text +5V (at 88.7 120.9) (layer B.SilkS))
  (gr_text GND (at 84.35 120.9) (layer B.SilkS))
  (gr_text GND (at 84.35 143.3) (layer B.SilkS))
  (gr_text +5V (at 88.7 143.3) (layer B.SilkS))
  (gr_text CAN_H (at 111.3 131.3) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 110.65 138.4) (layer B.SilkS))
  (gr_text +5V (at 88.7 98.5) (layer B.SilkS))
  (gr_text GND (at 84.35 98.5) (layer B.SilkS))
  (gr_text RX (at 100.45 75.9) (layer F.SilkS))
  (gr_text T (at 111.8 85.5 90) (layer F.SilkS))
  (gr_text B (at 57.6 92.9 90) (layer F.SilkS))
  (gr_text T (at 71.7 85.5 90) (layer F.SilkS))
  (gr_text RX (at 60.35 75.9) (layer F.SilkS))
  (gr_text PWR (at 54 75.9) (layer F.SilkS))
  (gr_text TX (at 57.15 75.9) (layer F.SilkS))
  (gr_text B (at 97.7 92.9 90) (layer F.SilkS))
  (gr_text TX (at 97.25 75.9) (layer F.SilkS))
  (gr_text PWR (at 94.1 75.9) (layer F.SilkS))
  (gr_text T (at 192 85.5 90) (layer F.SilkS))
  (gr_text B (at 177.9 92.9 90) (layer F.SilkS))
  (gr_text PWR (at 134.2 75.9) (layer F.SilkS))
  (gr_text RX (at 140.55 75.9) (layer F.SilkS))
  (gr_text TX (at 137.35 75.9) (layer F.SilkS))
  (gr_text TX (at 177.45 75.9) (layer F.SilkS))
  (gr_text RX (at 180.65 75.9) (layer F.SilkS))
  (gr_text PWR (at 174.3 75.9) (layer F.SilkS))
  (gr_text T (at 151.9 85.5 90) (layer F.SilkS))
  (gr_text B (at 137.8 92.9 90) (layer F.SilkS))
  (gr_arc (start 166.5 81.9) (end 166.5 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 81.1) (end 166.5 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 75) (end 161.7 81.1) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 88.1) (end 167.3 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 88.1) (end 127.2 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 88.9) (end 126.4 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 81.9) (end 126.4 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 81.1) (end 126.4 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 95) (end 121.6 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 75) (end 121.6 81.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 88.9) (end 166.5 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 75) (end 199.4 75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 95) (end 161.7 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 75) (end 199.4 95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 95) (end 161.7 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.3 81.9) (end 167.3 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 75) (end 119.2 95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 95) (end 81.5 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.1 81.9) (end 87.1 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 81.9) (end 86.3 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 88.1) (end 87.1 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 75) (end 119.2 75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.2 81.9) (end 127.2 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 75) (end 159.3 95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 75) (end 159.3 75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 95) (end 121.6 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 88.9) (end 86.3 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 75) (end 81.5 81.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 81.1) (end 86.3 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 95) (end 81.5 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 75) (end 79.1 95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 88.9) (end 46.2 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 88.1) (end 47 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 81.9) (end 46.2 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 81.1) (end 46.2 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47 81.9) (end 47 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 75) (end 41.4 81.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 75) (end 79.1 75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 95) (end 41.4 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 95) (end 41.4 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text http://bytewerk.org (at 150.75 93.6) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 149.3 77.3) (layer B.SilkS))
  (gr_text CAN_H (at 151.4 86.5) (layer B.SilkS))
  (gr_text CAN_H (at 191.5 86.5) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 190.85 93.6) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 189.4 77.3) (layer B.SilkS))
  (gr_text +5V (at 168.9 76.1) (layer B.SilkS))
  (gr_text GND (at 164.55 76.1) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 109.2 77.3) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 110.65 93.6) (layer B.SilkS))
  (gr_text CAN_H (at 111.3 86.5) (layer B.SilkS))
  (gr_text GND (at 124.45 76.1) (layer B.SilkS))
  (gr_text +5V (at 128.8 76.1) (layer B.SilkS))
  (gr_text GND (at 84.35 76.1) (layer B.SilkS))
  (gr_text +5V (at 88.7 76.1) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 69.1 77.3) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 70.55 93.6) (layer B.SilkS))
  (gr_text CAN_H (at 71.2 86.5) (layer B.SilkS))
  (gr_text +5V (at 48.6 76.1) (layer B.SilkS))
  (gr_text GND (at 44.25 76.1) (layer B.SilkS))
  (gr_text RX (at 100.45 53.5) (layer F.SilkS))
  (gr_text T (at 111.8 63.1 90) (layer F.SilkS))
  (gr_text B (at 57.6 70.5 90) (layer F.SilkS))
  (gr_text T (at 71.7 63.1 90) (layer F.SilkS))
  (gr_text RX (at 60.35 53.5) (layer F.SilkS))
  (gr_text PWR (at 54 53.5) (layer F.SilkS))
  (gr_text TX (at 57.15 53.5) (layer F.SilkS))
  (gr_text B (at 97.7 70.5 90) (layer F.SilkS))
  (gr_text TX (at 97.25 53.5) (layer F.SilkS))
  (gr_text PWR (at 94.1 53.5) (layer F.SilkS))
  (gr_text T (at 192 63.1 90) (layer F.SilkS))
  (gr_text B (at 177.9 70.5 90) (layer F.SilkS))
  (gr_text PWR (at 134.2 53.5) (layer F.SilkS))
  (gr_text RX (at 140.55 53.5) (layer F.SilkS))
  (gr_text TX (at 137.35 53.5) (layer F.SilkS))
  (gr_text TX (at 177.45 53.5) (layer F.SilkS))
  (gr_text RX (at 180.65 53.5) (layer F.SilkS))
  (gr_text PWR (at 174.3 53.5) (layer F.SilkS))
  (gr_text T (at 151.9 63.1 90) (layer F.SilkS))
  (gr_text B (at 137.8 70.5 90) (layer F.SilkS))
  (gr_arc (start 166.5 59.5) (end 166.5 58.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 58.7) (end 166.5 58.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 52.6) (end 161.7 58.7) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 65.7) (end 167.3 65.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 65.7) (end 127.2 65.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 66.5) (end 126.4 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 59.5) (end 126.4 58.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 58.7) (end 126.4 58.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 72.6) (end 121.6 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 52.6) (end 121.6 58.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 66.5) (end 166.5 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 52.6) (end 199.4 52.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 72.6) (end 161.7 72.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 52.6) (end 199.4 72.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 72.6) (end 161.7 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.3 59.5) (end 167.3 65.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 52.6) (end 119.2 72.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 72.6) (end 81.5 72.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.1 59.5) (end 87.1 65.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 59.5) (end 86.3 58.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 65.7) (end 87.1 65.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 52.6) (end 119.2 52.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.2 59.5) (end 127.2 65.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 52.6) (end 159.3 72.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 52.6) (end 159.3 52.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 72.6) (end 121.6 72.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 66.5) (end 86.3 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 52.6) (end 81.5 58.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 58.7) (end 86.3 58.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 72.6) (end 81.5 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 52.6) (end 79.1 72.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 66.5) (end 46.2 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 65.7) (end 47 65.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 59.5) (end 46.2 58.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 58.7) (end 46.2 58.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47 59.5) (end 47 65.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 52.6) (end 41.4 58.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 52.6) (end 79.1 52.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 72.6) (end 41.4 72.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 72.6) (end 41.4 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text http://bytewerk.org (at 150.75 71.2) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 149.3 54.9) (layer B.SilkS))
  (gr_text CAN_H (at 151.4 64.1) (layer B.SilkS))
  (gr_text CAN_H (at 191.5 64.1) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 190.85 71.2) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 189.4 54.9) (layer B.SilkS))
  (gr_text +5V (at 168.9 53.7) (layer B.SilkS))
  (gr_text GND (at 164.55 53.7) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 109.2 54.9) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 110.65 71.2) (layer B.SilkS))
  (gr_text CAN_H (at 111.3 64.1) (layer B.SilkS))
  (gr_text GND (at 124.45 53.7) (layer B.SilkS))
  (gr_text +5V (at 128.8 53.7) (layer B.SilkS))
  (gr_text GND (at 84.35 53.7) (layer B.SilkS))
  (gr_text +5V (at 88.7 53.7) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 69.1 54.9) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 70.55 71.2) (layer B.SilkS))
  (gr_text CAN_H (at 71.2 64.1) (layer B.SilkS))
  (gr_text +5V (at 48.6 53.7) (layer B.SilkS))
  (gr_text GND (at 44.25 53.7) (layer B.SilkS))
  (gr_text T (at 192 40.7 90) (layer F.SilkS))
  (gr_text RX (at 180.65 31.1) (layer F.SilkS))
  (gr_text TX (at 177.45 31.1) (layer F.SilkS))
  (gr_text PWR (at 174.3 31.1) (layer F.SilkS))
  (gr_text B (at 177.9 48.1 90) (layer F.SilkS))
  (gr_line (start 161.7 36.3) (end 166.5 36.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 44.1) (end 166.5 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 43.3) (end 167.3 43.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.5 37.1) (end 166.5 36.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 50.2) (end 161.7 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 30.2) (end 161.7 36.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7 30.2) (end 199.4 30.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 50.2) (end 161.7 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 30.2) (end 199.4 50.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.3 37.1) (end 167.3 43.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text http://bytewerk.org (at 190.85 48.8) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 189.4 32.5) (layer B.SilkS))
  (gr_text CAN_H (at 191.5 41.7) (layer B.SilkS))
  (gr_text +5V (at 168.9 31.3) (layer B.SilkS))
  (gr_text GND (at 164.55 31.3) (layer B.SilkS))
  (gr_text T (at 151.9 40.7 90) (layer F.SilkS))
  (gr_text RX (at 140.55 31.1) (layer F.SilkS))
  (gr_text TX (at 137.35 31.1) (layer F.SilkS))
  (gr_text PWR (at 134.2 31.1) (layer F.SilkS))
  (gr_text B (at 137.8 48.1 90) (layer F.SilkS))
  (gr_line (start 121.6 36.3) (end 126.4 36.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 44.1) (end 126.4 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 43.3) (end 127.2 43.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 126.4 37.1) (end 126.4 36.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 50.2) (end 121.6 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 30.2) (end 121.6 36.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.6 30.2) (end 159.3 30.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 50.2) (end 121.6 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.3 30.2) (end 159.3 50.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.2 37.1) (end 127.2 43.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text http://bytewerk.org (at 150.75 48.8) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 149.3 32.5) (layer B.SilkS))
  (gr_text CAN_H (at 151.4 41.7) (layer B.SilkS))
  (gr_text +5V (at 128.8 31.3) (layer B.SilkS))
  (gr_text GND (at 124.45 31.3) (layer B.SilkS))
  (gr_text T (at 111.8 40.7 90) (layer F.SilkS))
  (gr_text RX (at 100.45 31.1) (layer F.SilkS))
  (gr_text TX (at 97.25 31.1) (layer F.SilkS))
  (gr_text PWR (at 94.1 31.1) (layer F.SilkS))
  (gr_text B (at 97.7 48.1 90) (layer F.SilkS))
  (gr_line (start 81.5 36.3) (end 86.3 36.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 44.1) (end 86.3 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 43.3) (end 87.1 43.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.3 37.1) (end 86.3 36.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 50.2) (end 81.5 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 30.2) (end 81.5 36.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.5 30.2) (end 119.2 30.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 50.2) (end 81.5 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.2 30.2) (end 119.2 50.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.1 37.1) (end 87.1 43.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text http://bytewerk.org (at 110.65 48.8) (layer B.SilkS))
  (gr_text "candleLight v1.1" (at 109.2 32.5) (layer B.SilkS))
  (gr_text CAN_H (at 111.3 41.7) (layer B.SilkS))
  (gr_text +5V (at 88.7 31.3) (layer B.SilkS))
  (gr_text GND (at 84.35 31.3) (layer B.SilkS))
  (gr_text T (at 71.7 40.7 90) (layer F.SilkS))
  (gr_text B (at 57.6 48.1 90) (layer F.SilkS))
  (gr_text PWR (at 54 31.1) (layer F.SilkS))
  (gr_text RX (at 60.35 31.1) (layer F.SilkS))
  (gr_text TX (at 57.15 31.1) (layer F.SilkS))
  (gr_text "candleLight v1.1" (at 69.1 32.5) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 70.55 48.8) (layer B.SilkS))
  (gr_text CAN_H (at 71.2 41.7) (layer B.SilkS))
  (gr_text +5V (at 48.6 31.3) (layer B.SilkS))
  (gr_text GND (at 44.25 31.3) (layer B.SilkS))
  (gr_line (start 41.4 30.2) (end 41.4 36.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 30.2) (end 79.1 50.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47 37.1) (end 47 43.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 36.3) (end 46.2 36.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 37.1) (end 46.2 36.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 43.3) (end 47 43.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 44.1) (end 46.2 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 50.2) (end 41.4 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 50.2) (end 41.4 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 30.2) (end 79.1 30.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 29.2) (xy 80 29.2) (xy 80 51.2) (xy 40.5 51.2) (xy 40.5 29.2)
        (xy 40.5 29.2)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 40 28.7) (xy 80.5 28.7) (xy 80.5 51.7) (xy 40 51.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.6 29.2) (xy 120.1 29.2) (xy 120.1 51.2) (xy 80.6 51.2) (xy 80.6 29.2)
        (xy 80.6 29.2)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 80.1 28.7) (xy 120.6 28.7) (xy 120.6 51.7) (xy 80.1 51.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.7 29.2) (xy 160.2 29.2) (xy 160.2 51.2) (xy 120.7 51.2) (xy 120.7 29.2)
        (xy 120.7 29.2)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 120.2 28.7) (xy 160.7 28.7) (xy 160.7 51.7) (xy 120.2 51.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8 29.2) (xy 200.3 29.2) (xy 200.3 51.2) (xy 160.8 51.2) (xy 160.8 29.2)
        (xy 160.8 29.2)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 160.3 28.7) (xy 200.8 28.7) (xy 200.8 51.7) (xy 160.3 51.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.6 51.6) (xy 120.1 51.6) (xy 120.1 73.6) (xy 80.6 73.6) (xy 80.6 51.6)
        (xy 80.6 51.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 51.6) (xy 80 51.6) (xy 80 73.6) (xy 40.5 73.6) (xy 40.5 51.6)
        (xy 40.5 51.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.7 51.6) (xy 160.2 51.6) (xy 160.2 73.6) (xy 120.7 73.6) (xy 120.7 51.6)
        (xy 120.7 51.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8 51.6) (xy 200.3 51.6) (xy 200.3 73.6) (xy 160.8 73.6) (xy 160.8 51.6)
        (xy 160.8 51.6)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 40 51.1) (xy 80.5 51.1) (xy 80.5 74.1) (xy 40 74.1)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 80.1 51.1) (xy 120.6 51.1) (xy 120.6 74.1) (xy 80.1 74.1)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 160.3 51.1) (xy 200.8 51.1) (xy 200.8 74.1) (xy 160.3 74.1)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 120.2 51.1) (xy 160.7 51.1) (xy 160.7 74.1) (xy 120.2 74.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.6 74) (xy 120.1 74) (xy 120.1 96) (xy 80.6 96) (xy 80.6 74)
        (xy 80.6 74)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 74) (xy 80 74) (xy 80 96) (xy 40.5 96) (xy 40.5 74)
        (xy 40.5 74)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.7 74) (xy 160.2 74) (xy 160.2 96) (xy 120.7 96) (xy 120.7 74)
        (xy 120.7 74)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8 74) (xy 200.3 74) (xy 200.3 96) (xy 160.8 96) (xy 160.8 74)
        (xy 160.8 74)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 40 73.5) (xy 80.5 73.5) (xy 80.5 96.5) (xy 40 96.5)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 80.1 73.5) (xy 120.6 73.5) (xy 120.6 96.5) (xy 80.1 96.5)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 160.3 73.5) (xy 200.8 73.5) (xy 200.8 96.5) (xy 160.3 96.5)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 120.2 73.5) (xy 160.7 73.5) (xy 160.7 96.5) (xy 120.2 96.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.6 96.4) (xy 120.1 96.4) (xy 120.1 118.4) (xy 80.6 118.4) (xy 80.6 96.4)
        (xy 80.6 96.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.7 118.8) (xy 160.2 118.8) (xy 160.2 140.8) (xy 120.7 140.8) (xy 120.7 118.8)
        (xy 120.7 118.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.7 141.2) (xy 160.2 141.2) (xy 160.2 163.2) (xy 120.7 163.2) (xy 120.7 141.2)
        (xy 120.7 141.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8 118.8) (xy 200.3 118.8) (xy 200.3 140.8) (xy 160.8 140.8) (xy 160.8 118.8)
        (xy 160.8 118.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.7 96.4) (xy 160.2 96.4) (xy 160.2 118.4) (xy 120.7 118.4) (xy 120.7 96.4)
        (xy 120.7 96.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8 96.4) (xy 200.3 96.4) (xy 200.3 118.4) (xy 160.8 118.4) (xy 160.8 96.4)
        (xy 160.8 96.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.8 141.2) (xy 200.3 141.2) (xy 200.3 163.2) (xy 160.8 163.2) (xy 160.8 141.2)
        (xy 160.8 141.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.6 141.2) (xy 120.1 141.2) (xy 120.1 163.2) (xy 80.6 163.2) (xy 80.6 141.2)
        (xy 80.6 141.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.6 118.8) (xy 120.1 118.8) (xy 120.1 140.8) (xy 80.6 140.8) (xy 80.6 118.8)
        (xy 80.6 118.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 96.4) (xy 80 96.4) (xy 80 118.4) (xy 40.5 118.4) (xy 40.5 96.4)
        (xy 40.5 96.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 141.2) (xy 80 141.2) (xy 80 163.2) (xy 40.5 163.2) (xy 40.5 141.2)
        (xy 40.5 141.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 118.8) (xy 80 118.8) (xy 80 140.8) (xy 40.5 140.8) (xy 40.5 118.8)
        (xy 40.5 118.8)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 40 140.7) (xy 80.5 140.7) (xy 80.5 163.7) (xy 40 163.7)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 40 95.9) (xy 80.5 95.9) (xy 80.5 118.9) (xy 40 118.9)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 40 118.3) (xy 80.5 118.3) (xy 80.5 141.3) (xy 40 141.3)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 80.1 95.9) (xy 120.6 95.9) (xy 120.6 118.9) (xy 80.1 118.9)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 80.1 118.3) (xy 120.6 118.3) (xy 120.6 141.3) (xy 80.1 141.3)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 80.1 140.7) (xy 120.6 140.7) (xy 120.6 163.7) (xy 80.1 163.7)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 120.2 95.9) (xy 160.7 95.9) (xy 160.7 118.9) (xy 120.2 118.9)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 120.2 118.3) (xy 160.7 118.3) (xy 160.7 141.3) (xy 120.2 141.3)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 120.2 140.7) (xy 160.7 140.7) (xy 160.7 163.7) (xy 120.2 163.7)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 160.3 95.9) (xy 200.8 95.9) (xy 200.8 118.9) (xy 160.3 118.9)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 160.3 118.3) (xy 200.8 118.3) (xy 200.8 141.3) (xy 160.3 141.3)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 160.3 140.7) (xy 200.8 140.7) (xy 200.8 163.7) (xy 160.3 163.7)
      )
    )
  )
)
