<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="10.16" y2="0" width="0.254" layer="20"/>
<wire x1="10.16" y1="0" x2="10.16" y2="10.16" width="0.254" layer="20"/>
<wire x1="10.16" y1="10.16" x2="0" y2="10.16" width="0.254" layer="20"/>
<wire x1="0" y1="10.16" x2="0" y2="0" width="0.254" layer="20"/>
<text>CS</text>
<text>SCK</text>
<text>SDI</text>
<text>REF</text>
<text>VOA</text>
<text>GND</text>
<text>VCC</text>
<text>VOB</text>
<text>LTC2602</text>
<text>KD0GLS 2017</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="MSOP8">
</package>
<package name="PIN_SQUARE">
</package>
<package name="PIN_ROUND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="kd0gls" package="MSOP8" value="LTC2602"/>
<element name="CS" library="kd0gls" package="PIN_SQUARE" value="PIN_SQUARE"/>
<element name="SCK" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="SDI" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="REF" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="VOUTB" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="VCC" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="GND" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="VOUTA" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
</elements>
<signals>
<signal name="CS">
<contactref element="U1" pad="1"/>
<contactref element="CS" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="2"/>
<contactref element="SCK" pad="1"/>
</signal>
<signal name="SDI">
<contactref element="U1" pad="3"/>
<contactref element="SDI" pad="1"/>
</signal>
<signal name="REF">
<contactref element="U1" pad="4"/>
<contactref element="REF" pad="1"/>
</signal>
<signal name="VOUTB">
<contactref element="U1" pad="5"/>
<contactref element="VOUTB" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="6"/>
<contactref element="VCC" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="7"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="VOUTA">
<contactref element="U1" pad="8"/>
<contactref element="VOUTA" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
