(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 88)
    (tracks 32)
    (zones 0)
    (modules 10)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers(double)/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
  )
  (module misc_footprints:makho_micro_fmask (layer B.Cu) (tedit 5F25B3E4)
    (at 9 3.1 90)
    (fp_text reference Ref** (at 0 -1.7 90) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 1.45 90) (layer B.SilkS) hide)
  )
  (module misc_footprints:RM_4.75mm_fmask (layer F.Cu) (tedit 5F06772A)
    (at 8 9 270)
    (fp_text reference Ref** (at 0 -3.45 90) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 2.9 90) (layer F.SilkS) hide)
  )
  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 8.2 21.5)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference + (at 0 -2.898) (layer F.SilkS))
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.9) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask))
  )
  (module "misc_footprints:JST_BM02B-ACHSS-GAN-TF(LF)(SN)" (layer B.Cu) (tedit 5F4715CE)
    (at 8.2 24.75)
    (fp_text reference J1 (at 1.075 3.635) (layer B.SilkS) hide)
    (fp_text value "BM02B-ACHSS-GAN-TF(LF)(SN)" (at 16.95 -3.365) (layer B.Fab))
    (pad 1 smd rect (at -0.675 1.975) (size 0.8 1.05) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.675 1.975) (size 0.8 1.05) (layers B.Cu B.Paste B.Mask))
    (pad S1 smd rect (at -1.825 -1.95) (size 0.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad S2 smd rect (at 1.825 -1.95) (size 0.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 8.2 15.5)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference - (at 0 -2.898) (layer F.SilkS))
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.9) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask))
  )
  (module "misc_footprints:JST_BM02B-ACHSS-GAN-TF(LF)(SN)" (layer B.Cu) (tedit 5F3EEB13)
    (at 2.5 24.75)
    (fp_text reference J1 (at 1.075 3.635) (layer B.SilkS) hide)
    (fp_text value "BM02B-ACHSS-GAN-TF(LF)(SN)" (at 16.95 -3.365) (layer B.Fab))
    (pad S2 smd rect (at 1.825 -1.95) (size 0.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad S1 smd rect (at -1.825 -1.95) (size 0.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.675 1.975) (size 0.8 1.05) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -0.675 1.975) (size 0.8 1.05) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad1)"))
  )
  (module misc_footprints:makho_micro_fmask (layer B.Cu) (tedit 5F25B3E4)
    (at 3.3 3.1 90)
    (fp_text reference Ref** (at 0 -1.7 90) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 1.45 90) (layer B.SilkS) hide)
  )
  (module misc_footprints:RM_4.75mm_fmask (layer F.Cu) (tedit 5F06772A)
    (at 2.3 9 270)
    (fp_text reference Ref** (at 0 -3.45 90) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 2.9 90) (layer F.SilkS) hide)
  )
  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 2.5 21.5)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference + (at 0 -2.898) (layer F.SilkS))
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.9) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 2.5 15.5)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference - (at 0 -2.898) (layer F.SilkS))
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.9) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 2 "Net-(J1-Pad2)"))
  )
  (gr_line (start 9.7 3.8) (end 9.7 0.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 10.5 4) (end 9.9 4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 9.7 31.3) (end 9.7 27.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 10.5 27.5) (end 9.9 27.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 9.9 27.7) (end 9.9 27.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 9.5 31.3) (end 9.5 31.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 10.5 27.3) (end 10.5 27.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 9.5 0.2) (end 9.7 0.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 6.7 30.5) (end 5.7 30.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5.9 5.7) (end 6.5 5.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5.9 8.2) (end 6.5 8.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 9.5 31.5) (end 6.7 31.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5.7 5.5) (end 5.7 1) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 9.9 3.8) (end 9.7 3.8) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 10.7 27.3) (end 10.7 4.2) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 10.5 4.2) (end 10.7 4.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 6.7 5.9) (end 6.7 8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 9.5 0) (end 6.7 0) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 6.7 1) (end 6.7 0) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5.9 27.7) (end 6.5 27.7) (layer Edge.Cuts) (width 0.05))
  (gr_text AGS_LIPO (at 6.9 2.8 270) (layer B.Cu))
  (gr_text "+\n-" (at 8.7 7.1 90) (layer B.Cu))
  (gr_text AGS_LIPO (at 6.9 2.8 270) (layer B.Mask))
  (gr_text "+\n-" (at 8.7 7.1 90) (layer B.Mask))
  (gr_arc (start 6.5 8) (end 6.5 8.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 5.9 5.5) (end 5.7 5.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5.7 8.4) (end 5.7 27.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 6.5 30) (end 6.5 30.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 5.9 30.4) (end 5.9 30.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 5.9 8.4) (end 5.9 8.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5.9 30.2) (end 6.5 30.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 6.7 27.9) (end 6.7 30) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5.7 30.4) (end 5.7 30.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 5.9 27.5) (end 5.7 27.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 6.5 27.9) (end 6.7 27.9) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 6.5 5.9) (end 6.7 5.9) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 4 31.3) (end 4 27.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 4.8 27.5) (end 4.2 27.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 4.2 27.7) (end 4.2 27.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 3.8 31.3) (end 3.8 31.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 4.8 27.3) (end 4.8 27.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 4.8 4) (end 4.2 4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 4 3.8) (end 4 0.2) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 3.8 0.2) (end 4 0.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 4.8 4.2) (end 5 4.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 4.2 3.8) (end 4 3.8) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "+\n-" (at 3 7.1 90) (layer B.Mask))
  (gr_text "+\n-" (at 3 7.1 90) (layer B.Cu))
  (gr_text AGS_LIPO (at 1.2 2.8 270) (layer B.Mask))
  (gr_text AGS_LIPO (at 1.2 2.8 270) (layer B.Cu))
  (gr_arc (start 0.2 5.5) (end 0 5.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0.8 5.9) (end 1 5.9) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0.8 8) (end 0.8 8.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0.2 8.4) (end 0.2 8.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0.8 30) (end 0.8 30.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0.8 27.9) (end 1 27.9) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0.2 27.5) (end 0 27.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0.2 30.4) (end 0.2 30.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 30.4) (end 0 30.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 8.4) (end 0 27.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 1 27.9) (end 1 30) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.2 30.2) (end 0.8 30.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.2 27.7) (end 0.8 27.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 1 5.9) (end 1 8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.2 8.2) (end 0.8 8.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.2 5.7) (end 0.8 5.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 3.8 31.5) (end 1 31.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 5.5) (end 0 1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 3.8 0) (end 1 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5 27.3) (end 5 4.2) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 1 1) (end 1 0) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 1 30.5) (end 0 30.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 5 31.5) (xy 0 31.5) (xy 0 0) (xy 5 0)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.7 31.5) (xy 5.7 31.5) (xy 5.7 0) (xy 10.7 0)
      )
    )
  )
)
