<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<hole x="53.142" y="3.5" drill="2.75"/>
<hole x="53.142" y="61.5" drill="2.75"/>
<hole x="4.142" y="3.5" drill="2.75"/>
<hole x="4.142" y="61.5" drill="2.75"/>
<wire x1="121.031" y1="71.92" x2="121.031" y2="2.746" width="0.4064" layer="20"/>
<wire x1="121.031" y1="2.746" x2="118.031" y2="0" width="0.4064" layer="20" curve="-90"/>
<wire x1="118.031" y1="0" x2="3.142" y2="0" width="0.4064" layer="20"/>
<wire x1="3.142" y1="0" x2="0.142" y2="3" width="0.4064" layer="20" curve="-90"/>
<wire x1="0.142" y1="3" x2="0.142" y2="65.062" width="0.4064" layer="20"/>
<wire x1="0.142" y1="65.062" x2="2.634" y2="66.792" width="0.4064" layer="20" curve="-90"/>
<wire x1="2.634" y1="66.792" x2="34.8413625" y2="66.80178125" width="0.4064" layer="20"/>
<wire x1="34.8413625" y1="66.80178125" x2="35.56" y2="66.0833625" width="0.4064" layer="20" curve="-89.870856"/>
<wire x1="35.56" y1="66.0833625" x2="35.56" y2="64.516" width="0.4064" layer="20"/>
<wire x1="35.56" y1="64.516" x2="57.15" y2="64.516" width="0.4064" layer="20"/>
<wire x1="57.15" y1="64.516" x2="57.15" y2="66.08343125" width="0.4064" layer="20"/>
<wire x1="57.15" y1="66.08343125" x2="57.86856875" y2="66.80185" width="0.4064" layer="20" curve="-90.011963"/>
<wire x1="57.86856875" y1="66.80185" x2="66.167" y2="66.802" width="0.4064" layer="20"/>
<wire x1="66.167" y1="66.802" x2="66.167" y2="74.93" width="0.4064" layer="20"/>
<wire x1="66.167" y1="74.93" x2="102.616" y2="74.93" width="0.4064" layer="20"/>
<wire x1="102.616" y1="74.93" x2="102.616" y2="72.517" width="0.4064" layer="20"/>
<wire x1="102.616" y1="72.517" x2="117.856" y2="72.517" width="0.4064" layer="20"/>
<wire x1="117.856" y1="72.517" x2="117.856" y2="74.93" width="0.4064" layer="20"/>
<wire x1="117.856" y1="74.93" x2="117.904" y2="74.93" width="0.4064" layer="20"/>
<wire x1="117.904" y1="74.93" x2="121.031" y2="71.92" width="0.4064" layer="20" curve="-90"/>
<text>Volvo 240 Pi Dash Adapter
Rev C. Apr 2022
@whitfijs</text>
<text>+3.3V</text>
<text>GND</text>
<text>TACH</text>
<hole x="107.752" y="3.5" drill="2.75"/>
<hole x="118.039" y="58.325" drill="2.75"/>
<text>GND</text>
<text>GND</text>
<text>FUSE 16</text>
<text>FUSE 8</text>
<text>12V Switched</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X20">
<description>&lt;h3&gt;Plated Through Hole - 2x20&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_2MM">
<description>&lt;h3&gt;Plated Through Hole - 2mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_XTRA_BIG">
<description>&lt;h3&gt;Plated Through Hole - 0.1" holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.2"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="digital_dash">
<packages>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="SO16">
<description>&lt;h3&gt;SOIC-16&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Width:0.15"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;HEX_CONVERTER&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DIL8-SMD">
<description>&lt;b&gt;Dual  In Line SMD&lt;/b&gt; 8 pol.&lt;p&gt;
Source: LITE-ON ELECTRONICS, LTV816.pdf</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="VOLVO_CON_31">
</package>
<package name="VOLVO_CON_32">
</package>
<package name="SMD16">
<description>&lt;b&gt;SMD 4&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/83673/sfh618.pdf</description>
</package>
<package name="UMAX10">
<description>&lt;b&gt;micro MAX Package&lt;/b&gt;</description>
</package>
<package name="ECX-34RR">
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="YC248">
</package>
<package name="VOLVO_CONN_VSS">
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="MOLEX-1053102108">
</package>
<package name="MOLEX-1053141204">
</package>
<package name="MOLEX-1053101104">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_NO_SILK">
</package>
<package name="SMT-JUMPER_2_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM">
<description>&lt;h3&gt;12mm Coin Cell (CR1225) Battery Holder - SMD&lt;/h3&gt;
&lt;p&gt;Holds battery in place with friction. The metal housing connects to the positive side of the battery and the PCB pad underneath is connected to the negative side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/KEY-3000.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_6.0X3.5MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.0 x 3.5 mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/1101.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT323">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X20" value="CONN_20X2"/>
<element name="IC1" library="digital_dash" package="TSSOP14" value="LMV614"/>
<element name="C1" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE" value="100n"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C5" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="digital_dash" package="0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="digital_dash" package="0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE" value="100n"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="R6" library="digital_dash" package="0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="digital_dash" package="0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="digital_dash" package="SO16" value="MCP3X083008"/>
<element name="C6" library="digital_dash" package="0603" value="1u">
<attribute name="VOLTAGE" value="25V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C8" library="digital_dash" package="0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="IC3" library="microchip" package="SSOP28" value="MCP23017SS">
<attribute name="MPN" value="MCP23017-E/SS"/>
<attribute name="OC_NEWARK" value="31K2960"/>
<attribute name="MF" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="1467674"/>
</element>
<element name="OK1" library="digital_dash" package="SMD16" value="ILQ1X009"/>
<element name="R17" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="digital_dash" package="0603" value="470R"/>
<element name="R19" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="digital_dash" package="0603" value="470R"/>
<element name="R24" library="digital_dash" package="0603" value="470R"/>
<element name="R25" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OK2" library="digital_dash" package="SMD16" value="ILQ1X009"/>
<element name="R29" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="digital_dash" package="0603" value="470R"/>
<element name="R37" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C10" library="digital_dash" package="0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="OK3" library="digital_dash" package="SMD16" value="ILQ1X009"/>
<element name="R41" library="digital_dash" package="0603" value="470R"/>
<element name="R42" library="digital_dash" package="0603" value="470R"/>
<element name="R43" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="digital_dash" package="0603" value="470R"/>
<element name="R48" library="digital_dash" package="0603" value="470R"/>
<element name="R49" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="digital_dash" package="0603" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C13" library="digital_dash" package="0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="R57" library="digital_dash" package="0603" value="100R"/>
<element name="IC5" library="digital_dash" package="DIL8-SMD" value="IL300"/>
<element name="R53" library="digital_dash" package="0603" value="100k 1%"/>
<element name="R55" library="digital_dash" package="0603" value="270 1%"/>
<element name="R56" library="digital_dash" package="0603" value="20k 1%">
<attribute name="NAME"/>
<attribute name="VALUE" value="20k 1%"/>
</element>
<element name="IC6" library="digital_dash" package="SO08" value="TSV912D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C14" library="digital_dash" package="0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="R58" library="digital_dash" package="0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R59" library="digital_dash" package="0603" value="100k 1%">
<attribute name="NAME"/>
<attribute name="VALUE" value="100k 1%"/>
</element>
<element name="IC7" library="digital_dash" package="DIL8-SMD" value="IL300"/>
<element name="R61" library="digital_dash" package="0603" value="270 1%"/>
<element name="R62" library="digital_dash" package="0603" value="20k 1%">
<attribute name="NAME"/>
<attribute name="VALUE" value="20k 1%"/>
</element>
<element name="IC4" library="digital_dash" package="SO08" value="LM358D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="digital_dash" package="VOLVO_CON_31" value="VOLVO_CONN_31"/>
<element name="J7" library="digital_dash" package="VOLVO_CON_32" value="VOLVO_CONN_32"/>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN1_SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN2_SEL"/>
<element name="JP3" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN3_SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN4_SEL"/>
<element name="JP5" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN5_SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN6_SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN7_SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN8_SEL"/>
<element name="JP9" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN9_SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN10_SEL"/>
<element name="JP11" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN11_SEL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP12" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="IN12_SEL"/>
<element name="JP17" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="JUMPER-SMT_3_NO_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP18" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="JUMPER-SMT_3_NO_SILK"/>
<element name="JP13" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="JUMPER-SMT_3_NO_SILK"/>
<element name="JP14" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="JUMPER-SMT_3_NO_SILK"/>
<element name="IC8" library="digital_dash" package="SO08" value="TSV912D"/>
<element name="C15" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C16" library="digital_dash" package="0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="R63" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE" value="100n"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="R65" library="digital_dash" package="0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R67" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R69" library="digital_dash" package="0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP22" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="SPI_CS_SEL"/>
<element name="J13" library="SparkFun-Connectors" package="1X01_2MM" value=""/>
<element name="J14" library="SparkFun-Connectors" package="1X01_2MM" value=""/>
<element name="R71" library="digital_dash" package="0603" value="100k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R72" library="digital_dash" package="0603" value="100k 1%">
<attribute name="NAME"/>
<attribute name="VALUE" value="100k 1%"/>
</element>
<element name="R73" library="digital_dash" package="0603" value="100k 1%">
<attribute name="NAME"/>
<attribute name="VALUE" value="100k 1%"/>
</element>
<element name="R74" library="digital_dash" package="0603" value="100k 1%"/>
<element name="D7" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="diode" package="SOT23" value="BAT54S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="digital_dash" package="UMAX10" value="DS1374">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BT1" library="SparkFun-Batteries" package="BATTCON_12MM" value="">
<attribute name="PROD_ID" value="BATT-08044"/>
<attribute name="SF_SKU" value="PRT-10592"/>
</element>
<element name="Y1" library="digital_dash" package="ECX-34RR" value="ECX-.327-6-34RR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="digital_dash" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="50V"/>
</element>
<element name="C20" library="digital_dash" package="0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="R75" library="digital_dash" package="0603" value="1k"/>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.0X3.5MM" value="RST_SW">
<attribute name="PROD_ID" value="SWCH-14278"/>
<attribute name="SF_SKU" value="COM-08229"/>
</element>
<element name="J16" library="SparkFun-Connectors" package="1X03" value="TACH_IN">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="R76" library="digital_dash" package="0603" value="20k"/>
<element name="R82" library="digital_dash" package="0617/17" value="RES_D+">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J20" library="SparkFun-Connectors" package="1X02_XTRA_BIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J21" library="SparkFun-Connectors" package="1X02_XTRA_BIG" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J22" library="SparkFun-Connectors" package="1X02_XTRA_BIG" value=""/>
<element name="J17" library="SparkFun-Connectors" package="1X02_XTRA_BIG" value=""/>
<element name="C21" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="digital_dash" package="YC248" value="8.2k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="R3" library="digital_dash" package="YC248" value="15k">
<attribute name="TOLERANCE" value="5%"/>
</element>
<element name="J11" library="digital_dash" package="VOLVO_CONN_VSS" value="VOLVO_CONN_VSS"/>
<element name="IC10" library="digital_dash" package="UMAX10" value="MAX9924">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC11" library="digital_dash" package="SOT23" value="ZXTR2105FQ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="digital_dash" package="0603" value="1u">
<attribute name="VOLTAGE" value="25V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="digital_dash" package="0603" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="digital_dash" package="0603" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="digital_dash" package="0603" value="1n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP21" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_SILK" value="SPI_CS_SEL"/>
<element name="R14" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="digital_dash" package="0603" value="100n">
<attribute name="VOLTAGE" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="digital_dash" package="0603" value="10u">
<attribute name="VOLTAGE" value="6.3V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT323" value="310mA/60V/1.6Ω">
<attribute name="PROD_ID" value="TRANS-11151"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT323" value="310mA/60V/1.6Ω">
<attribute name="PROD_ID" value="TRANS-11151"/>
</element>
<element name="R15" library="digital_dash" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="digital_dash" package="0603" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE" value="20k"/>
</element>
<element name="R54" library="digital_dash" package="0603" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE" value="20k"/>
</element>
<element name="J2" library="digital_dash" package="MOLEX-1053102108" value="CONN_04X2"/>
<element name="JP15" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="VSS- Jumper"/>
<element name="J3" library="digital_dash" package="MOLEX-1053141204" value="CONN_04RIGHT-ANGLE"/>
<element name="J4" library="digital_dash" package="MOLEX-1053101104" value="CONN_04"/>
<element name="J5" library="SparkFun-Connectors" package="1X03" value="PWM_OUT">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="R60" library="digital_dash" package="0603" value="20k"/>
<element name="R64" library="digital_dash" package="0603" value="1k"/>
<element name="R66" library="digital_dash" package="0603" value="1k"/>
<element name="R68" library="digital_dash" package="0603" value="1k"/>
<element name="R70" library="digital_dash" package="0603" value="1k"/>
</elements>
<signals>
<signal name="SENSOR1_IN">
<contactref element="JP13" pad="1"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="SENSOR2_IN">
<contactref element="JP14" pad="1"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="SENSOR3_IN">
<contactref element="R6" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="SENSOR4_IN">
<contactref element="R8" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="11"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="39"/>
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="25"/>
<contactref element="J1" pad="30"/>
<contactref element="J1" pad="20"/>
<contactref element="J1" pad="14"/>
<contactref element="J1" pad="6"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC2" pad="14"/>
<contactref element="OK1" pad="16"/>
<contactref element="OK1" pad="13"/>
<contactref element="OK2" pad="16"/>
<contactref element="OK2" pad="13"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC3" pad="15"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC3" pad="17"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="OK3" pad="16"/>
<contactref element="OK3" pad="13"/>
<contactref element="OK2" pad="12"/>
<contactref element="OK2" pad="9"/>
<contactref element="OK3" pad="12"/>
<contactref element="OK3" pad="9"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC6" pad="4"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC6" pad="5"/>
<contactref element="OK1" pad="12"/>
<contactref element="OK1" pad="9"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="IC8" pad="4"/>
<contactref element="C18" pad="2"/>
<contactref element="D6" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="BT1" pad="GND"/>
<contactref element="IC9" pad="5"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="J16" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R3" pad="3"/>
<contactref element="R3" pad="4"/>
<contactref element="R3" pad="5"/>
<contactref element="R3" pad="6"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="J2" pad="8"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="IC8" pad="8"/>
<contactref element="R63" pad="2"/>
<contactref element="R67" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="J2" pad="7"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="ADC1_IN">
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="R2" pad="16"/>
<contactref element="R3" pad="16"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="3"/>
</signal>
<signal name="ADC2_IN">
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="R2" pad="15"/>
<contactref element="R3" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="D2" pad="3"/>
</signal>
<signal name="ADC3_IN">
<contactref element="C3" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="R2" pad="14"/>
<contactref element="R3" pad="14"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="D3" pad="3"/>
</signal>
<signal name="ADC4_IN">
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="4"/>
<contactref element="R2" pad="13"/>
<contactref element="R3" pad="13"/>
</signal>
<signal name="N$15">
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="12"/>
<contactref element="D4" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="6"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="13"/>
<contactref element="R2" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="9"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="17"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC2" pad="15"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="R39" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC3" pad="9"/>
<contactref element="R43" pad="2"/>
<contactref element="R46" pad="2"/>
<contactref element="R51" pad="2"/>
<contactref element="R52" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="IC6" pad="8"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="IC9" pad="10"/>
<contactref element="R75" pad="2"/>
<contactref element="J16" pad="3"/>
<contactref element="R76" pad="2"/>
<contactref element="R54" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="R64" pad="1"/>
<contactref element="R70" pad="1"/>
<contactref element="R68" pad="1"/>
<contactref element="R66" pad="1"/>
</signal>
<signal name="!SPI_CS">
<contactref element="IC2" pad="10"/>
<contactref element="JP22" pad="2"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="J1" pad="19"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="SPI_MISO">
<contactref element="J1" pad="21"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="SPI_CLK">
<contactref element="J1" pad="23"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="SPI_CE0_N">
<contactref element="J1" pad="24"/>
<contactref element="JP22" pad="3"/>
</signal>
<signal name="SPI_CE1_N">
<contactref element="J1" pad="26"/>
<contactref element="JP22" pad="1"/>
</signal>
<signal name="IN1P">
<contactref element="OK1" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="IN1N">
<contactref element="OK1" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="12V">
<contactref element="R17" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="R35" pad="2"/>
<contactref element="R37" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="R47" pad="2"/>
<contactref element="R49" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC4" pad="8"/>
<contactref element="D7" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="R82" pad="2"/>
<contactref element="IC11" pad="3"/>
<contactref element="C24" pad="1"/>
<contactref element="J11" pad="+"/>
<contactref element="R15" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="OUT1">
<contactref element="OK1" pad="15"/>
<contactref element="R19" pad="1"/>
<contactref element="IC3" pad="21"/>
</signal>
<signal name="OUT2">
<contactref element="R22" pad="1"/>
<contactref element="OK1" pad="14"/>
<contactref element="IC3" pad="22"/>
</signal>
<signal name="IN2P">
<contactref element="OK1" pad="4"/>
<contactref element="R20" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="IN2N">
<contactref element="OK1" pad="3"/>
<contactref element="R21" pad="2"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="IN3P">
<contactref element="OK1" pad="5"/>
<contactref element="R23" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="IN3N">
<contactref element="OK1" pad="6"/>
<contactref element="R24" pad="2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="IN4P">
<contactref element="OK1" pad="8"/>
<contactref element="R25" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="IN4N">
<contactref element="OK1" pad="7"/>
<contactref element="R26" pad="2"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="OUT4">
<contactref element="OK1" pad="10"/>
<contactref element="R28" pad="1"/>
<contactref element="IC3" pad="24"/>
</signal>
<signal name="OUT3">
<contactref element="OK1" pad="11"/>
<contactref element="R27" pad="1"/>
<contactref element="IC3" pad="23"/>
</signal>
<signal name="IN5P">
<contactref element="OK2" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="IN5N">
<contactref element="OK2" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="IN6P">
<contactref element="OK2" pad="4"/>
<contactref element="R32" pad="1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="IN6N">
<contactref element="OK2" pad="3"/>
<contactref element="R33" pad="2"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="IN7P">
<contactref element="OK2" pad="5"/>
<contactref element="R35" pad="1"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="IN7N">
<contactref element="OK2" pad="6"/>
<contactref element="R36" pad="2"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="IN8P">
<contactref element="OK2" pad="8"/>
<contactref element="R37" pad="1"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="IN8N">
<contactref element="OK2" pad="7"/>
<contactref element="R38" pad="2"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="OUT8">
<contactref element="OK2" pad="10"/>
<contactref element="R40" pad="1"/>
<contactref element="IC3" pad="25"/>
</signal>
<signal name="OUT7">
<contactref element="OK2" pad="11"/>
<contactref element="R39" pad="1"/>
<contactref element="IC3" pad="26"/>
</signal>
<signal name="OUT6">
<contactref element="OK2" pad="14"/>
<contactref element="R34" pad="1"/>
<contactref element="IC3" pad="27"/>
</signal>
<signal name="OUT5">
<contactref element="OK2" pad="15"/>
<contactref element="R31" pad="1"/>
<contactref element="IC3" pad="28"/>
</signal>
<signal name="SCL">
<contactref element="IC3" pad="12"/>
<contactref element="J1" pad="5"/>
<contactref element="IC9" pad="7"/>
</signal>
<signal name="SDA">
<contactref element="IC3" pad="13"/>
<contactref element="J1" pad="3"/>
<contactref element="IC9" pad="6"/>
</signal>
<signal name="IN9P">
<contactref element="OK3" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="IN9N">
<contactref element="OK3" pad="2"/>
<contactref element="R42" pad="2"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="IN10P">
<contactref element="OK3" pad="4"/>
<contactref element="R44" pad="1"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="IN10N">
<contactref element="OK3" pad="3"/>
<contactref element="R45" pad="2"/>
<contactref element="JP10" pad="3"/>
</signal>
<signal name="OUT10">
<contactref element="OK3" pad="14"/>
<contactref element="R46" pad="1"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="OUT9">
<contactref element="OK3" pad="15"/>
<contactref element="R43" pad="1"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="IN11P">
<contactref element="OK3" pad="5"/>
<contactref element="R47" pad="1"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="IN11N">
<contactref element="OK3" pad="6"/>
<contactref element="R48" pad="2"/>
<contactref element="JP11" pad="3"/>
</signal>
<signal name="OUT11">
<contactref element="OK3" pad="11"/>
<contactref element="R51" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="IN12P">
<contactref element="OK3" pad="8"/>
<contactref element="R49" pad="1"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="IN12N">
<contactref element="OK3" pad="7"/>
<contactref element="R50" pad="2"/>
<contactref element="JP12" pad="3"/>
</signal>
<signal name="OUT12">
<contactref element="OK3" pad="10"/>
<contactref element="R52" pad="1"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="R57" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="D7" pad="3"/>
</signal>
<signal name="IN1_12V_SIGNAL">
<contactref element="R57" pad="1"/>
<contactref element="R73" pad="2"/>
<contactref element="R74" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC5" pad="4"/>
<contactref element="R53" pad="2"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R55" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R55" pad="2"/>
<contactref element="IC5" pad="2"/>
</signal>
<signal name="SIG_3V3_IN1">
<contactref element="R56" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R58" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="D8" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="R59" pad="2"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="R61" pad="1"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="N$26">
<contactref element="R61" pad="2"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="SIG_3V3_IN2">
<contactref element="R62" pad="2"/>
<contactref element="IC6" pad="7"/>
<contactref element="IC2" pad="8"/>
<contactref element="C22" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="R62" pad="1"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC6" pad="6"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="GND-ISO">
<contactref element="R53" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="R59" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="R38" pad="1"/>
<contactref element="R36" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="R45" pad="1"/>
<contactref element="R50" pad="1"/>
<contactref element="R48" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC7" pad="1"/>
<contactref element="J7" pad="4"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R72" pad="1"/>
<contactref element="R74" pad="1"/>
<contactref element="D7" pad="1"/>
<contactref element="D8" pad="1"/>
<contactref element="J20" pad="1"/>
<contactref element="J21" pad="1"/>
<contactref element="J21" pad="2"/>
<contactref element="J20" pad="2"/>
<contactref element="IC11" pad="1"/>
<contactref element="C24" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="IC10" pad="5"/>
<contactref element="JP21" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="JP15" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="BRAKE_FAILURE_N">
<contactref element="J6" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="COOLANT_TEMP_SENSOR">
<contactref element="J6" pad="2"/>
<contactref element="JP13" pad="3"/>
</signal>
<signal name="HIGH_BEAM_P">
<contactref element="J6" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="OD_LAMP_P">
<contactref element="J6" pad="4"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="BULB_FAILURE_N">
<contactref element="J6" pad="12"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="CHARGING_N">
<contactref element="J6" pad="11"/>
<contactref element="JP6" pad="2"/>
<contactref element="R82" pad="1"/>
</signal>
<signal name="DIMMER_VOUT">
<contactref element="J6" pad="10"/>
<contactref element="JP17" pad="3"/>
</signal>
<signal name="BLINKER_LEFT_P">
<contactref element="J6" pad="8"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="BLINKER_RIGHT_P">
<contactref element="J6" pad="7"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="AC_RELAY/VSS_TO_ECU">
<contactref element="J6" pad="6"/>
<contactref element="IC10" pad="7"/>
<contactref element="Q1" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="OIL_PRESS_SW_N">
<contactref element="J6" pad="5"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="CONN_32_PIN3">
<contactref element="J7" pad="3"/>
<contactref element="JP12" pad="2"/>
</signal>
<signal name="PARKING_BRAKE_N">
<contactref element="J7" pad="2"/>
<contactref element="JP11" pad="2"/>
</signal>
<signal name="FUEL_LVL_SENDER">
<contactref element="J7" pad="1"/>
<contactref element="JP14" pad="3"/>
</signal>
<signal name="SIG_12V_IN1">
<contactref element="JP17" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R4" pad="1"/>
<contactref element="JP14" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R1" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="JP13" pad="2"/>
</signal>
<signal name="12V-FUSE_8">
<contactref element="J6" pad="9"/>
<contactref element="JP18" pad="3"/>
<contactref element="J22" pad="1"/>
<contactref element="J22" pad="2"/>
</signal>
<signal name="12V-FUSE_16">
<contactref element="J7" pad="A"/>
<contactref element="J17" pad="2"/>
<contactref element="J17" pad="1"/>
</signal>
<signal name="OD_LAMP_AUTO_P">
<contactref element="JP9" pad="2"/>
<contactref element="J13" pad="1"/>
</signal>
<signal name="CHECK_ENGINE_N">
<contactref element="JP10" pad="2"/>
<contactref element="J14" pad="1"/>
</signal>
<signal name="SIG_12V_IN2">
<contactref element="JP18" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="JP18" pad="2"/>
<contactref element="R71" pad="1"/>
</signal>
<signal name="SENSOR5_IN">
<contactref element="R65" pad="1"/>
<contactref element="R63" pad="1"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="SENSOR6_IN">
<contactref element="R69" pad="1"/>
<contactref element="R67" pad="1"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$28">
<contactref element="IC8" pad="2"/>
<contactref element="IC8" pad="1"/>
<contactref element="R2" pad="5"/>
</signal>
<signal name="N$29">
<contactref element="R65" pad="2"/>
<contactref element="IC8" pad="3"/>
<contactref element="D5" pad="3"/>
</signal>
<signal name="N$35">
<contactref element="IC8" pad="6"/>
<contactref element="IC8" pad="7"/>
<contactref element="R2" pad="6"/>
</signal>
<signal name="N$36">
<contactref element="R69" pad="2"/>
<contactref element="IC8" pad="5"/>
<contactref element="D6" pad="3"/>
</signal>
<signal name="ADC5_IN">
<contactref element="C17" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="R2" pad="12"/>
<contactref element="R3" pad="12"/>
</signal>
<signal name="ADC6_IN">
<contactref element="C18" pad="1"/>
<contactref element="IC2" pad="6"/>
<contactref element="R2" pad="11"/>
<contactref element="R3" pad="11"/>
</signal>
<signal name="N$17">
<contactref element="R58" pad="1"/>
<contactref element="R71" pad="2"/>
<contactref element="R72" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="JP17" pad="2"/>
<contactref element="R73" pad="1"/>
</signal>
<signal name="GPIO17">
<contactref element="J1" pad="11"/>
</signal>
<signal name="GPIO27">
<contactref element="J1" pad="13"/>
</signal>
<signal name="GPIO22">
<contactref element="J1" pad="15"/>
</signal>
<signal name="N$24">
<contactref element="IC9" pad="1"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="IC9" pad="2"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="BT1" pad="PWR@1"/>
<contactref element="IC9" pad="3"/>
</signal>
<signal name="N$39">
<contactref element="IC9" pad="9"/>
<contactref element="R75" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="IC9" pad="4"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="GPIO26">
<contactref element="J1" pad="37"/>
</signal>
<signal name="GPIO19">
<contactref element="J1" pad="35"/>
<contactref element="Q2" pad="3"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="GPIO13">
<contactref element="J1" pad="33"/>
</signal>
<signal name="GPIO6">
<contactref element="J1" pad="31"/>
<contactref element="J16" pad="2"/>
<contactref element="R76" pad="1"/>
</signal>
<signal name="N$42">
</signal>
<signal name="N$10">
<contactref element="C21" pad="2"/>
<contactref element="IC5" pad="6"/>
<contactref element="R56" pad="1"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="VCCA">
<contactref element="IC11" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="IC10" pad="10"/>
<contactref element="R13" pad="2"/>
<contactref element="JP21" pad="3"/>
</signal>
<signal name="N$46">
<contactref element="IC10" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="IC10" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="C26" pad="2"/>
</signal>
<signal name="VSS+">
<contactref element="J11" pad="G"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VSS-">
<contactref element="J11" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="JP15" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="IC10" pad="4"/>
<contactref element="R13" pad="1"/>
<contactref element="C28" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="IC10" pad="6"/>
<contactref element="IC10" pad="9"/>
<contactref element="JP21" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Q1" pad="3"/>
<contactref element="R16" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="USER_IN1">
<contactref element="IC3" pad="5"/>
<contactref element="J4" pad="1"/>
<contactref element="R64" pad="2"/>
</signal>
<signal name="USER_IN2">
<contactref element="IC3" pad="6"/>
<contactref element="J4" pad="2"/>
<contactref element="R66" pad="2"/>
</signal>
<signal name="USER_IN3">
<contactref element="IC3" pad="7"/>
<contactref element="J4" pad="3"/>
<contactref element="R68" pad="2"/>
</signal>
<signal name="USER_IN4">
<contactref element="IC3" pad="8"/>
<contactref element="J4" pad="4"/>
<contactref element="R70" pad="2"/>
</signal>
<signal name="GPIO18">
<contactref element="J1" pad="12"/>
<contactref element="J5" pad="2"/>
<contactref element="R60" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
