(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 43)
    (tracks 148)
    (zones 0)
    (modules 32)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2.032)
    (user_trace_width 2.032)
    (user_trace_width 3.81)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad16)")
  (net 2 "Net-(A1-Pad17)")
  (net 3 "Net-(A1-Pad3)")
  (net 4 "Net-(A1-Pad18)")
  (net 5 "Net-(A1-Pad4)")
  (net 6 GND)
  (net 7 "Net-(A1-Pad5)")
  (net 8 "Net-(A1-Pad20)")
  (net 9 "Net-(A1-Pad6)")
  (net 10 "Net-(A1-Pad21)")
  (net 11 "Net-(A1-Pad7)")
  (net 12 "Net-(A1-Pad22)")
  (net 13 "Net-(A1-Pad8)")
  (net 14 "Net-(A1-Pad23)")
  (net 15 "Net-(A1-Pad9)")
  (net 16 "Net-(A1-Pad24)")
  (net 17 "Net-(A1-Pad10)")
  (net 18 "Net-(A1-Pad25)")
  (net 19 "Net-(A1-Pad11)")
  (net 20 "Net-(A1-Pad26)")
  (net 21 "Net-(A1-Pad12)")
  (net 22 "Net-(A1-Pad27)")
  (net 23 "Net-(A1-Pad13)")
  (net 24 "Net-(A1-Pad28)")
  (net 25 "Net-(A1-Pad29)")
  (net 26 "Net-(A1-Pad15)")
  (net 27 "Net-(A1-Pad30)")
  (net 28 "Net-(A1-Pad1)")
  (net 29 "Net-(C1-Pad1)")
  (net 30 "Net-(J1-Pad3)")
  (net 31 "Net-(J1-Pad1)")
  (net 32 "Net-(J2-Pad1)")
  (net 33 "Net-(U1-Pad6)")
  (net 34 "Net-(A1-Pad2)")
  (net 35 "Net-(J2-Pad3)")
  (net 36 "Net-(D1-Pad2)")
  (net 37 "Net-(D2-PadA)")
  (net 38 "Net-(C4-Pad1)")
  (net 39 "Net-(J3-Pad4)")
  (net 40 "Net-(J3-Pad3)")
  (net 41 "Net-(J3-Pad2)")
  (net 42 "Net-(J3-Pad1)")
  (net 43 "Net-(J5-Pad5)")
  (net 44 "Net-(J5-Pad2)")
  (net 45 "Net-(J5-Pad1)")
  (net 46 "Net-(J10-Pad2)")
  (net 47 "Net-(L1-Pad12)")
  (net 48 "Net-(L1-Pad11)")
  (net 49 "Net-(L1-Pad6)")
  (net 50 "Net-(L1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1.27)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad29)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-PadA)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(L1-Pad11)")
    (add_net "Net-(L1-Pad12)")
    (add_net "Net-(L1-Pad5)")
    (add_net "Net-(L1-Pad6)")
    (add_net "Net-(U1-Pad6)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 130.556 97.028 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 2.032 7.62) (layer F.SilkS))
    (fp_text value SCL (at -0.254 -2.794 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad9)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "my library:Phoenix_6_pin_5mm_terminal_block" (layer F.Cu) (tedit 5DFECE68)
    (at 157.734 120.363 90)
    (fp_text reference J8 (at 0.221 -0.762 90) (layer F.SilkS))
    (fp_text value "Power Out" (at 30.701 4.572 180) (layer F.SilkS))
    (pad 6 thru_hole circle (at 27.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 46 "Net-(J10-Pad2)"))
    (pad 5 thru_hole circle (at 22.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 17.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 12.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad1)"))
    (pad 1 thru_hole circle (at 2.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad1)"))
  )
  (module "my library:Phoenix_9_pin_5mm_terminal_block" (layer F.Cu) (tedit 5DFECDCE)
    (at 96.52 95.25 270)
    (fp_text reference J6 (at 2 -1 90) (layer F.SilkS))
    (fp_text value Ground (at 20.828 10.16 90) (layer F.SilkS))
    (pad 9 thru_hole circle (at 42.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 8 thru_hole circle (at 37.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 7 thru_hole circle (at 32.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 6 thru_hole circle (at 27.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 5 thru_hole circle (at 22.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 4 thru_hole circle (at 17.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 3 thru_hole circle (at 12.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole circle (at 7.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 2.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module "my library:Phoenix_7_pin_5mm_terminal_block" (layer F.Cu) (tedit 5DFECD81)
    (at 96.52 59.69 270)
    (fp_text reference J5 (at 2 -1 90) (layer F.SilkS))
    (fp_text value GPIO's (at 19.558 7.874 90) (layer F.Fab))
    (pad 7 thru_hole circle (at 32.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad27)"))
    (pad 6 thru_hole circle (at 27.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad26)"))
    (pad 5 thru_hole circle (at 22.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 43 "Net-(J5-Pad5)"))
    (pad 4 thru_hole circle (at 17.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad24)"))
    (pad 3 thru_hole circle (at 12.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad23)"))
    (pad 2 thru_hole circle (at 7.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 44 "Net-(J5-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 45 "Net-(J5-Pad1)"))
  )
  (module "my library:Phoenix_4_pin_5mm_terminal_block" (layer F.Cu) (tedit 5D6B1E0B)
    (at 157.734 87.63 90)
    (fp_text reference J3 (at 21.082 -0.254 90) (layer F.SilkS))
    (fp_text value Analog (at 20.828 4.318 180) (layer F.SilkS))
    (pad 4 thru_hole circle (at 17.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at 12.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 40 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 7.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 41 "Net-(J3-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad1)"))
  )
  (module "my library:1N5400" (layer F.Cu) (tedit 5DFAB2C1)
    (at 151.13 131.064 90)
    (descr "<B>DIODE</B><p>\ndiameter 5.6 mm, horizontal, grid 15.24 mm")
    (fp_text reference D2 (at 3.556 -3.048 90) (layer F.SilkS))
    (fp_text value 1N5400 (at -3.048 -1.016 90) (layer F.SilkS))
    (pad C thru_hole circle (at -7.62 0 90) (size 3.5 3.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad1)") (solder_mask_margin 0.1016))
    (pad A thru_hole circle (at 7.62 0 90) (size 3.5 3.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 37 "Net-(D2-PadA)") (solder_mask_margin 0.1016))
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 130.048 130.048 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 5.08 0) (layer F.SilkS))
    (fp_text value "2.2 uF" (at 1.016 -2.54) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 130.048 115.062 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 5.08 0) (layer F.SilkS))
    (fp_text value "10 uF" (at 1.25 2.5) (layer F.SilkS))
    (fp_text user %R (at 1.25 0.762) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 99.822 60.452 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 4.064 1.778 90) (layer F.SilkS))
    (fp_text value 330 (at 3.81 -2.032 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad20)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "my library:LLC" (layer F.Cu) (tedit 5DBF56E8)
    (at 157.48 78.74 90)
    (fp_text reference L1 (at -14.986 -18.288 90) (layer F.SilkS))
    (fp_text value LLC (at -8.382 -19.939 90) (layer F.Fab))
    (fp_text user HV3 (at -5.08 -7.62 90) (layer F.SilkS))
    (fp_text user HV4 (at -5.08 -5.08 90) (layer F.SilkS))
    (fp_text user GND (at -5.08 -10.16 90) (layer F.SilkS))
    (fp_text user HV (at -5.08 -12.7 90) (layer F.SilkS))
    (fp_text user HV2 (at -5.08 -15.24 90) (layer F.SilkS))
    (fp_text user HV1 (at -5.08 -17.78 90) (layer F.SilkS))
    (fp_text user LV4 (at -10.16 -5.08 90) (layer F.SilkS))
    (fp_text user LV3 (at -10.16 -7.62 90) (layer F.SilkS))
    (fp_text user GND (at -10.16 -10.16 90) (layer F.SilkS))
    (fp_text user LV (at -10.16 -12.7 90) (layer F.SilkS))
    (fp_text user LV2 (at -10.16 -15.24 90) (layer F.SilkS))
    (fp_text user LV1 (at -10.16 -17.78 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at -2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(L1-Pad12)"))
    (pad 11 thru_hole circle (at -2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(L1-Pad11)"))
    (pad 10 thru_hole circle (at -2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 9 thru_hole circle (at -2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 8 thru_hole circle (at -2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad3)"))
    (pad 7 thru_hole circle (at -2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad3)"))
    (pad 6 thru_hole circle (at -12.7 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(L1-Pad6)"))
    (pad 5 thru_hole circle (at -12.7 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(L1-Pad5)"))
    (pad 4 thru_hole circle (at -12.7 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 3 thru_hole circle (at -12.7 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(A1-Pad2)"))
    (pad 2 thru_hole circle (at -12.7 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at -12.7 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad1)"))
  )
  (module "my library:ads1115" (layer F.Cu) (tedit 5DBF5633)
    (at 129.032 76.454)
    (fp_text reference U1 (at 13.1318 -12.3444) (layer F.SilkS))
    (fp_text value ADS1115 (at 25.4 -9.398 270) (layer F.SilkS))
    (fp_text user A3 (at 24.5364 -4.2672 90) (layer F.SilkS))
    (fp_text user A2 (at 21.971 -4.1402 90) (layer F.SilkS))
    (fp_text user A1 (at 19.4564 -4.2672 90) (layer F.SilkS))
    (fp_text user A0 (at 16.7894 -4.2164 90) (layer F.SilkS))
    (fp_text user Alrt (at 14.4526 -4.5212 90) (layer F.SilkS))
    (fp_text user Addr (at 11.9126 -4.8514 90) (layer F.SilkS))
    (fp_text user SDA (at 9.398 -4.7244 90) (layer F.SilkS))
    (fp_text user SCL (at 6.7818 -4.699 90) (layer F.SilkS))
    (fp_text user GND (at 4.2672 -4.6482 90) (layer F.SilkS))
    (fp_text user VDD (at 1.6256 -4.7752 90) (layer F.SilkS))
    (pad 10 thru_hole circle (at 24.5364 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad1)"))
    (pad 9 thru_hole circle (at 21.9964 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J3-Pad2)"))
    (pad 8 thru_hole circle (at 19.4564 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J3-Pad3)"))
    (pad 7 thru_hole circle (at 16.9164 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad4)"))
    (pad 6 thru_hole circle (at 14.3764 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at 11.8364 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 4 thru_hole circle (at 9.2964 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 6.7564 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at 4.2164 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 1.6764 -1.5494) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 129.794 109.982 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 0 -2.286) (layer F.SilkS))
    (fp_text value 4.7K (at 4.064 -1.778 270) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad9)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 46 "Net-(J10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 123.952 109.982 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 0 -2.286) (layer F.SilkS))
    (fp_text value 4.7K (at 3.302 -2.032 270) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad8)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 46 "Net-(J10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "my library:mEZD71201A" (layer F.Cu) (tedit 5DB4C6B1)
    (at 121.513 127.56 90)
    (fp_text reference RG1 (at 11.228 -1.371 180) (layer F.SilkS))
    (fp_text value mEZD71201A (at 5.1054 -1.4478 90) (layer F.SilkS))
    (fp_text user Vin (at 2.4384 3.0226) (layer F.SilkS))
    (fp_text user GND (at 5.0038 2.8448) (layer F.SilkS))
    (fp_text user Vout (at 7.5184 2.6416) (layer F.SilkS))
    (pad 3 thru_hole circle (at 7.4168 8.5 180) (size 1.59 1.59) (drill 0.89) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 4.8768 8.5 180) (size 1.59 1.59) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 2.3368 8.5 180) (size 1.59 1.59) (drill 0.89) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad1)"))
  )
  (module "my library:Phoenix_2_pin_5mm_terminal_block" (layer F.Cu) (tedit 5D6B1C47)
    (at 157.734 132.588 90)
    (fp_text reference J9 (at -1.524 8.128 90) (layer F.SilkS))
    (fp_text value "Power In" (at 10.668 4.826 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(D2-PadA)"))
    (pad 1 thru_hole circle (at 2.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 124.46 64.516 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 5.08 -0.254) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 2.032 2.54 270) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 83.566 137.291)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 83.566 62.915001)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -3.048 -3.225001) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.254) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 163.322 137.291)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 1.016 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 163.322 62.915001)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -6.096 -4.241001) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 99.822 70.866 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 4.064 1.778 90) (layer F.SilkS))
    (fp_text value 330 (at 3.81 -2.032 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad22)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 99.822 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 3.81 1.778 90) (layer F.SilkS))
    (fp_text value 330 (at 3.556 -2.032 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad25)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 "Net-(J5-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 149.352 102.362 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 4.064 -2.032 90) (layer F.SilkS))
    (fp_text value 1K (at 4.318 2.032 90) (layer F.SilkS))
    (fp_text user %R (at 3.72 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 144.78 97.282)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J10 (at 0 7.62) (layer F.SilkS))
    (fp_text value VCC (at 0 -2.794) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(A1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 124.506 68.58)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at -0.046 7.874) (layer F.SilkS))
    (fp_text value "Power Source" (at 2.494 2.794 90) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad12)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad15)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 135.128 82.042)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value I2C-5V (at 0.508 12.192 90) (layer F.SilkS))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 124.714 97.028 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 1.778 7.62) (layer F.SilkS))
    (fp_text value SDA (at 0 -2.794 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad8)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 149.352 115.57 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at -0.762 3.302 180) (layer F.SilkS))
    (fp_text value LED (at 4.572 3.302 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 139.954 131.318 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C6 (at 2.5 -6.25 90) (layer F.SilkS))
    (fp_text value "1000 uF" (at 2.5 6.25 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 129.54 78.994 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 4.826 0 270) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 1.524 -2.54) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 139.954 112.268 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 2.5 -6.25 90) (layer F.SilkS))
    (fp_text value "1000 uF" (at 3.81 5.891334 90) (layer F.SilkS))
    (fp_text user %R (at 2.54 -1.27 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "my library:Nano_33" (layer F.Cu) (tedit 5D5AD926)
    (at 104.394 63.525001)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference A1 (at -2.54 -3.073001) (layer F.SilkS))
    (fp_text value Nano_33/Nano (at 8.89 19.05 90) (layer F.SilkS))
    (fp_text user D13 (at 12.1158 35.6362) (layer F.SilkS))
    (fp_text user +3V3 (at 11.6586 32.9946) (layer F.SilkS))
    (fp_text user Aref (at 12.1158 30.5308) (layer F.SilkS))
    (fp_text user A0 (at 12.7508 27.8892) (layer F.SilkS))
    (fp_text user A1 (at 12.6746 25.4) (layer F.SilkS))
    (fp_text user A2 (at 12.7508 22.8346) (layer F.SilkS))
    (fp_text user A3 (at 12.7508 20.2692) (layer F.SilkS))
    (fp_text user A4 (at 12.6746 17.78) (layer F.SilkS))
    (fp_text user A5 (at 12.7508 15.1384) (layer F.SilkS))
    (fp_text user A6 (at 12.6746 12.8016) (layer F.SilkS))
    (fp_text user A7 (at 12.5222 10.3886) (layer F.SilkS))
    (fp_text user Vusb (at 11.9634 7.4422) (layer F.SilkS))
    (fp_text user RST (at 12.1158 5.1816) (layer F.SilkS))
    (fp_text user GND (at 12.1158 2.4638) (layer F.SilkS))
    (fp_text user VIN (at 12.4206 0.0508) (layer F.SilkS))
    (fp_text user D12 (at 2.9464 35.7124) (layer F.SilkS))
    (fp_text user D11 (at 2.9464 33.0708) (layer F.SilkS))
    (fp_text user D10 (at 3.0226 30.5308) (layer F.SilkS))
    (fp_text user D9 (at 2.5654 27.9654) (layer F.SilkS))
    (fp_text user D8 (at 2.6416 25.4) (layer F.SilkS))
    (fp_text user D7 (at 2.6416 22.987) (layer F.SilkS))
    (fp_text user D6 (at 2.6416 20.3454) (layer F.SilkS))
    (fp_text user D5 (at 2.6416 17.8562) (layer F.SilkS))
    (fp_text user D4 (at 2.5654 15.2908) (layer F.SilkS))
    (fp_text user D3 (at 2.7178 12.8016) (layer F.SilkS))
    (fp_text user D2 (at 2.794 10.3124) (layer F.SilkS))
    (fp_text user GND (at 3.0988 7.747) (layer F.SilkS))
    (fp_text user RST (at 2.8702 5.1054) (layer F.SilkS))
    (fp_text user RX (at 2.54 2.54) (layer F.SilkS))
    (fp_text user TX (at 2.413 0.127) (layer F.SilkS))
    (fp_text user %R (at 6.35 19.05 90) (layer F.Fab))
    (pad 16 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad16)"))
    (pad 2 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 34 "Net-(A1-Pad2)"))
    (pad 17 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad17)"))
    (pad 3 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad3)"))
    (pad 18 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad18)"))
    (pad 4 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad4)"))
    (pad 19 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 5 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad5)"))
    (pad 20 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad20)"))
    (pad 6 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad6)"))
    (pad 21 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad21)"))
    (pad 7 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad7)"))
    (pad 22 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad22)"))
    (pad 8 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad8)"))
    (pad 23 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad23)"))
    (pad 9 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad9)"))
    (pad 24 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad24)"))
    (pad 10 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad10)"))
    (pad 25 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad25)"))
    (pad 11 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad11)"))
    (pad 26 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad26)"))
    (pad 12 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad12)"))
    (pad 27 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad27)"))
    (pad 13 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad13)"))
    (pad 28 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad28)"))
    (pad 14 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 29 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad29)"))
    (pad 15 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad15)"))
    (pad 30 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad30)"))
    (pad 1 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad1)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 3 (at 141.986 102.616) (layer F.SilkS))
  (gr_text 2 (at 141.986 99.822) (layer F.SilkS))
  (gr_text 1 (at 141.986 97.282) (layer F.SilkS))
  (gr_text 1 (at 127.508 97.028) (layer F.SilkS))
  (gr_text 2 (at 127.508 94.488) (layer F.SilkS))
  (gr_text 3 (at 127.508 92.202) (layer F.SilkS))
  (gr_text 1 (at 121.92 68.58) (layer F.SilkS))
  (gr_text 2 (at 121.92 71.12) (layer F.SilkS))
  (gr_text 3 (at 121.92 73.914) (layer F.SilkS))
  (gr_text 12V (at 155.844857 124.206) (layer F.SilkS))
  (gr_text 5V (at 156.321048 97.79) (layer F.SilkS))
  (gr_text "12V\n" (at 155.844857 107.95) (layer F.SilkS))
  (gr_text 5V (at 156.321048 102.87) (layer F.SilkS))
  (gr_text WAS (at 156.972 85.09 90) (layer F.SilkS))
  (gr_text "Steer SW" (at 83.685143 82.55) (layer F.SilkS))
  (gr_text "Work SW" (at 83.875619 67.564) (layer F.SilkS))
  (gr_text "Serial TX" (at 83.637524 77.47) (layer F.SilkS))
  (gr_text "Serial RX" (at 83.518476 72.39) (layer F.SilkS))
  (gr_text VCC (at 155.797238 92.964) (layer F.SilkS))
  (gr_text Encoder (at 84.074 59.944) (layer F.SilkS))
  (gr_arc (start 165 139) (end 165 142) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 82 139) (end 82 142) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 82 61) (end 82 58) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 165 61) (end 165 58) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168 139) (end 168 61) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82 142) (end 165 142) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 79 61) (end 79 139) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165 58) (end 82 58) (layer Edge.Cuts) (width 0.05))
  (gr_text 5V (at 132.326 82.296) (layer F.SilkS))
  (gr_text GND (at 131.706952 84.582) (layer F.SilkS))
  (gr_text SCL (at 131.849809 87.122) (layer F.SilkS))
  (gr_text SDA (at 131.826 89.662) (layer F.SilkS))
  (gr_text GND (at 155.702 129.032) (layer F.SilkS))
  (gr_text 12V (at 155.844857 118.11) (layer F.SilkS))
  (gr_text "Steer DIR" (at 83.494667 87.376) (layer F.SilkS))
  (gr_text "Steer PWM" (at 83.089905 92.456) (layer F.SilkS))
  (gr_text AIN0 (at 156.972 70.104 90) (layer F.SilkS))
  (gr_text Roll (at 156.972 80.01 90) (layer F.SilkS))
  (gr_text AIN1 (at 156.972 75.184 90) (layer F.SilkS))
  (gr_text 12V (at 155.844857 113.284) (layer F.SilkS))
  (gr_text "AutoSteer 6.0  22-Dec-2019" (at 109.982 133.858) (layer F.SilkS))
  (gr_text "Nano - 2 & 3" (at 104.394 139.192) (layer F.SilkS))
  (gr_text "Nano33 - 1 & 2" (at 105.156 136.398) (layer F.SilkS))
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.846 58.166) (xy 81.28 58.42) (xy 79.502 60.198) (xy 79.756 140.462) (xy 82.931 141.478)
        (xy 163.068 141.732) (xy 167.386 140.208) (xy 167.64 60.198)
      )
    )
  )
)
