(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A5")
	(title_block
		(date "2024-07-22")
		(rev "1.0")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010f0_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "manufacturing/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(J1-5V)")
	(net 3 "/SCL_MCU")
	(net 4 "/SDA_MCU")
	(net 5 "unconnected-(U2-NC-Pad4)")
	(net 6 "/POW_A")
	(net 7 "Net-(D1-K)")
	(net 8 "/shutdown")
	(net 9 "/POW_B")
	(net 10 "+3.3V")
	(net 11 "/Vmotor")
	(net 12 "unconnected-(U1-GPIO1-Pad7)")
	(net 13 "unconnected-(U1-DNC-Pad8)")
	(footprint "asl_footprints:board_to_board_joint_4"
		(layer "F.Cu")
		(at 100 59.2973)
		(property "Reference" "J2"
			(at 0 1.27 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at -11.7586 0.2767 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "asl_footprints:board_to_board_joint_4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -4.7625 -1.373)
			(size 1.905 2.7432)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/POW_B")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.5875 -1.373)
			(size 1.905 2.7432)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/Vmotor")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.5875 -1.373)
			(size 1.905 2.7432)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/POW_A")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 4.7625 -1.373)
			(size 1.905 2.7432)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(J1-5V)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "asl_footprints:MountingHole_2.7mm_M2.5_pad"
		(layer "F.Cu")
		(at 116.5 70)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H2"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Mount hole"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "asl_footprints:MountingHole_2.7mm_M2.5_pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.4 4.4)
			(drill 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "asl_footprints:MountingHole_2.7mm_M2.5_pad"
		(layer "F.Cu")
		(at 83.5 70)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H1"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Mount hole"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "asl_footprints:MountingHole_2.7mm_M2.5_pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.4 4.4)
			(drill 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "asl_footprints:RJ45_SMD_Vertical"
		(layer "F.Cu")
		(at 99.764 69.245 -90)
		(property "Reference" "J1"
			(at -6.995 8.514 0)
			(layer "F.SilkS")
		)
		(property "Value" "0855135013"
			(at 0.635 -1.755 90)
			(layer "F.Fab")
		)
		(property "Footprint" "asl_footprints:RJ45_SMD_Vertical"
			(at 0 0.785 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/molex/0855135013/2404862"
			(at 0 0.785 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RJ45 Jack"
			(at 0 0.785 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB Rotation Offset" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -4.445 -7.525)
			(size 5 0.76)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/SCL_MCU")
			(pinfunction "DIO-A")
			(pintype "passive")
			(solder_mask_margin 0.1016)
		)
		(pad "2" smd rect
			(at -3.175 -7.525)
			(size 5 0.76)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.1016)
		)
		(pad "3" smd rect
			(at -1.905 -7.525)
			(size 5 0.76)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/POW_A")
			(pinfunction "POW-A")
			(pintype "passive")
			(solder_mask_margin 0.1016)
		)
		(pad "4" smd rect
			(at -0.635 -7.525)
			(size 5 0.76)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/SDA_MCU")
			(pinfunction "DIO-B")
			(pintype "passive")
			(solder_mask_margin 0.1016)
		)
		(pad "5" smd rect
			(at 0.635 -7.525)
			(size 5 0.76)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D1-K)")
			(pinfunction "SPECIAL")
			(pintype "passive")
			(solder_mask_margin 0.1016)
		)
		(pad "6" smd rect
			(at 1.905 -7.525)
			(size 5 0.76)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(J1-5V)")
			(pinfunction "5V")
			(pintype "passive")
			(solder_mask_margin 0.1016)
		)
		(pad "7" smd rect
			(at 3.175 -7.525)
			(size 5 0.76)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/POW_B")
			(pinfunction "POW-B")
			(pintype "passive")
			(solder_mask_margin 0.1016)
		)
		(pad "8" smd rect
			(at 4.445 -7.525)
			(size 5 0.76)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/Vmotor")
			(pinfunction "12V")
			(pintype "passive")
			(solder_mask_margin 0.1016)
		)
		(pad "MNT" smd roundrect
			(at 0 8.405)
			(size 4.5 8.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1111111111)
			(solder_mask_margin 0.1016)
		)
		(model "${KIPRJMOD}/libs/3d/RJ45_smd_vertical.step"
			(offset
				(xyz 0 -0.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 95.5 65.1 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.1 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10µF"
			(at 0 -1.43 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10A106KQ8NNNC/3886696"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLCPCB Rotation Offset" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 96.1 69.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.5 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "470Ω"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603JR-07470RL/726791"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB Rotation Offset" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C25197"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/SDA_MCU")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 96.1 71.4)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.5 0.1 180)
			(layer "B.SilkS")
		)
		(property "Value" "470Ω"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603JR-07470RL/726791"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB Rotation Offset" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C25197"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/SCL_MCU")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 99.5 75 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.5 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.43 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KB8NNNC/3886658"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB Rotation Offset" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "asl_footprints:D_SOD-123F"
		(layer "B.Cu")
		(at 101.4 65.4 180)
		(descr "D_SOD-123F")
		(tags "D_SOD-123F")
		(property "Reference" "D1"
			(at -0.1 1.8 180)
			(layer "B.SilkS")
		)
		(property "Value" "MMSD4148T1G"
			(at 0 -2.1 180)
			(layer "B.Fab")
		)
		(property "Footprint" "asl_footprints:D_SOD-123F"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/onsemi/MMSD4148T1G/919705"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.127 1.905 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.4 0 180)
			(size 1.1 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.4 0 180)
			(size 1.1 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "/shutdown")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 97.7 65.1 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 2.1 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10KΩ"
			(at 0 -1.43 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603FR-0710KL/726880"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C25197"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLCPCB Rotation Offset" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/shutdown")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "B.Cu")
		(at 102.4 75 180)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at 0 -2.5 180)
			(layer "B.SilkS")
		)
		(property "Value" "AP2112K-3.3"
			(at 0 -2.4 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/product-detail/en/diodes-incorporated/AP2112K-3.3TRG1/AP2112K-3.3TRG1DICT-ND/4505257"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB Rotation Offset" "90"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C51118"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23?5*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(J1-5V)")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(J1-5V)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "unconnected-(U2-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "asl_footprints:VL53L4CD"
		(layer "B.Cu")
		(at 100 70 90)
		(descr "VL53L1x distance sensor")
		(tags "VL53L1CXV0FY1 VL53L1x")
		(property "Reference" "U1"
			(at 0 2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "VL53L4CD"
			(at 0 -2.3 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "asl_footprints:VL53L4CD"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/stmicroelectronics/VL53L4CDV0DH-1/16123783"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "ToF sensor, Optical LGA12"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "ST*VL53L1x*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.6 1 180)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 10 "+3.3V")
			(pinfunction "AVDDVCSEL")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at -0.8 1 180)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "AVSSVCSEL")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 0 1 180)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at 0.8 1 180)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd rect
			(at 1.6 1 180)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 8 "/shutdown")
			(pinfunction "XSHUT")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at 2.05 0 90)
			(size 1.4 0.5)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" smd rect
			(at 1.6 -1)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 12 "unconnected-(U1-GPIO1-Pad7)")
			(pinfunction "GPIO1")
			(pintype "open_collector+no_connect")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" smd rect
			(at 0.8 -1)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 13 "unconnected-(U1-DNC-Pad8)")
			(pinfunction "DNC")
			(pintype "no_connect")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" smd rect
			(at 0 -1)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 4 "/SDA_MCU")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" smd rect
			(at -0.8 -1)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "/SCL_MCU")
			(pinfunction "SCL")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" smd rect
			(at -1.6 -1)
			(size 0.9 0.5)
			(layers "B.Cu" "B.Mask")
			(net 10 "+3.3V")
			(pinfunction "AVDD")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" smd rect
			(at -2.05 0 270)
			(size 1.4 0.5)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(model "${KICAD8_3DMODEL_DIR}/Sensor_Distance.3dshapes/ST_VL53L1x.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 97.9 75 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "10µF"
			(at 0 -1.43 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10A106KQ8NNNC/3886696"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLCPCB Rotation Offset" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C19702"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DNP" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "rear.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 84.16491 80.500037)
		(end 115.83509 80.500037)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.16491 80.500037)
		(mid 81.099433 68.058496)
		(end 86.630244 56.499983)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.36974 56.5)
		(end 86.63026 56.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 113.36974 56.5)
		(mid 118.900543 68.058498)
		(end 115.83507 80.500023)
		(layer "Edge.Cuts")
	)
	(gr_text "DIO_B"
		(at 109.7788 68.12 0)
		(layer "F.SilkS")
	)
	(gr_text "DIO_A\n"
		(at 109.7788 64.31 0)
		(layer "F.SilkS")
	)
	(gr_text "POW_A"
		(at 109.7788 66.85 0)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 98.4 59.6492 0)
		(layer "F.SilkS")
	)
	(gr_text "July\n2024"
		(at 86.6 80.2 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 104.8 60.2 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 109.7788 65.58 0)
		(layer "F.SilkS")
	)
	(gr_text "POW_B"
		(at 109.7788 71.93 0)
		(layer "F.SilkS")
	)
	(gr_text "DIO_C\n"
		(at 109.7788 69.39 0)
		(layer "F.SilkS")
	)
	(gr_text "PB"
		(at 95.2 60.2 0)
		(layer "F.SilkS")
	)
	(gr_text "PA"
		(at 101.6 59.7 0)
		(layer "F.SilkS")
	)
	(gr_text "Nosepoke ToF v${REVISION}"
		(at 106 78.6 0)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 109.7788 73.2 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 109.7788 70.66 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 141.931005 92.841) (xy 60.456005 92.714) (xy 60.583005 43.565) (xy 142.312005 43.692)
			)
		)
	)
)
