(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 20)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6002)
    (drawings 10)
    (tracks 86)
    (zones 0)
    (modules 9)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 AO1)
  (net 3 AO2)
  (net 4 AO3)
  (net 5 GND)
  (net 6 AO4)
  (net 7 AO5)
  (net 8 AO6)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net AO1)
    (add_net AO2)
    (add_net AO3)
    (add_net AO4)
    (add_net AO5)
    (add_net AO6)
    (add_net GND)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A7BB8A5)
    (at 175.26 106.68)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 11.43 2.54) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 16.51 5.08) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A7BB882)
    (at 133.35 88.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 50.8 17.78) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 54.61 12.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Potentiometers:Potentiometer_Alps_RK09K_Horizontal (layer F.Cu) (tedit 5A7BB877)
    (at 162.56 88.9 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09K/RK09D1130C1B.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single")
    (fp_text reference P2 (at 11.43 1.27 180) (layer F.SilkS))
    (fp_text value POT2 (at -25.4 -3.81 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 0 -2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 AO2))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 0 np_thru_hole circle (at 7 -6.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 0 np_thru_hole circle (at 7 1.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK09K_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microfit3_Header_02x05_Straight_43045-1028 (layer F.Cu) (tedit 5A7BB891)
    (at 128.27 91.44 90)
    (descr "Microfit3 Header Straight 02x05 43045-1028")
    (tags "connector Microfit 02x05 header straight 3mm")
    (fp_text reference Mlx43045 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 1028 (at -6 -7 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -15 -4 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at -3 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 AO4))
    (pad 3 thru_hole circle (at -6 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 AO5))
    (pad 4 thru_hole circle (at -9 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 AO6))
    (pad 5 thru_hole circle (at -12 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole circle (at 0 -3 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 7 thru_hole circle (at -3 -3 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 AO1))
    (pad 8 thru_hole circle (at -6 -3 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 AO2))
    (pad 9 thru_hole circle (at -9 -3 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 AO3))
    (pad 10 thru_hole circle (at -12 -3 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad "" np_thru_hole circle (at 3 -3.94 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microfit3_Header_02x05_Straight_43045-1028.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Alps_RK09K_Horizontal (layer F.Cu) (tedit 5A7BB87D)
    (at 148.59 88.9 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09K/RK09D1130C1B.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single")
    (fp_text reference P1 (at 11.43 1.27 180) (layer F.SilkS))
    (fp_text value POT1 (at -43.18 0 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 0 -2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 AO1))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 0 np_thru_hole circle (at 7 -6.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 0 np_thru_hole circle (at 7 1.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK09K_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Alps_RK09K_Horizontal (layer F.Cu) (tedit 5A7BB87A)
    (at 176.53 88.9 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09K/RK09D1130C1B.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single")
    (fp_text reference P3 (at 11.43 1.27 180) (layer F.SilkS))
    (fp_text value POT3 (at -10.16 3.81 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 0 -2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 AO3))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 0 np_thru_hole circle (at 7 -6.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 0 np_thru_hole circle (at 7 1.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK09K_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Alps_RK09K_Horizontal (layer F.Cu) (tedit 5A7BB86F)
    (at 144.78 100.33 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09K/RK09D1130C1B.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single")
    (fp_text reference P4 (at 2.54 -6.35 180) (layer F.SilkS))
    (fp_text value POT4 (at -43.18 -5.08 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 0 -2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 AO4))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 0 np_thru_hole circle (at 7 -6.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 0 np_thru_hole circle (at 7 1.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK09K_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Alps_RK09K_Horizontal (layer F.Cu) (tedit 5A7BB860)
    (at 158.75 100.33 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09K/RK09D1130C1B.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single")
    (fp_text reference P5 (at 2.54 -6.35 180) (layer F.SilkS))
    (fp_text value POT5 (at -26.67 1.27 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 0 -2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 AO5))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 0 np_thru_hole circle (at 7 -6.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 0 np_thru_hole circle (at 7 1.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK09K_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Alps_RK09K_Horizontal (layer F.Cu) (tedit 5A7BB856)
    (at 172.72 100.33 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09K/RK09D1130C1B.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single")
    (fp_text reference P6 (at 2.54 -6.35 180) (layer F.SilkS))
    (fp_text value POT6 (at -12.7 3.81 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 0 -2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 AO6))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 0 np_thru_hole circle (at 7 -6.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 0 np_thru_hole circle (at 7 1.9 180) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK09K_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Marcavius\nFox" (at 133.35 93.98 90) (layer F.SilkS))
  (gr_text "freespy\n" (at 176.53 100.33 90) (layer F.SilkS))
  (gr_line (start 124.46 85.09) (end 176.53 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 86.36) (end 124.46 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 107.95) (end 123.19 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 109.22) (end 123.19 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.53 109.22) (end 124.46 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 107.95) (end 176.53 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 86.36) (end 177.8 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.53 85.09) (end 177.8 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 85.09) (xy 176.53 85.09) (xy 177.8 86.36) (xy 177.8 107.95) (xy 176.53 109.22)
        (xy 124.46 109.22) (xy 123.19 107.95) (xy 123.19 86.36)
      )
    )
  )
)
