<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<hole x="10.16" y="3.429" drill="2.8"/>
<hole x="40.64" y="53.721" drill="2.8"/>
<wire x1="-0.254" y1="0" x2="51.054" y2="0" width="0.254" layer="20"/>
<wire x1="-0.254" y1="57.15" x2="51.054" y2="57.15" width="0.254" layer="20"/>
<wire x1="-0.254" y1="0" x2="-0.254" y2="57.15" width="0.254" layer="20"/>
<wire x1="51.054" y1="0" x2="51.054" y2="57.15" width="0.254" layer="20"/>
<text>LED+</text>
<text>Data</text>
<text>GND</text>
<text>GND</text>
<text>+12V</text>
<text>Mode 1</text>
<text>RV-Project.Com</text>
<text>CylonEye Driver</text>
<text>Ver 2.1</text>
<text>Mode 2</text>
<text>1591XXFL</text>
<text>GND</text>
<text>LED+</text>
<text>LED 
Data</text>
<text>+12V</text>
<text>GND</text>
<text>Mode 1</text>
<text>Mode 2</text>
<text>Golf Cart
 Version</text>
<text>Warning: LED Board
must have a 470Ohm
Resistor in DATA line.

Otherwise, insert a
470Ohm resistor in
the data line.</text>
</plain>
<libraries>
<library name="alsstuff">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_200MIL(10MM)">
</package>
<package name="RADIAL_ELECTROLYTIC_100MIL(5MM)">
<description>Generic Electrolytic Capacitor 0.100 spacing 0.200 diameter.</description>
</package>
<package name="GENERIC_0100_DEVICE_150_SPACING">
<description>&lt;h3&gt;Ceramic Capacitor&lt;/h3&gt;
Commonly used for small ceramic capacitors 0150 spacing.</description>
</package>
<package name="DIODE-1N4001">
</package>
<package name="1/4W_AXIAL">
<description>Standard Axial 1/4Watt Resistor&lt;p&gt;0.45" footprint</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SMTSO-256-ET">
</package>
<package name="TO-220-HEATSINK-2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="1000UF">
<attribute name="VOLTAGE" value="25V"/>
<attribute name="MARKING" value="108"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="1000UF">
<attribute name="VOLTAGE" value="25V"/>
<attribute name="MARKING" value="108"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="alsstuff" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="VOLTAGE" value="25v"/>
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="alsstuff" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="alsstuff" package="RADIAL_ELECTROLYTIC_200MIL(10MM)" value="1000UF">
<attribute name="VOLTAGE" value="25V"/>
<attribute name="MARKING" value="108"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="alsstuff" package="DIODE-1N4001" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="alsstuff" package="1/4W_AXIAL" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="alsstuff" package="TO-220-HEATSINK-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="alsstuff" package="DIP08" value="">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="alsstuff" package="SMTSO-256-ET" value=""/>
<element name="JP2" library="alsstuff" package="SMTSO-256-ET" value=""/>
<element name="JP3" library="alsstuff" package="SMTSO-256-ET" value=""/>
<element name="JP4" library="alsstuff" package="SMTSO-256-ET" value=""/>
<element name="JP5" library="alsstuff" package="SMTSO-256-ET" value=""/>
<element name="JP6" library="alsstuff" package="SMTSO-256-ET" value=""/>
<element name="JP7" library="alsstuff" package="SMTSO-256-ET" value=""/>
<element name="R2" library="alsstuff" package="1/4W_AXIAL" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="alsstuff" package="1/4W_AXIAL" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="alsstuff" package="1/4W_AXIAL" value="10k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="R5" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="JP3" pad="P$1"/>
<contactref element="JP7" pad="P$1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="12V">
<contactref element="U1" pad="IN"/>
<contactref element="D1" pad="C"/>
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP4" pad="P$1"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="OUT"/>
<contactref element="D1" pad="A"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="JP1" pad="P$1"/>
<contactref element="C5" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="5"/>
<contactref element="JP2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="JP5" pad="P$1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP6" pad="P$1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
