(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/SYNC")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "+12V")
  (net 4 "GND")
  (net 5 "-12V")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C4-Pad2)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C5-Pad2)")
  (net 10 "VCC")
  (net 11 "VSS")
  (net 12 "Net-(C11-Pad1)")
  (net 13 "Net-(C11-Pad2)")
  (net 14 "Net-(C12-Pad1)")
  (net 15 "Net-(C13-Pad1)")
  (net 16 "Net-(C13-Pad2)")
  (net 17 "Net-(D1-Pad1)")
  (net 18 "Net-(D1-Pad2)")
  (net 19 "Net-(D3-Pad1)")
  (net 20 "Net-(D3-Pad2)")
  (net 21 "Net-(D4-Pad2)")
  (net 22 "Net-(D5-Pad1)")
  (net 23 "Net-(J1-PadT)")
  (net 24 "unconnected-(J1-PadTN)")
  (net 25 "/CV2")
  (net 26 "unconnected-(J2-PadTN)")
  (net 27 "/CV1")
  (net 28 "unconnected-(J3-PadTN)")
  (net 29 "Net-(J4-PadT)")
  (net 30 "unconnected-(J4-PadTN)")
  (net 31 "Net-(J5-PadT)")
  (net 32 "unconnected-(J5-PadTN)")
  (net 33 "Net-(J6-PadT)")
  (net 34 "unconnected-(J6-PadTN)")
  (net 35 "/SINE")
  (net 36 "unconnected-(J7-PadTN)")
  (net 37 "/SAW")
  (net 38 "unconnected-(J8-PadTN)")
  (net 39 "/TRIANGLE")
  (net 40 "unconnected-(J9-PadTN)")
  (net 41 "/SQUARE")
  (net 42 "unconnected-(J10-PadTN)")
  (net 43 "Net-(J11-Pad1)")
  (net 44 "Net-(J11-Pad10)")
  (net 45 "Net-(R1-Pad1)")
  (net 46 "/EXP_CV")
  (net 47 "Net-(R11-Pad1)")
  (net 48 "/FINE")
  (net 49 "/COARSE")
  (net 50 "Net-(R8-Pad2)")
  (net 51 "Net-(R9-Pad2)")
  (net 52 "Net-(R10-Pad1)")
  (net 53 "Net-(R11-Pad2)")
  (net 54 "Net-(R14-Pad1)")
  (net 55 "/LIN_CV")
  (net 56 "Net-(R16-Pad2)")
  (net 57 "Net-(R18-Pad2)")
  (net 58 "Net-(R19-Pad1)")
  (net 59 "Net-(R22-Pad1)")
  (net 60 "Net-(R23-Pad1)")
  (net 61 "Net-(R23-Pad2)")
  (net 62 "Net-(R24-Pad1)")
  (net 63 "Net-(R24-Pad2)")
  (net 64 "Net-(R27-Pad1)")
  (net 65 "/PWM")
  (net 66 "Net-(R31-Pad2)")
  (net 67 "/PW")
  (net 68 "Net-(R33-Pad1)")
  (net 69 "Net-(R37-Pad2)")
  (net 70 "Net-(R39-Pad1)")
  (net 71 "Net-(R39-Pad2)")
  (net 72 "Net-(R41-Pad2)")
  (net 73 "Net-(R42-Pad2)")
  (net 74 "Net-(R49-Pad2)")
  (net 75 "Net-(R50-Pad2)")
  (net 76 "unconnected-(RV8-Pad3)")
  (net 77 "unconnected-(RV10-Pad3)")
  (net 78 "unconnected-(U4-Pad4)")
  (net 79 "unconnected-(U4-Pad8)")
  (net 80 "unconnected-(U3-Pad5)")
  (net 81 "unconnected-(U3-Pad4)")
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 41.275 92.71)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "EXP FM" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 24 "unconnected-(J1-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (tedit 0)
    (at 61.595 67.31)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV3" (at -9.779 -0.508 unlocked) (layer "F.SilkS"))
    (fp_text value "PWM LVL" (at 0 4.826 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.604 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 65 "/PWM") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-PadT)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole" (layer "F.Cu")
    (tedit 0)
    (at 67.13 212.84)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H1" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "1v/oct" (at 0 -6.858 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-2M_Switch-Hole" (layer "F.Cu")
    (tedit 0)
    (at 48.08 182.36)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H21" (at 0 -4.445 unlocked) (layer "F.Fab"))
    (fp_text value "SYNC HARDNESS" (at 0 4.445 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 7 7) (drill 4.95) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole" (layer "F.Cu")
    (tedit 0)
    (at 48.08 196.33)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H5" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "pwm" (at 0 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 28.575 106.68)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "Sine" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 35 "/SINE") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 36 "unconnected-(J7-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 53.975 92.71)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "1V/OCT" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 25 "/CV2") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J2-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_pan" (layer "F.Cu")
    (tedit 0)
    (at 62.05 136.64)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H12" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "fine tune" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "+" (at 1.905 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "-" (at -1.905 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -7.8 0) (size 1.3 3.1) (drill oval 1.2 3) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (tedit 0)
    (at 33.655 67.31)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV7" (at -6.35 -7.239 unlocked) (layer "F.SilkS"))
    (fp_text value "PW" (at 0 4.826 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.604 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "Net-(R9-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 67 "/PW") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 54 "Net-(R14-Pad1)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 47.625 76.2)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 3.302 -5.969 unlocked) (layer "F.SilkS"))
    (fp_text value "PWM" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 32 "unconnected-(J5-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_level" (layer "F.Cu")
    (tedit 0)
    (at 34.11 136.64)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H11" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "frequency" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "10" (at 6.35 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "0" (at -5.08 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -7.8 0) (size 1.3 3.1) (drill oval 1.2 3) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (tedit 0)
    (at 41.73 226.81)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H9" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "triangle" (at 0 8.255 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (tedit 0)
    (at 67.13 226.81)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H10" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "pulse" (at 0 8.255 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Switch_SPDT_Tayda_A-5751" (layer "F.Cu")
    (tedit 0)
    (at 47.625 62.23)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text value "Sync Mode" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(J6-PadT)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "/SYNC") (pinfunction "C") (pintype "passive"))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (tedit 0)
    (at 25.28 119.84)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H20" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "MountingHole" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (tedit 0)
    (at 71 119.84)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H17" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "MountingHole" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole" (layer "F.Cu")
    (tedit 0)
    (at 29.03 212.84)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H4" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "lin fm" (at 0 -6.858 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 66.675 106.68)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "Square" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 41 "/SQUARE") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 42 "unconnected-(J10-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_level" (layer "F.Cu")
    (tedit 0)
    (at 62.05 162.04)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H14" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "exp fm" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "10" (at 6.35 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "0" (at -5.08 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -7.8 0) (size 1.3 3.1) (drill oval 1.2 3) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 28.575 92.71)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "LIN FM" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(J4-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 30 "unconnected-(J4-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_pan" (layer "F.Cu")
    (tedit 0)
    (at 34.11 187.44)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H15" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "pw" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "-" (at -1.905 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "+" (at 1.905 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -7.8 0) (size 1.3 3.1) (drill oval 1.2 3) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (tedit 0)
    (at 71 242.34)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H19" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "MountingHole" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 47.625 50.8)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "SYNC" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 33 "Net-(J6-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J6-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (tedit 0)
    (at 54.43 226.81)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H8" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "saw" (at 0 8.255 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole" (layer "F.Cu")
    (tedit 0)
    (at 41.73 212.84)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H3" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "exp fm" (at 0 -6.858 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole" (layer "F.Cu")
    (tedit 0)
    (at 48.08 170.93)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H6" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "sync" (at 0 -6.858 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (tedit 0)
    (at 61.595 16.51)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV5" (at -9.906 3.556 unlocked) (layer "F.SilkS"))
    (fp_text value "Fine Tune" (at 0 4.826 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.604 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "-12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 48 "/FINE") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "+12V") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_level" (layer "F.Cu")
    (tedit 0)
    (at 62.05 187.44)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H16" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "pwm lvl" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "0" (at -5.08 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "10" (at 6.35 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -7.8 0) (size 1.3 3.1) (drill oval 1.2 3) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (tedit 0)
    (at 25.28 242.34)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H18" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "MountingHole" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_level" (layer "F.Cu")
    (tedit 0)
    (at 34.11 162.04)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H13" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "lin fm" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "0" (at -5.08 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "10" (at 6.35 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -7.8 0) (size 1.3 3.1) (drill oval 1.2 3) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 66.675 92.71)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "1V/OCT" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 27 "/CV1") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 28 "unconnected-(J3-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole" (layer "F.Cu")
    (tedit 0)
    (at 54.43 212.84)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H2" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "1v/oct" (at 0 -6.858 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (tedit 0)
    (at 61.595 41.91)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV1" (at -9.779 0.508 unlocked) (layer "F.SilkS"))
    (fp_text value "EXP FM LVL" (at 0 4.826 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.604 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 "/EXP_CV") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-PadT)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 53.975 106.68)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "Saw" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 37 "/SAW") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 38 "unconnected-(J8-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (tedit 0)
    (at 41.275 106.68)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "Triangle" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 39 "/TRIANGLE") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers *.Cu *.Mask)
      (net 40 "unconnected-(J9-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (tedit 0)
    (at 33.655 16.51)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV4" (at 5.461 9.779 unlocked) (layer "F.SilkS"))
    (fp_text value "Tune" (at 15.367 11.049 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 15.367 12.827 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "-12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "/COARSE") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "+12V") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (tedit 0)
    (at 29.03 226.81)
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H7" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "sine" (at 0 8.255 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers *.Cu *.Mask))
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (tedit 0)
    (at 33.655 41.91)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV2" (at -9.906 3.556 unlocked) (layer "F.SilkS"))
    (fp_text value "LIN FM LVL" (at 0 4.826 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.604 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 55 "/LIN_CV") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(J4-PadT)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 69.088 50.927 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R29" (at -3.048 0.127) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(C12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 60.96 78.359 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.6905 0 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 46 "/EXP_CV") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(R11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 61.595 49.276 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at -3.302 0.889) (layer "B.SilkS"))
    (fp_text value "10p" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 65.024 78.359 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -2.667 0 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 27 "/CV1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(R11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 37.465 49.53)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.651) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "VSS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 53.848 23.241 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R47" (at -3.302 -0.254) (layer "B.SilkS"))
    (fp_text value "150K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 22 "Net-(D5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 53.848 25.273 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R49" (at -3.302 -0.254) (layer "B.SilkS"))
    (fp_text value "1.5K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 74 "Net-(R49-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.769 62.23 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -3.175 -0.127) (layer "B.SilkS"))
    (fp_text value "1M" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 61.595 47.244 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at -3.302 0.381) (layer "B.SilkS"))
    (fp_text value "1M" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 12 "Net-(C11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 46.736 29.337 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R48" (at 3.048 -0.254 90) (layer "B.SilkS"))
    (fp_text value "22K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 22 "Net-(D5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 62.992 78.359 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 2.6905 0 90) (layer "B.SilkS"))
    (fp_text value "3M3" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 48 "/FINE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(R11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 54.864 70.993 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 3.175 0) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(C4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 55 "/LIN_CV") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.896 78.359 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -2.6905 0.127 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 25 "/CV2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(R11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 57.15 18.923 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R46" (at -3.302 0 90) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 39 "/TRIANGLE") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 37.084 22.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R43" (at 0 -1.778 90) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 41 "/SQUARE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 70 "Net-(R39-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "B.Cu")
    (tedit 58641739)
    (at 56.769 64.262 180)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -2.667 0) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85) (layer "B.Fab"))
    (pad "1" smd rect (at -1.05 0 180) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 180) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 69.596 44.196)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -2.667 0.762 180) (layer "B.SilkS"))
    (fp_text value "220p" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 63.5 53.213 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at -2.667 3.556) (layer "B.SilkS"))
    (fp_text value "LM311" (at 0 -3.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "VSS") (pinfunction "GND") (pintype "passive"))
    (pad "2" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C12-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R24-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "VSS") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "VCC") (pinfunction "BAL") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "VCC") (pinfunction "STRB") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C11-Pad1)") (pintype "open_collector"))
    (pad "8" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "VCC") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "B.Cu")
    (tedit 58641739)
    (at 58.012 50.927)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at -2.894 -0.127) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85) (layer "B.Fab"))
    (pad "1" smd rect (at -1.05 0) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "Net-(C11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(C11-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "B.Cu")
    (tedit 5A3D4994)
    (at 70.993 76.073 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV6" (at -8.509 -0.381 180) (layer "B.SilkS"))
    (fp_text value "220K" (at -2.54 -3.67 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 -0.005 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "-12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(R8-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+12V") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 54.864 66.929 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 2.794 -0.127) (layer "B.SilkS"))
    (fp_text value "100p" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:SOT457+thermco_resistor" (layer "B.Cu")
    (tedit 5D9F72B0)
    (at 52.832 61.849)
    (descr "SC-74, 6 Pin (https://www.nxp.com/docs/en/package-information/SOT457.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SC-74 SO")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at -1.778 2.54) (layer "B.SilkS"))
    (fp_text value "thermally_coupled_transistor_pair" (at 0 -3.81) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.1375 0.95) (size 1.425 0.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R19-Pad1)") (pinfunction "E1") (pintype "input"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.425 0.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D1-Pad2)") (pinfunction "B1") (pintype "input"))
    (pad "3" smd roundrect (at -1.1375 -0.95) (size 1.425 0.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C5-Pad1)") (pinfunction "C2") (pintype "output"))
    (pad "4" smd roundrect (at 1.1375 -0.95) (size 1.425 0.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R19-Pad1)") (pinfunction "E2") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 0) (size 1.425 0.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "B2") (pintype "input"))
    (pad "6" smd roundrect (at 1.1375 0.95) (size 1.425 0.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C4-Pad2)") (pinfunction "C1") (pintype "output"))
    (pad "7" thru_hole circle (at 0 2.54) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "8" thru_hole circle (at 0 -2.54) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SC-74-6_1.5x2.9mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 34.925 63.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 3 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 44 "Net-(J11-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 36.195 76.2 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 1.25 3.75 90) (layer "B.SilkS"))
    (fp_text value "22U 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "-12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 65.786 40.259 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.794 -0.254) (layer "B.SilkS"))
    (fp_text value "50K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 45 "Net-(R1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.769 60.071)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 3.175 0.127) (layer "B.SilkS"))
    (fp_text value "1M" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 58 "Net-(R19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 17 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 69.088 54.991 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at -3.048 0.127) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 62 "Net-(R24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 63 "Net-(R24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 66.167 72.263)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 3.175 0.127) (layer "B.SilkS"))
    (fp_text value "47K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 52 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 43.053 60.706 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "47p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "/SYNC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 66.548 35.433 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R42" (at 0.127 -1.651 90) (layer "B.SilkS"))
    (fp_text value "150K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(C13-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 73 "Net-(R42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "B.Cu")
    (tedit 58641739)
    (at 54.61 34.925 180)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 2.794 0) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85) (layer "B.Fab"))
    (pad "1" smd rect (at -1.05 0 180) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "Net-(D3-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 180) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 48.26 22.733 180)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at -3.048 5.588 90) (layer "B.SilkS"))
    (fp_text value "TL074" (at 0 -5.28) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(C13-Pad1)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C13-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "+12V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 -1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D5-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 -2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(R49-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 -3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(R50-Pad2)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(R41-Pad2)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 -2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(R37-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 -1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(R31-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R33-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(R39-Pad2)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 42.672 22.225)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R34" (at -3.048 0) (layer "B.SilkS"))
    (fp_text value "470K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 66 "Net-(R31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 65.786 42.291 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at -3.302 0) (layer "B.SilkS"))
    (fp_text value "5K6" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 59 "Net-(R22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 5 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 42.672 29.083)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R44" (at -3.302 0) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 37 "/SAW") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 72 "Net-(R41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 53.848 29.337)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R51" (at 3.302 0) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 75 "Net-(R50-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 35 "/SINE") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 54.864 68.961 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 3.175 0) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 58 "Net-(R19-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 36.195 66.08 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 1.25 3.75 90) (layer "B.SilkS"))
    (fp_text value "22U 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 55.118 18.923 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R45" (at 3.302 0 90) (layer "B.SilkS"))
    (fp_text value "200K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(C13-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(C13-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 54.61 43.053)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at -3.048 0) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 60 "Net-(R23-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 61 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 58.547 66.421)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 2.667 -0.508) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "VSS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 54.61 38.989 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R30" (at 3.048 0) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 19 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R27-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 69.596 47.498 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 2.4 90) (layer "B.SilkS"))
    (fp_text value "MMBFJ111" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C5-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C5-Pad2)") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C11-Pad2)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 54.864 73.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -3.048 0.127) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 56 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 60.198 41.529 180)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -1.27 5.28) (layer "B.SilkS"))
    (fp_text value "TL074" (at 0 -5.28) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C5-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C5-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(R1-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "+12V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 -1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C5-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 -2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(R24-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 -3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(R24-Pad1)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(R27-Pad1)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 -2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R23-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 -1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D3-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D3-Pad2)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 42.672 17.907)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R39" (at -3.048 0 180) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 70 "Net-(R39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 71 "Net-(R39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 69.088 52.959)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R28" (at 3.048 -0.127) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 1 "/SYNC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 57.912 48.895 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 3.175 0) (layer "B.SilkS"))
    (fp_text value "33K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 12 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 10 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 42.672 20.076 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R33" (at 3.048 0.01) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 68 "Net-(R33-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R27-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 57.912 54.991)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at -3.302 0) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 13 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 57.912 52.959)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -3.175 0) (layer "B.SilkS"))
    (fp_text value "47p" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 37.465 53.34 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at -2.794 3.302) (layer "B.SilkS"))
    (fp_text value "L79L12_SO8" (at 0 -3.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "VSS") (pinfunction "OUT") (pintype "power_out"))
    (pad "2" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J11-Pad1)") (pinfunction "IN") (pintype "power_in"))
    (pad "3" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J11-Pad1)") (pinfunction "IN") (pintype "passive"))
    (pad "4" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 78 "unconnected-(U4-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J11-Pad1)") (pinfunction "IN") (pintype "passive"))
    (pad "7" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J11-Pad1)") (pinfunction "IN") (pintype "passive"))
    (pad "8" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 79 "unconnected-(U4-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 37.084 25.781 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R36" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 36.195 82.55 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -1.397 -1.651 90) (layer "B.SilkS"))
    (fp_text value "7.5K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 5 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 51 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 42.672 27.031)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R41" (at -3.048 0.02) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 69 "Net-(R37-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 72 "Net-(R41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "B.Cu")
    (tedit 58641739)
    (at 50.8 29.337 90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at -2.54 0 90) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.05 0 90) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 90) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 58.232 35.687 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 34.925 85.598)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R32" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 67 "/PW") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 66 "Net-(R31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 28.829 49.53 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 65.786 38.227)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.667 0.889) (layer "B.SilkS"))
    (fp_text value "70K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 45 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 10 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 48.768 16.637 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 41.455 82.55 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "7.5K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 54 "Net-(R14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 3 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 67.056 78.359 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 2.6905 0 90) (layer "B.SilkS"))
    (fp_text value "470K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 50 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "B.Cu")
    (tedit 5A3D4994)
    (at 70.993 30.597 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV11" (at 1.143 -3.429 90) (layer "B.SilkS"))
    (fp_text value "220K" (at -2.54 -3.67 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 -0.005 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(R42-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "B.Cu")
    (tedit 58641739)
    (at 48.768 29.337 90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at -2.794 0 90) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.05 0 90) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 90) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "Net-(D5-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 53.086 18.923 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -3.302 0 90) (layer "B.SilkS"))
    (fp_text value "47p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 37.084 18.669 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R40" (at -0.227064 -1.778 90) (layer "B.SilkS"))
    (fp_text value "4.7K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 70 "Net-(R39-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 53.848 27.305 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R50" (at -3.302 -0.254) (layer "B.SilkS"))
    (fp_text value "15K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 74 "Net-(R49-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 75 "Net-(R50-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 54.61 41.021 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R35" (at 3.048 0) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 19 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 21 "Net-(D4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 60.579 70.231 180)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at -2.667 3.302) (layer "B.SilkS"))
    (fp_text value "OPA2134" (at 0 -3.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.575 1.905 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(R18-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -2.575 0.635 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(R11-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.575 -0.635 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R10-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.575 -1.905 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "VSS") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.575 -1.905 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(R16-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.575 -0.635 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C4-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at 2.575 0.635 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad1)") (pintype "output"))
    (pad "8" smd roundrect (at 2.575 1.905 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "VCC") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 54.61 45.085 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R27" (at 3.048 0) (layer "B.SilkS"))
    (fp_text value "220K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 61 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 58.928 78.359 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 2.6905 -0.127 90) (layer "B.SilkS"))
    (fp_text value "220K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 49 "/COARSE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(R11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "B.Cu")
    (tedit 58641739)
    (at 54.61 36.957 180)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 2.794 0) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0.1 -1.9) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.85) (layer "B.Fab"))
    (pad "1" smd rect (at -1.05 0 180) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 180) (size 0.6 0.45) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 66.167 70.231)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 3.175 0) (layer "B.SilkS"))
    (fp_text value "33K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 53 "Net-(R11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "B.Cu")
    (tedit 5A3D4994)
    (at 45.72 41.793 -90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV10" (at 0.498 -3.302 90) (layer "B.SilkS"))
    (fp_text value "100K" (at -2.54 -3.67 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 -0.005 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(R23-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R24-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "unconnected-(RV10-Pad3)") (pinfunction "3") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "B.Cu")
    (tedit 5A3D4994)
    (at 70.993 59.553 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV8" (at -6.233 -3.429 90) (layer "B.SilkS"))
    (fp_text value "25K" (at -2.54 -3.67 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 -0.005 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(R18-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(R11-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "unconnected-(RV8-Pad3)") (pinfunction "3") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 66.167 68.072 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at -3.175 0) (layer "B.SilkS"))
    (fp_text value "22K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 57 "Net-(R18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "B.Cu")
    (tedit 5A3D4994)
    (at 70.993 19.929 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV9" (at -5.344 -3.302 90) (layer "B.SilkS"))
    (fp_text value "220K" (at -2.54 -3.67 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 -0.005 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(R22-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R23-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 60.833 85.598 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R31" (at -0.381 -1.651) (layer "B.SilkS"))
    (fp_text value "180K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 65 "/PWM") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 66 "Net-(R31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:PinHeader_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 21.5773 76.1619)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at 0.6477 5.8801) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.2446 -16.2052) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J11-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J11-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J11-Pad10)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J11-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 43.561 32.766 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R38" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "50K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 21 "Net-(D4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 16 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 34.925 78.74)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 43 "Net-(J11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 5 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 42.672 25.019)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R37" (at -3.048 0) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 69 "Net-(R37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 28.575 53.34 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "vco.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at -3.175 3.302) (layer "B.SilkS"))
    (fp_text value "L78L12_SO8" (at 0 -3.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "VCC") (pinfunction "OUT") (pintype "power_out"))
    (pad "2" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "4" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "unconnected-(U3-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 80 "unconnected-(U3-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "7" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J11-Pad10)") (pinfunction "IN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 75.565 114.3) (end 17.78 12.7) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_rect (start 17.78 116.84) (end 78.38 245.34) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "thismatters/vco/v1" (at 19.685 105.41 -90) (layer "B.SilkS"))
  (gr_text "red\nline" (at 29.845 76.1919) (layer "B.SilkS"))
  (gr_text "soft" (at 48.08 187.44) (layer "F.SilkS"))
  (gr_text "thismatters/vco/v1" (at 76.655 232.525 90) (layer "F.SilkS"))
  (gr_text "vco" (at 48.08 240.03) (layer "F.SilkS"))
  (gr_text "hard" (at 48.08 177.28) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.56 245.86)
        (xy 17.6 245.86)
        (xy 17.6 116.32)
        (xy 78.56 116.32)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.565 114.3)
        (xy 17.78 114.3)
        (xy 17.78 12.7)
        (xy 75.565 12.7)
      )
    )
  )
)
