<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="20.681" y2="0" width="0" layer="20"/>
<wire x1="20.681" y1="0" x2="20.681" y2="28.88" width="0" layer="20"/>
<wire x1="20.681" y1="28.88" x2="2.54" y2="28.88" width="0" layer="20"/>
<wire x1="2.54" y1="28.88" x2="2.54" y2="0" width="0" layer="20"/>
<text>LM317</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220-ADJ">
</package>
</packages>
</library>
<library name="$RJPO8VP">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="TT5D10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 10 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LM317" library="SparkFun" package="TO220-ADJ" value="LM317"/>
<element name="R1" library="$RJPO8VP" package="0207/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="$RJPO8VP" package="0207/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="$RJPO8VP" package="C050-024X044" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="$RJPO8VP" package="TT5D10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V-OUT" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V-IN" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="LM317" pad="OUT"/>
<contactref element="R1" pad="1"/>
<contactref element="V-OUT" pad="1"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="V-IN" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="LM317" pad="IN"/>
</signal>
<signal name="N$2">
<contactref element="LM317" pad="ADJ"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
