(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 261)
    (zones 0)
    (modules 46)
    (nets 67)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.8128)
    (user_trace_width 0.4064)
    (user_trace_width 0.8128)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.651 1.651)
    (pad_drill 0.889)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U$1-PadJ3_20)")
  (net 2 "Net-(U$1-PadJ3_18)")
  (net 3 "Net-(U$1-PadJ3_17)")
  (net 4 "Net-(U$1-PadJ3_16)")
  (net 5 "Net-(U$1-PadJ3_13)")
  (net 6 "Net-(U$1-PadJ3_10)")
  (net 7 "Net-(U$1-PadJ3_9)")
  (net 8 "Net-(U$1-PadJ3_7)")
  (net 9 "Net-(U$1-PadJ3_5)")
  (net 10 "Net-(U$1-PadJ3_4)")
  (net 11 "Net-(U$1-PadJ2_9)")
  (net 12 "Net-(U$1-PadJ2_8)")
  (net 13 "Net-(U$1-PadJ2_7)")
  (net 14 "Net-(U$1-PadJ2_4)")
  (net 15 "Net-(U$1-PadJ2_3)")
  (net 16 "Net-(U$1-PadJ1_20)")
  (net 17 "Net-(U$1-PadJ1_19)")
  (net 18 "Net-(U$1-PadJ1_18)")
  (net 19 "Net-(U$1-PadJ1_17)")
  (net 20 "Net-(CHAN5OUT1-Pad1)")
  (net 21 "Net-(CHAN1OUT1-Pad1)")
  (net 22 "Net-(CHAN1OUT1-Pad2)")
  (net 23 "Net-(A1-Pad16)")
  (net 24 "Net-(A1-Pad15)")
  (net 25 "Net-(A1-Pad30)")
  (net 26 "Net-(A1-Pad14)")
  (net 27 "Net-(A1-Pad29)")
  (net 28 "Net-(A1-Pad13)")
  (net 29 "Net-(A1-Pad28)")
  (net 30 "Net-(A1-Pad12)")
  (net 31 "Net-(A1-Pad27)")
  (net 32 "Net-(A1-Pad11)")
  (net 33 "Net-(A1-Pad26)")
  (net 34 "Net-(A1-Pad10)")
  (net 35 "Net-(A1-Pad25)")
  (net 36 "Net-(A1-Pad9)")
  (net 37 "Net-(A1-Pad24)")
  (net 38 "Net-(A1-Pad8)")
  (net 39 "Net-(A1-Pad23)")
  (net 40 "Net-(A1-Pad7)")
  (net 41 "Net-(A1-Pad22)")
  (net 42 "Net-(A1-Pad6)")
  (net 43 "Net-(A1-Pad21)")
  (net 44 "Net-(A1-Pad5)")
  (net 45 "Net-(A1-Pad20)")
  (net 46 "Net-(A1-Pad4)")
  (net 47 "Net-(A1-Pad19)")
  (net 48 "Net-(A1-Pad3)")
  (net 49 "Net-(A1-Pad18)")
  (net 50 "Net-(A1-Pad2)")
  (net 51 "Net-(A1-Pad17)")
  (net 52 "Net-(A1-Pad1)")
  (net 53 "Net-(A1-Pad31)")
  (net 54 "Net-(A1-Pad32)")
  (net 55 "Net-(CHAN2OUT1-Pad1)")
  (net 56 "Net-(CHAN3OUT1-Pad1)")
  (net 57 "Net-(CHAN4OUT1-Pad1)")
  (net 58 "Net-(CHAN6OUT1-Pad1)")
  (net 59 "Net-(CHAN7OUT1-Pad1)")
  (net 60 "Net-(CHAN8OUT1-Pad1)")
  (net 61 "Net-(+23V1-Pad1)")
  (net 62 "Net-(-23V1-Pad1)")
  (net 63 "Net-(+15cap+1-Pad1)")
  (net 64 "Net-(+15capG1-Pad1)")
  (net 65 "Net-(-15cap-1-Pad1)")
  (net 66 "Net-(5Vcap+1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(+15cap+1-Pad1)")
    (add_net "Net-(+15capG1-Pad1)")
    (add_net "Net-(+23V1-Pad1)")
    (add_net "Net-(-15cap-1-Pad1)")
    (add_net "Net-(-23V1-Pad1)")
    (add_net "Net-(5Vcap+1-Pad1)")
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad29)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad31)")
    (add_net "Net-(A1-Pad32)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(CHAN1OUT1-Pad1)")
    (add_net "Net-(CHAN1OUT1-Pad2)")
    (add_net "Net-(CHAN2OUT1-Pad1)")
    (add_net "Net-(CHAN3OUT1-Pad1)")
    (add_net "Net-(CHAN4OUT1-Pad1)")
    (add_net "Net-(CHAN5OUT1-Pad1)")
    (add_net "Net-(CHAN6OUT1-Pad1)")
    (add_net "Net-(CHAN7OUT1-Pad1)")
    (add_net "Net-(CHAN8OUT1-Pad1)")
    (add_net "Net-(U$1-PadJ1_17)")
    (add_net "Net-(U$1-PadJ1_18)")
    (add_net "Net-(U$1-PadJ1_19)")
    (add_net "Net-(U$1-PadJ1_20)")
    (add_net "Net-(U$1-PadJ2_3)")
    (add_net "Net-(U$1-PadJ2_4)")
    (add_net "Net-(U$1-PadJ2_7)")
    (add_net "Net-(U$1-PadJ2_8)")
    (add_net "Net-(U$1-PadJ2_9)")
    (add_net "Net-(U$1-PadJ3_10)")
    (add_net "Net-(U$1-PadJ3_13)")
    (add_net "Net-(U$1-PadJ3_16)")
    (add_net "Net-(U$1-PadJ3_17)")
    (add_net "Net-(U$1-PadJ3_18)")
    (add_net "Net-(U$1-PadJ3_20)")
    (add_net "Net-(U$1-PadJ3_4)")
    (add_net "Net-(U$1-PadJ3_5)")
    (add_net "Net-(U$1-PadJ3_7)")
    (add_net "Net-(U$1-PadJ3_9)")
  )
  (module dacBoard:AMP_227161 (layer Bottom) (tedit 0)
    (at 156.21 16.51 180)
    (descr "<b>JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC</b><p>\nSource: amp_227161.pdf")
    (fp_text reference CHAN3OUT1 (at -6.985 -8.89) (layer B.SilkS))
    (fp_text value ?2271611- (at -0.635 -8.89) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "Net-(CHAN3OUT1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module randomfootprints:custompuad2 (layer Top) (tedit 5D0BE152)
    (at 212.09 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompuad2 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.81 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompuad2 (layer Top) (tedit 5D0BE152)
    (at 186.69 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompuad2 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.81 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompuad2 (layer Top) (tedit 5D0BE152)
    (at 161.29 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompuad2 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.81 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompuad2 (layer Top) (tedit 5D0BE152)
    (at 135.89 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompuad2 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.81 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompuad2 (layer Top) (tedit 5D0BE152)
    (at 110.49 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompuad2 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.81 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompuad2 (layer Top) (tedit 5D0BE152)
    (at 85.09 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompuad2 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.81 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompuad2 (layer Top) (tedit 5D0BE152)
    (at 59.69 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompuad2 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.81 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompuad2 (layer Top) (tedit 5D0BE152)
    (at 34.29 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompuad2 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.81 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompad1 (layer Top) (tedit 5D0BE0C0)
    (at 24.13 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompad1 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompad1 (layer Top) (tedit 5D0BE0C0)
    (at 49.53 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompad1 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompad1 (layer Top) (tedit 5D0BE0C0)
    (at 74.93 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompad1 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompad1 (layer Top) (tedit 5D0BE0C0)
    (at 100.33 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompad1 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompad1 (layer Top) (tedit 5D0BE0C0)
    (at 125.73 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompad1 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompad1 (layer Top) (tedit 5D0BE0C0)
    (at 151.13 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompad1 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 5.08) (layers Top F.Paste F.Mask))
  )
  (module randomfootprints:custompad1 (layer Top) (tedit 5D0BE0C0)
    (at 176.53 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompad1 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 5.08) (layers Top F.Paste F.Mask))
  )
  (module dacBoard:AMP_227161 (layer Bottom) (tedit 0)
    (at 207.01 16.51 180)
    (descr "<b>JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC</b><p>\nSource: amp_227161.pdf")
    (fp_text reference CHAN1OUT1 (at -6.985 -8.89) (layer B.SilkS))
    (fp_text value ?2271611- (at -0.635 -8.89) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(CHAN1OUT1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module randomfootprints:custompad1 (layer Top) (tedit 5D0BE0C0)
    (at 201.93 16.51)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value custompad1 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 5.08) (layers Top F.Paste F.Mask))
  )
  (module dacBoard:TO220S (layer Top) (tedit 0)
    (at 143.51 97.79 180)
    (descr "<b>VOLTAGE REGULATOR</b>")
    (fp_text reference DVDD_REG1 (at -5.08 5.9182 180) (layer F.SilkS))
    (fp_text value LT1084CT (at -5.08 7.62 180) (layer F.Fab))
    (fp_text user 3 (at 1.905 3.81 180) (layer F.Fab))
    (fp_text user 2 (at -0.635 3.81 180) (layer F.Fab))
    (fp_text user 1 (at -3.175 3.81 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 2.54 2.54 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 "Net-(5Vcap+1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole oval (at -2.54 2.54 270) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 "Net-(+23V1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 196.85 109.22 90)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference -capG1 (at -0.762 -1.016 90) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 199.39 109.22)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference -cap-1 (at 2.54 1.27) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 62 "Net-(-23V1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 180.34 114.3)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference +15capG1 (at -8.89 2.54) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 5D0BBEB2)
    (at 163.83 119.38)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference GND1 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 143.51 104.14 180)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference 5VcapG1 (at -1.27 0 180) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 140.97 104.14)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference 5Vcap+1 (at -2.54 3.81 90) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 66 "Net-(5Vcap+1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 5D0BBEBE)
    (at 199.39 118.11)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference -23V1 (at 1.27 0) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 62 "Net-(-23V1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 208.28 95.25 180)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference -15capG1 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 5D0BBDB3)
    (at 156.21 101.6)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference +23V1 (at -1.27 3.81 90) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 61 "Net-(+23V1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 182.88 114.3 180)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference +15cap+1 (at -2.54 -7.62 270) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 63 "Net-(+15cap+1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 163.83 106.68 180)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference +capG1 (at 1.27 -2.54 180) (layer F.SilkS))
    (fp_text value +capG (at 0 -0.6 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 5D0BBEA6)
    (at 147.32 118.11 180)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference ardG1 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 5D0BBE9A)
    (at 139.7 118.11)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference ard+1 (at -0.762 2.54) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 66 "Net-(5Vcap+1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 161.29 106.68)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference +cap+1 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 61 "Net-(+23V1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:AMP_227161 (layer Bottom) (tedit 0)
    (at 105.41 16.51 180)
    (descr "<b>JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC</b><p>\nSource: amp_227161.pdf")
    (fp_text reference CHAN5OUT1 (at -6.985 -8.89) (layer B.SilkS))
    (fp_text value ?2271611- (at -0.635 -8.89) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(CHAN5OUT1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module Module:Arduino_UNO_R3 (layer Bottom) (tedit 58AB60FC)
    (at 102.87 88.9 90)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (fp_text reference A1 (at 1.27 3.81 -90) (layer B.SilkS))
    (fp_text value Arduino_UNO_R3 (at 0 -22.86 90) (layer B.Fab))
    (fp_text user %R (at 0 -20.32 -90) (layer B.Fab))
    (pad 16 thru_hole oval (at 33.02 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad16)"))
    (pad 15 thru_hole oval (at 35.56 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad15)"))
    (pad 30 thru_hole oval (at -4.06 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad30)"))
    (pad 14 thru_hole oval (at 35.56 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad14)"))
    (pad 29 thru_hole oval (at -1.52 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad29)"))
    (pad 13 thru_hole oval (at 33.02 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad13)"))
    (pad 28 thru_hole oval (at 1.02 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-Pad28)"))
    (pad 12 thru_hole oval (at 30.48 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(A1-Pad12)"))
    (pad 27 thru_hole oval (at 3.56 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(A1-Pad27)"))
    (pad 11 thru_hole oval (at 27.94 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(A1-Pad11)"))
    (pad 26 thru_hole oval (at 6.1 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(A1-Pad26)"))
    (pad 10 thru_hole oval (at 25.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(A1-Pad10)"))
    (pad 25 thru_hole oval (at 8.64 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(A1-Pad25)"))
    (pad 9 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(A1-Pad9)"))
    (pad 24 thru_hole oval (at 11.18 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(A1-Pad24)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(A1-Pad8)"))
    (pad 23 thru_hole oval (at 13.72 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(A1-Pad23)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(A1-Pad7)"))
    (pad 22 thru_hole oval (at 17.78 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(A1-Pad22)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(A1-Pad6)"))
    (pad 21 thru_hole oval (at 20.32 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(A1-Pad21)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(A1-Pad5)"))
    (pad 20 thru_hole oval (at 22.86 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(A1-Pad20)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(A1-Pad4)"))
    (pad 19 thru_hole oval (at 25.4 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(A1-Pad19)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(A1-Pad3)"))
    (pad 18 thru_hole oval (at 27.94 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(A1-Pad18)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(A1-Pad2)"))
    (pad 17 thru_hole oval (at 30.48 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(A1-Pad17)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(A1-Pad1)"))
    (pad 31 thru_hole oval (at -6.6 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(A1-Pad31)"))
    (pad 32 thru_hole oval (at -9.14 -48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(A1-Pad32)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_UNO_R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 5D0BBE8F)
    (at 147.32 111.76)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference isoG1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 5D0BBE7A)
    (at 139.7 111.76)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference iso+1 (at 1.27 2.54) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 66 "Net-(5Vcap+1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:DAC8718PACKAGE (layer Bottom) (tedit 5D09647E)
    (at 161.2011 80.2386 180)
    (fp_text reference U$1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value DAC8718 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text user value (at -40.64 -10.795 180) (layer B.Fab))
    (fp_text user >Name (at -40.64 36.83 180) (layer B.SilkS))
    (pad J3_20 thru_hole circle (at 35.56 2.54 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(U$1-PadJ3_20)") (solder_mask_margin 0.1016))
    (pad J3_19 thru_hole circle (at 33.02 2.54) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "Net-(A1-Pad20)") (solder_mask_margin 0.1016))
    (pad J3_18 thru_hole circle (at 35.56 5.08 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(U$1-PadJ3_18)") (solder_mask_margin 0.1016))
    (pad J3_17 thru_hole circle (at 33.02 5.08) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(U$1-PadJ3_17)") (solder_mask_margin 0.1016))
    (pad J3_16 thru_hole circle (at 35.56 7.62 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(U$1-PadJ3_16)") (solder_mask_margin 0.1016))
    (pad J3_15 thru_hole circle (at 33.02 7.62) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "Net-(A1-Pad19)") (solder_mask_margin 0.1016))
    (pad J3_14 thru_hole circle (at 35.56 10.16 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(A1-Pad27)") (solder_mask_margin 0.1016))
    (pad J3_13 thru_hole circle (at 33.02 10.16) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(U$1-PadJ3_13)") (solder_mask_margin 0.1016))
    (pad J3_12 thru_hole circle (at 35.56 12.7 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(A1-Pad26)") (solder_mask_margin 0.1016))
    (pad J3_11 thru_hole circle (at 33.02 12.7) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "Net-(A1-Pad18)") (solder_mask_margin 0.1016))
    (pad J3_10 thru_hole circle (at 35.56 15.24 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(U$1-PadJ3_10)") (solder_mask_margin 0.1016))
    (pad J3_9 thru_hole circle (at 33.02 15.24) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(U$1-PadJ3_9)") (solder_mask_margin 0.1016))
    (pad J3_8 thru_hole circle (at 35.56 17.78 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(A1-Pad25)") (solder_mask_margin 0.1016))
    (pad J3_7 thru_hole circle (at 33.02 17.78) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(U$1-PadJ3_7)") (solder_mask_margin 0.1016))
    (pad J3_6 thru_hole circle (at 35.56 20.32 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(A1-Pad24)") (solder_mask_margin 0.1016))
    (pad J3_5 thru_hole circle (at 33.02 20.32) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(U$1-PadJ3_5)") (solder_mask_margin 0.1016))
    (pad J3_4 thru_hole circle (at 35.56 22.86 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(U$1-PadJ3_4)") (solder_mask_margin 0.1016))
    (pad J3_3 thru_hole circle (at 33.02 22.86) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(A1-Pad17)") (solder_mask_margin 0.1016))
    (pad J3_2 thru_hole circle (at 35.56 25.4 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(A1-Pad23)") (solder_mask_margin 0.1016))
    (pad J3_1 thru_hole circle (at 33.02 25.4) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "Net-(A1-Pad22)") (solder_mask_margin 0.1016))
    (pad J2_10 thru_hole circle (at 5.08 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 "Net-(5Vcap+1-Pad1)") (solder_mask_margin 0.1016))
    (pad J2_9 thru_hole circle (at 5.08 -2.54 270) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(U$1-PadJ2_9)") (solder_mask_margin 0.1016))
    (pad J2_8 thru_hole circle (at 2.54 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(U$1-PadJ2_8)") (solder_mask_margin 0.1016))
    (pad J2_7 thru_hole circle (at 2.54 -2.54 270) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(U$1-PadJ2_7)") (solder_mask_margin 0.1016))
    (pad J2_6 thru_hole circle (at 0 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
    (pad J2_5 thru_hole circle (at 0 -2.54 270) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
    (pad J2_4 thru_hole circle (at -2.54 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(U$1-PadJ2_4)") (solder_mask_margin 0.1016))
    (pad J2_3 thru_hole circle (at -2.54 -2.54 270) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(U$1-PadJ2_3)") (solder_mask_margin 0.1016))
    (pad J2_2 thru_hole circle (at -5.08 0 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(-15cap-1-Pad1)") (solder_mask_margin 0.1016))
    (pad J2_1 thru_hole circle (at -5.08 -2.54 270) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "Net-(+15cap+1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_20 thru_hole circle (at -33.02 1.27 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(U$1-PadJ1_20)") (solder_mask_margin 0.1016))
    (pad J1_19 thru_hole circle (at -35.56 1.27) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(U$1-PadJ1_19)") (solder_mask_margin 0.1016))
    (pad J1_18 thru_hole circle (at -33.02 3.81 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(U$1-PadJ1_18)") (solder_mask_margin 0.1016))
    (pad J1_17 thru_hole circle (at -35.56 3.81) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(U$1-PadJ1_17)") (solder_mask_margin 0.1016))
    (pad J1_16 thru_hole circle (at -33.02 6.35 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 "Net-(CHAN8OUT1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_15 thru_hole circle (at -35.56 6.35) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad J1_14 thru_hole circle (at -33.02 8.89 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 "Net-(CHAN7OUT1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_13 thru_hole circle (at -35.56 8.89) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad J1_12 thru_hole circle (at -33.02 11.43 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 "Net-(CHAN6OUT1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_11 thru_hole circle (at -35.56 11.43) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad J1_10 thru_hole circle (at -33.02 13.97 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(CHAN5OUT1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_9 thru_hole circle (at -35.56 13.97) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad J1_8 thru_hole circle (at -33.02 16.51 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 "Net-(CHAN4OUT1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_7 thru_hole circle (at -35.56 16.51) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad J1_6 thru_hole circle (at -33.02 19.05 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 "Net-(CHAN3OUT1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_5 thru_hole circle (at -35.56 19.05) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad J1_4 thru_hole circle (at -33.02 21.59 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 "Net-(CHAN2OUT1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_3 thru_hole circle (at -35.56 21.59) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad J1_2 thru_hole circle (at -33.02 24.13 180) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(CHAN1OUT1-Pad1)") (solder_mask_margin 0.1016))
    (pad J1_1 thru_hole circle (at -35.56 24.13) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:AMP_227161 (layer Bottom) (tedit 0)
    (at 29.21 16.51 180)
    (descr "<b>JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC</b><p>\nSource: amp_227161.pdf")
    (fp_text reference CHAN8OUT1 (at -6.985 -8.89) (layer B.SilkS))
    (fp_text value ?2271611- (at -0.635 -8.89) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 "Net-(CHAN8OUT1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:AMP_227161 (layer Bottom) (tedit 0)
    (at 54.61 16.51 180)
    (descr "<b>JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC</b><p>\nSource: amp_227161.pdf")
    (fp_text reference CHAN7OUT1 (at -6.985 -8.89) (layer B.SilkS))
    (fp_text value ?2271611- (at -0.635 -8.89) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 "Net-(CHAN7OUT1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:AMP_227161 (layer Bottom) (tedit 0)
    (at 80.01 16.51 180)
    (descr "<b>JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC</b><p>\nSource: amp_227161.pdf")
    (fp_text reference CHAN6OUT1 (at -6.985 -8.89) (layer B.SilkS))
    (fp_text value ?2271611- (at -0.635 -8.89) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 "Net-(CHAN6OUT1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:AMP_227161 (layer Bottom) (tedit 0)
    (at 130.81 16.51 180)
    (descr "<b>JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC</b><p>\nSource: amp_227161.pdf")
    (fp_text reference CHAN4OUT1 (at -6.985 -8.89) (layer B.SilkS))
    (fp_text value ?2271611- (at -0.635 -8.89) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 "Net-(CHAN4OUT1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:AMP_227161 (layer Bottom) (tedit 0)
    (at 181.61 16.51 180)
    (descr "<b>JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC</b><p>\nSource: amp_227161.pdf")
    (fp_text reference CHAN2OUT1 (at -6.985 -8.89) (layer B.SilkS))
    (fp_text value ?2271611- (at -0.635 -8.89) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(CHAN1OUT1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -5.08 180) (size 1.27 1.27) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "Net-(CHAN2OUT1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:TO220S (layer Top) (tedit 0)
    (at 180.34 106.68)
    (descr "<b>VOLTAGE REGULATOR</b>")
    (fp_text reference U$3 (at -5.08 5.9182) (layer F.SilkS))
    (fp_text value LT1084CT (at -5.08 7.62) (layer F.Fab))
    (fp_text user 3 (at 1.905 3.81) (layer F.Fab))
    (fp_text user 2 (at -0.635 3.81) (layer F.Fab))
    (fp_text user 1 (at -3.175 3.81) (layer F.Fab))
    (pad 3 thru_hole oval (at 2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 "Net-(+15cap+1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole oval (at -2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 "Net-(+23V1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:TO220S (layer Top) (tedit 0)
    (at 201.93 97.79)
    (descr "<b>VOLTAGE REGULATOR</b>")
    (fp_text reference U$4 (at -5.08 5.9182) (layer F.SilkS))
    (fp_text value LT1084CT (at -5.08 7.62) (layer F.Fab))
    (fp_text user 3 (at 1.905 3.81) (layer F.Fab))
    (fp_text user 2 (at -0.635 3.81) (layer F.Fab))
    (fp_text user 1 (at -3.175 3.81) (layer F.Fab))
    (pad 3 thru_hole oval (at 2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "Net-(-15cap-1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 "Net-(-23V1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole oval (at -2.54 2.54 90) (size 3.048 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "Net-(+15capG1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module dacBoard:1,6_0,8 (layer Top) (tedit 0)
    (at 205.74 95.25 90)
    (descr "<b>THROUGH-HOLE PAD</b>")
    (fp_text reference -15cap-1 (at 1.27 0 90) (layer F.SilkS))
    (fp_text value 1,6_0,8 (at 0 -0.6 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 65 "Net-(-15cap-1-Pad1)") (solder_mask_margin 0.1016))
  )
  (gr_line (start 20.32 124.46) (end 215.9 124.46) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 124.46) (end 215.9 8.89) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 8.89) (end 20.32 8.89) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.32 8.89) (end 20.32 124.46) (layer Edge.Cuts) (width 0.15))
)
