<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>SDA</text>
<text>SCL</text>
<text>3V3</text>
<text>GND</text>
<text>RST</text>
<text>INT</text>
<text>Pesky 
Products</text>
<text>v.03a</text>
<text>18 channel
20 nm FWHM
spectrometer</text>
<text>AS72651
AS72652
AS72653</text>
<text>410 - 940 nm</text>
<text>410-940nm</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>nCS</text>
<text>SO</text>
<text>SI</text>
<text>SCK</text>
<text>I2C</text>
<text>UART</text>
<text>SDA</text>
<text>SCL</text>
<text>3V3</text>
<text>GND</text>
<text>INT</text>
<text>RST</text>
<wire x1="1.27" y1="8.89" x2="1.27" y2="0" width="0.002540625" layer="20"/>
<wire x1="1.27" y1="0" x2="19.05" y2="0" width="0.002540625" layer="20"/>
<wire x1="19.05" y1="0" x2="19.05" y2="8.89" width="0.002540625" layer="20"/>
<wire x1="1.27" y1="8.89" x2="10.16" y2="17.78" width="0" layer="20" curve="-90"/>
<wire x1="10.16" y1="17.78" x2="19.05" y2="8.89" width="0" layer="20" curve="-90"/>
<text>AS7265X</text>
</plain>
<libraries>
<library name="kris">
<packages>
<package name="AS7265X">
<description>AS7265X AMG Smart Spectral Sensor
http://ams.com/eng/Products/Spectral-Sensing/Multi-spectral-Sensing/AS7265x</description>
</package>
<package name="USON-8">
<description>uson-8 package for Macronix MX25L4006E 4 Mbit SPI Fash</description>
</package>
<package name="LUXEON-Z-ES">
<description>Luxeon Z ES flash LED by Phillips</description>
</package>
<package name="0402LED">
<description>0402 led</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_NO_SILK">
</package>
</packages>
</library>
<library name="Spark">
<packages>
<package name="R0402_B">
</package>
<package name="C0402_B">
</package>
</packages>
</library>
<library name="PWSONN6">
<packages>
<package name="HN01">
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="LED_SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="kris" package="AS7265X" value="AS7265X"/>
<element name="GND/VCC" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="GND/VCC2" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="GND/VCC3" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="R5" library="Spark" package="R0402_B" value="10 K"/>
<element name="C9" library="Spark" package="C0402_B" value="100 nF"/>
<element name="C1" library="Spark" package="C0402_B" value="10 uF"/>
<element name="C2" library="Spark" package="C0402_B" value="100 nF"/>
<element name="C3" library="Spark" package="C0402_B" value="10 uF"/>
<element name="C4" library="Spark" package="C0402_B" value="100 nF"/>
<element name="C5" library="Spark" package="C0402_B" value="10 uF"/>
<element name="R1" library="Spark" package="R0402_B" value="10 K"/>
<element name="R2" library="Spark" package="R0402_B" value="4K7"/>
<element name="R3" library="Spark" package="R0402_B" value="4K7"/>
<element name="R6" library="Spark" package="R0402_B" value="10 K"/>
<element name="R7" library="Spark" package="R0402_B" value="10 K"/>
<element name="R8" library="Spark" package="R0402_B" value="10 K"/>
<element name="U2" library="kris" package="AS7265X" value="AS72652"/>
<element name="U3" library="kris" package="AS7265X" value="AS72652"/>
<element name="U4" library="kris" package="USON-8" value="MX25L4006E"/>
<element name="C6" library="Spark" package="C0402_B" value="1 uF"/>
<element name="L3" library="kris" package="LUXEON-Z-ES" value="LUXEON-Z-ES"/>
<element name="R11" library="Spark" package="R0402_B" value="4K7"/>
<element name="R12" library="Spark" package="R0402_B" value="4K7"/>
<element name="U$7" library="PWSONN6" package="HN01" value="HN01"/>
<element name="U$8" library="PWSONN6" package="HN01" value="HN01"/>
<element name="U$1" library="PWSONN6" package="HN01" value="HN01"/>
<element name="U$2" library="PWSONN6" package="HN01" value="HN01"/>
<element name="R13" library="Spark" package="R0402_B" value="100K"/>
<element name="850NM" library="eagle-ltspice" package="LED_SML0603" value="">
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="940NM1" library="eagle-ltspice" package="LED_SML0603" value="">
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="RED" library="kris" package="0402LED" value="0402LED"/>
<element name="SJ1" library="jumper" package="SJ_2" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="GND/VCC2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U1" pad="P$16"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="P$16"/>
<contactref element="U3" pad="P$16"/>
<contactref element="U4" pad="P$4"/>
<contactref element="C6" pad="1"/>
<contactref element="L3" pad="P$3"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="GND/VCC2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="P$17"/>
<contactref element="C9" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="P$14"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U2" pad="P$14"/>
<contactref element="U2" pad="P$17"/>
<contactref element="U3" pad="P$14"/>
<contactref element="U3" pad="P$17"/>
<contactref element="U4" pad="P$8"/>
<contactref element="C6" pad="2"/>
<contactref element="U4" pad="P$7"/>
<contactref element="U4" pad="P$3"/>
<contactref element="L3" pad="P$2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="850NM" pad="A"/>
<contactref element="940NM1" pad="A"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="RED" pad="P$1"/>
</signal>
<signal name="SDA">
<contactref element="GND/VCC3" pad="1"/>
<contactref element="U1" pad="P$12"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="GND/VCC3" pad="2"/>
<contactref element="U1" pad="P$11"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="!RST">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="P$2"/>
<contactref element="GND/VCC" pad="1"/>
</signal>
<signal name="I2C_EN">
<contactref element="U1" pad="P$8"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="!INT">
<contactref element="R1" pad="1"/>
<contactref element="GND/VCC" pad="2"/>
<contactref element="U1" pad="P$13"/>
</signal>
<signal name="SCL_M">
<contactref element="U2" pad="P$9"/>
<contactref element="U3" pad="P$9"/>
<contactref element="R12" pad="1"/>
<contactref element="U1" pad="P$9"/>
</signal>
<signal name="SDA_M">
<contactref element="U2" pad="P$10"/>
<contactref element="U3" pad="P$10"/>
<contactref element="R11" pad="1"/>
<contactref element="U1" pad="P$10"/>
</signal>
<signal name="!CS">
<contactref element="U1" pad="P$6"/>
<contactref element="U4" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="SO">
<contactref element="U1" pad="P$5"/>
<contactref element="U4" pad="P$2"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="SI">
<contactref element="U1" pad="P$4"/>
<contactref element="U4" pad="P$5"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="P$3"/>
<contactref element="U4" pad="P$6"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="IND1">
<contactref element="U1" pad="P$18"/>
<contactref element="RED" pad="P$2"/>
</signal>
<signal name="DRV1">
<contactref element="U1" pad="P$15"/>
<contactref element="850NM" pad="C"/>
</signal>
<signal name="DRV3">
<contactref element="U2" pad="P$15"/>
<contactref element="940NM1" pad="C"/>
</signal>
<signal name="DRV2">
<contactref element="U3" pad="P$15"/>
<contactref element="L3" pad="P$1"/>
</signal>
<signal name="SLV2_RESN">
<contactref element="U1" pad="P$20"/>
<contactref element="U2" pad="P$2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="SLV1_RESN">
<contactref element="U1" pad="P$1"/>
<contactref element="U3" pad="P$2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R6" pad="1"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
