(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 1139)
    (no_connects 0)
    (area 14.157143 13.916999 125.842858 194.655)
    (thickness 1.6)
    (drawings 7372)
    (tracks 3841)
    (zones 0)
    (modules 522)
    (nets 301)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 2.54)
    (trace_clearance 0.15)
    (zone_clearance 0.02)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (user_via 1.2 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.2 5.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.12)
    (solder_mask_min_width 0.1524)
    (aux_axis_origin 20 189.9)
    (grid_origin 20 189.9)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(AWG1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(AWG2-Pad1)")
  (net 4 +VCC_USB_P)
  (net 5 +1V2)
  (net 6 +3V3)
  (net 7 "Net-(C22-Pad1)")
  (net 8 Va)
  (net 9 IOUT2)
  (net 10 ~IOUT2)
  (net 11 ~IOUT1)
  (net 12 IOUT1)
  (net 13 "Net-(C31-Pad1)")
  (net 14 -Va)
  (net 15 +2.88V)
  (net 16 -2.88V)
  (net 17 CH1_OFFSET)
  (net 18 CH2_OFFSET)
  (net 19 "Net-(C59-Pad2)")
  (net 20 "Net-(C59-Pad1)")
  (net 21 "Net-(C60-Pad1)")
  (net 22 "Net-(C62-Pad1)")
  (net 23 "Net-(C63-Pad2)")
  (net 24 "Net-(C63-Pad1)")
  (net 25 "Net-(C64-Pad2)")
  (net 26 "Net-(C64-Pad1)")
  (net 27 "Net-(C65-Pad2)")
  (net 28 "Net-(C65-Pad1)")
  (net 29 "Net-(C67-Pad1)")
  (net 30 "Net-(C68-Pad1)")
  (net 31 CH1_GAIN)
  (net 32 "/ADC, DAC/CH1+")
  (net 33 "Net-(C73-Pad1)")
  (net 34 "/ADC, DAC/CH1-")
  (net 35 CH1_CM)
  (net 36 "/ADC, DAC/CH2+")
  (net 37 "Net-(C81-Pad2)")
  (net 38 "Net-(C81-Pad1)")
  (net 39 "Net-(C82-Pad2)")
  (net 40 "Net-(C82-Pad1)")
  (net 41 "/ADC, DAC/CH2-")
  (net 42 CH2_CM)
  (net 43 "Net-(C88-Pad2)")
  (net 44 "Net-(C99-Pad2)")
  (net 45 A_D15_J19)
  (net 46 D15_J19)
  (net 47 A_D13_J17)
  (net 48 D13_J17)
  (net 49 A_D11_J15)
  (net 50 D11_J15)
  (net 51 A_D9_J13)
  (net 52 D9_J13)
  (net 53 A_D7_J7)
  (net 54 D7_J7)
  (net 55 A_D5_J5)
  (net 56 D5_J5)
  (net 57 A_D3_J3)
  (net 58 D3_J3)
  (net 59 A_D1_J1)
  (net 60 D1_J1)
  (net 61 A_D0_J2)
  (net 62 D0_J2)
  (net 63 A_D2_J4)
  (net 64 D2_J4)
  (net 65 A_D4_J6)
  (net 66 D4_J6)
  (net 67 A_D6_J8)
  (net 68 D6_J8)
  (net 69 +VCC_DIG)
  (net 70 A_D8_J14)
  (net 71 D8_J14)
  (net 72 A_D10_J16)
  (net 73 D10_J16)
  (net 74 A_D12_J18)
  (net 75 D12_J18)
  (net 76 A_D14_J20)
  (net 77 D14_J20)
  (net 78 "Net-(C117-Pad1)")
  (net 79 "Net-(C125-Pad2)")
  (net 80 "Net-(C127-Pad1)")
  (net 81 "Net-(C129-Pad2)")
  (net 82 "Net-(C129-Pad1)")
  (net 83 -5V)
  (net 84 "Net-(C131-Pad1)")
  (net 85 "Net-(C133-Pad2)")
  (net 86 CH2_GAIN)
  (net 87 +3.3V_PD)
  (net 88 "Net-(C139-Pad2)")
  (net 89 "/ANALOG INPUTS/CH1_VGA")
  (net 90 "Net-(C140-Pad2)")
  (net 91 "/ANALOG INPUTS/CH2_VGA")
  (net 92 D+)
  (net 93 "Net-(D18-Pad2)")
  (net 94 "Net-(D20-Pad2)")
  (net 95 "Net-(D21-Pad2)")
  (net 96 "Net-(D22-Pad2)")
  (net 97 "Net-(D23-Pad3)")
  (net 98 RE3)
  (net 99 RE4)
  (net 100 "Net-(D26-Pad3)")
  (net 101 "Net-(D27-Pad3)")
  (net 102 RE2)
  (net 103 "Net-(D29-Pad3)")
  (net 104 RE1)
  (net 105 "Net-(F1-Pad2)")
  (net 106 "Net-(L1-Pad1)")
  (net 107 "Net-(LED1-Pad2)")
  (net 108 "Net-(LED2-Pad2)")
  (net 109 "Net-(LED3-Pad2)")
  (net 110 D-)
  (net 111 "Net-(Q1-Pad2)")
  (net 112 "Net-(Q1-Pad5)")
  (net 113 "Net-(Q2-Pad2)")
  (net 114 "Net-(Q2-Pad5)")
  (net 115 FD12)
  (net 116 "Net-(R1-Pad1)")
  (net 117 FD11)
  (net 118 "Net-(R2-Pad1)")
  (net 119 FD10)
  (net 120 "Net-(R3-Pad1)")
  (net 121 FD9)
  (net 122 "Net-(R4-Pad1)")
  (net 123 FD8)
  (net 124 "Net-(R5-Pad1)")
  (net 125 "Net-(R6-Pad2)")
  (net 126 FLAGD)
  (net 127 "Net-(R7-Pad2)")
  (net 128 PA6/PKTEND)
  (net 129 "Net-(R8-Pad2)")
  (net 130 FIFOADDR1_INIT_B)
  (net 131 "Net-(R9-Pad2)")
  (net 132 FIFOADDR0)
  (net 133 "Net-(R10-Pad2)")
  (net 134 PA3)
  (net 135 LED1)
  (net 136 CH2_K)
  (net 137 CH2_GND)
  (net 138 "Net-(R16-Pad2)")
  (net 139 CH1_DC)
  (net 140 "Net-(R17-Pad2)")
  (net 141 CH2_DC)
  (net 142 LED3)
  (net 143 LED2)
  (net 144 EN_CLK)
  (net 145 "Net-(R23-Pad2)")
  (net 146 "Net-(R24-Pad2)")
  (net 147 "Net-(R25-Pad2)")
  (net 148 "Net-(R25-Pad1)")
  (net 149 "Net-(R26-Pad2)")
  (net 150 "Net-(R27-Pad2)")
  (net 151 "Net-(R27-Pad1)")
  (net 152 "Net-(R28-Pad1)")
  (net 153 "Net-(R29-Pad2)")
  (net 154 "Net-(R29-Pad1)")
  (net 155 CH1_GND)
  (net 156 CH1_K)
  (net 157 "Net-(R35-Pad1)")
  (net 158 "Net-(R36-Pad1)")
  (net 159 "Net-(R37-Pad2)")
  (net 160 "Net-(R37-Pad1)")
  (net 161 "Net-(R38-Pad1)")
  (net 162 "Net-(R39-Pad2)")
  (net 163 "Net-(R39-Pad1)")
  (net 164 "Net-(R40-Pad1)")
  (net 165 "Net-(R41-Pad2)")
  (net 166 "Net-(R104-Pad1)")
  (net 167 "Net-(R45-Pad2)")
  (net 168 "Net-(R45-Pad1)")
  (net 169 "Net-(R47-Pad2)")
  (net 170 AN_TRIG)
  (net 171 AN_TRIG_LEVEL)
  (net 172 "Net-(R51-Pad1)")
  (net 173 "Net-(R52-Pad1)")
  (net 174 IFCLK)
  (net 175 "Net-(R53-Pad1)")
  (net 176 SLWR)
  (net 177 "Net-(R54-Pad1)")
  (net 178 SLRD)
  (net 179 "Net-(R55-Pad1)")
  (net 180 CCLK)
  (net 181 "Net-(R56-Pad1)")
  (net 182 FD15)
  (net 183 "Net-(R57-Pad1)")
  (net 184 FD14)
  (net 185 "Net-(R58-Pad1)")
  (net 186 FD13)
  (net 187 "Net-(R59-Pad1)")
  (net 188 "Net-(R79-Pad2)")
  (net 189 "Net-(R80-Pad2)")
  (net 190 "Net-(R83-Pad1)")
  (net 191 "Net-(R85-Pad1)")
  (net 192 "Net-(R86-Pad1)")
  (net 193 "Net-(R107-Pad1)")
  (net 194 "Net-(R108-Pad2)")
  (net 195 "Net-(R92-Pad1)")
  (net 196 "Net-(R101-Pad2)")
  (net 197 "Net-(R102-Pad2)")
  (net 198 "Net-(R104-Pad2)")
  (net 199 "Net-(R109-Pad1)")
  (net 200 EN_PWR)
  (net 201 "Net-(R113-Pad1)")
  (net 202 V_OV)
  (net 203 V_UV)
  (net 204 "Net-(R118-Pad1)")
  (net 205 "Net-(R119-Pad1)")
  (net 206 "Net-(R121-Pad1)")
  (net 207 "Net-(R123-Pad1)")
  (net 208 "Net-(R127-Pad2)")
  (net 209 "Net-(R131-Pad1)")
  (net 210 "Net-(R133-Pad2)")
  (net 211 "Net-(R135-Pad2)")
  (net 212 "Net-(R141-Pad2)")
  (net 213 "Net-(U27-Pad49)")
  (net 214 RESERVED)
  (net 215 DORB)
  (net 216 DCLKB)
  (net 217 D0B)
  (net 218 D1B)
  (net 219 D2B)
  (net 220 D3B)
  (net 221 D4B)
  (net 222 D5B)
  (net 223 D6B)
  (net 224 D7B)
  (net 225 D8B)
  (net 226 D9B)
  (net 227 SDIN)
  (net 228 SCLK)
  (net 229 ~CS)
  (net 230 CH2_OFFSET_ADJ)
  (net 231 CH2_GAIN_ADJ)
  (net 232 CH1_OFFSET_ADJ)
  (net 233 CH1_GAIN_ADJ)
  (net 234 DPOT_SCK)
  (net 235 DPOT_CS)
  (net 236 DPOT_SI)
  (net 237 DAC_D11)
  (net 238 DAC_D10)
  (net 239 DAC_D9)
  (net 240 DAC_D8)
  (net 241 DAC_D7)
  (net 242 DAC_D6)
  (net 243 DAC_D5)
  (net 244 DAC_D4)
  (net 245 DAC_D3)
  (net 246 DAC_D2)
  (net 247 DAC_D1)
  (net 248 DAC_D0)
  (net 249 DAC_CLK)
  (net 250 DASDIN)
  (net 251 DASCLK)
  (net 252 ~DASYNC)
  (net 253 PROG_B)
  (net 254 FD5)
  (net 255 FD4)
  (net 256 FD3)
  (net 257 FD7)
  (net 258 FLAGA)
  (net 259 FLAGB)
  (net 260 SLOE)
  (net 261 DIR1)
  (net 262 DIR2)
  (net 263 FD2)
  (net 264 FD1)
  (net 265 CTL2_CSI_B)
  (net 266 FD0)
  (net 267 SUSPEND)
  (net 268 B_D14_J20)
  (net 269 B_D15_J19)
  (net 270 B_D12_J18)
  (net 271 B_D13_J17)
  (net 272 B_D10_J16)
  (net 273 B_D11_J15)
  (net 274 B_D8_J14)
  (net 275 B_D9_J13)
  (net 276 B_D7_J7)
  (net 277 B_D6_J8)
  (net 278 B_D5_J5)
  (net 279 B_D4_J6)
  (net 280 B_D2_J4)
  (net 281 B_D1_J1)
  (net 282 B_D0_J2)
  (net 283 B_D3_J3)
  (net 284 FD6)
  (net 285 "Net-(J2-Pad3)")
  (net 286 "Net-(J2-Pad4)")
  (net 287 "Net-(J2-Pad5)")
  (net 288 "Net-(J2-Pad6)")
  (net 289 "Net-(R100-Pad2)")
  (net 290 "Net-(RE1-Pad3)")
  (net 291 "Net-(RE3-Pad3)")
  (net 292 "Net-(R11-Pad2)")
  (net 293 "Net-(R12-Pad2)")
  (net 294 "Net-(R143-Pad1)")
  (net 295 AWG2_PROT)
  (net 296 AWG1_PROT)
  (net 297 "Net-(R138-Pad1)")
  (net 298 AWG2_PROTECT)
  (net 299 AWG1_PROTECT)
  (net 300 "Net-(P1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V2)
    (add_net +2.88V)
    (add_net +3.3V_PD)
    (add_net +3V3)
    (add_net +VCC_DIG)
    (add_net +VCC_USB_P)
    (add_net -2.88V)
    (add_net -5V)
    (add_net -Va)
    (add_net "/ADC, DAC/CH1+")
    (add_net "/ADC, DAC/CH1-")
    (add_net "/ADC, DAC/CH2+")
    (add_net "/ADC, DAC/CH2-")
    (add_net "/ANALOG INPUTS/CH1_VGA")
    (add_net "/ANALOG INPUTS/CH2_VGA")
    (add_net AN_TRIG)
    (add_net AN_TRIG_LEVEL)
    (add_net AWG1_PROT)
    (add_net AWG1_PROTECT)
    (add_net AWG2_PROT)
    (add_net AWG2_PROTECT)
    (add_net A_D0_J2)
    (add_net A_D10_J16)
    (add_net A_D11_J15)
    (add_net A_D12_J18)
    (add_net A_D13_J17)
    (add_net A_D14_J20)
    (add_net A_D15_J19)
    (add_net A_D1_J1)
    (add_net A_D2_J4)
    (add_net A_D3_J3)
    (add_net A_D4_J6)
    (add_net A_D5_J5)
    (add_net A_D6_J8)
    (add_net A_D7_J7)
    (add_net A_D8_J14)
    (add_net A_D9_J13)
    (add_net B_D0_J2)
    (add_net B_D10_J16)
    (add_net B_D11_J15)
    (add_net B_D12_J18)
    (add_net B_D13_J17)
    (add_net B_D14_J20)
    (add_net B_D15_J19)
    (add_net B_D1_J1)
    (add_net B_D2_J4)
    (add_net B_D3_J3)
    (add_net B_D4_J6)
    (add_net B_D5_J5)
    (add_net B_D6_J8)
    (add_net B_D7_J7)
    (add_net B_D8_J14)
    (add_net B_D9_J13)
    (add_net CCLK)
    (add_net CH1_CM)
    (add_net CH1_DC)
    (add_net CH1_GAIN)
    (add_net CH1_GAIN_ADJ)
    (add_net CH1_GND)
    (add_net CH1_K)
    (add_net CH1_OFFSET)
    (add_net CH1_OFFSET_ADJ)
    (add_net CH2_CM)
    (add_net CH2_DC)
    (add_net CH2_GAIN)
    (add_net CH2_GAIN_ADJ)
    (add_net CH2_GND)
    (add_net CH2_K)
    (add_net CH2_OFFSET)
    (add_net CH2_OFFSET_ADJ)
    (add_net CTL2_CSI_B)
    (add_net D+)
    (add_net D-)
    (add_net D0B)
    (add_net D0_J2)
    (add_net D10_J16)
    (add_net D11_J15)
    (add_net D12_J18)
    (add_net D13_J17)
    (add_net D14_J20)
    (add_net D15_J19)
    (add_net D1B)
    (add_net D1_J1)
    (add_net D2B)
    (add_net D2_J4)
    (add_net D3B)
    (add_net D3_J3)
    (add_net D4B)
    (add_net D4_J6)
    (add_net D5B)
    (add_net D5_J5)
    (add_net D6B)
    (add_net D6_J8)
    (add_net D7B)
    (add_net D7_J7)
    (add_net D8B)
    (add_net D8_J14)
    (add_net D9B)
    (add_net D9_J13)
    (add_net DAC_CLK)
    (add_net DAC_D0)
    (add_net DAC_D1)
    (add_net DAC_D10)
    (add_net DAC_D11)
    (add_net DAC_D2)
    (add_net DAC_D3)
    (add_net DAC_D4)
    (add_net DAC_D5)
    (add_net DAC_D6)
    (add_net DAC_D7)
    (add_net DAC_D8)
    (add_net DAC_D9)
    (add_net DASCLK)
    (add_net DASDIN)
    (add_net DCLKB)
    (add_net DIR1)
    (add_net DIR2)
    (add_net DORB)
    (add_net DPOT_CS)
    (add_net DPOT_SCK)
    (add_net DPOT_SI)
    (add_net EN_CLK)
    (add_net EN_PWR)
    (add_net FD0)
    (add_net FD1)
    (add_net FD10)
    (add_net FD11)
    (add_net FD12)
    (add_net FD13)
    (add_net FD14)
    (add_net FD15)
    (add_net FD2)
    (add_net FD3)
    (add_net FD4)
    (add_net FD5)
    (add_net FD6)
    (add_net FD7)
    (add_net FD8)
    (add_net FD9)
    (add_net FIFOADDR0)
    (add_net FIFOADDR1_INIT_B)
    (add_net FLAGA)
    (add_net FLAGB)
    (add_net FLAGD)
    (add_net IFCLK)
    (add_net IOUT1)
    (add_net IOUT2)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net "Net-(AWG1-Pad1)")
    (add_net "Net-(AWG2-Pad1)")
    (add_net "Net-(C117-Pad1)")
    (add_net "Net-(C125-Pad2)")
    (add_net "Net-(C127-Pad1)")
    (add_net "Net-(C129-Pad1)")
    (add_net "Net-(C129-Pad2)")
    (add_net "Net-(C131-Pad1)")
    (add_net "Net-(C133-Pad2)")
    (add_net "Net-(C139-Pad2)")
    (add_net "Net-(C140-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C59-Pad1)")
    (add_net "Net-(C59-Pad2)")
    (add_net "Net-(C60-Pad1)")
    (add_net "Net-(C62-Pad1)")
    (add_net "Net-(C63-Pad1)")
    (add_net "Net-(C63-Pad2)")
    (add_net "Net-(C64-Pad1)")
    (add_net "Net-(C64-Pad2)")
    (add_net "Net-(C65-Pad1)")
    (add_net "Net-(C65-Pad2)")
    (add_net "Net-(C67-Pad1)")
    (add_net "Net-(C68-Pad1)")
    (add_net "Net-(C73-Pad1)")
    (add_net "Net-(C81-Pad1)")
    (add_net "Net-(C81-Pad2)")
    (add_net "Net-(C82-Pad1)")
    (add_net "Net-(C82-Pad2)")
    (add_net "Net-(C88-Pad2)")
    (add_net "Net-(C99-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D21-Pad2)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(D23-Pad3)")
    (add_net "Net-(D26-Pad3)")
    (add_net "Net-(D27-Pad3)")
    (add_net "Net-(D29-Pad3)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(LED3-Pad2)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad5)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad5)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R100-Pad2)")
    (add_net "Net-(R101-Pad2)")
    (add_net "Net-(R102-Pad2)")
    (add_net "Net-(R104-Pad1)")
    (add_net "Net-(R104-Pad2)")
    (add_net "Net-(R107-Pad1)")
    (add_net "Net-(R108-Pad2)")
    (add_net "Net-(R109-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R113-Pad1)")
    (add_net "Net-(R118-Pad1)")
    (add_net "Net-(R119-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R121-Pad1)")
    (add_net "Net-(R123-Pad1)")
    (add_net "Net-(R127-Pad2)")
    (add_net "Net-(R131-Pad1)")
    (add_net "Net-(R133-Pad2)")
    (add_net "Net-(R135-Pad2)")
    (add_net "Net-(R138-Pad1)")
    (add_net "Net-(R141-Pad2)")
    (add_net "Net-(R143-Pad1)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R27-Pad1)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad1)")
    (add_net "Net-(R29-Pad1)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R35-Pad1)")
    (add_net "Net-(R36-Pad1)")
    (add_net "Net-(R37-Pad1)")
    (add_net "Net-(R37-Pad2)")
    (add_net "Net-(R38-Pad1)")
    (add_net "Net-(R39-Pad1)")
    (add_net "Net-(R39-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R40-Pad1)")
    (add_net "Net-(R41-Pad2)")
    (add_net "Net-(R45-Pad1)")
    (add_net "Net-(R45-Pad2)")
    (add_net "Net-(R47-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R51-Pad1)")
    (add_net "Net-(R52-Pad1)")
    (add_net "Net-(R53-Pad1)")
    (add_net "Net-(R54-Pad1)")
    (add_net "Net-(R55-Pad1)")
    (add_net "Net-(R56-Pad1)")
    (add_net "Net-(R57-Pad1)")
    (add_net "Net-(R58-Pad1)")
    (add_net "Net-(R59-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R79-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R80-Pad2)")
    (add_net "Net-(R83-Pad1)")
    (add_net "Net-(R85-Pad1)")
    (add_net "Net-(R86-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(R92-Pad1)")
    (add_net "Net-(RE1-Pad3)")
    (add_net "Net-(RE3-Pad3)")
    (add_net "Net-(U27-Pad49)")
    (add_net PA3)
    (add_net PA6/PKTEND)
    (add_net PROG_B)
    (add_net RE1)
    (add_net RE2)
    (add_net RE3)
    (add_net RE4)
    (add_net RESERVED)
    (add_net SCLK)
    (add_net SDIN)
    (add_net SLOE)
    (add_net SLRD)
    (add_net SLWR)
    (add_net SUSPEND)
    (add_net V_OV)
    (add_net V_UV)
    (add_net Va)
    (add_net ~CS)
    (add_net ~DASYNC)
    (add_net ~IOUT1)
    (add_net ~IOUT2)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 188.4)
    (fp_text reference REF**1112210 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 185.86)
    (fp_text reference REF**111229 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 183.32)
    (fp_text reference REF**111228 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 180.78)
    (fp_text reference REF**111227 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 178.24)
    (fp_text reference REF**111226 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 175.7)
    (fp_text reference REF**111225 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 173.16)
    (fp_text reference REF**111224 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 170.62)
    (fp_text reference REF**111223 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 168.08)
    (fp_text reference REF**111222 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 188.4)
    (fp_text reference REF**11 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 163)
    (fp_text reference REF**111 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 88.8 105.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R112 (at -1.507834 0.02155 360) (layer F.SilkS))
    (fp_text value R_47k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 103.693 145.45 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C125 (at 0 -2.286 180) (layer F.SilkS))
    (fp_text value C_10n (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C125-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:USB_B (layer F.Cu) (tedit 5717ED53)
    (at 38.8342 183.3 270)
    (descr "USB B connector")
    (tags "USB_B USB_DEV")
    (fp_text reference P1 (at -7.4 7.3342 540) (layer F.SilkS))
    (fp_text value USB_B (at -0.5 9.25 450) (layer F.Fab))
    (pad 2 thru_hole circle (at -6.5 1.25 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask F.SilkS)
      (net 110 D-))
    (pad 1 thru_hole circle (at -6.5 -1.25 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(F1-Pad2)"))
    (pad 4 thru_hole circle (at -4.50102 -1.25 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at -4.50102 1.25 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask F.SilkS)
      (net 92 D+))
    (pad 5 thru_hole circle (at -1.79 6.02 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask F.SilkS)
      (net 300 "Net-(P1-Pad5)"))
    (pad 5 thru_hole circle (at -1.79 -6.02 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask F.SilkS)
      (net 300 "Net-(P1-Pad5)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/USB_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:QFN48_EP (layer F.Cu) (tedit 572B9249)
    (at 39.959674 120.305415 270)
    (fp_text reference U5 (at 4.951585 0.020674 360) (layer F.SilkS))
    (fp_text value MAX19516 (at 0 5.2 270) (layer F.Fab))
    (pad 1 smd oval (at -3.5 -2.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd oval (at -3.5 -2.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 35 CH1_CM))
    (pad 3 smd oval (at -3.5 -1.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 32 "/ADC, DAC/CH1+"))
    (pad 4 smd oval (at -3.5 -1.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 34 "/ADC, DAC/CH1-"))
    (pad 5 smd oval (at -3.5 -0.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd oval (at -3.5 -0.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C88-Pad2)"))
    (pad 7 smd oval (at -3.5 0.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd oval (at -3.5 0.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd oval (at -3.5 1.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 36 "/ADC, DAC/CH2+"))
    (pad 10 smd oval (at -3.5 1.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 41 "/ADC, DAC/CH2-"))
    (pad 11 smd oval (at -3.5 2.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 42 CH2_CM))
    (pad 12 smd oval (at -3.5 2.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 13 smd oval (at -2.75 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 14 smd oval (at -2.25 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd oval (at -1.75 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C81-Pad1)"))
    (pad 16 smd oval (at -1.25 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C82-Pad1)"))
    (pad 17 smd oval (at -0.75 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd oval (at -0.25 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd oval (at 0.25 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 215 DORB))
    (pad 20 smd oval (at 0.75 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 216 DCLKB))
    (pad 21 smd oval (at 1.25 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 217 D0B))
    (pad 22 smd oval (at 1.75 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 218 D1B))
    (pad 23 smd oval (at 2.25 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 219 D2B))
    (pad 24 smd oval (at 2.75 3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 220 D3B))
    (pad 25 smd oval (at 3.5 2.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 26 smd oval (at 3.5 2.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 221 D4B))
    (pad 27 smd oval (at 3.5 1.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 222 D5B))
    (pad 28 smd oval (at 3.5 1.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 223 D6B))
    (pad 29 smd oval (at 3.5 0.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 224 D7B))
    (pad 30 smd oval (at 3.5 0.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 225 D8B))
    (pad 31 smd oval (at 3.5 -0.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 226 D9B))
    (pad 32 smd oval (at 3.5 -0.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd oval (at 3.5 -1.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd oval (at 3.5 -1.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd oval (at 3.5 -2.25) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd oval (at 3.5 -2.75) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 37 smd oval (at 2.75 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd oval (at 2.25 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd oval (at 1.75 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd oval (at 1.25 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd oval (at 0.75 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd oval (at 0.25 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 43 smd oval (at -0.25 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd oval (at -0.75 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask))
    (pad 45 smd oval (at -1.25 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 227 SDIN))
    (pad 46 smd oval (at -1.75 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 228 SCLK))
    (pad 47 smd oval (at -2.25 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 229 ~CS))
    (pad 48 smd oval (at -2.75 -3.5 270) (size 0.2794 0.762) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad EP smd rect (at 0 0 270) (size 5.5 5.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/qfn48_ep.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:S-PQFP-G48 (layer F.Cu) (tedit 572B8DD8)
    (at 71.8 117.2 180)
    (fp_text reference U25 (at 0 -6.2865 180) (layer F.SilkS))
    (fp_text value DAC2932 (at 0 6.1595 180) (layer F.Fab))
    (pad 1 smd rect (at 2.75 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 237 DAC_D11))
    (pad 2 smd rect (at 2.25 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 238 DAC_D10))
    (pad 3 smd rect (at 1.75 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 239 DAC_D9))
    (pad 4 smd rect (at 1.25 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 240 DAC_D8))
    (pad 5 smd rect (at 0.75 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 241 DAC_D7))
    (pad 6 smd rect (at 0.25 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 242 DAC_D6))
    (pad 7 smd rect (at -0.25 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 243 DAC_D5))
    (pad 8 smd rect (at -0.75 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 244 DAC_D4))
    (pad 9 smd rect (at -1.25 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 245 DAC_D3))
    (pad 10 smd rect (at -1.75 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 246 DAC_D2))
    (pad 11 smd rect (at -2.25 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 247 DAC_D1))
    (pad 12 smd rect (at -2.75 -4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 248 DAC_D0))
    (pad 13 smd rect (at -4 -2.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -4 -2.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 15 smd rect (at -4 -1.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 249 DAC_CLK))
    (pad 16 smd rect (at -4 -1.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -4 -0.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -4 -0.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -4 0.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at -4 0.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 21 smd rect (at -4 1.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at -4 1.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at -4 2.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at -4 2.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(R80-Pad2)"))
    (pad 25 smd rect (at -2.75 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (pad 26 smd rect (at -2.25 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 ~IOUT1))
    (pad 27 smd rect (at -1.75 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 IOUT1))
    (pad 28 smd rect (at -1.25 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 29 smd rect (at -0.75 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 30 smd rect (at -0.25 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 31 smd rect (at 0.25 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 32 smd rect (at 0.75 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 33 smd rect (at 1.25 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 IOUT2))
    (pad 34 smd rect (at 1.75 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 ~IOUT2))
    (pad 35 smd rect (at 2.25 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 36 smd rect (at 2.75 4 180) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at 4 2.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 231 CH2_GAIN_ADJ))
    (pad 38 smd rect (at 4 2.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 233 CH1_GAIN_ADJ))
    (pad 39 smd rect (at 4 1.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 232 CH1_OFFSET_ADJ))
    (pad 40 smd rect (at 4 1.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 230 CH2_OFFSET_ADJ))
    (pad 41 smd rect (at 4 0.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 42 smd rect (at 4 0.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 43 smd rect (at 4 -0.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 44 smd rect (at 4 -0.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 45 smd rect (at 4 -1.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 250 DASDIN))
    (pad 46 smd rect (at 4 -1.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 251 DASCLK))
    (pad 47 smd rect (at 4 -2.25 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 252 ~DASYNC))
    (pad 48 smd rect (at 4 -2.75 90) (size 0.28 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/PQFP-48_7x7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT363 (layer F.Cu) (tedit 5675A3C3)
    (at 28.8901 68.3821)
    (fp_text reference Q1 (at -2.6401 -0.1321) (layer F.SilkS))
    (fp_text value BSS138BKS (at 0 2.667) (layer F.Fab))
    (pad 1 smd rect (at 0.762 -0.889 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.762 0.889 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 RE1))
    (pad 4 smd rect (at -0.762 0.889 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.762 -0.889 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 RE2))
    (pad 2 smd rect (at 0 -0.889 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(Q1-Pad2)"))
    (pad 5 smd rect (at 0 0.889 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(Q1-Pad5)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/sot363.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TQG144 (layer F.Cu) (tedit 5692BE7F)
    (at 54.584588 139.71292 270)
    (fp_text reference U26 (at -7.46292 13.584588 360) (layer F.SilkS))
    (fp_text value XC6SLX9 (at 0 13 270) (layer F.Fab))
    (pad 1 smd rect (at -8.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 223 D6B))
    (pad 2 smd rect (at -8.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 222 D5B))
    (pad 3 smd rect (at -7.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -7.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 5 smd rect (at -6.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 221 D4B))
    (pad 6 smd rect (at -6.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 220 D3B))
    (pad 7 smd rect (at -5.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 219 D2B))
    (pad 8 smd rect (at -5.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 218 D1B))
    (pad 9 smd rect (at -4.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 217 D0B))
    (pad 10 smd rect (at -4.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 214 RESERVED))
    (pad 11 smd rect (at -3.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 144 EN_CLK))
    (pad 12 smd rect (at -3.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 156 CH1_K))
    (pad 13 smd rect (at -2.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -2.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 216 DCLKB))
    (pad 15 smd rect (at -1.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 215 DORB))
    (pad 16 smd rect (at -1.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 155 CH1_GND))
    (pad 17 smd rect (at -0.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 136 CH2_K))
    (pad 18 smd rect (at -0.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 19 smd rect (at 0.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 20 smd rect (at 0.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 21 smd rect (at 1.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 137 CH2_GND))
    (pad 22 smd rect (at 1.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 139 CH1_DC))
    (pad 23 smd rect (at 2.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 141 CH2_DC))
    (pad 24 smd rect (at 2.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 142 LED3))
    (pad 25 smd rect (at 3.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 3.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 143 LED2))
    (pad 27 smd rect (at 4.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 135 LED1))
    (pad 28 smd rect (at 4.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 29 smd rect (at 5.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 115 FD12))
    (pad 30 smd rect (at 5.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 117 FD11))
    (pad 31 smd rect (at 6.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 32 smd rect (at 6.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 119 FD10))
    (pad 33 smd rect (at 7.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 121 FD9))
    (pad 34 smd rect (at 7.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 123 FD8))
    (pad 35 smd rect (at 8.25 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 134 PA3))
    (pad 36 smd rect (at 8.75 10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 37 smd rect (at 10.8 8.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 253 PROG_B))
    (pad 38 smd rect (at 10.8 8.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 126 FLAGD))
    (pad 39 smd rect (at 10.8 7.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 130 FIFOADDR1_INIT_B))
    (pad 40 smd rect (at 10.8 7.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 132 FIFOADDR0))
    (pad 41 smd rect (at 10.8 6.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 128 PA6/PKTEND))
    (pad 42 smd rect (at 10.8 6.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 43 smd rect (at 10.8 5.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 284 FD6))
    (pad 44 smd rect (at 10.8 5.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 254 FD5))
    (pad 45 smd rect (at 10.8 4.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 255 FD4))
    (pad 46 smd rect (at 10.8 4.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 256 FD3))
    (pad 47 smd rect (at 10.8 3.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 48 smd rect (at 10.8 3.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 257 FD7))
    (pad 49 smd rect (at 10.8 2.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 50 smd rect (at 10.8 2.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 258 FLAGA))
    (pad 51 smd rect (at 10.8 1.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 259 FLAGB))
    (pad 52 smd rect (at 10.8 1.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 53 smd rect (at 10.8 0.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 54 smd rect (at 10.8 0.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 55 smd rect (at 10.8 -0.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 260 SLOE))
    (pad 56 smd rect (at 10.8 -0.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 174 IFCLK))
    (pad 57 smd rect (at 10.8 -1.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 58 smd rect (at 10.8 -1.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 261 DIR1))
    (pad 59 smd rect (at 10.8 -2.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 262 DIR2))
    (pad 60 smd rect (at 10.8 -2.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 61 smd rect (at 10.8 -3.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 263 FD2))
    (pad 62 smd rect (at 10.8 -3.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 264 FD1))
    (pad 63 smd rect (at 10.8 -4.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 64 smd rect (at 10.8 -4.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 265 CTL2_CSI_B))
    (pad 65 smd rect (at 10.8 -5.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 266 FD0))
    (pad 66 smd rect (at 10.8 -5.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 176 SLWR))
    (pad 67 smd rect (at 10.8 -6.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 178 SLRD))
    (pad 68 smd rect (at 10.8 -6.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 69 smd rect (at 10.8 -7.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 70 smd rect (at 10.8 -7.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 180 CCLK))
    (pad 71 smd rect (at 10.8 -8.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(R52-Pad1)"))
    (pad 72 smd rect (at 10.8 -8.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 73 smd rect (at 8.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 267 SUSPEND))
    (pad 74 smd rect (at 8.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 184 FD14))
    (pad 75 smd rect (at 7.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 200 EN_PWR))
    (pad 76 smd rect (at 7.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 77 smd rect (at 6.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 78 smd rect (at 6.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 182 FD15))
    (pad 79 smd rect (at 5.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 186 FD13))
    (pad 80 smd rect (at 5.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 268 B_D14_J20))
    (pad 81 smd rect (at 4.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 269 B_D15_J19))
    (pad 82 smd rect (at 4.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 270 B_D12_J18))
    (pad 83 smd rect (at 3.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 271 B_D13_J17))
    (pad 84 smd rect (at 3.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 272 B_D10_J16))
    (pad 85 smd rect (at 2.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 273 B_D11_J15))
    (pad 86 smd rect (at 2.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 87 smd rect (at 1.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 235 DPOT_CS))
    (pad 88 smd rect (at 1.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 89 smd rect (at 0.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 90 smd rect (at 0.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 91 smd rect (at -0.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 92 smd rect (at -0.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 274 B_D8_J14))
    (pad 93 smd rect (at -1.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 275 B_D9_J13))
    (pad 94 smd rect (at -1.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 276 B_D7_J7))
    (pad 95 smd rect (at -2.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 277 B_D6_J8))
    (pad 96 smd rect (at -2.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 97 smd rect (at -3.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 278 B_D5_J5))
    (pad 98 smd rect (at -3.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 279 B_D4_J6))
    (pad 99 smd rect (at -4.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 280 B_D2_J4))
    (pad 100 smd rect (at -4.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 281 B_D1_J1))
    (pad 101 smd rect (at -5.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 282 B_D0_J2))
    (pad 102 smd rect (at -5.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 283 B_D3_J3))
    (pad 103 smd rect (at -6.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 104 smd rect (at -6.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 236 DPOT_SI))
    (pad 105 smd rect (at -7.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 234 DPOT_SCK))
    (pad 106 smd rect (at -7.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(R51-Pad1)"))
    (pad 107 smd rect (at -8.25 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 288 "Net-(J2-Pad6)"))
    (pad 108 smd rect (at -8.75 -10.8 90) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 109 smd rect (at -10.8 -8.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 285 "Net-(J2-Pad3)"))
    (pad 110 smd rect (at -10.8 -8.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 287 "Net-(J2-Pad5)"))
    (pad 111 smd rect (at -10.8 -7.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 248 DAC_D0))
    (pad 112 smd rect (at -10.8 -7.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 247 DAC_D1))
    (pad 113 smd rect (at -10.8 -6.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 114 smd rect (at -10.8 -6.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 246 DAC_D2))
    (pad 115 smd rect (at -10.8 -5.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 245 DAC_D3))
    (pad 116 smd rect (at -10.8 -5.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 244 DAC_D4))
    (pad 117 smd rect (at -10.8 -4.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 243 DAC_D5))
    (pad 118 smd rect (at -10.8 -4.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 242 DAC_D6))
    (pad 119 smd rect (at -10.8 -3.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 241 DAC_D7))
    (pad 120 smd rect (at -10.8 -3.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 240 DAC_D8))
    (pad 121 smd rect (at -10.8 -2.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 239 DAC_D9))
    (pad 122 smd rect (at -10.8 -2.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 123 smd rect (at -10.8 -1.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 238 DAC_D10))
    (pad 124 smd rect (at -10.8 -1.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 237 DAC_D11))
    (pad 125 smd rect (at -10.8 -0.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 126 smd rect (at -10.8 -0.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 294 "Net-(R143-Pad1)"))
    (pad 127 smd rect (at -10.8 0.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 252 ~DASYNC))
    (pad 128 smd rect (at -10.8 0.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 129 smd rect (at -10.8 1.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 130 smd rect (at -10.8 1.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 131 smd rect (at -10.8 2.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 251 DASCLK))
    (pad 132 smd rect (at -10.8 2.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 250 DASDIN))
    (pad 133 smd rect (at -10.8 3.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 170 AN_TRIG))
    (pad 134 smd rect (at -10.8 3.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 170 AN_TRIG))
    (pad 135 smd rect (at -10.8 4.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 136 smd rect (at -10.8 4.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 137 smd rect (at -10.8 5.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 171 AN_TRIG_LEVEL))
    (pad 138 smd rect (at -10.8 5.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 139 smd rect (at -10.8 6.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 229 ~CS))
    (pad 140 smd rect (at -10.8 6.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 228 SCLK))
    (pad 141 smd rect (at -10.8 7.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 227 SDIN))
    (pad 142 smd rect (at -10.8 7.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 226 D9B))
    (pad 143 smd rect (at -10.8 8.25) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 225 D8B))
    (pad 144 smd rect (at -10.8 8.75) (size 0.28 1.2) (layers F.Cu F.Paste F.Mask)
      (net 224 D7B))
    (model ${KIPRJMOD}/ScopefunPackages3D/TQG144C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 69.428599 174.897 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R57 (at 0 -3.178599 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 182 FD15))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(R57-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 89.281 133.985 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C124 (at -1.615 1.719 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 100.076 56.261 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R135 (at -1.542 0.176 360) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(R135-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 74.2 72.112)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C40 (at 0 2.288) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOD123 (layer F.Cu) (tedit 5709196A)
    (at 53.4265 63.918812 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D24 (at 1.613188 -0.0405 360) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 3.3 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.575 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 98 RE3))
    (pad 1 smd rect (at 0 -1.575 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/sod123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:G6K-2F-Y (layer F.Cu) (tedit 56755A3F)
    (at 53.6805 56.533 180)
    (fp_text reference RE3 (at 0 -5.9 180) (layer F.SilkS))
    (fp_text value G6K-2F-Y-DC4.5 (at 0 6.2 180) (layer F.Fab))
    (pad 7 smd rect (at 3.5 -0.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.5 -3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 98 RE3))
    (pad 1 smd rect (at -3.5 -3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 6 smd rect (at 3.5 1.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 3.5 3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.5 -0.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.5 1.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 291 "Net-(RE3-Pad3)"))
    (pad 4 smd rect (at -3.5 3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C64-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/G6K-2F-Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 79.7 119.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C32 (at 1.515602 -0.1 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 25.8 134.7 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at -2.4 0.8 180) (layer F.SilkS))
    (fp_text value R_2.2k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 144 EN_CLK))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 79.398 170.3885 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R78 (at -0.104 3.8915 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 A_D15_J19))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 D15_J19))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 85.494 174.9605 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R62 (at 10.691 -4.8715 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 72 A_D10_J16))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 73 D10_J16))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:CSM-7X (layer F.Cu) (tedit 56955EC4)
    (at 67.2314 161.5112 180)
    (fp_text reference X1 (at -3.7616 -0.0328 180) (layer F.SilkS))
    (fp_text value Crystal_24Mhz (at 0 9 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -4.75 90) (size 5.5 2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C99-Pad2)"))
    (pad 2 smd rect (at 0 4.75 90) (size 5.5 2) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C117-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/xtal_csm-7x.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SSOP56 (layer F.Cu) (tedit 56955947)
    (at 54.049994 168.07456 180)
    (fp_text reference U27 (at 0 -10.16 180) (layer F.SilkS))
    (fp_text value CY7C68013A-56PVXC (at 0 10.16 180) (layer F.Fab))
    (pad 56 smd rect (at 4.723 -8.5725 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R1-Pad1)"))
    (pad 1 smd rect (at -4.723 -8.5725 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(R59-Pad1)"))
    (pad 55 smd rect (at 4.723 -7.9375 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at -4.723 -7.9375 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(R58-Pad1)"))
    (pad 54 smd rect (at 4.723 -7.3025 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R3-Pad1)"))
    (pad 3 smd rect (at -4.723 -7.3025 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(R57-Pad1)"))
    (pad 53 smd rect (at 4.723 -6.6675 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R4-Pad1)"))
    (pad 4 smd rect (at -4.723 -6.6675 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 52 smd rect (at 4.723 -6.0325 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R5-Pad1)"))
    (pad 5 smd rect (at -4.723 -6.0325 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R56-Pad1)"))
    (pad 51 smd rect (at 4.723 -5.3975 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(R79-Pad2)"))
    (pad 6 smd rect (at -4.723 -5.3975 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 50 smd rect (at 4.723 -4.7625 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 7 smd rect (at -4.723 -4.7625 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 49 smd rect (at 4.723 -4.1275 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(U27-Pad49)"))
    (pad 8 smd rect (at -4.723 -4.1275 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(R55-Pad1)"))
    (pad 48 smd rect (at 4.723 -3.4925 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -4.723 -3.4925 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(R54-Pad1)"))
    (pad 47 smd rect (at 4.723 -2.8575 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R6-Pad2)"))
    (pad 10 smd rect (at -4.723 -2.8575 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 46 smd rect (at 4.723 -2.2225 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R7-Pad2)"))
    (pad 11 smd rect (at -4.723 -2.2225 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C99-Pad2)"))
    (pad 45 smd rect (at 4.723 -1.5875 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R8-Pad2)"))
    (pad 12 smd rect (at -4.723 -1.5875 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C117-Pad1)"))
    (pad 44 smd rect (at 4.723 -0.9525 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R9-Pad2)"))
    (pad 13 smd rect (at -4.723 -0.9525 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 43 smd rect (at 4.723 -0.3175 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(R10-Pad2)"))
    (pad 14 smd rect (at -4.723 -0.3175 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 42 smd rect (at 4.723 0.3175 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 260 SLOE))
    (pad 15 smd rect (at -4.723 0.3175 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 92 D+))
    (pad 41 smd rect (at 4.723 0.9525 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 253 PROG_B))
    (pad 16 smd rect (at -4.723 0.9525 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 110 D-))
    (pad 40 smd rect (at 4.723 1.5875 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 267 SUSPEND))
    (pad 17 smd rect (at -4.723 1.5875 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 39 smd rect (at 4.723 2.2225 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 18 smd rect (at -4.723 2.2225 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 38 smd rect (at 4.723 2.8575 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 265 CTL2_CSI_B))
    (pad 19 smd rect (at -4.723 2.8575 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 37 smd rect (at 4.723 3.4925 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 259 FLAGB))
    (pad 20 smd rect (at -4.723 3.4925 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(R53-Pad1)"))
    (pad 36 smd rect (at 4.723 4.1275 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 258 FLAGA))
    (pad 21 smd rect (at -4.723 4.1275 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 35 smd rect (at 4.723 4.7625 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at -4.723 4.7625 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 293 "Net-(R12-Pad2)"))
    (pad 34 smd rect (at 4.723 5.3975 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 23 smd rect (at -4.723 5.3975 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(R11-Pad2)"))
    (pad 33 smd rect (at 4.723 6.0325 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -4.723 6.0325 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 32 smd rect (at 4.723 6.6675 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 257 FD7))
    (pad 25 smd rect (at -4.723 6.6675 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 266 FD0))
    (pad 31 smd rect (at 4.723 7.3025 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 284 FD6))
    (pad 26 smd rect (at -4.723 7.3025 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 264 FD1))
    (pad 30 smd rect (at 4.723 7.9375 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 254 FD5))
    (pad 27 smd rect (at -4.723 7.9375 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 263 FD2))
    (pad 29 smd rect (at 4.723 8.5725 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 255 FD4))
    (pad 28 smd rect (at -4.723 8.5725 90) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 256 FD3))
    (model ${KIPRJMOD}/ScopefunPackages3D/SSOP56.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 48 186.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D1 (at 2.106 0.1015) (layer F.SilkS))
    (fp_text value PGB1010603MR (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 92 D+))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 48 183.8)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D2 (at 1.856 0.1535) (layer F.SilkS))
    (fp_text value PGB1010603MR (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 110 D-))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:LED_0805 (layer F.Cu) (tedit 57058062)
    (at 77.0485 149.72433 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D18 (at -1.78667 -0.0865 360) (layer F.SilkS))
    (fp_text value HSMD-C170 (at 0 2.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 180) (size 1.1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(D18-Pad2)"))
    (pad 1 smd rect (at 0 -1.1 180) (size 1.1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_1206 (layer F.Cu) (tedit 56FEE4E5)
    (at 56.261 184.277 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference F1 (at -2.177 -0.0532 360) (layer F.SilkS))
    (fp_text value 1206L150 (at 0 3.302 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.45 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(F1-Pad2)"))
    (pad 1 smd rect (at 0 -1.45 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.383701 0.383701 0.383701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:LED_0805 (layer F.Cu) (tedit 57058062)
    (at 71.27 187.471016 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference LED1 (at -1.377984 -4.468 180) (layer F.SilkS))
    (fp_text value HSMD-C170 (at 0 2.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1) (size 1.1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(LED1-Pad2)"))
    (pad 1 smd rect (at 0 -1.1) (size 1.1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:LED_0805 (layer F.Cu) (tedit 57058062)
    (at 93.876 32.315984 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference LED2 (at 0.668816 -4.3204 360) (layer F.SilkS))
    (fp_text value HSMD-C170 (at 0 2.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 180) (size 1.1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(LED2-Pad2)"))
    (pad 1 smd rect (at 0 -1.1 180) (size 1.1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:LED_0805 (layer F.Cu) (tedit 57058062)
    (at 46.124 32.315984 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference LED3 (at 1.126016 -4.2188 360) (layer F.SilkS))
    (fp_text value HSMD-C170 (at 0 2.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 180) (size 1.1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(LED3-Pad2)"))
    (pad 1 smd rect (at 0 -1.1 180) (size 1.1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 60.513 186.725 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference MLV1 (at 2.817 0.0815 180) (layer F.SilkS))
    (fp_text value V5.5MLA0603NH (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 173.881 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.119 -2.5675 360) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 115 FD12))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R1-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 172.357 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.107 -2.5675 360) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 117 FD11))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R2-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 170.833 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.083 -2.5675 360) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 119 FD10))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R3-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 169.182 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.068 -2.5675 360) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 121 FD9))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R4-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 167.658 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.092 -2.5675 360) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 123 FD8))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R5-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 166.134 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0.134 -2.5675 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 126 FLAGD))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 164.483 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.017 -2.5675 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 128 PA6/PKTEND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 162.832 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.168 -2.5675 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R8-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 130 FIFOADDR1_INIT_B))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 38.5675 161.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -0.069 -2.5675 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R9-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 132 FIFOADDR0))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 42.418 159.4665)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -2.286 -0.0815) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 134 PA3))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 28.1408 154.5897 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -0.7592 -2.3103 180) (layer F.SilkS))
    (fp_text value R_2.2k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(R11-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 26.2612 154.5897 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0.6612 -2.3103 180) (layer F.SilkS))
    (fp_text value R_2.2k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 293 "Net-(R12-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 37.361 148.6715 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -2.286 180) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 135 LED1))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(LED1-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 34.059 139.4005)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -0.059 2.9665) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 136 CH2_K))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(Q1-Pad5)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 32.408 139.4005 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 2.3495 180) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 137 CH2_GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 30.757 139.4005 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 3.8495 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R16-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 139 CH1_DC))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 29.106 139.4005 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at -0.106 2.3495 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R17-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 141 CH2_DC))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 27.455 139.4005)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0.045 3.8495) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 142 LED3))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(LED3-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 25.804 139.4005)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at -0.054 2.3495) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 143 LED2))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(LED2-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 30.5665 123.081 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 2.9335 180) (layer F.SilkS))
    (fp_text value R_150R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C82-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 27.8 119.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 2.5 2.6 180) (layer F.SilkS))
    (fp_text value R_150R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C81-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 31.138 106.888398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0.588 2.138398 180) (layer F.SilkS))
    (fp_text value R_249R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R23-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 41 "/ADC, DAC/CH2-"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 32.915999 106.888398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at -2.484001 0.038398 180) (layer F.SilkS))
    (fp_text value R_249R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(R24-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 36 "/ADC, DAC/CH2+"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 33.8685 97.935 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at -0.018 -3.2155 360) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R25-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R25-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 33.043 95.204398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at -2.517 -0.045602 180) (layer F.SilkS))
    (fp_text value R_402R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R26-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R25-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 31.011 95.204398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 2.563 -0.045602 180) (layer F.SilkS))
    (fp_text value R_402R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R27-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R27-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 30.1855 97.935 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0 -3.1855 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R27-Pad1)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R28-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 27.328 85.044398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at 2.309 0.843398 180) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R29-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R29-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 27.2645 82.314 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at -1.514 0.2645 360) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R29-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 30.734 75.057 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 0 2.921 360) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C140-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 91 "/ANALOG INPUTS/CH2_VGA"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 39.139 70.3125 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at 0.361 -2.3125 180) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 155 CH1_GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 41.171 70.3125)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at 2.329 1.4375) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 156 CH1_K))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(Q2-Pad5)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 46.678914 74.948 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at 0.109 3.007602 360) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C139-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 89 "/ANALOG INPUTS/CH1_VGA"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 43.2665 82.314 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at -0.018 3.1345 360) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R35-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 43.203 85.044398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R36 (at 2.436 1.097398 180) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R35-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(R36-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 46.886 95.204398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R37 (at 2.436 -0.045602 180) (layer F.SilkS))
    (fp_text value R_402R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(R37-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(R37-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 46.060602 97.935 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R38 (at 0 -3.310602 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(R37-Pad1)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(R38-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 49.022 95.204398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R39 (at -2.263 0.081398 180) (layer F.SilkS))
    (fp_text value R_402R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(R39-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(R39-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 49.743398 97.935 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R40 (at 1.506 -0.929602 360) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(R39-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(R40-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 57.109602 97.681 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R41 (at 0.931 -3.109602 180) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(R41-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 31 CH1_GAIN))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 57.109602 99.967 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R42 (at -1.796 3.134602 360) (layer F.SilkS))
    (fp_text value R_255R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 31 CH1_GAIN))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 57.109602 102.253 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R43 (at 2.503 -3.109602 180) (layer F.SilkS))
    (fp_text value R_255R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 86 CH2_GAIN))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 57.109602 104.666 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R44 (at -0.034 3.290398 180) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(R104-Pad1)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 86 CH2_GAIN))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 50.569 106.888398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R45 (at -2.331 -0.011602 180) (layer F.SilkS))
    (fp_text value R_348R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(R45-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(R45-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 48.791 106.888398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R46 (at 0.041 2.138398 180) (layer F.SilkS))
    (fp_text value R_249R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(R45-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 32 "/ADC, DAC/CH1+"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 47.013 106.888398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R47 (at 2.363 -0.061602 180) (layer F.SilkS))
    (fp_text value R_249R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(R47-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 34 "/ADC, DAC/CH1-"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 49.2 118.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R48 (at 0.0638 -3 180) (layer F.SilkS))
    (fp_text value R_6.8k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C22-Pad1)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C73-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 53.9 118.255 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R49 (at 1.495 0.065398 360) (layer F.SilkS))
    (fp_text value R_100k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(R45-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 170 AN_TRIG))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 50 124.668602)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R50 (at 0 -2.168602) (layer F.SilkS))
    (fp_text value R_6.8k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 171 AN_TRIG_LEVEL))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C22-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 72.603602 131.953 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R51 (at -1.406 -0.103602 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 286 "Net-(J2-Pad4)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(R51-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 72.730398 148.735 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R52 (at -1.76 -0.086398 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(D18-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(R52-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 56.769 155.575 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R53 (at -2.454 -0.0335 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 174 IFCLK))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(R53-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 69.428599 170.325 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R54 (at 0 3.071401 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 176 SLWR))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(R54-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 69.428599 171.849 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R55 (at 0 3.071401 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 178 SLRD))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(R55-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 69.428599 173.373 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R56 (at 0 -3.178599 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 180 CCLK))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R56-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 69.428599 176.421 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R58 (at 0 -3.178599 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 184 FD14))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(R58-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 69.428599 177.945 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R59 (at 0 -3.178599 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 186 FD13))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(R59-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 77.366 174.9605 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R60 (at 2.563 -2.3315 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 76 A_D14_J20))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 77 D14_J20))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 81.43 174.9605 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R61 (at 6.627 -3.6015 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 74 A_D12_J18))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 75 D12_J18))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 89.558 174.9605 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R63 (at 14.755 -6.1415 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 A_D8_J14))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 D8_J14))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 91.59 170.3885 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R64 (at 0.023 3.8915 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 A_D9_J13))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 D9_J13))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 95.5 170.3885 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R65 (at -0.131 3.8915 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 A_D7_J7))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 D7_J7))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 99.583 170.3885 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R66 (at 0 3.8915 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 A_D5_J5))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 56 D5_J5))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 103.647 170.3885 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R67 (at -0.112 3.8915 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 A_D3_J3))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 58 D3_J3))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 107.711 170.3885 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R68 (at 0.015 3.8915 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 A_D1_J1))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 60 D1_J1))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 111.521 170.8965)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R69 (at 0.493 2.2045) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 113.172 170.8965)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R70 (at 2.328 -0.1465) (layer F.SilkS))
    (fp_text value R_22k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(D20-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 112.3719 167.658 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R71 (at 0.158 3.1281 180) (layer F.SilkS))
    (fp_text value R_6.8k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(D20-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 109.743 174.9605 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R72 (at -2.398 -2.7125 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 A_D0_J2))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 62 D0_J2))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 105.679 174.9605 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R73 (at -6.462 -3.9825 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 A_D2_J4))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 D2_J4))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 101.615 174.9605 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R74 (at -10.526 -5.2525 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 A_D4_J6))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 D4_J6))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 97.551 174.9605 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R75 (at -14.59 -6.5225 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 A_D6_J8))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 68 D6_J8))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 87.526 170.3885 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R76 (at 0.023 3.8915 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 A_D11_J15))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 D11_J15))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 83.462 170.3885 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R77 (at 0 3.8915 180) (layer F.SilkS))
    (fp_text value R_1k_0.5W (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 A_D13_J17))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 D13_J17))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 63.078398 177.945 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R79 (at -1.415 -0.040602 360) (layer F.SilkS))
    (fp_text value R_10k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(R79-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 80.096398 114.064 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R80 (at 0.036 -3.003602 360) (layer F.SilkS))
    (fp_text value R_19.6k_0.1% (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(R80-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 75.6 106.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R81 (at 0 -3.048398 360) (layer F.SilkS))
    (fp_text value R_249R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 12 IOUT1))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 74.762398 104.539 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R82 (at -0.061 2.937602 180) (layer F.SilkS))
    (fp_text value R_249R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 9 IOUT2))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 73.238602 101.237 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R83 (at 1.633 0.975602 360) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R83-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 73.238602 98.951 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R84 (at 1.451 -0.988602 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R83-Pad1)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(R41-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 79.779 100.284398)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R85 (at 0.471 -2.286) (layer F.SilkS))
    (fp_text value R_249R_0.1% (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 9 IOUT2))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R85-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 77.62 100.284398)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R86 (at -0.37 -2.284398) (layer F.SilkS))
    (fp_text value R_249R_0.1% (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 10 ~IOUT2))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(R86-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 84.478 100.284398)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R87 (at -0.228 -2.286) (layer F.SilkS))
    (fp_text value R_249R_0.1% (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 12 IOUT1))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R107-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 86.764 100.284398)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R88 (at 0.486 -2.284398) (layer F.SilkS))
    (fp_text value R_249R_0.1% (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 11 ~IOUT1))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R108-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 81.747398 104.539 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R89 (at -0.061 2.952602 180) (layer F.SilkS))
    (fp_text value R_249R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 11 ~IOUT1))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 79.7 92.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R90 (at -2.418 -0.144602) (layer F.SilkS))
    (fp_text value R_2.2k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R85-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 79.75 87.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R91 (at -2.25 -0.207602) (layer F.SilkS))
    (fp_text value R_2.2k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(R86-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(D26-Pad3)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 73.238602 90.823 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R92 (at -1.669 0.086602 360) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(R92-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 73.238602 93.109 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R93 (at -1.641 0.011398 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(R92-Pad1)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(R100-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 68.73 84.917602)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R94 (at 0 -2.286) (layer F.SilkS))
    (fp_text value R_6.8k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(D21-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 71.765201 81.425 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R95 (at -0.175 3.065201 360) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(D21-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 71.714599 79.012 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R96 (at 0.012 -2.964599 180) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 63.459602 79.012 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R97 (at 0 -3.459602 180) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 63.459398 81.425 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R98 (at -0.125 3.459398 360) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(D22-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 60.013431 84.917602)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R99 (at 0 -2.286) (layer F.SilkS))
    (fp_text value R_6.8k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(D22-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 57.998602 90.823 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R100 (at 1.573 0.251398 180) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(R100-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 17 CH1_OFFSET))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 57.998602 93.109 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at -0.641 -3.248602 180) (layer F.SilkS))
    (fp_text value R_1.02k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(R101-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 18 CH2_OFFSET))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 62.570602 93.109 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at -1.641 -0.070602 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(R102-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(R101-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 62.570398 90.823 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R103 (at -1.542 -0.070398 360) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(R102-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 62.570602 98.951 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R104 (at 1.451 0.079398 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(R104-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(R104-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 62.570602 101.237 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R105 (at 1.513 0.070602 360) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(R104-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 68.6 106.8 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R106 (at 0.075 3.500001 360) (layer F.SilkS))
    (fp_text value R_249R (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 10 ~IOUT2))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 88.5 92.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R107 (at 2.724 -0.025602) (layer F.SilkS))
    (fp_text value R_2.2k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R107-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 90 87.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R108 (at 2.71 -0.07) (layer F.SilkS))
    (fp_text value R_2.2k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R108-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(D27-Pad3)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 100.226 89.489602 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R109 (at 0 -2.286 180) (layer F.SilkS))
    (fp_text value R_47k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 83 -5V))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(R109-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 100.2 94.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R110 (at 0 -2.286 180) (layer F.SilkS))
    (fp_text value R_51k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(R109-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 108.7 97.7 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R111 (at -0.065 -3.6635 180) (layer F.SilkS))
    (fp_text value R_2.2k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 200 EN_PWR))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 97.813 75.2655 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R113 (at -1.237 2.3155 180) (layer F.SilkS))
    (fp_text value R_49.9k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(R113-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 96.035 75.2655)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R114 (at -1.035 -2.2655) (layer F.SilkS))
    (fp_text value R_100k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(R113-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 98.6385 68.344 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R115 (at 1.499 -0.0155 360) (layer F.SilkS))
    (fp_text value R_49.9k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 202 V_OV))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 90.129602 66.185 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R116 (at 0.018 3.469398 180) (layer F.SilkS))
    (fp_text value R_1.5k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 203 V_UV))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 90.129602 68.344 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R117 (at 1.549 -0.070398 360) (layer F.SilkS))
    (fp_text value R_49.9k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 203 V_UV))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_1206 (layer F.Cu) (tedit 56FEE4E5)
    (at 80.772 62.865)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R118 (at 0.127 -3.048) (layer F.SilkS))
    (fp_text value R_48.7R_0.5W (at 0 3.302) (layer F.Fab))
    (pad 2 smd rect (at 0 1.45 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(D27-Pad3)"))
    (pad 1 smd rect (at 0 -1.45 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(R118-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.383701 0.383701 0.383701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_1206 (layer F.Cu) (tedit 56FEE4E5)
    (at 77.978 62.865)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R119 (at -1.016 -3.048) (layer F.SilkS))
    (fp_text value R_48.7R_0.5W (at 0 3.302) (layer F.Fab))
    (pad 2 smd rect (at 0 1.45 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(D26-Pad3)"))
    (pad 1 smd rect (at 0 -1.45 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(R119-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.383701 0.383701 0.383701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 70.762 59.3778 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R120 (at -0.138 -2.7222 180) (layer F.SilkS))
    (fp_text value R_953k_0.1% (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C67-Pad1)"))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C68-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 59.078 64.3435)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R121 (at 0 -2.286) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(D23-Pad3)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(R121-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 44.981 59.3778 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R122 (at -0.019 -3.6722 180) (layer F.SilkS))
    (fp_text value R_953k_0.1% (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C59-Pad2)"))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C59-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 33.17 64.3435)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R123 (at 0 -2.286) (layer F.SilkS))
    (fp_text value R_100R (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D29-Pad3)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(R123-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 35.075 46.6905)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R124 (at -0.023 2.5855) (layer F.SilkS))
    (fp_text value R_47k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C60-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C62-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 39.52 46.6778 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R125 (at 0.023 -2.8522 180) (layer F.SilkS))
    (fp_text value R_953k_0.1% (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C60-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 46.378 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R126 (at -0.128 -2.4405 180) (layer F.SilkS))
    (fp_text value R_47k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C59-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 55.522 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R127 (at 0.15 -2.3315 180) (layer F.SilkS))
    (fp_text value R_56R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(R127-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C64-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 60.729 46.6905)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R128 (at -0.023 2.3315) (layer F.SilkS))
    (fp_text value R_47k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C65-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C65-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 65.047 46.6778 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R129 (at 0 -2.8522 180) (layer F.SilkS))
    (fp_text value R_953k_0.1% (at 0 2.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C65-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 72.286 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R130 (at -0.036 -2.4405 180) (layer F.SilkS))
    (fp_text value R_47k (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C67-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 86.065398 46.246 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R131 (at -1.446 -0.134602 360) (layer F.SilkS))
    (fp_text value R_22k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(R131-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 91.018602 46.246 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R132 (at -1.446 -0.131398 360) (layer F.SilkS))
    (fp_text value R_499k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(R131-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(AWG2-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 96.7335 46.246 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R133 (at 1.496 -0.2335 180) (layer F.SilkS))
    (fp_text value R_499k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(R133-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AWG1-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 101.6865 46.246 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R134 (at 1.496 0.3135 180) (layer F.SilkS))
    (fp_text value R_22k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(R133-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 100.1 58.166 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R136 (at -2.866 -3.8 360) (layer F.SilkS))
    (fp_text value R_100k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 296 AWG1_PROT))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 86.75 58.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R137 (at -0.05 3.7 360) (layer F.SilkS))
    (fp_text value R_100k (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 295 AWG2_PROT))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 86.75 56.261 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R138 (at 0 -3.708602 180) (layer F.SilkS))
    (fp_text value R_499R (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 297 "Net-(R138-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 109.6 75.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R139 (at 0 -2.286) (layer F.SilkS))
    (fp_text value R_97.6k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C133-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 112.1 75.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R140 (at 0.225 2.2345) (layer F.SilkS))
    (fp_text value R_51k (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C133-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 30.503 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R141 (at 0 -2.4405 180) (layer F.SilkS))
    (fp_text value R_56R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(R141-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C63-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 98.6385 66.185 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R142 (at 0.018 4.2315 180) (layer F.SilkS))
    (fp_text value R_1.5k (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 202 V_OV))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:CP-16-2 (layer F.Cu) (tedit 56787FE1)
    (at 47.902 101.725899)
    (fp_text reference U7 (at -2.152 -2.225899) (layer F.SilkS))
    (fp_text value ADA4932-1 (at -0.1 3.2) (layer F.Fab))
    (pad 5 smd oval (at -1.37 -0.75) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd oval (at 0.75 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(R40-Pad1)"))
    (pad 12 smd oval (at 0.75 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 11 smd oval (at 0.25 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(R45-Pad2)"))
    (pad 2 smd oval (at 0.25 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(R39-Pad1)"))
    (pad 3 smd oval (at -0.25 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(R37-Pad1)"))
    (pad 10 smd oval (at -0.25 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(R47-Pad2)"))
    (pad 9 smd oval (at -0.75 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 35 CH1_CM))
    (pad 4 smd oval (at -0.75 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(R38-Pad1)"))
    (pad EP smd rect (at 0 0 270) (size 1.37 1.37) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at 1.37 -0.75) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 15 smd oval (at 1.37 -0.25) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 6 smd oval (at -1.37 -0.25) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 7 smd oval (at -1.37 0.25) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 14 smd oval (at 1.37 0.25) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 13 smd oval (at 1.37 0.75) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 8 smd oval (at -1.37 0.75) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/LFCSP16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:CP-16-2 (layer F.Cu) (tedit 56787FE1)
    (at 32.0778 101.725899)
    (fp_text reference U14 (at -2.5778 -2.225899) (layer F.SilkS))
    (fp_text value ADA4932-1 (at -0.1 3.2) (layer F.Fab))
    (pad 5 smd oval (at -1.37 -0.75) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd oval (at 0.75 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R25-Pad1)"))
    (pad 12 smd oval (at 0.75 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 11 smd oval (at 0.25 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(R24-Pad2)"))
    (pad 2 smd oval (at 0.25 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R25-Pad2)"))
    (pad 3 smd oval (at -0.25 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R27-Pad1)"))
    (pad 10 smd oval (at -0.25 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R23-Pad2)"))
    (pad 9 smd oval (at -0.75 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 42 CH2_CM))
    (pad 4 smd oval (at -0.75 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R28-Pad1)"))
    (pad EP smd rect (at 0 0 270) (size 1.37 1.37) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at 1.37 -0.75) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 15 smd oval (at 1.37 -0.25) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 6 smd oval (at -1.37 -0.25) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 7 smd oval (at -1.37 0.25) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 14 smd oval (at 1.37 0.25) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 13 smd oval (at 1.37 0.75) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 8 smd oval (at -1.37 0.75) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/LFCSP16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:CP-8-2 (layer F.Cu) (tedit 56787BF2)
    (at 45.997 84.740665)
    (fp_text reference U9 (at 0.253 -3.490665) (layer F.SilkS))
    (fp_text value AD8337 (at -0.1 3.2) (layer F.Fab))
    (pad 1 smd oval (at 0.75 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(R37-Pad2)"))
    (pad 8 smd oval (at 0.75 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 7 smd oval (at 0.25 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 31 CH1_GAIN))
    (pad 2 smd oval (at 0.25 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd oval (at -0.25 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 89 "/ANALOG INPUTS/CH1_VGA"))
    (pad 6 smd oval (at -0.25 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 5 smd oval (at -0.75 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(R36-Pad1)"))
    (pad 4 smd oval (at -0.75 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(R35-Pad1)"))
    (pad EP smd rect (at 0 0 270) (size 1.53 1.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.1) (solder_paste_margin -0.2))
    (model ${KIPRJMOD}/ScopefunPackages3D/LFCSP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:CP-8-2 (layer F.Cu) (tedit 56787BF2)
    (at 30.122 84.740665)
    (fp_text reference U12 (at 0.128 -3.490665) (layer F.SilkS))
    (fp_text value AD8337 (at -0.1 3.2) (layer F.Fab))
    (pad 1 smd oval (at 0.75 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R27-Pad2)"))
    (pad 8 smd oval (at 0.75 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 7 smd oval (at 0.25 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 86 CH2_GAIN))
    (pad 2 smd oval (at 0.25 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd oval (at -0.25 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 91 "/ANALOG INPUTS/CH2_VGA"))
    (pad 6 smd oval (at -0.25 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 5 smd oval (at -0.75 1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R29-Pad1)"))
    (pad 4 smd oval (at -0.75 -1.37 270) (size 0.71 0.254) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R29-Pad2)"))
    (pad EP smd rect (at 0 0 270) (size 1.53 1.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin -0.1) (solder_paste_margin -0.2))
    (model ${KIPRJMOD}/ScopefunPackages3D/LFCSP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOD123 (layer F.Cu) (tedit 5709196A)
    (at 64.0945 63.918812 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D25 (at 1.581188 -0.1555 360) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 3.3 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.575 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 99 RE4))
    (pad 1 smd rect (at 0 -1.575 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/sod123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOD123 (layer F.Cu) (tedit 5709196A)
    (at 38.4151 63.918812 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D28 (at 1.581188 -0.0849 360) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 3.3 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.575 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 102 RE2))
    (pad 1 smd rect (at 0 -1.575 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/sod123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOD123 (layer F.Cu) (tedit 5709196A)
    (at 27.5185 63.918812 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D30 (at 1.581188 -0.0315 360) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 3.3 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.575 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 104 RE1))
    (pad 1 smd rect (at 0 -1.575 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/sod123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TZC3 (layer F.Cu) (tedit 56732153)
    (at 46.124 52.85)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference CV1 (at 0 3.411) (layer F.SilkS))
    (fp_text value CVar_1.4-3.0_pF (at 0 3.429) (layer F.Fab))
    (pad 1 smd rect (at 0 2.032 90) (size 0.85 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C59-Pad1)"))
    (pad 2 smd rect (at 0 -2.032 90) (size 0.85 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C59-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/TZC3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TZC3 (layer F.Cu) (tedit 56732153)
    (at 71.905 52.85)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference CV2 (at 0.104 3.538) (layer F.SilkS))
    (fp_text value CVar_1.4-3.0_pF (at 0 3.429) (layer F.Fab))
    (pad 1 smd rect (at 0 2.032 90) (size 0.85 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C68-Pad1)"))
    (pad 2 smd rect (at 0 -2.032 90) (size 0.85 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C67-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/TZC3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TZC3 (layer F.Cu) (tedit 56732153)
    (at 68.603 40.785)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference CV3 (at 0 -3.302) (layer F.SilkS))
    (fp_text value CVar_1.4-3.0_pF (at 0 3.429) (layer F.Fab))
    (pad 1 smd rect (at 0 2.032 90) (size 0.85 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C65-Pad2)"))
    (pad 2 smd rect (at 0 -2.032 90) (size 0.85 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/TZC3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TZC3 (layer F.Cu) (tedit 56732153)
    (at 42.949 40.785)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference CV4 (at 0 -3.302) (layer F.SilkS))
    (fp_text value CVar_1.4-3.0_pF (at 0 3.429) (layer F.Fab))
    (pad 1 smd rect (at 0 2.032 90) (size 0.85 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C60-Pad1)"))
    (pad 2 smd rect (at 0 -2.032 90) (size 0.85 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/TZC3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOP-4 (layer F.Cu) (tedit 5675591C)
    (at 50.569 46.285878 90)
    (tags SOP-4)
    (fp_text reference RE5 (at 5.035878 -0.569 180) (layer F.SilkS))
    (fp_text value AQY282SX (at 0 3.4 270) (layer F.Fab))
    (pad 1 smd rect (at 3 1.27 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R16-Pad2)"))
    (pad 4 smd rect (at -3 1.27 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(R127-Pad2)"))
    (pad 2 smd rect (at 3 -1.27 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3 -1.27 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C64-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/sop4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOP-4 (layer F.Cu) (tedit 5675591C)
    (at 25.804 46.285878 90)
    (tags SOP-4)
    (fp_text reference RE6 (at 5.035878 -0.804 180) (layer F.SilkS))
    (fp_text value AQY282SX (at 0 3.4 270) (layer F.Fab))
    (pad 1 smd rect (at 3 1.27 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R17-Pad2)"))
    (pad 4 smd rect (at -3 1.27 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(R141-Pad2)"))
    (pad 2 smd rect (at 3 -1.27 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3 -1.27 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C63-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/sop4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOP-4 (layer F.Cu) (tedit 5675591C)
    (at 87.740097 51.58)
    (tags SOP-4)
    (fp_text reference RE7 (at 0 -3.3) (layer F.SilkS))
    (fp_text value AQY282SX (at 0 3.4 180) (layer F.Fab))
    (pad 1 smd rect (at 3 1.27 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 297 "Net-(R138-Pad1)"))
    (pad 4 smd rect (at -3 1.27 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(R119-Pad1)"))
    (pad 2 smd rect (at 3 -1.27 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 298 AWG2_PROTECT))
    (pad 3 smd rect (at -3 -1.27 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(AWG2-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/sop4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOP-4 (layer F.Cu) (tedit 5675591C)
    (at 101.075122 51.58)
    (tags SOP-4)
    (fp_text reference RE8 (at 0 -3.3) (layer F.SilkS))
    (fp_text value AQY282SX (at 0 3.4 180) (layer F.Fab))
    (pad 1 smd rect (at 3 1.27 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(R135-Pad2)"))
    (pad 4 smd rect (at -3 1.27 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(R118-Pad1)"))
    (pad 2 smd rect (at 3 -1.27 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 299 AWG1_PROTECT))
    (pad 3 smd rect (at -3 -1.27 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AWG1-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/sop4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 79.398 164.2925 180)
    (fp_text reference D3 (at 0 2.2925 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 45 A_D15_J19))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 83.462 164.2925 180)
    (fp_text reference D4 (at 0 2.2925 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 47 A_D13_J17))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 87.526 164.2925 180)
    (fp_text reference D5 (at 0.026 2.2925 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 49 A_D11_J15))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 91.59 164.2925 180)
    (fp_text reference D6 (at 0 2.2925 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 51 A_D9_J13))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 95.5 164.2925 180)
    (fp_text reference D7 (at 0.019 2.2925 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 53 A_D7_J7))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 99.583 164.2925 180)
    (fp_text reference D8 (at 0.083 2.2925 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 55 A_D5_J5))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 103.647 164.2925 180)
    (fp_text reference D9 (at 0 2.2925 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 57 A_D3_J3))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 107.711 164.2925 180)
    (fp_text reference D10 (at -0.039 2.2925 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 59 A_D1_J1))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 105.679 159.4665 180)
    (fp_text reference D11 (at 0 2.2165 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 63 A_D2_J4))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 101.615 159.4665 180)
    (fp_text reference D12 (at 0 2.2165 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 65 A_D4_J6))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 97.551 159.4665 180)
    (fp_text reference D13 (at 0 2.2165 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 67 A_D6_J8))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 89.558 159.4665 180)
    (fp_text reference D14 (at 0 2.2165 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 70 A_D8_J14))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 85.494 159.4665 180)
    (fp_text reference D15 (at -0.006 2.2165 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 72 A_D10_J16))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 81.43 159.4665 180)
    (fp_text reference D16 (at -0.07 2.2165 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 74 A_D12_J18))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 77.366 159.4665 180)
    (fp_text reference D17 (at 0 2.2165 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 76 A_D14_J20))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 109.743 159.4665 180)
    (fp_text reference D19 (at 0 2.2165 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 61 A_D0_J2))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 112.3338 164.25)
    (fp_text reference D20 (at 0.1662 -2.25) (layer F.SilkS))
    (fp_text value LM431 (at 0 2.2) (layer F.Fab))
    (pad 3 smd rect (at 0 -1) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 1) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(D20-Pad2)"))
    (pad 1 smd rect (at -0.95 1) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 71.788711 84.791389 180)
    (fp_text reference D21 (at -0.211289 -2.458611 180) (layer F.SilkS))
    (fp_text value LM431 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(D21-Pad2)"))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 63.48015 84.77432 180)
    (fp_text reference D22 (at 0.01985 -2.22568 180) (layer F.SilkS))
    (fp_text value LM431 (at 0 2.2 180) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (pad 2 smd rect (at 0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(D22-Pad2)"))
    (pad 1 smd rect (at -0.95 1 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 50.1245 72.3318 90)
    (fp_text reference D23 (at 2.5818 -0.1245 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(D23-Pad3)"))
    (pad 2 smd rect (at 0.95 1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (pad 1 smd rect (at -0.95 1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 77.5565 70.4522 270)
    (fp_text reference D26 (at 2.7022 -0.0565 360) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 270) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(D26-Pad3)"))
    (pad 2 smd rect (at 0.95 1 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (pad 1 smd rect (at -0.95 1 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 84.7955 70.4522 270)
    (fp_text reference D27 (at 2.7022 -0.0455 360) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 270) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(D27-Pad3)"))
    (pad 2 smd rect (at 0.95 1 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (pad 1 smd rect (at -0.95 1 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23 (layer F.Cu) (tedit 567584C3)
    (at 33.952574 72.3318 90)
    (fp_text reference D29 (at 2.5818 0.047426 180) (layer F.SilkS))
    (fp_text value BAV199 (at 0 2.2 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D29-Pad3)"))
    (pad 2 smd rect (at 0.95 1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (pad 1 smd rect (at -0.95 1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TSSOP8 (layer F.Cu) (tedit 57168719)
    (at 84.892706 87.943402)
    (fp_text reference U16 (at -0.592706 -2.443402) (layer F.SilkS))
    (fp_text value OPA2830 (at 0 2.5) (layer F.Fab))
    (pad 8 smd rect (at 2.2 -0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at -2.2 -0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(D26-Pad3)"))
    (pad 7 smd rect (at 2.2 -0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(D27-Pad3)"))
    (pad 2 smd rect (at -2.2 -0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(R86-Pad1)"))
    (pad 6 smd rect (at 2.2 0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(R108-Pad2)"))
    (pad 3 smd rect (at -2.2 0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(R85-Pad1)"))
    (pad 5 smd rect (at 2.2 0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(R107-Pad1)"))
    (pad 4 smd rect (at -2.2 0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/TSSOP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TSSOP8 (layer F.Cu) (tedit 57168719)
    (at 100.097476 60.978)
    (fp_text reference U20 (at 2.102524 2.522) (layer F.SilkS))
    (fp_text value LM393DGK (at 0 2.5) (layer F.Fab))
    (pad 8 smd rect (at 2.2 -0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at -2.2 -0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 296 AWG1_PROT))
    (pad 7 smd rect (at 2.2 -0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 296 AWG1_PROT))
    (pad 2 smd rect (at -2.2 -0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(R133-Pad2)"))
    (pad 6 smd rect (at 2.2 0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 203 V_UV))
    (pad 3 smd rect (at -2.2 0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 202 V_OV))
    (pad 5 smd rect (at 2.2 0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(R133-Pad2)"))
    (pad 4 smd rect (at -2.2 0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/TSSOP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TSSOP8 (layer F.Cu) (tedit 57168719)
    (at 86.762501 60.978)
    (fp_text reference U21 (at 4.937499 -0.028) (layer F.SilkS))
    (fp_text value LM393DGK (at 0 2.5) (layer F.Fab))
    (pad 8 smd rect (at 2.2 -0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at -2.2 -0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 295 AWG2_PROT))
    (pad 7 smd rect (at 2.2 -0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 295 AWG2_PROT))
    (pad 2 smd rect (at -2.2 -0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(R131-Pad1)"))
    (pad 6 smd rect (at 2.2 0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 203 V_UV))
    (pad 3 smd rect (at -2.2 0.325 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 202 V_OV))
    (pad 5 smd rect (at 2.2 0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(R131-Pad1)"))
    (pad 4 smd rect (at -2.2 0.975 270) (size 0.425 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/TSSOP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SIL6 (layer F.Cu) (tedit 569B6C35)
    (at 76.223 129.431 180)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference J2 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value SIL6 (at 0 2.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.35 0) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 6 +3V3))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 285 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at 1.27 0) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 286 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 287 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 6.35 0) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 288 "Net-(J2-Pad6)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/SIL6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-6 (layer F.Cu) (tedit 56914D5A)
    (at 54.504679 115.128082 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U6 (at -2.128082 0.254679 360) (layer F.SilkS))
    (fp_text value TLV3501 (at 0 3.6 270) (layer F.Fab))
    (pad 5 smd rect (at 0 -1.35) (size 1.05 0.6) (layers F.Cu F.Paste F.Mask)
      (net 170 AN_TRIG))
    (pad 1 smd rect (at -0.95 1.35) (size 1.05 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C73-Pad1)"))
    (pad 2 smd rect (at 0 1.35) (size 1.05 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.95 1.35) (size 1.05 0.6) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(R45-Pad1)"))
    (pad 4 smd rect (at 0.95 -1.35) (size 1.05 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 6 smd rect (at -0.95 -1.35) (size 1.05 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 29.16696 171.030866)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS))
    (fp_text value LM3674MF-1.2 (at 0 3.556) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 2 smd rect (at 0 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 4 smd rect (at 0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 5 smd rect (at -0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(L1-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 27.201 149.51986)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at 0 -2.9) (layer F.SilkS))
    (fp_text value 24LC00_SOT-23 (at 0 3.556) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 293 "Net-(R12-Pad2)"))
    (pad 2 smd rect (at 0 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 292 "Net-(R11-Pad2)"))
    (pad 4 smd rect (at 0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 34.11996 149.59606)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U3 (at 0 -2.9) (layer F.SilkS))
    (fp_text value TPS3820-33 (at 0 3.556) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(U27-Pad49)"))
    (pad 2 smd rect (at 0 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 4 smd rect (at 0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 52.793989 91.176111)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U8 (at 0 -2.9) (layer F.SilkS))
    (fp_text value LMH6559 (at 0 3.556) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(R39-Pad2)"))
    (pad 2 smd rect (at 0 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 3 smd rect (at 0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 CH1_OFFSET))
    (pad 5 smd rect (at -0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 47.424709 78.3008 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U10 (at -2.1992 1.825291 180) (layer F.SilkS))
    (fp_text value AD8065 (at 0 3.556 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 89 "/ANALOG INPUTS/CH1_VGA"))
    (pad 2 smd rect (at 0 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 3 smd rect (at 0.95 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(D23-Pad3)"))
    (pad 4 smd rect (at 0.95 -1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C139-Pad2)"))
    (pad 5 smd rect (at -0.95 -1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 31.422734 78.3008 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U11 (at -2.1992 2.077266 180) (layer F.SilkS))
    (fp_text value AD8065 (at 0 3.556 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 91 "/ANALOG INPUTS/CH2_VGA"))
    (pad 2 smd rect (at 0 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 3 smd rect (at 0.95 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D29-Pad3)"))
    (pad 4 smd rect (at 0.95 -1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C140-Pad2)"))
    (pad 5 smd rect (at -0.95 -1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 36.91904 91.243091)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U13 (at 0 -2.9) (layer F.SilkS))
    (fp_text value LMH6559 (at 0 3.556) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 0 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 3 smd rect (at 0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 CH2_OFFSET))
    (pad 5 smd rect (at -0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 107.05 80.85)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U19 (at 3.3 0 180) (layer F.SilkS))
    (fp_text value SP6205EM5-L (at 0 3.556) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 2 smd rect (at 0 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 200 EN_PWR))
    (pad 4 smd rect (at 0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C133-Pad2)"))
    (pad 5 smd rect (at -0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 108.70706 104.539 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U22 (at 0.039 -3.70706 180) (layer F.SilkS))
    (fp_text value SP6205EM5-L-3-3 (at 0 3.556 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 2 smd rect (at 0 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.95 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 4 smd rect (at 0.95 -1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C127-Pad1)"))
    (pad 5 smd rect (at -0.95 -1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 108.647116 145.687 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U23 (at 2.142 -0.043116 180) (layer F.SilkS))
    (fp_text value SP6205EM5-L (at 0 3.556 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 2 smd rect (at 0 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.95 1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 200 EN_PWR))
    (pad 4 smd rect (at 0.95 -1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C125-Pad2)"))
    (pad 5 smd rect (at -0.95 -1.1 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT363 (layer F.Cu) (tedit 5675A3C3)
    (at 45.1461 68.3821)
    (fp_text reference Q2 (at 2.6039 -0.1321) (layer F.SilkS))
    (fp_text value BSS138BKS (at 0 2.667) (layer F.Fab))
    (pad 1 smd rect (at 0.762 -0.889 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.762 0.889 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 98 RE3))
    (pad 4 smd rect (at -0.762 0.889 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.762 -0.889 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 99 RE4))
    (pad 2 smd rect (at 0 -0.889 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(Q2-Pad2)"))
    (pad 5 smd rect (at 0 0.889 270) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(Q2-Pad5)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/sot363.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT363 (layer F.Cu) (tedit 5675A3C3)
    (at 94.2189 57.7649 180)
    (fp_text reference Q3 (at -0.0311 2.2649 180) (layer F.SilkS))
    (fp_text value BSS138BKS (at 0 2.667 180) (layer F.Fab))
    (pad 1 smd rect (at 0.762 -0.889 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.762 0.889 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 298 AWG2_PROTECT))
    (pad 4 smd rect (at -0.762 0.889 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.762 -0.889 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 299 AWG1_PROTECT))
    (pad 2 smd rect (at 0 -0.889 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 295 AWG2_PROT))
    (pad 5 smd rect (at 0 0.889 90) (size 0.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 296 AWG1_PROT))
    (model ${KIPRJMOD}/ScopefunPackages3D/sot363.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TSSOP14 (layer F.Cu) (tedit 56AE30D1)
    (at 67.682001 96.470588 90)
    (fp_text reference U15 (at 4.420588 0.117999 180) (layer F.SilkS))
    (fp_text value TS9224 (at 0 3.175 90) (layer F.Fab))
    (pad 14 smd rect (at 2.75 -1.95) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(R101-Pad2)"))
    (pad 1 smd rect (at -2.75 -1.95) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(R104-Pad1)"))
    (pad 13 smd rect (at 2.75 -1.3) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(R102-Pad2)"))
    (pad 2 smd rect (at -2.75 -1.3) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(R104-Pad2)"))
    (pad 12 smd rect (at 2.75 -0.65) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 230 CH2_OFFSET_ADJ))
    (pad 3 smd rect (at -2.75 -0.65) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 231 CH2_GAIN_ADJ))
    (pad 11 smd rect (at 2.75 0) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 4 smd rect (at -2.75 0) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 10 smd rect (at 2.75 0.65) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 232 CH1_OFFSET_ADJ))
    (pad 5 smd rect (at -2.75 0.65) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 233 CH1_GAIN_ADJ))
    (pad 9 smd rect (at 2.75 1.3) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(R92-Pad1)"))
    (pad 6 smd rect (at -2.75 1.3) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(R83-Pad1)"))
    (pad 8 smd rect (at 2.75 1.95) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 289 "Net-(R100-Pad2)"))
    (pad 7 smd rect (at -2.75 1.95) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(R41-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/tssop14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOIC8 (layer F.Cu) (tedit 56A66AB5)
    (at 106.520374 90.073395 270)
    (fp_text reference U18 (at 3.826605 0.020374 360) (layer F.SilkS))
    (fp_text value MAX889S (at 0 5.08 270) (layer F.Fab))
    (pad 8 smd rect (at 1.905 2.465 90) (size 0.53 1.98) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.905 -2.465 90) (size 0.53 1.98) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 7 smd rect (at 0.635 2.465 90) (size 0.53 1.98) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(R109-Pad1)"))
    (pad 2 smd rect (at 0.635 -2.465 90) (size 0.53 1.98) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(C129-Pad2)"))
    (pad 6 smd rect (at -0.635 2.465 90) (size 0.53 1.98) (layers F.Cu F.Paste F.Mask)
      (net 200 EN_PWR))
    (pad 3 smd rect (at -0.635 -2.465 90) (size 0.53 1.98) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.905 2.465 90) (size 0.53 1.98) (layers F.Cu F.Paste F.Mask)
      (net 83 -5V))
    (pad 4 smd rect (at -1.905 -2.465 90) (size 0.53 1.98) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C129-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/soic8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-F (layer F.Cu) (tedit 569278F2)
    (at 82.3825 108.2982 90)
    (fp_text reference D31 (at -2.7018 0.6175 180) (layer F.SilkS))
    (fp_text value ZXRE125 (at 0 2.2 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.95 1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.95 1 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23_TO236AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOIC14 (layer F.Cu) (tedit 56A521E8)
    (at 103.157242 138.658488 270)
    (fp_text reference U24 (at -0.658488 -6.142758 540) (layer F.SilkS))
    (fp_text value MCP42100 (at 0 5.5 270) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at -2.7 -3.81 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 235 DPOT_CS))
    (pad 13 smd rect (at 2.7 -2.54 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.7 -2.54 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 234 DPOT_SCK))
    (pad 12 smd rect (at 2.7 -1.27 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 3 smd rect (at -2.7 -1.27 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 236 DPOT_SI))
    (pad 11 smd rect (at 2.7 0 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 4 smd rect (at -2.7 0 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2.7 1.27 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C125-Pad2)"))
    (pad 5 smd rect (at -2.7 1.27 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 2.54 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (pad 6 smd rect (at -2.7 2.54 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C125-Pad2)"))
    (pad 8 smd rect (at 2.7 3.81 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (pad 7 smd rect (at -2.7 3.81 180) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C125-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/soic14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:DIL20_RA (layer F.Cu) (tedit 5717F266)
    (at 92.479 182.15)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference J1 (at -17.549 4.159 180) (layer F.SilkS))
    (fp_text value DIL20_RA (at 0 11.43 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 11.43 -2.54 180) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 60 D1_J1))
    (pad 2 thru_hole circle (at 11.43 0 180) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 62 D0_J2))
    (pad 3 thru_hole circle (at 8.89 -2.54 180) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 58 D3_J3))
    (pad 4 thru_hole circle (at 8.89 0 180) (size 1.8 1.8) (drill 0.889) (layers *.Cu *.SilkS *.Mask)
      (net 64 D2_J4))
    (pad 5 thru_hole circle (at 6.35 -2.54 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 56 D5_J5))
    (pad 6 thru_hole circle (at 6.35 0 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 66 D4_J6))
    (pad 7 thru_hole circle (at 3.81 -2.54 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 54 D7_J7))
    (pad 8 thru_hole circle (at 3.81 0 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 68 D6_J8))
    (pad 9 thru_hole circle (at 1.27 -2.54 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 69 +VCC_DIG))
    (pad 10 thru_hole circle (at 1.27 0 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 11 thru_hole circle (at -1.27 -2.54 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 69 +VCC_DIG))
    (pad 12 thru_hole circle (at -1.27 0 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 13 thru_hole circle (at -3.81 -2.54 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 52 D9_J13))
    (pad 14 thru_hole circle (at -3.81 0 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 71 D8_J14))
    (pad 15 thru_hole circle (at -6.35 -2.54 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 50 D11_J15))
    (pad 16 thru_hole circle (at -6.35 0 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 73 D10_J16))
    (pad 17 thru_hole circle (at -8.89 -2.54 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 48 D13_J17))
    (pad 18 thru_hole circle (at -8.89 0 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 75 D12_J18))
    (pad 19 thru_hole circle (at -11.43 -2.54 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 46 D15_J19))
    (pad 20 thru_hole circle (at -11.43 0 180) (size 1.8 1.8) (drill 0.9144) (layers *.Cu *.SilkS *.Mask)
      (net 77 D14_J20))
    (model ${KIPRJMOD}/ScopefunPackages3D/CON20POS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:CLCC (layer F.Cu) (tedit 5691775D)
    (at 28.075522 128.116906 90)
    (fp_text reference U4 (at 0 5.124478 180) (layer F.SilkS))
    (fp_text value NBXSBA010 (at 0 4.953 90) (layer F.Fab))
    (pad 6 smd rect (at 2.53 -2.54) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at -2.53 -2.54 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 144 EN_CLK))
    (pad 5 smd rect (at 2.53 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C81-Pad2)"))
    (pad 2 smd rect (at -2.53 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 214 RESERVED))
    (pad 4 smd rect (at 2.53 2.54) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C82-Pad2)"))
    (pad 3 smd rect (at -2.53 2.54) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/NBXSBA010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 90.551 58.166 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C142 (at 1.75 0 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 104 58.166 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C141 (at 1.566 -0.1 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 30.725504 73.499946 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C140 (at -0.093946 3.547504 360) (layer F.SilkS))
    (fp_text value C_12p (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C140-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 91 "/ANALOG INPUTS/CH2_VGA"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 46.678914 73.406 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C139 (at 0 3.498914 360) (layer F.SilkS))
    (fp_text value C_12p (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C139-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 89 "/ANALOG INPUTS/CH1_VGA"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 63.307 186.725)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C138 (at 2.898 -0.0815) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 57.109602 107.079 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C135 (at 0.079 3.490398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 86 CH2_GAIN))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 68.072 102.108 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C134 (at 1.651 0 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 107.75 75.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C133 (at -0.211 -3.7655) (layer F.SilkS))
    (fp_text value C_10n (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(C133-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 99.7 82.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C131 (at 1.45 0 180) (layer F.SilkS))
    (fp_text value C_10n (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C131-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 104.8 85.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C130 (at -0.05 -3.5 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 83 -5V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 112.3 89.362602)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C129 (at 0 -2.286) (layer F.SilkS))
    (fp_text value C_1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(C129-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C129-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 112.3 93.9 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C128 (at 0 -2.2 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 108.7 101.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C127 (at 0 -3.6 180) (layer F.SilkS))
    (fp_text value C_10n (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C127-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 112.850944 102.816588 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C126 (at 0 2.3 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 89.281 150.622 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C123 (at 0.017 3.771398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 78.445602 145.052 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C122 (at -1.415 0.054398 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 78.445602 139.337 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C121 (at -1.663 0.054398 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 70.254 140.7213 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C119 (at -2.771 2.2913 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 70.889 157.607)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C117 (at 2.861 -0.1845) (layer F.SilkS))
    (fp_text value C_12p (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C117-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 75.715 174.9605 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C116 (at 2.69 -0.0455 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 76 A_D14_J20))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 77 D14_J20))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 79.779 174.9605 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C115 (at 0.023 -2.7125 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 74 A_D12_J18))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 75 D12_J18))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 83.843 174.9605 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C114 (at 0 -2.7125 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 72 A_D10_J16))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 73 D10_J16))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 87.907 174.9605 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C113 (at -0.023 -2.7125 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 70 A_D8_J14))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 71 D8_J14))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 92.456 175.895 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C112 (at -0.127 2.286 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 95.4 174.9605 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C111 (at 0.023 -2.7125 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 67 A_D6_J8))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 68 D6_J8))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 99.964 174.9605 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C110 (at 0.015 -2.7125 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 65 A_D4_J6))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 66 D4_J6))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 104.028 174.9605 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C109 (at -0.112 -2.7125 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 63 A_D2_J4))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 64 D2_J4))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 107.95 174.9605 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C108 (at 0 -2.7125 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 61 A_D0_J2))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 62 D0_J2))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 106.06 170.3885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C107 (at 0 2.6215 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 59 A_D1_J1))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 60 D1_J1))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 101.996 170.3885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C106 (at 0.004 2.6215 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 57 A_D3_J3))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 58 D3_J3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 97.932 170.3885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C105 (at 0.015 2.6215 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 55 A_D5_J5))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 56 D5_J5))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 93.75 170.3885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C104 (at 0.024 2.6215 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 53 A_D7_J7))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 54 D7_J7))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 89.939 170.3885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C103 (at 0.023 2.6215 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 51 A_D9_J13))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 52 D9_J13))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 85.875 170.3885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C102 (at 0.023 2.6215 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 49 A_D11_J15))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 50 D11_J15))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 81.788 170.3885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C101 (at 0 2.6215 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 47 A_D13_J17))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 48 D13_J17))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 70.889 165.481)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C99 (at 2.361 -0.0625) (layer F.SilkS))
    (fp_text value C_12p (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C99-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 61.681398 173.482 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C98 (at -1.524 0.040602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 62.357 170.942 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C97 (at 0 2.921 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 61.681398 165.227 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C95 (at 4.318 0.040602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 61.681398 167.404 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C94 (at -1.506 0.040602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 45.679398 171.849 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C93 (at -1.669 0.086398 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 45.679398 165.499 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C92 (at 1.633 -0.086398 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 45.679398 162.832 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C91 (at -1.542 -0.040602 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 36.726 127.462602)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C89 (at 0.024 2.287398) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 40 113.937 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C88 (at 1.437 -0.0915 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C88-Pad2)"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 28.217 103.332398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C87 (at 2.436 -0.045602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 27.074 106.888602)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C86 (at -2.324 -0.138602) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 42 CH2_CM))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 30.3125 109.746 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C85 (at -0.004 -3.1125 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 41 "/ADC, DAC/CH2-"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 24.8 121.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C84 (at -3.3 -0.4 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 24.8 123 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C83 (at -3.7 -0.4 360) (layer F.SilkS))
    (fp_text value C_10n (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 30.5665 121.303 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C82 (at -0.003 -2.9335 360) (layer F.SilkS))
    (fp_text value C_10n (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C82-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C82-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 30.5665 119.525 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C81 (at 0.025 -2.9335 360) (layer F.SilkS))
    (fp_text value C_10n (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C81-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C81-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 34.567 116.032602 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C80 (at 0 2.232602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 33.7415 109.746 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C79 (at -0.004 3.1085 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 36 "/ADC, DAC/CH2+"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 35.837 103.332398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C78 (at -0.104 2.240398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 44.092 103.332398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C77 (at 2.309 0.081398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 41.806 106.888602)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C76 (at -2.436 -0.081602) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 35 CH1_CM))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 46.2 109.746 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C75 (at -1.754 -0.037398 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 34 "/ADC, DAC/CH1-"))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 45.362 116.032398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C74 (at -0.038 2.232398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 49.2 116.1 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C73 (at 1.596 -0.235602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C73-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 49.65 109.746 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C72 (at -1.704 0.033602 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 32 "/ADC, DAC/CH1+"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 51.712 103.332602 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C71 (at -0.104 2.240602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 57.109602 95.395 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C70 (at 0.145 -3.109602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 31 CH1_GAIN))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 67.777599 89.934 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C69 (at 1.434 -0.027599 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 72.921 59.5175 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C68 (at 0.021 -3.8325 180) (layer F.SilkS))
    (fp_text value C_13p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C67-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C68-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 70.127 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C67 (at 0.373 2.3095 180) (layer F.SilkS))
    (fp_text value C_300p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C67-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 67.206 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C66 (at 0.294 2.3095 180) (layer F.SilkS))
    (fp_text value C_2p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C65-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 62.888 46.6905)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C65 (at -0.15 -2.3675) (layer F.SilkS))
    (fp_text value C_300p (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C65-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C65-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 57.681 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C64 (at 0.023 2.2405 180) (layer F.SilkS))
    (fp_text value C_22n (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C64-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C64-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 32.662 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C63 (at 0 2.3095 180) (layer F.SilkS))
    (fp_text value C_22n (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C63-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C63-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 37.361 46.6905)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C62 (at -0.361 -2.2405) (layer F.SilkS))
    (fp_text value C_300p (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C60-Pad1)"))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C62-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 44.092 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C61 (at -0.485 2.5595 180) (layer F.SilkS))
    (fp_text value C_300p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C59-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 41.679 46.6905 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C60 (at 0 2.5595 180) (layer F.SilkS))
    (fp_text value C_2p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C60-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 47.267 59.5175 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C59 (at -0.533 -2.3325 180) (layer F.SilkS))
    (fp_text value C_13p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C59-Pad2)"))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C59-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 36.599 70.5665 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C58 (at 0.099 2.2165 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 43.053 77.6785)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C57 (at -2.318 0.8215) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 35.329 77.6785 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C56 (at -2.263 0.0815 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 36.599 74.041)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C55 (at 2.401 0.1529) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 26.797 77.6785)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C54 (at -2.189 0.0715) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 28.321 89.281 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C53 (at 0.023 -2.331398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 31.877 89.281 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C52 (at 0.023 -2.331398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 39.647 87.584398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C51 (at -0.003 2.234398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 18 CH2_OFFSET))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 44.196 89.281 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C50 (at -0.104 -2.331398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 47.775 89.281 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C49 (at 0.023 -2.331398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 55.522 87.584398 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C48 (at 0.172 2.234398 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 17 CH1_OFFSET))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 51.204 77.6785 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C47 (at -2.517 -0.0455 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 53.236 70.588 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C46 (at 0.036 2.2165 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 53.236 74.062)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C45 (at 2.514 0.1529) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 63.459398 76.599 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C44 (at 0.051 3.309398 360) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 71.714599 76.599 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C43 (at 0 -3.214599 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 81.7 68.738 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C42 (at -0.191 2.2825 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 74.191 68.738 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C41 (at 0.041 2.188 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 16 -2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 81.7 72.162)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C39 (at 0 2.2825) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 15 +2.88V))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 88.519 83.693 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C37 (at 0 2.159 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 82.7 92.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C36 (at 0 2.4 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 108.900284 140.624 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C33 (at -2.412716 0 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 80.096398 111.778 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C31 (at 1.4912 -0.492798 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 75.651602 109.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C30 (at -1.5 0.098398 180) (layer F.SilkS))
    (fp_text value C_12p (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 11 ~IOUT1))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 12 IOUT1))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 72.3 109.9 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C29 (at 0 2.1 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 68.6 109.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C28 (at 0.111 -3.289599 180) (layer F.SilkS))
    (fp_text value C_12p (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 9 IOUT2))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 10 ~IOUT2))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 67 111.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C27 (at 0 3.1 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 64.3 117.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C26 (at -1.4 0 360) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 180) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 58.824 115.143602)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C25 (at 0 -2.286) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 53.934602 124.605 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C23 (at 2.105 -0.034602 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 49.2 121 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C22 (at 0 -2.985602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C22-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 46.124 124.922398)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C21 (at 0 -2.286) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 54.1 154.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C12 (at 0.0008 -3.065398 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 39.012 140.462)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -2.286) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 30.503 148.6715)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -2.286) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 270) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 25.169 171.43625 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -2.286 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 4 +VCC_USB_P))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 61.681398 162.451 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C96 (at 2.812 0.040602 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 77.747 170.3885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C100 (at 0.023 2.6215 180) (layer F.SilkS))
    (fp_text value C_18p (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 45 A_D15_J19))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 46 D15_J19))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 112.776 159.3395 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C137 (at 2.959 0.1605 180) (layer F.SilkS))
    (fp_text value C_10u (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 87 +3.3V_PD))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:G6K-2F-Y (layer F.Cu) (tedit 56755A3F)
    (at 64.3485 56.533 180)
    (fp_text reference RE4 (at 0 -5.9 180) (layer F.SilkS))
    (fp_text value G6K-2F-Y-DC4.5 (at 0 6.2 180) (layer F.Fab))
    (pad 7 smd rect (at 3.5 -0.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C68-Pad1)"))
    (pad 8 smd rect (at 3.5 -3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 99 RE4))
    (pad 1 smd rect (at -3.5 -3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 6 smd rect (at 3.5 1.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 291 "Net-(RE3-Pad3)"))
    (pad 5 smd rect (at 3.5 3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C65-Pad1)"))
    (pad 2 smd rect (at -3.5 -0.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C67-Pad1)"))
    (pad 3 smd rect (at -3.5 1.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(R121-Pad1)"))
    (pad 4 smd rect (at -3.5 3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C65-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/G6K-2F-Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:G6K-2F-Y (layer F.Cu) (tedit 56755A3F)
    (at 38.5675 56.533 180)
    (fp_text reference RE2 (at 0 -5.9 180) (layer F.SilkS))
    (fp_text value G6K-2F-Y-DC4.5 (at 0 6.2 180) (layer F.Fab))
    (pad 7 smd rect (at 3.5 -0.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C59-Pad1)"))
    (pad 8 smd rect (at 3.5 -3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 102 RE2))
    (pad 1 smd rect (at -3.5 -3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 6 smd rect (at 3.5 1.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 290 "Net-(RE1-Pad3)"))
    (pad 5 smd rect (at 3.5 3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C62-Pad1)"))
    (pad 2 smd rect (at -3.5 -0.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C59-Pad2)"))
    (pad 3 smd rect (at -3.5 1.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(R123-Pad1)"))
    (pad 4 smd rect (at -3.5 3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C60-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/G6K-2F-Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:G6K-2F-Y (layer F.Cu) (tedit 56755A3F)
    (at 27.8995 56.533 180)
    (fp_text reference RE1 (at 0 -5.9 180) (layer F.SilkS))
    (fp_text value G6K-2F-Y-DC4.5 (at 0 6.2 180) (layer F.Fab))
    (pad 7 smd rect (at 3.5 -0.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 3.5 -3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 104 RE1))
    (pad 1 smd rect (at -3.5 -3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 Va))
    (pad 6 smd rect (at 3.5 1.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 3.5 3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.5 -0.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.5 1.6 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 290 "Net-(RE1-Pad3)"))
    (pad 4 smd rect (at -3.5 3.8 90) (size 0.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C63-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/G6K-2F-Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:BNC-5-1634556-0 (layer F.Cu) (tedit 570155F2)
    (at 58.062 36.85)
    (tags "BNC 5-1634556-0")
    (fp_text reference CH1 (at -0.062 6.25) (layer F.SilkS))
    (fp_text value BNC (at 0 8.763) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.004 -0.004) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.SilkS *.Mask)
      (net 25 "Net-(C64-Pad2)"))
    (pad 2 thru_hole circle (at -3.302 -3.302) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.298 -3.302) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.302 3.298) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.298 3.298) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/BNC-5-1634556-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:BNC-5-1634556-0 (layer F.Cu) (tedit 570155F2)
    (at 81.938 36.85)
    (tags "BNC 5-1634556-0")
    (fp_text reference AWG2 (at 0.162 6.25) (layer F.SilkS))
    (fp_text value BNC (at 0 8.763) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.004 -0.004) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(AWG2-Pad1)"))
    (pad 2 thru_hole circle (at -3.302 -3.302) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.298 -3.302) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.302 3.298) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.298 3.298) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/BNC-5-1634556-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:BNC-5-1634556-0 (layer F.Cu) (tedit 570155F2)
    (at 105.814 36.85)
    (tags "BNC 5-1634556-0")
    (fp_text reference AWG1 (at 0.286 6.25) (layer F.SilkS))
    (fp_text value BNC (at 0 8.763) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.004 -0.004) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(AWG1-Pad1)"))
    (pad 2 thru_hole circle (at -3.302 -3.302) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.298 -3.302) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.302 3.298) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.298 3.298) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/BNC-5-1634556-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:BNC-5-1634556-0 (layer F.Cu) (tedit 570155F2)
    (at 34.186 36.85)
    (tags "BNC 5-1634556-0")
    (fp_text reference CH2 (at 0.014 6.25) (layer F.SilkS))
    (fp_text value BNC (at 0 8.763) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.004 -0.004) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.SilkS *.Mask)
      (net 23 "Net-(C63-Pad2)"))
    (pad 2 thru_hole circle (at -3.302 -3.302) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.298 -3.302) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.302 3.298) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.298 3.298) (size 3.55 3.55) (drill 1.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/BNC-5-1634556-0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:L_3X3MM (layer F.Cu) (tedit 56A67E0D)
    (at 30.40267 164.003702 90)
    (descr "MURATA Inductor")
    (tags "MURATA Inductor")
    (attr smd)
    (fp_text reference L1 (at 2.753702 0.09733 180) (layer F.SilkS))
    (fp_text value L_4.7u (at 0 3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.075 0 90) (size 1.15 3.3) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.075 0 90) (size 1.15 3.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (model ${KIPRJMOD}/ScopefunPackages3D/L_3x3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer F.Cu) (tedit 56FD7C61)
    (at 67.841 140.625288 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C120 (at -0.485 2.195288 180) (layer F.SilkS))
    (fp_text value C_0.47u (at 0 1.905 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.45 90) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.45 90) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer F.Cu) (tedit 56FD7C61)
    (at 67.691 146.685 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C118 (at -1.12 1.980912 180) (layer F.SilkS))
    (fp_text value C_0.47u (at 0 1.905 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.45 90) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.45 90) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 46.574012 148.6588 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C90 (at 1.4552 -0.034988 360) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 270) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer F.Cu) (tedit 56FD7C61)
    (at 53.9 126.8148 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C24 (at 0.0648 2.686988 180) (layer F.SilkS))
    (fp_text value C_0.47u (at 0 1.905 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.45) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.45) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 46.124 132.079788)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at 0 1.778) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 90) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 90) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 50.0888 130.7518 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C19 (at -1.4982 0.000012 180) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 90) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 180) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 180) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 55.776 131.20181 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at -0.026 2.298186 180) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 180) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 270) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 270) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 57.3 131.20181 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at -0.0024 -2.04659 180) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 180) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 270) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 270) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 63.627 133.985 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at 0 1.779588 180) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 180) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 270) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 270) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 63.627 139.954)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 0 1.778) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 90) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 90) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V2))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 59.817 148.6588 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at -1.4658 -0.127 360) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 270) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer F.Cu) (tedit 56FD7C61)
    (at 54.1 152.5958 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at -0.1542 -2.559988 180) (layer F.SilkS))
    (fp_text value C_0.47u (at 0 1.905 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.45) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.45) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 52.705 148.6588 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 1.4088 0.083012 180) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 90) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 180) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 180) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V2))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 49.403 148.6588 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 1.4552 -0.127 360) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 270) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 46.124 146.568888 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at -1.882 0.010888 180) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 180) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 270) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 270) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 46.124 143.636712)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 1.626 0.113288) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 90) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 90) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V2))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 46.124 139.217112)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 1.626 0.032888) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 90) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 90) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V2))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer F.Cu) (tedit 56FD7C61)
    (at 41.3742 140.462)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -1.778) (layer F.SilkS))
    (fp_text value C_0.47u (at 0 1.905) (layer F.Fab))
    (pad 2 smd rect (at 0 0.45 270) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.45 270) (size 0.45 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0402 (layer B.Cu) (tedit 56FD7C61)
    (at 53.467 130.7518 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C18 (at -1.4982 -0.174988 180) (layer B.SilkS))
    (fp_text value C_0.47u (at 0 -1.905 90) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.45 180) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0.45 180) (size 0.45 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V2))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:R_0603 (layer F.Cu) (tedit 56FD7D95)
    (at 57.3 123.8 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R143 (at -0.1 2.2 180) (layer F.SilkS))
    (fp_text value R_82R (at 0 2.413 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 249 DAC_CLK))
    (pad 1 smd rect (at 0 -0.762 90) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 294 "Net-(R143-Pad1)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:TSSOP48 (layer F.Cu) (tedit 572B9530)
    (at 85.609189 142.547052)
    (fp_text reference U28 (at 0 -7.5 180) (layer F.SilkS))
    (fp_text value 74AVCH16T245 (at 0 7.5) (layer F.Fab))
    (pad 48 smd rect (at 3.75 -5.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.75 -5.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 261 DIR1))
    (pad 47 smd rect (at 3.75 -5.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 61 A_D0_J2))
    (pad 2 smd rect (at -3.75 -5.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 282 B_D0_J2))
    (pad 46 smd rect (at 3.75 -4.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 59 A_D1_J1))
    (pad 3 smd rect (at -3.75 -4.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 281 B_D1_J1))
    (pad 45 smd rect (at 3.75 -4.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -3.75 -4.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd rect (at 3.75 -3.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 63 A_D2_J4))
    (pad 5 smd rect (at -3.75 -3.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 280 B_D2_J4))
    (pad 43 smd rect (at 3.75 -3.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 57 A_D3_J3))
    (pad 6 smd rect (at -3.75 -3.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 283 B_D3_J3))
    (pad 42 smd rect (at 3.75 -2.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (pad 7 smd rect (at -3.75 -2.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 41 smd rect (at 3.75 -2.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 65 A_D4_J6))
    (pad 8 smd rect (at -3.75 -2.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 279 B_D4_J6))
    (pad 40 smd rect (at 3.75 -1.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 55 A_D5_J5))
    (pad 9 smd rect (at -3.75 -1.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 278 B_D5_J5))
    (pad 39 smd rect (at 3.75 -1.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -3.75 -1.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 38 smd rect (at 3.75 -0.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 67 A_D6_J8))
    (pad 11 smd rect (at -3.75 -0.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 277 B_D6_J8))
    (pad 37 smd rect (at 3.75 -0.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 53 A_D7_J7))
    (pad 12 smd rect (at -3.75 -0.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 276 B_D7_J7))
    (pad 36 smd rect (at 3.75 0.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 51 A_D9_J13))
    (pad 13 smd rect (at -3.75 0.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 275 B_D9_J13))
    (pad 35 smd rect (at 3.75 0.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 70 A_D8_J14))
    (pad 14 smd rect (at -3.75 0.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 274 B_D8_J14))
    (pad 34 smd rect (at 3.75 1.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at -3.75 1.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 33 smd rect (at 3.75 1.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 49 A_D11_J15))
    (pad 16 smd rect (at -3.75 1.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 273 B_D11_J15))
    (pad 32 smd rect (at 3.75 2.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 72 A_D10_J16))
    (pad 17 smd rect (at -3.75 2.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 272 B_D10_J16))
    (pad 31 smd rect (at 3.75 2.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 69 +VCC_DIG))
    (pad 18 smd rect (at -3.75 2.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 30 smd rect (at 3.75 3.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 47 A_D13_J17))
    (pad 19 smd rect (at -3.75 3.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 271 B_D13_J17))
    (pad 29 smd rect (at 3.75 3.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 74 A_D12_J18))
    (pad 20 smd rect (at -3.75 3.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 270 B_D12_J18))
    (pad 28 smd rect (at 3.75 4.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 21 smd rect (at -3.75 4.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 27 smd rect (at 3.75 4.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 45 A_D15_J19))
    (pad 22 smd rect (at -3.75 4.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 269 B_D15_J19))
    (pad 26 smd rect (at 3.75 5.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 76 A_D14_J20))
    (pad 23 smd rect (at -3.75 5.25 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 268 B_D14_J20))
    (pad 25 smd rect (at 3.75 5.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -3.75 5.75 270) (size 0.28 1.5) (layers F.Cu F.Paste F.Mask)
      (net 262 DIR2))
    (model ${KIPRJMOD}/ScopefunPackages3D/TSSOP48.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 572BAB02)
    (at 114.5 35.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MH3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.2 5.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module ScopefunPackagesLibrary:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 57378471)
    (at 25.5 183.3)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MH1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 1.1) (size 5.2 5.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module ScopefunPackagesLibrary:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 572BAB02)
    (at 25.5 35.5 90)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MH2 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.2 5.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module ScopefunPackagesLibrary:VIA-0.5mm-0.3mm (layer F.Cu) (tedit 572BB523)
    (at 39.939 120.177)
    (fp_text reference REF**3 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.5-0.3mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.5mm-0.3mm (layer F.Cu) (tedit 572BB523)
    (at 38.415 121.828)
    (fp_text reference REF**4 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.5-0.3mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.5mm-0.3mm (layer F.Cu) (tedit 572BB523)
    (at 41.463 118.78)
    (fp_text reference REF**2 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.5-0.3mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.5mm-0.3mm (layer F.Cu) (tedit 572BB523)
    (at 41.463 121.828)
    (fp_text reference REF**5 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.5-0.3mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.5mm-0.3mm (layer F.Cu) (tedit 572BB523)
    (at 38.415 118.78)
    (fp_text reference REF**1 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.5-0.3mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:R_0805 (layer F.Cu) (tedit 56FD91CC)
    (at 26.985 179.105 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R144 (at -1.705 -0.015 360) (layer F.SilkS))
    (fp_text value R_0R (at 0 2.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0 1.1 180) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -1.1 180) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask)
      (net 300 "Net-(P1-Pad5)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:3528-21 (layer F.Cu) (tedit 56FEFBB9)
    (at 110.871 150.622 270)
    (fp_text reference C136 (at 0.035 5.273 360) (layer F.SilkS))
    (fp_text value CP_47u (at 0 3.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.46 90) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 1.46 90) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 69 +VCC_DIG))
    (model ${KIPRJMOD}/ScopefunPackages3D/3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:3528-21 (layer F.Cu) (tedit 56FEFBB9)
    (at 102.743 76.327 90)
    (fp_text reference C132 (at -2.500886 -0.028954 180) (layer F.SilkS))
    (fp_text value CP_47u (at 0 3.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.46 270) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 1.46 270) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 8 Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:3528-21 (layer F.Cu) (tedit 56FEFBB9)
    (at 91.149691 76.327 270)
    (fp_text reference C38 (at 2.805114 -0.100309 360) (layer F.SilkS))
    (fp_text value CP_47u (at 0 3.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.46 90) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 14 -Va))
    (pad 1 smd rect (at 0 1.46 90) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/ScopefunPackages3D/3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:3528-21 (layer F.Cu) (tedit 56FEFBB9)
    (at 92.963988 97.536)
    (fp_text reference C35 (at 0 -3.3) (layer F.SilkS))
    (fp_text value CP_47u (at 0 3.5) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.46 180) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 1.46 180) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 6 +3V3))
    (model ${KIPRJMOD}/ScopefunPackages3D/3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:3528-21 (layer F.Cu) (tedit 56FEFBB9)
    (at 26.246214 163.968396 180)
    (fp_text reference C2 (at -0.003786 3.468396 180) (layer F.SilkS))
    (fp_text value CP_47u (at 0 3.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.46) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 1.46) (size 2.35 1.8) (layers F.Cu F.Paste F.SilkS F.Mask)
      (net 5 +1V2))
    (model ${KIPRJMOD}/ScopefunPackages3D/3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 98.679 63.881 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C143 (at -0.019 -4.079 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:C_0603 (layer F.Cu) (tedit 56FD82E3)
    (at 85.344 64.007999 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C144 (at 0.007999 3.756 180) (layer F.SilkS))
    (fp_text value C_0.1u (at 0 2.413 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -0.762) (size 0.635 0.889) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5737843A)
    (at 114.5 184.4)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference MH4 (at -76.585 -65.485) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.2 5.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 160.46)
    (fp_text reference REF**112 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 157.92)
    (fp_text reference REF**113 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 155.38)
    (fp_text reference REF**114 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 152.84)
    (fp_text reference REF**115 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 150.3)
    (fp_text reference REF**116 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 147.76)
    (fp_text reference REF**117 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 145.22)
    (fp_text reference REF**118 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 142.68)
    (fp_text reference REF**119 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 165.54)
    (fp_text reference REF**111221 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 163)
    (fp_text reference REF**1111 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 160.46)
    (fp_text reference REF**1112 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 157.92)
    (fp_text reference REF**1113 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 155.38)
    (fp_text reference REF**1114 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 152.84)
    (fp_text reference REF**1115 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 150.3)
    (fp_text reference REF**1116 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 147.76)
    (fp_text reference REF**1117 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 145.22)
    (fp_text reference REF**1118 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 142.68)
    (fp_text reference REF**1119 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 140.14)
    (fp_text reference REF**1120 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 137.6)
    (fp_text reference REF**1121 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 135.06)
    (fp_text reference REF**1122 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 132.52)
    (fp_text reference REF**1123 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 129.979998)
    (fp_text reference REF**1124 (at 0 0.635002) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 127.44)
    (fp_text reference REF**1125 (at 0 0.634998) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 124.9)
    (fp_text reference REF**1126 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 122.36)
    (fp_text reference REF**1127 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 119.82)
    (fp_text reference REF**1128 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 117.28)
    (fp_text reference REF**1129 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 114.74)
    (fp_text reference REF**1130 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 112.2)
    (fp_text reference REF**1131 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 109.66)
    (fp_text reference REF**1132 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 107.12)
    (fp_text reference REF**1133 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 104.58)
    (fp_text reference REF**1134 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 102.04)
    (fp_text reference REF**1135 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 99.5)
    (fp_text reference REF**1136 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 96.96)
    (fp_text reference REF**1137 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 94.42)
    (fp_text reference REF**1138 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 91.88)
    (fp_text reference REF**1139 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 89.34)
    (fp_text reference REF**1140 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 86.8)
    (fp_text reference REF**1141 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 84.26)
    (fp_text reference REF**1142 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 81.72)
    (fp_text reference REF**1143 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 79.18)
    (fp_text reference REF**1144 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 76.64)
    (fp_text reference REF**1145 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 74.1)
    (fp_text reference REF**1146 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 71.56)
    (fp_text reference REF**1147 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 69.02)
    (fp_text reference REF**1148 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 66.48)
    (fp_text reference REF**1149 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 63.94)
    (fp_text reference REF**1150 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 61.4)
    (fp_text reference REF**1151 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 58.86)
    (fp_text reference REF**1152 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 56.32)
    (fp_text reference REF**1153 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 53.78)
    (fp_text reference REF**1154 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 51.24)
    (fp_text reference REF**1155 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 48.7)
    (fp_text reference REF**1156 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 46.16)
    (fp_text reference REF**1157 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 43.62)
    (fp_text reference REF**1158 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 41.08)
    (fp_text reference REF**1159 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 38.54)
    (fp_text reference REF**1160 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 36)
    (fp_text reference REF**1161 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 33.46)
    (fp_text reference REF**1162 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 118.5 30.92)
    (fp_text reference REF**1163 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 185.86)
    (fp_text reference REF**12 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 183.32)
    (fp_text reference REF**13 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 180.78)
    (fp_text reference REF**14 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 178.24)
    (fp_text reference REF**15 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 175.7)
    (fp_text reference REF**16 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 173.16)
    (fp_text reference REF**17 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 170.62)
    (fp_text reference REF**18 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 168.08)
    (fp_text reference REF**19 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 165.54)
    (fp_text reference REF**110 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 163)
    (fp_text reference REF**111 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 160.46)
    (fp_text reference REF**112 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 157.92)
    (fp_text reference REF**113 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 155.38)
    (fp_text reference REF**114 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 152.84)
    (fp_text reference REF**115 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 150.3)
    (fp_text reference REF**116 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 147.76)
    (fp_text reference REF**117 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 145.22)
    (fp_text reference REF**118 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 142.68)
    (fp_text reference REF**119 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 140.14)
    (fp_text reference REF**120 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 137.6)
    (fp_text reference REF**121 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 135.06)
    (fp_text reference REF**122 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 132.52)
    (fp_text reference REF**123 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 129.979998)
    (fp_text reference REF**124 (at 0 0.635002) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 127.44)
    (fp_text reference REF**125 (at 0 0.634998) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 124.9)
    (fp_text reference REF**126 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 122.36)
    (fp_text reference REF**127 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 119.82)
    (fp_text reference REF**128 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 117.28)
    (fp_text reference REF**129 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 114.74)
    (fp_text reference REF**130 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 112.2)
    (fp_text reference REF**131 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 109.66)
    (fp_text reference REF**132 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 107.12)
    (fp_text reference REF**133 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 104.58)
    (fp_text reference REF**134 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 102.04)
    (fp_text reference REF**135 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 99.5)
    (fp_text reference REF**136 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 96.96)
    (fp_text reference REF**137 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 94.42)
    (fp_text reference REF**138 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 91.88)
    (fp_text reference REF**139 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 89.34)
    (fp_text reference REF**140 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 86.8)
    (fp_text reference REF**141 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 84.26)
    (fp_text reference REF**142 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 81.72)
    (fp_text reference REF**143 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 79.18)
    (fp_text reference REF**144 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 76.64)
    (fp_text reference REF**145 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 74.1)
    (fp_text reference REF**146 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 71.56)
    (fp_text reference REF**147 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 69.02)
    (fp_text reference REF**148 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 66.48)
    (fp_text reference REF**149 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 63.94)
    (fp_text reference REF**150 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 61.4)
    (fp_text reference REF**151 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 58.86)
    (fp_text reference REF**152 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 56.32)
    (fp_text reference REF**153 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 53.78)
    (fp_text reference REF**154 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 51.24)
    (fp_text reference REF**155 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 48.7)
    (fp_text reference REF**156 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 46.16)
    (fp_text reference REF**157 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 43.62)
    (fp_text reference REF**158 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 41.08)
    (fp_text reference REF**159 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 38.54)
    (fp_text reference REF**160 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 36)
    (fp_text reference REF**161 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 33.46)
    (fp_text reference REF**162 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:VIA-0.8mm-0.6mm (layer F.Cu) (tedit 572B9A41)
    (at 21.5 30.92)
    (fp_text reference REF**163 (at 0 0.635) (layer F.SilkS) hide)
    (fp_text value VIA-0.8-0.6mm (at 0 -1.143) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module ScopefunPackagesLibrary:SLP3-300-100-R (layer F.Cu) (tedit 5738419E)
    (at 71.247 187.4 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference SLP1 (at -4.901 -0.809 540) (layer F.SilkS))
    (fp_text value SLP3-300-100-R (at -0.254 -3.302 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.6924 1.28925 270) (size 1.6764 1.6764) (drill 1.1684) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.6924 -1.28925 270) (size 1.6764 1.6764) (drill 1.1684) (layers *.Cu *.SilkS *.Mask)
      (net 107 "Net-(LED1-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/SLP3-300-100-R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SLP3-300-100-R (layer F.Cu) (tedit 5738419E)
    (at 93.9 32.299999 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference SLP2 (at -2.184401 4.3688 180) (layer F.SilkS))
    (fp_text value SLP3-300-100-R (at -0.254 -3.302 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.6924 1.28925 90) (size 1.6764 1.6764) (drill 1.1684) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.6924 -1.28925 90) (size 1.6764 1.6764) (drill 1.1684) (layers *.Cu *.SilkS *.Mask)
      (net 108 "Net-(LED2-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/SLP3-300-100-R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SLP3-300-100-R (layer F.Cu) (tedit 5738419E)
    (at 46.1 32.299999 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference SLP3 (at -2.794001 4.318 180) (layer F.SilkS))
    (fp_text value SLP3-300-100-R (at -0.254 -3.302 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.6924 1.28925 90) (size 1.6764 1.6764) (drill 1.1684) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.6924 -1.28925 90) (size 1.6764 1.6764) (drill 1.1684) (layers *.Cu *.SilkS *.Mask)
      (net 109 "Net-(LED3-Pad2)"))
    (model ${KIPRJMOD}/ScopefunPackages3D/SLP3-300-100-R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ScopefunPackagesLibrary:SOT23-5 (layer F.Cu) (tedit 57094B30)
    (at 95.527 80.829116)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U17 (at 0 -2.9) (layer F.SilkS))
    (fp_text value LT1964-BYP (at 0 3.556) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 83 -5V))
    (pad 3 smd rect (at 0.95 1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(C131-Pad1)"))
    (pad 4 smd rect (at 0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(R113-Pad1)"))
    (pad 5 smd rect (at -0.95 -1.1 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 -Va))
    (model ${KIPRJMOD}/ScopefunPackages3D/SOT23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Licensed under\nCERN OHL v.1.2" (at 114.488 48.168 90) (layer F.SilkS))
  (gr_line (start 20 189.9) (end 20 29.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120 189.9) (end 20 189.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120 29.9) (end 120 189.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20 29.9) (end 120 29.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 80.772 139.573) (xy 82.55 139.573) (xy 82.55 140.081) (xy 78.867 140.081) (xy 78.867 138.938)
        (xy 80.137 138.938)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 80.772 145.034) (xy 82.55 145.034) (xy 82.55 145.542) (xy 78.867 145.542) (xy 78.867 144.399)
        (xy 80.137 144.399)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 64.77 139.319) (xy 72.009 139.319) (xy 72.009 140.462) (xy 67.564 140.462) (xy 67.056 139.954)
        (xy 66.675 139.573) (xy 66.548 139.573) (xy 64.77 139.573)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.304 29.396) (xy 120.65 29.396) (xy 120.65 190.432) (xy 19.304 190.432)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 72.009 141.097) (xy 72.0065 142.0845) (xy 64.8945 142.0845) (xy 64.8945 141.8305) (xy 66.0375 141.8305)
        (xy 66.294 141.605) (xy 66.294 140.335) (xy 66.04 140.081) (xy 64.897 140.081) (xy 64.897 139.827)
        (xy 66.421 139.827) (xy 67.31 140.716) (xy 72.009 140.716)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 37.7 139.2) (xy 44.05 139.2) (xy 44.069 140.589) (xy 42.545 140.589) (xy 42.164 140.208)
        (xy 37.719 140.208)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 53.9725 155.737) (xy 53.9725 150.022) (xy 53.655 150.022) (xy 53.655 151.673) (xy 52.893 152.4985)
        (xy 52.893 155.737)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 52.5 123.1) (xy 53.8 123.1) (xy 53.8 127.4) (xy 53.6 127.6) (xy 53.6 129.329813)
        (xy 53.1 129.329813) (xy 53.1 127.329813) (xy 52.5 126.729813)
      )
    )
  )
  (zone (net 4) (net_name +VCC_USB_P) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.125 173.228) (xy 115.443 173.228) (xy 115.443 176.784) (xy 111.125 176.784)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.379 163.703) (xy 113.284 163.703) (xy 113.284 162.306) (xy 111.379 162.306)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.826503 159.004) (xy 113.731503 159.004) (xy 113.731503 157.607) (xy 111.826503 157.607)
      )
    )
  )
  (zone (net 87) (net_name +3.3V_PD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.649 159.766) (xy 110.744 159.766) (xy 110.744 161.29) (xy 113.284 161.29) (xy 113.284 159.766)
      )
    )
  )
  (zone (net 87) (net_name +3.3V_PD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.565 163.484) (xy 75.565 157.008066) (xy 109.728 157.005934) (xy 109.728 158.623) (xy 110.49 159.385)
        (xy 113.157 159.385) (xy 113.157 163.484)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.638 171.069) (xy 24.638 164.592) (xy 27.432 164.592) (xy 27.432 168.529) (xy 27.432 171.069)
      )
    )
  )
  (zone (net 106) (net_name "Net-(L1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.131 164.465) (xy 32.131 167.64) (xy 31.369 168.402) (xy 29.337 168.402) (xy 28.448 169.291)
        (xy 28.448 170.561) (xy 27.94 170.561) (xy 27.94 168.148) (xy 28.702 167.386) (xy 28.702 164.465)
      )
    )
  )
  (zone (net 5) (net_name +1V2) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.1 163.5) (xy 24.6 163.5) (xy 24.6 158.7) (xy 32.1 158.7)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.5 149.1) (xy 33.5 147.5) (xy 30 147.5) (xy 30 148.3) (xy 31 148.3)
        (xy 31.8 149.1)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37.3 127.1) (xy 36.2 127.1) (xy 36.2 124.7) (xy 37 123.9) (xy 37 123.7)
        (xy 37.1 123.6) (xy 37.1 123.4) (xy 37.4 123.4) (xy 37.4 124.2) (xy 37.3 124.3)
      )
    )
  )
  (zone (net 4) (net_name +VCC_USB_P) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.2 105.2) (xy 111.8 105.2) (xy 111.8 103.2) (xy 115.199996 103.2) (xy 115.2 105.8)
        (xy 109.2 105.8)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.2 105.8) (xy 106.6 105.8) (xy 106.3 106.1) (xy 91.6 106.1) (xy 91.6 98.1)
        (xy 94.2 98.1) (xy 94.2 98.7) (xy 98.95 98.7) (xy 104.5 98.7) (xy 106.3 100.5)
        (xy 106.3 104.8) (xy 106.6 105.1) (xy 108.2 105.1)
      )
    )
  )
  (zone (net 4) (net_name +VCC_USB_P) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 91.694) (xy 115.316 91.694) (xy 115.316 93.472) (xy 107.95 93.472)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.997 91.694) (xy 105.537 91.694) (xy 105.537 85.852) (xy 105.283 85.852) (xy 105.283 84.963)
        (xy 106.68 84.963) (xy 107.442 85.725) (xy 107.442 87.0585) (xy 107.442 88.9) (xy 107.696 89.154)
        (xy 109.982 89.154) (xy 109.982 89.662) (xy 107.696 89.662) (xy 107.442 89.916) (xy 107.442 92.456)
        (xy 105.791 92.456) (xy 105.537 92.202) (xy 102.997 92.202)
      )
    )
  )
  (zone (net 14) (net_name -Va) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.806 79.502) (xy 98.552 79.756) (xy 94.869 79.756) (xy 94.234 79.756) (xy 90.932 79.756)
        (xy 87.122 83.566) (xy 87.122 93.472) (xy 70.358 93.472) (xy 67.818 96.012) (xy 67.818 100.838)
        (xy 58.674 109.982) (xy 49.276 109.982) (xy 46.99 112.268) (xy 23.876 112.268) (xy 23.876 87.376)
        (xy 28.956 87.376) (xy 28.956 89.154) (xy 25.4 92.71) (xy 25.4 103.886) (xy 34.036 103.886)
        (xy 34.036 100.584) (xy 35.433 99.187) (xy 35.433 93.853) (xy 37.084 92.202) (xy 37.084 83.566)
        (xy 34.29 80.772) (xy 34.29 78.232) (xy 40.132 78.232) (xy 40.132 80.01) (xy 41.91 81.788)
        (xy 41.91 87.376) (xy 44.704 87.376) (xy 44.704 89.154) (xy 40.64 93.218) (xy 40.64 103.886)
        (xy 49.911 103.886) (xy 49.911 100.7618) (xy 51.308 99.3648) (xy 51.308 93.853) (xy 52.959 92.202)
        (xy 52.959 83.566) (xy 50.2 80.8) (xy 50.2 78.2) (xy 66.6 78.2) (xy 66.6 80.744852)
        (xy 78.8 80.7) (xy 78.8 67.1) (xy 84.074 61.722) (xy 98.806 61.722)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.554 142.91) (xy 107.376 142.91) (xy 107.376 129.794) (xy 86.36 129.794) (xy 86.36 178.181)
        (xy 52.959 178.181) (xy 49.784 175.006) (xy 23.876 175.006) (xy 23.876 163.576) (xy 41.529 163.576)
        (xy 44.958 160.147) (xy 44.958 145.669) (xy 50.546 145.669) (xy 50.546 148.082) (xy 49.403 148.082)
        (xy 49.403 150.114) (xy 56.642 150.114) (xy 56.642 148.082) (xy 66.04 148.082) (xy 66.04 138.43)
        (xy 62.738 138.43) (xy 62.738 136.398) (xy 59.182 132.842) (xy 56.134 132.842) (xy 55.499 132.207)
        (xy 55.499 130.429) (xy 54.102 129.032) (xy 52.324 129.032) (xy 52.324 131.826) (xy 51.054 133.096)
        (xy 44.45 133.096) (xy 42.418 135.128) (xy 42.418 139.446) (xy 34.798 147.066) (xy 34.798 155.194)
        (xy 33.528 156.464) (xy 23.876 156.464) (xy 23.876 113.03) (xy 30.226 113.03) (xy 30.226 118.11)
        (xy 50.292 118.11) (xy 53.213 115.189) (xy 79.629 115.189) (xy 92.202 102.616) (xy 100.838 102.616)
        (xy 100.838 101.854) (xy 91.948 101.854) (xy 79.375 114.427) (xy 52.959 114.427) (xy 50.038 117.348)
        (xy 31.115 117.348) (xy 31.115 113.03) (xy 47.244 113.03) (xy 49.53 110.744) (xy 59.436 110.744)
        (xy 66.675 103.505) (xy 71.374 103.505) (xy 71.374 97.79) (xy 114.554 97.79)
      )
    )
  )
  (zone (net 69) (net_name +VCC_DIG) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.411126 178.181) (xy 95.123 178.181) (xy 95.123 180.848) (xy 89.916 180.848) (xy 89.916 178.181)
        (xy 87.122 178.181) (xy 87.122 130.555081) (xy 106.487 130.558063) (xy 106.487 143.672) (xy 114.554 143.672)
        (xy 114.554 174.498)
      )
    )
  )
  (zone (net 5) (net_name +1V2) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.864 132.588) (xy 55.88 133.604) (xy 58.928 133.604) (xy 62.23 136.906) (xy 62.23 138.938)
        (xy 65.532 138.938) (xy 65.532 147.574) (xy 55.88 147.574) (xy 55.88 149.606) (xy 51.054 149.606)
        (xy 51.054 145.034) (xy 44.196 145.034) (xy 44.196 160.02) (xy 41.148 163.068) (xy 23.876 163.068)
        (xy 23.876 156.972) (xy 34.036 156.972) (xy 35.56 155.448) (xy 35.56 147.066) (xy 43.18 139.446)
        (xy 43.18 135.128) (xy 44.704 133.604) (xy 51.562 133.604) (xy 52.578 132.588) (xy 52.578 129.54)
        (xy 53.848 129.54) (xy 54.864 130.556)
      )
    )
  )
  (zone (net 8) (net_name Va) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27.178 100.584) (xy 30.099 100.584) (xy 30.099 102.87) (xy 27.178 102.87)
      )
    )
  )
  (zone (net 8) (net_name Va) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45.974 100.584) (xy 43.053 100.584) (xy 43.053 102.87) (xy 45.974 102.87)
      )
    )
  )
  (zone (net 14) (net_name -Va) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.036 100.584) (xy 36.957 100.584) (xy 36.957 102.87) (xy 34.036 102.87)
      )
    )
  )
  (zone (net 14) (net_name -Va) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49.911 100.584) (xy 52.705 100.584) (xy 52.705 102.863685) (xy 49.911 102.863685)
      )
    )
  )
  (zone (net 69) (net_name +VCC_DIG) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.138 146.339) (xy 108.138 147.99) (xy 108.773 148.625) (xy 110.932 148.625) (xy 110.932 152.562)
        (xy 106.868 152.562) (xy 106.868 146.339)
      )
    )
  )
  (zone (net 69) (net_name +VCC_DIG) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.154 132.334) (xy 89.154 133.096) (xy 89.154 134.874) (xy 87.376 136.652) (xy 87.376 144.862985)
        (xy 87.376 145.681661) (xy 87.376 149.225) (xy 88.138 149.987) (xy 88.9 149.987) (xy 88.9 152.019)
        (xy 87.249 152.019) (xy 85.598 150.495) (xy 85.598 136.652) (xy 87.376 134.874) (xy 87.376 132.334)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.02))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.7086 93.472) (xy 28.6766 95.504) (xy 28.6766 99.568) (xy 29.6926 100.584) (xy 34.036 100.584)
        (xy 35.4076 99.2124) (xy 35.4076 95.504) (xy 33.3756 93.472) (xy 32.3596 93.472)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.02))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.609 93.472) (xy 44.577 95.504) (xy 44.577 99.568) (xy 45.593 100.584) (xy 50.038 100.584)
        (xy 51.308 99.314) (xy 51.308 95.504) (xy 49.276 93.472) (xy 48.26 93.472)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.02))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.32 112.268) (xy 31.115 112.268) (xy 31.115 117.348) (xy 35.687 117.348) (xy 35.687 118.11)
        (xy 30.226 118.11) (xy 30.226 113.03) (xy 20.32 113.03)
      )
    )
  )
  (zone (net 8) (net_name Va) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 85.598) (xy 96.266 85.598) (xy 96.266 96.774) (xy 71.374 96.774) (xy 70.612 97.536)
        (xy 70.612 102.616) (xy 68.58 102.616) (xy 68.58 96.266) (xy 70.358 94.488) (xy 88.138 94.488)
        (xy 88.138 83.566) (xy 90.932 80.772) (xy 99.568 80.772) (xy 99.568 61.214) (xy 83.82 61.214)
        (xy 78 67) (xy 78 79.8) (xy 67.8 79.8) (xy 67.8 77.5) (xy 49 77.5)
        (xy 49 81.3) (xy 52.07 84.328) (xy 52.07 91.44) (xy 50.038 93.472) (xy 46.609 93.472)
        (xy 44.5516 95.5294) (xy 44.5516 99.5426) (xy 45.593 100.584) (xy 45.974 100.584) (xy 45.974 102.87)
        (xy 41.148 102.87) (xy 41.148 93.726) (xy 45.466 89.408) (xy 45.466 86.614) (xy 42.418 86.614)
        (xy 42.418 81.026) (xy 40.894 79.502) (xy 40.894 77.47) (xy 33.528 77.47) (xy 33.528 81.28)
        (xy 36.576 84.328) (xy 36.576 91.44) (xy 34.544 93.472) (xy 30.734 93.472) (xy 28.702 95.504)
        (xy 28.702 99.568) (xy 29.718 100.584) (xy 30.099 100.584) (xy 30.099 102.87) (xy 25.908 102.87)
        (xy 25.908 92.964) (xy 29.464 89.408) (xy 29.464 86.614) (xy 23.876 86.614) (xy 23.876 44.196)
        (xy 114.554 44.196) (xy 114.554 85.598)
      )
    )
  )
  (zone (net 14) (net_name -Va) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.694 74.041) (xy 94.869 74.041) (xy 94.869 80.391) (xy 94.234 80.391) (xy 94.234 79.121)
        (xy 93.472 78.359) (xy 91.694 78.359)
      )
    )
  )
  (zone (net 8) (net_name Va) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.251 74.041) (xy 106.426 74.041) (xy 106.426 80.391) (xy 105.791 80.391) (xy 105.791 79.121)
        (xy 105.029 78.359) (xy 103.251 78.359)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37.3355 116.494) (xy 34.097 116.494) (xy 34.097 117.129) (xy 34.986 117.129) (xy 35.494 117.637)
        (xy 36.7005 117.637) (xy 36.7005 117.1925) (xy 36.8275 117.0655) (xy 37.3355 117.0655)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.606 116.5575) (xy 45.8445 116.5575) (xy 45.845836 117.129) (xy 44.8285 117.129) (xy 44.3205 117.637)
        (xy 43.241 117.637) (xy 43.241 117.1925) (xy 43.114 117.0655) (xy 42.606 117.0655)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.309 119.034) (xy 78.547 119.034) (xy 77.023 119.034) (xy 76.769 119.288) (xy 75.245 119.288)
        (xy 75.245 119.6055) (xy 76.769 119.6055) (xy 77.0865 119.923) (xy 79.309 119.923)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.6415 113.827) (xy 72.6415 110.398) (xy 71.943 110.398) (xy 71.943 113.827)
      )
    )
  )
  (zone (net 300) (net_name "Net-(P1-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 33.843 183.677) (xy 31.43 183.677) (xy 30.033 182.28) (xy 27.493 179.74) (xy 27.493 178.47)
        (xy 32.954 178.47) (xy 34.986 180.502) (xy 34.986 182.534)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 20.5 189.4) (xy 111.5 189.4) (xy 111.5 187.614) (xy 28.5 187.614) (xy 28.5 182.9)
        (xy 27 181.4) (xy 22.5 181.4) (xy 22.5 38.4) (xy 27 38.4) (xy 28.5 36.9)
        (xy 28.5 30.4) (xy 20.5 30.4)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 111.5 189.4) (xy 119.5 189.4) (xy 119.5 30.4) (xy 111.5 30.4) (xy 111.5 36.9)
        (xy 113 38.4) (xy 117.5 38.4) (xy 117.5 181.4) (xy 113 181.4) (xy 111.5 182.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 22.5 189.4) (xy 22.5 181.525845) (xy 22.5 30.4) (xy 20.5 30.4) (xy 20.5 189.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 119.5 189.4) (xy 119.5 30.4) (xy 117.5 30.4) (xy 117.5 189.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 119.5 189.4) (xy 119.5 30.4) (xy 117.5 30.4) (xy 117.5 189.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 22.5 189.4) (xy 22.5 30.4) (xy 20.5 30.4) (xy 20.5 189.4)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 111.5 187.614) (xy 111.5 182.9) (xy 113 181.4) (xy 117.5 181.4) (xy 117.5 38.4)
        (xy 113 38.4) (xy 111.5 36.9) (xy 111.5 30.4) (xy 117.5 30.4) (xy 119.5 30.4)
        (xy 119.5 187.4) (xy 119.5 189.4) (xy 117.5 189.4) (xy 22.5 189.4) (xy 20.5 189.4)
        (xy 20.5 30.4) (xy 28.5 30.4) (xy 28.5 36.9) (xy 27 38.4) (xy 22.5 38.4)
        (xy 22.5 181.4) (xy 27 181.4) (xy 28.5 182.9) (xy 28.5 187.614)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.02))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 26.477 178.47) (xy 26.477 179.74) (xy 20.635 179.74) (xy 20.635 178.47)
      )
    )
  )
)
