(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 10)
    (no_connects 0)
    (area 131.242999 81.712999 148.157001 95.325001)
    (thickness 1.6)
    (drawings 14)
    (tracks 30)
    (zones 0)
    (modules 9)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 VIDEO_IN)
  (net 3 GND)
  (net 4 VIDEO_OUT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net VIDEO_IN)
    (add_net VIDEO_OUT)
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A5E4ACF)
    (at 133.223 83.693)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.159 1.27 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -6.985 -0.127) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A5E4892)
    (at 133.223 88.392)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 2.159 1.27 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -6.985 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VIDEO_IN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A5E4AE9)
    (at 133.223 93.345)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 2.159 1.27 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -7.112 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A5E4876)
    (at 146.177 88.392)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -2.159 1.27 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 7.112 -0.381) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 VIDEO_OUT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5A5E4834)
    (at 146.177 93.345)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -2.159 1.27 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 7.112 0.127) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A5E4AAA)
    (at 140.716 88.392 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.651 -1.524 180) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 VIDEO_IN))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VIDEO_OUT))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5A5E4A93)
    (at 140.589 85.0265)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -1.905 -1.4605) (layer F.SilkS))
    (fp_text value 2.2K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VIDEO_IN))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5A5E48D6)
    (at 136.9695 88.646 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.921 -0.0635 180) (layer F.SilkS))
    (fp_text value 3.3K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VIDEO_IN))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5A5E4ABC)
    (at 140.6525 92.1385)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -1.9685 1.4605) (layer F.SilkS))
    (fp_text value 75 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 VIDEO_OUT))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ATARI 2600\nATARI 7800\nVIDEO AMP" (at 139.7 88.519) (layer B.SilkS))
  (gr_text "VIDEO IN" (at 133.477 86.233) (layer F.SilkS))
  (gr_text "VIDEO\nOUT" (at 146.177 85.725) (layer F.SilkS))
  (gr_text GND (at 146.177 91.186) (layer F.SilkS))
  (gr_text GND (at 135.89 93.345) (layer F.SilkS))
  (gr_text 75R (at 142.24 93.599) (layer F.SilkS))
  (gr_text 3.3K (at 137.033 91.567) (layer F.SilkS))
  (gr_text BC817 (at 140.843 90.551) (layer F.SilkS))
  (gr_text 2.2K (at 141.986 83.566) (layer F.SilkS))
  (gr_text +5V (at 135.89 83.312) (layer F.SilkS))
  (gr_line (start 148.082 81.788) (end 131.318 81.788) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.082 95.25) (end 148.082 81.788) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.318 95.25) (end 148.082 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.318 81.788) (end 131.318 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.445 81.915) (xy 131.445 95.123) (xy 147.955 95.123) (xy 147.955 81.915)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.955 95.123) (xy 131.445 95.123) (xy 131.445 81.915) (xy 147.955 81.915)
      )
    )
  )
)
