<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="44.44" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="55.88" y2="44.45" width="0" layer="20"/>
<wire x1="55.88" y1="44.45" x2="55.88" y2="13.97" width="0" layer="20"/>
<wire x1="55.88" y1="13.97" x2="38.735" y2="13.97" width="0" layer="20"/>
<wire x1="38.735" y1="13.97" x2="38.735" y2="0" width="0" layer="20"/>
<wire x1="38.735" y1="0" x2="0" y2="0" width="0" layer="20"/>
<text>dunn effects</text>
<text>obviously
cloned
distortion</text>
<text>DIY ver 1.0
Aug. 2017</text>
</plain>
<libraries>
<library name="capacitors-elec">
<packages>
<package name="063_025">
<description>&lt;b&gt;6.3mm diameter, 2.5 mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitors-film">
<packages>
<package name="BOX_SMALL">
</package>
</packages>
</library>
<library name="diodes">
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
<package name="3MM_B">
</package>
<package name="DO35-4">
<description>&lt;B&gt;DO-35 0.4" spacing&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="mb_supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="16MM">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;
&lt;p&gt;potentiometer for showing off-board connections</description>
</package>
</packages>
</library>
<library name="integrated circuits">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistors">
<packages>
<package name="TO92-">
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="switches">
<packages>
<package name="M9040P">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
Marquardt</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitors-elec" package="063_025" value="100u"/>
<element name="C10" library="capacitors-film" package="BOX_SMALL" value="47n"/>
<element name="C2" library="capacitors-elec" package="050_020_1" value="10u"/>
<element name="C3" library="capacitors-film" package="BOX_SMALL" value="22n"/>
<element name="C4" library="capacitors-film" package="BOX_SMALL" value="68n"/>
<element name="C5" library="capacitors-film" package="BOX_SMALL" value="220p"/>
<element name="C6" library="capacitors-film" package="BOX_SMALL" value="1n"/>
<element name="C7" library="capacitors-film" package="BOX_SMALL" value="100n"/>
<element name="C8" library="capacitors-film" package="BOX_SMALL" value="220p"/>
<element name="C9" library="capacitors-elec" package="050_020_1" value="10u"/>
<element name="D1" library="diodes" package="DO41-3" value="1N4001"/>
<element name="D2" library="diodes" package="3MM_B" value="LEDB"/>
<element name="D3" library="diodes" package="DO35-4" value="1N34A"/>
<element name="G" library="mb_supply" package="SQUARE" value=""/>
<element name="GAIN" library="potentiometers" package="16MM" value="1MA"/>
<element name="G1" library="mb_supply" package="SQUARE" value="out2"/>
<element name="IC1" library="integrated circuits" package="DIL08" value="TL082"/>
<element name="I" library="mb_supply" package="SQUARE" value="in1"/>
<element name="L" library="mb_supply" package="SQUARE" value=""/>
<element name="O" library="mb_supply" package="SQUARE" value="out1"/>
<element name="Q1" library="transistors" package="TO92-" value="2N7000"/>
<element name="Q2" library="transistors" package="TO92-" value="2N7000"/>
<element name="R1" library="resistors" package="R0207/3" value="10k"/>
<element name="R10" library="resistors" package="R0207/3" value="10K"/>
<element name="R11" library="resistors" package="R0207/3" value="220K"/>
<element name="R12" library="resistors" package="R0207/3" value="39K"/>
<element name="R13" library="resistors" package="R0207/3" value="150K"/>
<element name="R14" library="resistors" package="R0207/3" value="22K"/>
<element name="R15" library="resistors" package="R0207/3" value="33K"/>
<element name="R2" library="resistors" package="R0207/3" value="10k"/>
<element name="R3" library="resistors" package="R0207/3" value="10k"/>
<element name="R4" library="resistors" package="R0207/3" value="1M"/>
<element name="R5" library="resistors" package="R0207/3" value="2.2K"/>
<element name="R6" library="resistors" package="R0207/3" value="10K"/>
<element name="R7" library="resistors" package="R0207/3" value="470K"/>
<element name="R8" library="resistors" package="R0207/3" value="18K"/>
<element name="R9" library="resistors" package="R0207/3" value="10K"/>
<element name="SW1" library="switches" package="M9040P" value=""/>
<element name="TONE" library="potentiometers" package="16MM" value="10KB"/>
<element name="V" library="mb_supply" package="SQUARE" value="out2"/>
<element name="VOL" library="potentiometers" package="16MM" value="500KB"/>
</elements>
<signals>
<signal name="GND">
<contactref element="G" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="G1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="IC1" pad="4"/>
<contactref element="R12" pad="1"/>
<contactref element="VOL" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="TONE" pad="3"/>
<contactref element="TONE" pad="2"/>
</signal>
<signal name="+9V">
<contactref element="IC1" pad="8"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="C3" pad="2"/>
<contactref element="I" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C3" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="VB">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="R7" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="D3" pad="A"/>
<contactref element="C6" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="C7" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R13" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="R13" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="+"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="D3" pad="C"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="C9" pad="-"/>
<contactref element="R15" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="VOL" pad="2"/>
<contactref element="O" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="GAIN" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="C10" pad="1"/>
<contactref element="VOL" pad="3"/>
<contactref element="R15" pad="2"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="A"/>
<contactref element="V" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="SW1" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="L" pad="1"/>
<contactref element="D2" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="R8" pad="1"/>
<contactref element="GAIN" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C10" pad="2"/>
<contactref element="TONE" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
