(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 25)
    (no_connects 0)
    (area 129.667 66.10858 182.753002 122.682002)
    (thickness 1.6002)
    (drawings 21)
    (tracks 114)
    (zones 0)
    (modules 10)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(JL1-Pad3)")
  (net 4 "Net-(JL1-Pad4)")
  (net 5 "Net-(JN1-Pad1)")
  (net 6 "Net-(JN1-Pad2)")
  (net 7 "Net-(JN1-Pad3)")
  (net 8 "Net-(JN1-Pad4)")
  (net 9 "Net-(JN1-Pad5)")
  (net 10 "Net-(JN1-Pad6)")
  (net 11 "Net-(JN1-Pad7)")
  (net 12 "Net-(JN1-Pad8)")
  (net 13 "Net-(JN1-Pad9)")
  (net 14 "Net-(JN1-Pad10)")
  (net 15 "Net-(JN1-Pad11)")
  (net 16 "Net-(JN1-Pad12)")
  (net 17 "Net-(JR1-Pad1)")
  (net 18 "Net-(LED1-Pad2-DO)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(JL1-Pad3)")
    (add_net "Net-(JL1-Pad4)")
    (add_net "Net-(JN1-Pad1)")
    (add_net "Net-(JN1-Pad10)")
    (add_net "Net-(JN1-Pad11)")
    (add_net "Net-(JN1-Pad12)")
    (add_net "Net-(JN1-Pad2)")
    (add_net "Net-(JN1-Pad3)")
    (add_net "Net-(JN1-Pad4)")
    (add_net "Net-(JN1-Pad5)")
    (add_net "Net-(JN1-Pad6)")
    (add_net "Net-(JN1-Pad7)")
    (add_net "Net-(JN1-Pad8)")
    (add_net "Net-(JN1-Pad9)")
    (add_net "Net-(JR1-Pad1)")
    (add_net "Net-(LED1-Pad2-DO)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 164.211 96.54 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.107 1.651 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X04_NO_SILK (layer F.Cu) (tedit 59930C2F)
    (at 160.02 110.49 180)
    (descr "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference JL1 (at 0.254 -1.7018 180) (layer F.SilkS) hide)
    (fp_text value led (at 3.937 1.143 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(JL1-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(JL1-Pad4)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X12_NO_SILK (layer F.Cu) (tedit 599307C6)
    (at 170.18 68.58 180)
    (descr "PLATED THROUGH HOLE -12 PIN NO SILK")
    (tags "PLATED THROUGH HOLE -12 PIN NO SILK")
    (attr virtual)
    (fp_text reference JN1 (at 0.254 -1.7018 180) (layer F.SilkS) hide)
    (fp_text value nixie (at 0.5588 1.7272 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(JN1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(JN1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(JN1-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(JN1-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(JN1-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(JN1-Pad6)"))
    (pad 7 thru_hole circle (at 15.24 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(JN1-Pad7)"))
    (pad 8 thru_hole circle (at 17.78 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(JN1-Pad8)"))
    (pad 9 thru_hole circle (at 20.32 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(JN1-Pad9)"))
    (pad 10 thru_hole circle (at 22.86 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(JN1-Pad10)"))
    (pad 11 thru_hole circle (at 25.4 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(JN1-Pad11)"))
    (pad 12 thru_hole circle (at 27.94 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 16 "Net-(JN1-Pad12)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X02_NO_SILK (layer F.Cu) (tedit 599307D9)
    (at 143.51 70.993 180)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference JR1 (at 0.254 -1.7018 180) (layer F.SilkS) hide)
    (fp_text value jumper (at -2.794 -0.635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(JR1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 16 "Net-(JN1-Pad12)"))
  )
  (module adafruit:adafruit-WS2812B (layer F.Cu) (tedit 598E7B56)
    (at 143.51 96.52 90)
    (attr smd)
    (fp_text reference LED1 (at 3.8989 0.4445 360) (layer F.SilkS))
    (fp_text value WS2812B5050 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1-VD smd rect (at 2.44856 1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2-DO smd rect (at 2.44856 -1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED1-Pad2-DO)"))
    (pad 3-GN smd rect (at -2.44856 -1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4-DI smd rect (at -2.44856 1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JL1-Pad3)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 142.287 73.66 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(JR1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(JN1-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 147.955 96.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-WS2812B (layer F.Cu) (tedit 598E7BC6)
    (at 168.91254 96.52 90)
    (attr smd)
    (fp_text reference LED2 (at 3.8989 0.4445 360) (layer F.SilkS))
    (fp_text value WS2812B5050 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1-VD smd rect (at 2.44856 1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2-DO smd rect (at 2.44856 -1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JL1-Pad4)"))
    (pad 3-GN smd rect (at -2.44856 -1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4-DI smd rect (at -2.44856 1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED1-Pad2-DO)"))
  )
  (module logos:mermaid_l (layer F.Cu) (tedit 0)
    (at 153.289 104.648)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module NL7037:mynixies-RTS-5-DSUB (layer F.Cu) (tedit 59930F81)
    (at 156.210001 96.139001)
    (attr virtual)
    (fp_text reference N1 (at 0 -21.59) (layer F.SilkS))
    (fp_text value NL7037 (at 0 -12.7) (layer F.SilkS))
    (pad P$2 thru_hole circle (at 5.97154 16.4084) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(JR1-Pad1)"))
    (pad P$3 thru_hole circle (at 11.22426 13.37564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(JN1-Pad7)"))
    (pad P$4 thru_hole circle (at 15.12062 8.72998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(JN1-Pad11)"))
    (pad P$7 thru_hole circle (at 15.12062 -8.72998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(JN1-Pad3)"))
    (pad P$8 thru_hole circle (at 11.22426 -13.37564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(JN1-Pad5)"))
    (pad P$9 thru_hole circle (at 5.97154 -16.4084) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(JN1-Pad2)"))
    (pad P$12 thru_hole circle (at -11.22426 -13.37564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(JN1-Pad9)"))
    (pad P$13 thru_hole circle (at -15.12062 -8.72998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(JN1-Pad10)"))
    (pad P$14 thru_hole circle (at -17.1958 -3.03022) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(JN1-Pad6)"))
    (pad P$16 thru_hole circle (at -15.12062 8.72998) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(JN1-Pad8)"))
    (pad P$17 thru_hole circle (at -11.22426 13.37564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(JN1-Pad4)"))
    (pad "" np_thru_hole circle (at 0 0) (size 7.9375 7.9375) (drill 7.9375) (layers *.Cu *.Mask))
  )
  (gr_text NC (at 170.18 70.104) (layer F.SilkS))
  (gr_text 1 (at 167.64 70.104) (layer F.SilkS))
  (gr_text 2 (at 165.1 70.104) (layer F.SilkS))
  (gr_text 3 (at 162.56 70.104) (layer F.SilkS))
  (gr_text 4 (at 160.02 70.104) (layer F.SilkS))
  (gr_text 5 (at 157.48 70.104) (layer F.SilkS))
  (gr_text 6 (at 154.94 70.104) (layer F.SilkS))
  (gr_text 7 (at 152.4 70.104) (layer F.SilkS))
  (gr_text 8 (at 149.86 70.104) (layer F.SilkS))
  (gr_text 9 (at 147.32 70.104) (layer F.SilkS))
  (gr_text 0 (at 144.78 70.104) (layer F.SilkS))
  (gr_text A (at 142.24 70.104) (layer F.SilkS))
  (gr_text Dout (at 152.273 112.141) (layer F.SilkS))
  (gr_text Din (at 154.94 112.141) (layer F.SilkS))
  (gr_text Vin (at 157.48 112.141) (layer F.SilkS))
  (gr_text Gnd (at 160.02 112.141) (layer F.SilkS))
  (gr_text nixies.us (at 157.734 104.14) (layer F.Mask))
  (gr_arc (start 156.21 96.393) (end 172.72 83.82) (angle 254.5813338) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 172.72 67.31) (end 172.72 83.82) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 139.7 67.31) (end 139.7 83.82) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 172.724668 67.31) (end 139.699756 67.31) (layer Edge.Cuts) (width 0.127))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.876 108.839) (xy 150.876 100.711) (xy 161.29 100.711) (xy 161.29 108.585) (xy 150.876 108.585)
        (xy 150.876 108.585)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.749 108.712) (xy 150.749 100.457) (xy 161.544 100.457) (xy 161.544 108.839) (xy 150.876 108.839)
      )
    )
  )
)
