(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user)
		(11 "B.Adhes" user)
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user)
		(7 "B.SilkS" user)
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user)
		(19 "Cmts.User" user)
		(21 "Eco1.User" user)
		(23 "Eco2.User" user)
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user)
		(29 "B.CrtYd" user)
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755557f)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Gerber/")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-Pad3)")
	(net 2 "Net-(D1-Pad2)")
	(net 3 "Net-(D1-Pad1)")
	(net 4 "Net-(J1-Pad1)")
	(net 5 "Net-(J1-Pad3)")
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 170 135.9 180)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "Q1"
			(at 1.5 1.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "BC807"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1 -0.95 180)
			(size 1.2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(J1-Pad3)")
		)
		(pad "2" smd rect
			(at -1 0.95 180)
			(size 1.2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(J1-Pad1)")
		)
		(pad "3" smd rect
			(at 1 0 180)
			(size 1.2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(D1-Pad1)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 173.074999 140.674999 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J1"
			(at 0.924999 -1.575001 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "trig PNP"
			(at -2.075001 2.424999 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pad1)")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-Pad3)")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pad3)")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 167 138 -90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ext trig"
			(at 0 2.33 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D1-Pad2)")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 170 140)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "D1"
			(at 1.5 1.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT54C"
			(at 0 2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1 -0.95)
			(size 1.2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(D1-Pad1)")
		)
		(pad "2" smd rect
			(at -1 0.95)
			(size 1.2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(D1-Pad2)")
		)
		(pad "3" smd rect
			(at 1 0)
			(size 1.2 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-Pad3)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 168 142)
		(end 175 142)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175 133.75)
		(end 175 142)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.5 136.25)
		(end 165.5 139.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 168 142)
		(mid 166.232233 141.267767)
		(end 165.5 139.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168 133.75)
		(end 175 133.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 165.5 136.25)
		(mid 166.232233 134.482233)
		(end 168 133.75)
		(layer "Edge.Cuts")
	)
	(gr_text "trig"
		(at 168.25 140 0)
		(layer "F.SilkS")
	)
	(gr_text "E"
		(at 174 140.7 0)
		(layer "F.SilkS")
	)
	(gr_text "C"
		(at 174 138.2 0)
		(layer "F.SilkS")
	)
	(gr_text "B"
		(at 174 135.6 0)
		(layer "F.SilkS")
	)
	(gr_text "x0x"
		(at 166 135.75 0)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
