(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 17)
    (no_connects 0)
    (area 122.225999 117.145999 177.113001 123.646001)
    (thickness 1.6)
    (drawings 13)
    (tracks 64)
    (zones 0)
    (modules 11)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEDF79)
    (pcbplotparams
      (layerselection 0x01008_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/rick/Dropbox/AA LED Boost/gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(L1-Pad2)")
  (net 6 "Net-(C1-Pad1)")
  (net 7 "Net-(R1-Pad2)")
  (net 8 "Net-(R2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
  )
  (module "Rick's Custom:12BH311P-GR" (layer B.Cu) (tedit 5A63D9BC)
    (at 149.86 120.3071)
    (fp_text reference BT1 (at 0 -1.27) (layer B.SilkS) hide)
    (fp_text value "1.5v AA" (at 0 1.27) (layer B.Fab))
    (pad 1 thru_hole rect (at -26 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 26 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A63D9B1)
    (at 138.176 119.634)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A63D994)
    (at 138.176 118.11)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Rick's Custom:EPL2010-472MLB" (layer F.Cu) (tedit 5A63D9AB)
    (at 138.176 121.666 270)
    (fp_text reference L1 (at 0 2.286 270) (layer F.SilkS) hide)
    (fp_text value 4.7uH (at 0 -2.286 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.675 0 270) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(L1-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A63D97A)
    (at 147.574 122.3645)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1) (layer F.SilkS) hide)
    (fp_text value 56_Ohm (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A63D981)
    (at 144.272 122.3645)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1) (layer F.SilkS) hide)
    (fp_text value 340_Ohm (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SC-70-6 (layer F.Cu) (tedit 5A63D9A1)
    (at 134.874 121.158 180)
    (descr SC-70-6,)
    (tags SC-70-6)
    (attr smd)
    (fp_text reference U1 (at 0.01016 -3.05054 180) (layer F.SilkS) hide)
    (fp_text value TLV61225 (at 0.04064 4.191 180) (layer F.Fab))
    (pad 1 smd rect (at -0.65024 0.94996 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0 0.94996 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 0.65024 0.94996 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65024 -0.94996 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 0 -0.94996 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(L1-Pad2)"))
    (pad 6 smd rect (at -0.65024 -0.94996 180) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Rick's Custom:logo_5mm" (layer F.Cu) (tedit 0)
    (at 153.924 120.396)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "Rick's Custom:SMD_SPDT_SLIDE_SWITCH" (layer F.Cu) (tedit 55B2AB0C)
    (at 129.286 118.364 180)
    (fp_text reference SW1 (at 0 3.15 180) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -3.3 180) (layer F.Fab))
    (pad 3 smd rect (at 2.25 -1.75 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 -1.75 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at -2.25 -1.75 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at -1.5 0 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 1.5 0 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
  )
  (module "Rick's Custom:SMD_SPDT_SLIDE_SWITCH" (layer F.Cu) (tedit 55B2AB0C)
    (at 146.304 118.364 180)
    (fp_text reference SW2 (at 0 3.15 180) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -3.3 180) (layer F.Fab))
    (pad 3 smd rect (at 2.25 -1.75 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 -1.75 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -2.25 -1.75 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 4 thru_hole circle (at -1.5 0 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 1.5 0 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
  )
  (module "Rick's Custom:3014_led" (layer F.Cu) (tedit 5A8C8910)
    (at 173.482 120.65 90)
    (fp_text reference D1 (at 0 -1.524 270) (layer F.SilkS))
    (fp_text value LED (at 0 -1.524 90) (layer F.Fab))
    (pad 2 smd rect (at -1.11 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.695 0 90) (size 1.61 0.72) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (gr_text 10mA (at 150.368 118.618 270) (layer F.Mask))
  (gr_text 2mA (at 142.24 118.618 90) (layer F.Mask))
  (gr_text "Off    On" (at 129.54 122.174) (layer F.Mask))
  (gr_text 4.7uH (at 139.954 121.92 90) (layer F.SilkS))
  (gr_text 10uF (at 140.716 119.634) (layer F.SilkS))
  (gr_text 10uF (at 140.716 118.11) (layer F.SilkS))
  (gr_text 340Ω (at 141.478 122.428) (layer F.SilkS))
  (gr_text 56Ω (at 150.114 122.428) (layer F.SilkS))
  (gr_line (start 177.038 123.571) (end 177.038 117.221) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.301 117.221) (end 122.301 123.571) (layer Edge.Cuts) (width 0.15))
  (gr_text "AA LED Boost V1.1\nMad Electron Engineering 2018" (at 164.338 120.396) (layer F.Mask))
  (gr_line (start 177.038 123.571) (end 122.301 123.571) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.301 117.221) (end 177.038 117.221) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.784 117.348) (xy 176.784 123.444) (xy 122.428 123.444) (xy 122.428 117.348)
      )
    )
  )
  (zone (net 1) (net_name "Net-(BT1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.556 117.602) (xy 130.556 123.444) (xy 122.428 123.444) (xy 122.428 117.348) (xy 130.556 117.348)
      )
    )
  )
  (zone (net 6) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.064 117.602) (xy 131.064 117.348) (xy 135.89 117.348) (xy 135.89 118.872) (xy 138.176 118.872)
        (xy 138.176 120.396) (xy 138.938 120.396) (xy 138.938 123.444) (xy 131.064 123.444)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.684 117.348) (xy 138.684 119.38) (xy 139.954 120.904) (xy 139.954 123.444) (xy 176.784 123.444)
        (xy 176.784 117.348)
      )
    )
  )
)
