(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.955)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user "plugins.config")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.0254))
      (layer "F.Cu" (type "copper") (thickness 0.0711))
      (layer "dielectric 1" (type "core") (color "FR4 natural") (thickness 0.762) (material "KB-6167F") (epsilon_r 4.8) (loss_tangent 0.015))
      (layer "B.Cu" (type "copper") (thickness 0.0711))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.0254))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (footprint "Xer_Library:XT60U-M Reversible" (layer "F.Cu")
    (at 100 100)
    (descr "AMASS female XT60, through hole, vertical, https://www.tme.eu/Document/2d152ced3b7a446066e6c419d84bb460/XT60%20SPEC.pdf")
    (tags "XT60 female vertical")
    (property "Sheetfile" "CapCap.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "XT1" (at 0 -5.3 180) (layer "F.SilkS") hide)
    (fp_text value "~" (at 0.9 7.58) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.05) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.6 0) (size 6 6) (drill 4.4) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "power_in"))
    (pad "2" thru_hole circle (at 3.6 0) (size 6 6) (drill 4.4) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)") (pintype "power_in"))
    (model "D:/Documents/KiCad/7.0/3dmodels/XT60U-M.stp"
      (offset (xyz 0 0 4.25))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Xer_Library:470uf poly cap" (layer "F.Cu")
    (at 100 109.2 180)
    (property "Sheetfile" "CapCap.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 0 -7.62 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "C" (at 0 7.62 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 10.16 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.5 0 180) (size 2 2) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.5 0 180) (size 2 2) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "D:/Documents/KiCad/7.0/3dmodels/EEHAZSV471UB.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_line (start 96.3 96.5) (end 103.7 96.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 92.937626 100.971824) (mid 93.502556 97.896597) (end 96.3 96.5)
    (layer "Edge.Cuts"))
  (gr_line (start 107.062374 100.971824) (end 104.323052 110.449488)
    (layer "Edge.Cuts"))
  (gr_arc (start 104.323052 110.449488) (mid 100 113.7) (end 95.676948 110.449488)
    (layer "Edge.Cuts"))
  (gr_line (start 92.937626 100.971824) (end 95.676948 110.449488)
    (layer "Edge.Cuts"))
  (gr_arc (start 103.7 96.5) (mid 106.497444 97.896596) (end 107.062374 100.971824)
    (layer "Edge.Cuts"))
  (gr_text "{\n  \"ViaStitching\": \"0.2\",\n  \"stitch_zone_0\": {\n    \"HSpacing\": \".1\",\n    \"VSpacing\": \".1\",\n    \"Clearance\": \"0\",\n    \"Randomize\": false\n  }\n}" (at 0 0) (layer "User.9"))
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 100.1 95)
        (xy 100.1 115)
        (xy 110 115)
        (xy 110 95)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad1)") (layers "F&B.Cu") (name "stitch_zone_0") (hatch edge 0.5)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 99.9 95)
        (xy 99.9 115)
        (xy 90 115)
        (xy 90 95)
      )
    )
  )
)
