(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 9)
    (no_connects 1)
    (area 136.73 97.453599 158.060001 112.585)
    (thickness 1.6)
    (drawings 15)
    (tracks 13)
    (zones 0)
    (modules 5)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad4)")
  (net 2 "Net-(D1-Pad5)")
  (net 3 "Net-(D1-Pad6)")
  (net 4 "Net-(D1-Pad3)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class HIGH_CURRENT ""
    (clearance 0.2)
    (trace_width 0.65)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D1-Pad5)")
    (add_net "Net-(D1-Pad6)")
    (add_net "Net-(P1-Pad1)")
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58403E6F)
    (at 151.94 108.12 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.36 1.84 180) (layer F.SilkS))
    (fp_text value R (at 0.1 2 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.75) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 2 smd rect (at 0 0.75) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58403E6F)
    (at 151.94 106.27 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.32 1.81 180) (layer F.SilkS))
    (fp_text value R (at 0.1 2 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.75) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad5)"))
    (pad 2 smd rect (at 0 0.75) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58403E6F)
    (at 151.94 104.42 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.54 1.76 180) (layer F.SilkS))
    (fp_text value R (at 0.1 2 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.75) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad6)"))
    (pad 2 smd rect (at 0 0.75) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED:PLCC6_3-4MMSQR_LED locked (layer F.Cu) (tedit 58443E03)
    (at 147.3211 106.2736 90)
    (descr http://www.world-semi.com/en/Driver/Lighting/WS2811/WS212B/WS2822S/)
    (tags "LED RGB")
    (attr smd)
    (fp_text reference D1 (at -3.3264 1.3989 360) (layer F.SilkS))
    (fp_text value LED_RGB (at -5.7364 1.1789 180) (layer F.Fab))
    (pad 4 smd rect (at -1.025 1.5 90) (size 0.75 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 5 smd rect (at 0 1.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad5)"))
    (pad 6 smd rect (at 1.025 1.5 90) (size 0.75 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad6)"))
    (pad 3 smd rect (at -1.025 -1.5 90) (size 0.75 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 0 -1.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 1.025 -1.5 90) (size 0.75 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_WS2812-PLCC6.wrl
      (at (xyz 0 0 0.004))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn:M20-9750446 locked (layer B.Cu) (tedit 58443F54)
    (at 142.75 105.01 180)
    (fp_text reference P1 (at -2.09 -4.59 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 6.45 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 3.81 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 1.27 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at 0 -1.27 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 4 thru_hole circle (at 0 -3.81 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad3)"))
  )
  (gr_circle (center 142.7511 108.8136) (end 143.2511 108.8136) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 142.7511 106.2736) (end 143.2511 106.2736) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 153.7511 109.5036) (end 153.7511 110.5036) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2511 110.5036) (end 153.7511 110.5036) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.2511 109.5036) (end 141.2511 109.5036) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.2511 100.5036) (end 141.2511 109.5036) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.2511 100.5036) (end 142.2511 99.5036) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.769279 99.5036) (end 142.2511 99.5036) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.769279 100.5036) (end 143.514635 99.836933) (angle -48.1896851) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 146.123381 97.5036) (end 143.514635 99.836933) (angle -48.1896851) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.123381 101.0036) (end 153.7511 101.0036) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 153.7511 102.0036) (end 154.7511 102.0036) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.7511 109.5036) (end 154.7511 102.0036) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 142.7511 101.1936) (end 143.2511 101.1936) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 142.7511 103.7336) (end 143.2511 103.7336) (layer Edge.Cuts) (width 0.1))
  (zone (net 7) (net_name "Net-(P1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.9 99.24) (xy 140.9 102.5) (xy 143.5 102.5) (xy 143.9 102.9) (xy 150.8 102.9)
        (xy 152 104.1) (xy 152 110.8) (xy 154.98 110.8) (xy 154.99 99.24)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D1-Pad6)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 103.1) (xy 148 105.63) (xy 151.8 105.63) (xy 151.8 103.8) (xy 151.1 103.1)
      )
    )
  )
  (zone (net 2) (net_name "Net-(D1-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.02 105.92) (xy 148.02 106.63) (xy 149.8 106.63) (xy 150.46 107.29) (xy 151.8 107.29)
        (xy 151.8 105.25) (xy 150.47 105.25) (xy 149.8 105.92)
      )
    )
  )
  (zone (net 7) (net_name "Net-(P1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.75 98.4) (xy 136.73 112.38) (xy 158.06 112.4) (xy 158.06 98.41)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.9 102.66) (xy 143.36 102.66) (xy 143.8 103.1) (xy 146.61 103.1) (xy 146.61 105.62)
        (xy 144.24 105.62) (xy 143.62 105) (xy 140.9 105)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.9 105.2) (xy 144.1 105.2) (xy 144.82 105.92) (xy 146.62 105.92) (xy 146.62 106.63)
        (xy 144.82 106.63) (xy 144.09 107.36) (xy 140.9 107.36)
      )
    )
  )
  (zone (net 4) (net_name "Net-(D1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.9 107.5) (xy 144 107.5) (xy 144.57 106.93) (xy 146.62 106.93) (xy 146.62 107.67)
        (xy 146.62 110.8) (xy 140.9 110.8)
      )
    )
  )
  (zone (net 1) (net_name "Net-(D1-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.8 106.93) (xy 148.03 106.93) (xy 148.03 110.8) (xy 151.8 110.8)
      )
    )
  )
)
