(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 64)
    (no_connects 0)
    (area 137.65 -35.069401 261.293101 133.428601)
    (thickness 1.6)
    (drawings 279)
    (tracks 382)
    (zones 0)
    (modules 12)
    (nets 50)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2875 1.2875)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /~RST)
  (net 2 GND)
  (net 3 VDD)
  (net 4 /V_DEBUGGER)
  (net 5 +BATT)
  (net 6 "Net-(P1-Pad2)")
  (net 7 /RTS_TARGETOUT)
  (net 8 /CTS_TARGETIN)
  (net 9 /RX_TARGETIN)
  (net 10 /TX_TARGETOUT)
  (net 11 /TEST)
  (net 12 "Net-(P1-Pad10)")
  (net 13 /UI_IN5)
  (net 14 /UI_IN0)
  (net 15 /UI_IN1)
  (net 16 /UI_IN2)
  (net 17 /UI_IN3)
  (net 18 /UI_IN4)
  (net 19 "Net-(S1-Pad8)")
  (net 20 "Net-(S1-Pad7)")
  (net 21 "Net-(S1-Pad6)")
  (net 22 "Net-(U1-Pad8)")
  (net 23 "Net-(S1-Pad5)")
  (net 24 "Net-(U1-Pad10)")
  (net 25 "Net-(U1-Pad11)")
  (net 26 "Net-(U1-Pad12)")
  (net 27 "Net-(U1-Pad13)")
  (net 28 "Net-(U1-Pad14)")
  (net 29 "Net-(U1-Pad15)")
  (net 30 "Net-(U1-Pad18)")
  (net 31 "Net-(U1-Pad19)")
  (net 32 "Net-(U1-Pad27)")
  (net 33 "Net-(U1-Pad28)")
  (net 34 "Net-(U1-Pad29)")
  (net 35 "Net-(U1-Pad30)")
  (net 36 /SDA)
  (net 37 /SCL)
  (net 38 "Net-(U1-Pad33)")
  (net 39 /~INT)
  (net 40 "Net-(U1-Pad35)")
  (net 41 "Net-(U1-Pad42)")
  (net 42 "Net-(U1-Pad43)")
  (net 43 "Net-(U1-Pad45)")
  (net 44 "Net-(U1-Pad46)")
  (net 45 "Net-(P3-Pad2)")
  (net 46 "Net-(U1-Pad4)")
  (net 47 "Net-(U1-Pad5)")
  (net 48 "Net-(U1-Pad6)")
  (net 49 "Net-(U1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CTS_TARGETIN)
    (add_net /RTS_TARGETOUT)
    (add_net /RX_TARGETIN)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TEST)
    (add_net /TX_TARGETOUT)
    (add_net /UI_IN0)
    (add_net /UI_IN1)
    (add_net /UI_IN2)
    (add_net /UI_IN3)
    (add_net /UI_IN4)
    (add_net /UI_IN5)
    (add_net /~INT)
    (add_net /~RST)
    (add_net GND)
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(S1-Pad5)")
    (add_net "Net-(S1-Pad6)")
    (add_net "Net-(S1-Pad7)")
    (add_net "Net-(S1-Pad8)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net VDD)
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net /V_DEBUGGER)
  )
  (module Housings_DFN_QFN:QFN-48-1EP_7x7mm_Pitch0.5mm (layer B.Cu) (tedit 5881A9CB)
    (at 157.55 99.4 135)
    (descr "UK Package; 48-Lead Plastic QFN (7mm x 7mm); (see Linear Technology QFN_48_05-08-1704.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 5.267946 0.247487 135) (layer B.SilkS))
    (fp_text value MSP430FR5969RGZ (at 0 -4.75 135) (layer B.Fab))
    (pad 1 smd rect (at -3.4 2.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(S1-Pad8)"))
    (pad 2 smd rect (at -3.4 2.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(S1-Pad7)"))
    (pad 3 smd rect (at -3.4 1.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(S1-Pad6)"))
    (pad 4 smd rect (at -3.4 1.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -3.4 0.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -3.4 0.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -3.4 -0.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -3.4 -0.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -3.4 -1.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(S1-Pad5)"))
    (pad 10 smd rect (at -3.4 -1.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -3.4 -2.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -3.4 -2.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -2.75 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at -2.25 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -1.75 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -1.25 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 8 /CTS_TARGETIN))
    (pad 17 smd rect (at -0.75 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 /RTS_TARGETOUT))
    (pad 18 smd rect (at -0.25 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 0.25 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 0.75 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /UI_IN3))
    (pad 21 smd rect (at 1.25 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /UI_IN4))
    (pad 22 smd rect (at 1.75 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 11 /TEST))
    (pad 23 smd rect (at 2.25 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /~RST))
    (pad 24 smd rect (at 2.75 -3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 10 /TX_TARGETOUT))
    (pad 25 smd rect (at 3.4 -2.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /RX_TARGETIN))
    (pad 26 smd rect (at 3.4 -2.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /UI_IN0))
    (pad 27 smd rect (at 3.4 -1.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 3.4 -1.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 3.4 -0.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 3.4 -0.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 3.4 0.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 36 /SDA))
    (pad 32 smd rect (at 3.4 0.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 37 /SCL))
    (pad 33 smd rect (at 3.4 1.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U1-Pad33)"))
    (pad 34 smd rect (at 3.4 1.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 39 /~INT))
    (pad 35 smd rect (at 3.4 2.25 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U1-Pad35)"))
    (pad 36 smd rect (at 3.4 2.75 135) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 37 smd rect (at 2.75 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 38 smd rect (at 2.25 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 13 /UI_IN5))
    (pad 39 smd rect (at 1.75 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 15 /UI_IN1))
    (pad 40 smd rect (at 1.25 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 16 /UI_IN2))
    (pad 41 smd rect (at 0.75 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 42 smd rect (at 0.25 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at -0.25 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U1-Pad43)"))
    (pad 44 smd rect (at -0.75 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 45 smd rect (at -1.25 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U1-Pad45)"))
    (pad 46 smd rect (at -1.75 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(U1-Pad46)"))
    (pad 47 smd rect (at -2.25 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 48 smd rect (at -2.75 3.4 45) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 49 smd rect (at 1.93125 -1.93125 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -0.64375 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 0.64375 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 1.93125 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -1.93125 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -0.64375 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 0.64375 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 1.93125 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -1.93125 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -0.64375 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 0.64375 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 1.93125 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -1.93125 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -0.64375 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 0.64375 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 1.93125 135) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5881A16D)
    (at 160.65 106.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.2 1.45 270) (layer B.SilkS))
    (fp_text value 1nF (at 2.75 -0.7 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /~RST))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5881A088)
    (at 164.45 96.05 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.65165 -0.035355 135) (layer B.SilkS))
    (fp_text value 1µF (at -5.727565 -0.141421 135) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5881A04A)
    (at 163.35 97.2 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.404163 0.070711 135) (layer B.SilkS))
    (fp_text value 100nF (at -5.69221 -0.176777 135) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 150.51 92.75 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.39 90) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 7.47 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /V_DEBUGGER))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VDD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 147.4 92.54)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X10 (at 0 25.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /V_DEBUGGER))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RTS_TARGETOUT))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /CTS_TARGETIN))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /RX_TARGETIN))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /TX_TARGETOUT))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /~RST))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /TEST))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad10)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5881A167)
    (at 162.4 106.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 47kΩ (at -1.1 3.3 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /~RST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD_BF:SW_SPST_B3S-1000 (layer B.Cu) (tedit 5881A17C)
    (at 173.3 95.2 180)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at -6.7 2.5 180) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0 -4.5 180) (layer B.Fab))
    (pad 1 smd rect (at -3.975 2.25 180) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 /~RST))
    (pad 1 smd rect (at 3.975 2.25 180) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 /~RST))
    (pad 2 smd rect (at -3.975 -2.25 180) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.975 -2.25 180) (size 1.55 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Buttons_Switches_SMD_BF:SW_SPST_B3S-1000 (layer F.Cu) (tedit 58831664)
    (at 154.45 110.85)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW2 (at -3.2 0.1) (layer F.SilkS))
    (fp_text value SW_PUSH_Small_Horizontal (at 0 4.5) (layer F.Fab))
    (pad 1 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /UI_IN5))
    (pad 1 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /UI_IN5))
    (pad 2 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Buttons_Switches_SMD_BF:Sw_Navigation_JS5208 (layer F.Cu) (tedit 58831669)
    (at 170.5 110.15 180)
    (fp_text reference SW3 (at 1.55 3.05 180) (layer F.SilkS))
    (fp_text value Sw_Navigation_JS5208 (at 1.778 -7.366 180) (layer F.Fab))
    (pad "" np_thru_hole oval (at 3.5 5.525 180) (size 4.5 1.45) (drill oval 4.5 1.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -3.5 5.525 180) (size 4.5 1.45) (drill oval 4.5 1.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3 3 180) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -7.5 -4 180) (size 2 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -7.5 0 180) (size 2 1.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /UI_IN0))
    (pad 3 smd rect (at -7.5 4 180) (size 2 1.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /UI_IN1))
    (pad 4 smd rect (at 7.5 4 180) (size 2 1.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /UI_IN2))
    (pad 5 smd rect (at 7.5 0 180) (size 2 1.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /UI_IN3))
    (pad 6 smd rect (at 7.5 -4 180) (size 2 1.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /UI_IN4))
    (pad "" np_thru_hole circle (at 3 -3 180) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 0 -5.525 180) (size 4.5 1.45) (drill oval 4.5 1.45) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 167.15 122.95)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +BATT))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 /~INT))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /SCL))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /SDA))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Buttons_Switches_SMD_BF:Sw_DIP_x4_1.27mm_CTS_218-4LPSTR (layer B.Cu) (tedit 5881A7EF)
    (at 159.05 112.8 90)
    (fp_text reference S1 (at -0.05 -5.45 90) (layer B.SilkS))
    (fp_text value SW_DIP_x4 (at -1.3 -2.15 90) (layer B.Fab))
    (pad 6 smd rect (at -0.635 -3.81 90) (size 0.76 1.27) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(S1-Pad6)"))
    (pad 7 smd rect (at 0.635 -3.81 90) (size 0.76 1.27) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(S1-Pad7)"))
    (pad 8 smd rect (at 1.905 -3.81 90) (size 0.76 1.27) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(S1-Pad8)"))
    (pad 5 smd rect (at -1.905 -3.81 90) (size 0.76 1.27) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(S1-Pad5)"))
    (pad 4 smd rect (at -1.905 3.81 90) (size 0.76 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.905 3.81 90) (size 0.76 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.635 3.81 90) (size 0.76 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -0.635 3.81 90) (size 0.76 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (gr_text r0 (at 182.4 118.95) (layer F.Mask))
  (gr_text C-bage! (at 162.55 92.85) (layer F.SilkS))
  (gr_text X (at 154.25 106.25) (layer F.SilkS))
  (gr_text - (at 171.9 117.95) (layer F.SilkS))
  (gr_text + (at 172.1 101.8) (layer F.SilkS))
  (gr_line (start 187.1031 94.5526) (end 186.7721 94.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.7721 94.8296) (end 186.3671 94.9766) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.3671 94.9766) (end 185.9351 94.9766) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.9351 94.9766) (end 185.5301 94.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.5301 94.8296) (end 185.1991 94.5526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.1991 94.5526) (end 184.9841 94.1786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.9841 94.1786) (end 184.9091 93.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.9091 93.7536) (end 184.9841 93.3286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.9841 93.3286) (end 185.1991 92.9546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.1991 92.9546) (end 185.5301 92.6776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.5301 92.6776) (end 185.9351 92.5306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.9351 92.5306) (end 186.3671 92.5306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.3671 92.5306) (end 186.7721 92.6776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.7721 92.6776) (end 187.1031 92.9546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.1031 92.9546) (end 187.3181 93.3286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.3181 93.3286) (end 187.3931 93.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.3931 93.7536) (end 187.3181 94.1786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.3181 94.1786) (end 187.1031 94.5526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.9881 93.0516) (end 186.6971 92.8076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.6971 92.8076) (end 186.3411 92.6776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.3411 92.6776) (end 185.9611 92.6776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.9611 92.6776) (end 185.6051 92.8076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.6051 92.8076) (end 185.3141 93.0516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.3141 93.0516) (end 185.1251 93.3796) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.1251 93.3796) (end 185.0591 93.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.0591 93.7536) (end 185.1251 94.1276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.1251 94.1276) (end 185.3141 94.4556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.3141 94.4556) (end 185.6051 94.6996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.6051 94.6996) (end 185.9611 94.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.9611 94.8296) (end 186.3411 94.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.3411 94.8296) (end 186.6971 94.6996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.6971 94.6996) (end 186.9881 94.4556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.9881 94.4556) (end 187.1771 94.1276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.1771 94.1276) (end 187.2431 93.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.2431 93.7536) (end 187.1771 93.3796) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.1771 93.3796) (end 186.9881 93.0516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.2771 121.3796) (end 187.0881 121.0516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.3431 121.7536) (end 187.2771 121.3796) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.2771 122.1276) (end 187.3431 121.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.0881 122.4556) (end 187.2771 122.1276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.7971 122.6996) (end 187.0881 122.4556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.4411 122.8296) (end 186.7971 122.6996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.0611 122.8296) (end 186.4411 122.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.7051 122.6996) (end 186.0611 122.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.4141 122.4556) (end 185.7051 122.6996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2251 122.1276) (end 185.4141 122.4556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.1591 121.7536) (end 185.2251 122.1276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2251 121.3796) (end 185.1591 121.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.4141 121.0516) (end 185.2251 121.3796) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.7051 120.8076) (end 185.4141 121.0516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.0611 120.6776) (end 185.7051 120.8076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.4411 120.6776) (end 186.0611 120.6776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.7971 120.8076) (end 186.4411 120.6776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.0881 121.0516) (end 186.7971 120.8076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.4181 122.1786) (end 187.2031 122.5526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.4931 121.7536) (end 187.4181 122.1786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.4181 121.3286) (end 187.4931 121.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.2031 120.9546) (end 187.4181 121.3286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.8721 120.6776) (end 187.2031 120.9546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.4671 120.5306) (end 186.8721 120.6776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.0351 120.5306) (end 186.4671 120.5306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.6301 120.6776) (end 186.0351 120.5306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2991 120.9546) (end 185.6301 120.6776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.0841 121.3286) (end 185.2991 120.9546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.0091 121.7536) (end 185.0841 121.3286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.0841 122.1786) (end 185.0091 121.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2991 122.5526) (end 185.0841 122.1786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.6301 122.8296) (end 185.2991 122.5526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.0351 122.9766) (end 185.6301 122.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.4671 122.9766) (end 186.0351 122.9766) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.8721 122.8296) (end 186.4671 122.9766) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.2031 122.5526) (end 186.8721 122.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.9775 121.4796) (end 148.7878 121.1516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.0434 121.8536) (end 148.9775 121.4796) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.9775 122.2276) (end 149.0434 121.8536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.7878 122.5556) (end 148.9775 122.2276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.4972 122.7996) (end 148.7878 122.5556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.1408 122.9296) (end 148.4972 122.7996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7614 122.9296) (end 148.1408 122.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.405 122.7996) (end 147.7614 122.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.1144 122.5556) (end 147.405 122.7996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.9247 122.2276) (end 147.1144 122.5556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8588 121.8536) (end 146.9247 122.2276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.9247 121.4796) (end 146.8588 121.8536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.1144 121.1516) (end 146.9247 121.4796) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.405 120.9076) (end 147.1144 121.1516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7614 120.7776) (end 147.405 120.9076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.1408 120.7776) (end 147.7614 120.7776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.4972 120.9076) (end 148.1408 120.7776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.7878 121.1516) (end 148.4972 120.9076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.1184 122.2786) (end 148.9027 122.6526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.1934 121.8536) (end 149.1184 122.2786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.1184 121.4286) (end 149.1934 121.8536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.9027 121.0546) (end 149.1184 121.4286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.5722 120.7776) (end 148.9027 121.0546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.1668 120.6306) (end 148.5722 120.7776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7354 120.6306) (end 148.1668 120.6306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.33 120.7776) (end 147.7354 120.6306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.9995 121.0546) (end 147.33 120.7776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7838 121.4286) (end 146.9995 121.0546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7088 121.8536) (end 146.7838 121.4286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7838 122.2786) (end 146.7088 121.8536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.9995 122.6526) (end 146.7838 122.2786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.33 122.9296) (end 146.9995 122.6526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7354 123.0766) (end 147.33 122.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.1668 123.0766) (end 147.7354 123.0766) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.5722 122.9296) (end 148.1668 123.0766) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.9027 122.6526) (end 148.5722 122.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189 90.5786) (end 143.15 90.5786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.15 124.8536) (end 143.15 90.5786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189 124.8286) (end 143.15 124.8286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189 90.5786) (end 189 124.8286) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142 87.8) (xy 194.2 87.5) (xy 193.7 131.1) (xy 137.65 130) (xy 142.2 88)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.9 88.1) (xy 194.2 87.7) (xy 193.5 131.5) (xy 140.5 130.5) (xy 141.4 88)
      )
    )
  )
)
