(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 53)
    (no_connects 0)
    (area 132.8865 98.858 146.374 111.962)
    (thickness 1.6)
    (drawings 4)
    (tracks 301)
    (zones 0)
    (modules 21)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu mixed hide)
    (2 In2.Cu power hide)
    (31 B.Cu signal hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.127)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0 0)
    (mod_text_width 0)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance_ratio -0.075)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +BATT)
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(C6-Pad2)")
  (net 7 +3V3)
  (net 8 +1V8)
  (net 9 "Net-(L1-Pad1)")
  (net 10 "Net-(L2-Pad1)")
  (net 11 /ISET)
  (net 12 /Charge)
  (net 13 /LowBatt)
  (net 14 "Net-(R2-Pad2)")
  (net 15 "Net-(U1-Pad8)")
  (net 16 "Net-(U1-Pad3)")
  (net 17 "Net-(U2-Pad11)")
  (net 18 "Net-(U2-Pad5)")
  (net 19 "Net-(U3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +3V3)
    (add_net /Charge)
    (add_net /ISET)
    (add_net /LowBatt)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U3-Pad2)")
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.254)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L2-Pad1)")
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58307A8A)
    (at 137.8458 103.632 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value 536k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 135.9662 103.5304 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5415D599)
    (at 135.7884 107.3912)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 138.9888 106.7308 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +BATT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 137.7696 106.7308 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +BATT))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 139.0904 104.2797 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 5415D599)
    (at 144.272 104.3305 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.7 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 8 +1V8))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5415D631)
    (at 139.1412 106.5022 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5415D631)
    (at 144.272 106.553 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 +1V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:IND_SRN4026 (layer B.Cu) (tedit 58856FB5)
    (at 136.5885 103.886 270)
    (fp_text reference L1 (at 1.524 0 360) (layer B.SilkS))
    (fp_text value 4.7uH (at 1.5 3.5 270) (layer B.Fab))
    (pad 2 smd rect (at 3.05 0 270) (size 1.5 3.6) (layers B.Cu B.Paste B.Mask)
      (net 7 +3V3))
    (pad 1 smd rect (at 0 0 270) (size 1.5 3.6) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(L1-Pad1)"))
  )
  (module Footprints:IND_SRN4026 (layer B.Cu) (tedit 58856FBB)
    (at 141.732 103.886 270)
    (fp_text reference L2 (at 1.524 0 540) (layer B.SilkS))
    (fp_text value 4.7uH (at 1.5 3.5 270) (layer B.Fab))
    (pad 2 smd rect (at 3.05 0 270) (size 1.5 3.6) (layers B.Cu B.Paste B.Mask)
      (net 8 +1V8))
    (pad 1 smd rect (at 0 0 270) (size 1.5 3.6) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(L2-Pad1)"))
  )
  (module Footprints:DIP8_Header (layer F.Cu) (tedit 58854EB4)
    (at 138.43 106.68)
    (fp_text reference P1 (at 0 5.08) (layer F.SilkS))
    (fp_text value "DIP8 Header" (at 2.54 -7.62) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole circle (at 2.54 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 /ISET))
    (pad 4 thru_hole circle (at 5.08 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 /Charge))
    (pad 5 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +BATT))
    (pad 6 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 /LowBatt))
    (pad 7 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 8 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 +1V8))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58307A8A)
    (at 138.3792 104.902)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.8) (layer F.SilkS))
    (fp_text value 16.5k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /ISET))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58307A8A)
    (at 140.4874 107.1626)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 -1.8) (layer F.SilkS))
    (fp_text value 100k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58307A8A)
    (at 142.1638 107.1626)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.8) (layer F.SilkS))
    (fp_text value 120k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58307A8A)
    (at 138.9126 103.632 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value 120k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58307A8A)
    (at 143.9164 105.537 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.8 90) (layer F.SilkS))
    (fp_text value 200k (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 +1V8))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58307A8A)
    (at 143.9164 103.8352 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.8 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Footprints:10-TDFN_(AAT3693)" (layer F.Cu) (tedit 58855F55)
    (at 136.652 104.648 270)
    (fp_text reference U1 (at 1.5 3.05 270) (layer F.SilkS))
    (fp_text value AAT3693 (at 1.2 -1.55 270) (layer F.Fab))
    (pad 6 smd rect (at 1.78 1.6 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at 1.78 1.2 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /ISET))
    (pad 8 smd rect (at 1.78 0.8 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 1.78 0.4 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 10 smd rect (at 1.78 0 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +BATT))
    (pad 5 smd rect (at 0 1.6 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0 1.2 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0 0.8 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at 0 0.4 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /Charge))
    (pad 1 smd rect (at 0 0 270) (size 0.42 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 11 smd rect (at 0.9 0.8 270) (size 0.9 1.7) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module "Footprints:WDFN-12_(PAM2306D)" (layer F.Cu) (tedit 58856DB0)
    (at 142.6972 105.8926 180)
    (fp_text reference U2 (at 1.7 3.9 180) (layer F.SilkS))
    (fp_text value PAM2306DYPAA (at 2 -1.7 180) (layer F.Fab))
    (pad 7 smd rect (at 2.55 2.25 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +BATT))
    (pad 8 smd rect (at 2.55 1.8 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(L1-Pad1)"))
    (pad 9 smd rect (at 2.55 1.35 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2.55 0.9 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 11 smd rect (at 2.55 0.45 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 2.55 0 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +BATT))
    (pad 6 smd rect (at 0 2.25 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +BATT))
    (pad 5 smd rect (at 0 1.8 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at 0 1.35 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 3 smd rect (at 0 0.9 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 0.45 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(L2-Pad1)"))
    (pad 1 smd rect (at 0 0 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +BATT))
    (pad 13 smd rect (at 1.275 1.125 180) (size 1.6 2.5) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module "Footprints:6-UDFN_(NCS2202)" (layer F.Cu) (tedit 58857C8C)
    (at 144.0942 107.5182 180)
    (fp_text reference U3 (at 0.7 2 180) (layer F.SilkS))
    (fp_text value NCS2200 (at 0.5 -1.35 180) (layer F.Fab))
    (pad 6 smd rect (at 0.65 0 180) (size 0.42 0.22) (layers F.Cu F.Paste F.Mask)
      (net 13 /LowBatt))
    (pad 5 smd rect (at 0.65 0.4 180) (size 0.42 0.22) (layers F.Cu F.Paste F.Mask)
      (net 4 +BATT))
    (pad 3 smd rect (at 0 0.8 180) (size 0.42 0.22) (layers F.Cu F.Paste F.Mask)
      (net 8 +1V8))
    (pad 4 smd rect (at 0.65 0.8 180) (size 0.42 0.22) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 0 0.4 180) (size 0.42 0.22) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U3-Pad2)"))
    (pad 1 smd rect (at 0 0 180) (size 0.42 0.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (gr_line (start 144.78 100.33) (end 134.62 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 110.49) (end 144.78 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 110.49) (end 144.78 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 100.33) (end 134.62 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 100.33) (xy 144.78 100.33) (xy 144.78 110.49) (xy 134.62 110.49)
      )
    )
  )
  (zone (net 7) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.6365 107.8865) (xy 141.986 107.8865) (xy 141.986 110.49) (xy 134.62 110.49) (xy 134.62 106.045)
        (xy 139.6365 106.045)
      )
    )
  )
  (zone (net 8) (net_name +1V8) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.78 106.045) (xy 139.7635 106.045) (xy 139.7635 107.7595) (xy 142.113 107.7595) (xy 142.113 110.49)
        (xy 144.78 110.49)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.78 100.33) (xy 144.78 105.918) (xy 134.62 105.918) (xy 134.62 100.33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.5735 102.997) (xy 144.653 102.997) (xy 144.653 105.918) (xy 143.51 105.918) (xy 143.51 102.997)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.811 103.3145) (xy 138.4935 103.3145) (xy 138.4935 104.0765) (xy 138.811 104.0765)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 100.33) (xy 144.78 100.33) (xy 144.78 110.49) (xy 134.62 110.49)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 100.33) (xy 144.78 100.33) (xy 144.78 110.49) (xy 134.62 110.49)
      )
    )
  )
)
