(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.606)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "TPI Audio Switch")
		(rev "1.0")
		(company "HDM")
		(comment 1 "Drawn By: Aidan Medcalf")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
				(material "Liquid Photo")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Red")
				(thickness 0.01)
				(material "Liquid Ink")
				(epsilon_r 3.3)
				(loss_tangent 0)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.043)
			)
			(layer "dielectric 1"
				(type "core")
				(color "FR4 natural")
				(thickness 1.5)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.043)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Red")
				(thickness 0.01)
				(material "Liquid Ink")
				(epsilon_r 3.3)
				(loss_tangent 0)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
				(material "Liquid Photo")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 107.95 76.2)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-Pin_1)")
	(net 2 "/MIC")
	(net 3 "Net-(J1-Pin_3)")
	(net 4 "/AUDIO_R")
	(net 5 "Net-(J1-Pin_4)")
	(net 6 "/AUDIO_L")
	(net 7 "/GND")
	(net 8 "unconnected-(J2-Pad6)")
	(net 9 "unconnected-(J2-Pad7)")
	(net 10 "/AUDIO_L_SW")
	(net 11 "/MIC_SW")
	(footprint "Diode_SMD:D_SOD-123F"
		(locked yes)
		(layer "F.Cu")
		(at 124.95 98.2 180)
		(descr "D_SOD-123F")
		(tags "D_SOD-123F")
		(property "Reference" "D3"
			(at -3.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SMF10CA"
			(at 0 2.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bidirectional transient-voltage-suppression diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 3 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 180)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 6 "/AUDIO_L")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 180)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 7 "/GND")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 161.95 110.2)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at -3 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 157.48 100.33 180)
		(descr "Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x02 2.54mm double row")
		(property "Reference" "J3"
			(at 5.655 -2.87 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1\" Pin RA"
			(at 5.53 5.13 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.31 2.63 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/AUDIO_L_SW")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/MIC_SW")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(locked yes)
		(layer "F.Cu")
		(at 125.45 100.45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 3 0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AUDIO_L")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.15sqmm_1x04_P4mm_D0.5mm_OD1.5mm"
		(locked yes)
		(layer "F.Cu")
		(at 113.95 90.2 -90)
		(descr "Soldered wire connection, for 4 times 0.15 mm² wires, basic insulation, conductor diameter 0.5mm, outer diameter 1.5mm, size source Multi-Contact FLEXI-E 0.15 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.15sqmm")
		(property "Reference" "J1"
			(at 14.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "TRRS Cable"
			(at -5 -2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 6 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4 0 270)
			(size 1.7 1.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 8 0 270)
			(size 1.7 1.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 12 0 270)
			(size 1.7 1.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.15sqmm_1x04_P4mm_D0.5mm_OD1.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 113.95 110.2)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 2 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "TPI_MicSw Footprints:SAMESKY_SJ3-35024K-SMT-TR"
		(locked yes)
		(layer "F.Cu")
		(at 134.5 79.1 180)
		(property "Reference" "J2"
			(at 3.05 1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "SJ3-35024K-SMT-TR"
			(at -2.4892 5.461 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1.0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "5.575mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Same Sky"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr smd)
		(fp_text user "PCB EDGE"
			(at 2 3.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -3.45 -6.5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -3.45 0.5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/MIC")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0 -2.9 180)
			(size 2.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -5.8 180)
			(size 2.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/AUDIO_R")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 0 -8 180)
			(size 2.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/AUDIO_L_SW")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -6.9 0.9 180)
			(size 2.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/MIC_SW")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -6.9 -1 180)
			(size 2.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(J2-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -6.9 -3.9 180)
			(size 2.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(J2-Pad7)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -6.9 -6.1 180)
			(size 2.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/AUDIO_L")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(locked yes)
		(layer "F.Cu")
		(at 125.45 91.45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 9 1.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/MIC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123F"
		(locked yes)
		(layer "F.Cu")
		(at 124.95 93.7 180)
		(descr "D_SOD-123F")
		(tags "D_SOD-123F")
		(property "Reference" "D2"
			(at -3.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "SMF10CA"
			(at 0 2.1 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bidirectional transient-voltage-suppression diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 3 1.5 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 180)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 4 "/AUDIO_R")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 180)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 7 "/GND")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 128.45 82.2)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at -4.5 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-123F"
		(locked yes)
		(layer "F.Cu")
		(at 124.95 89.2 180)
		(descr "D_SOD-123F")
		(tags "D_SOD-123F")
		(property "Reference" "D1"
			(at -3.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SMF10CA"
			(at -9.5 -12.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bidirectional transient-voltage-suppression diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 3 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 180)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 2 "/MIC")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 180)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 7 "/GND")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 147.45 82.2)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 4.5 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(locked yes)
		(layer "F.Cu")
		(at 125.45 95.95)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J1-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AUDIO_R")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 162.56 100.33 180)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "J4"
			(at 1.27 -2.87 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1\" Pin"
			(at 1.27 5.13 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "TPI_MicSw.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at -2.89 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/AUDIO_L_SW")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/MIC_SW")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 107.95 116.2) (xy 167.95 116.2) (xy 167.95 78.2) (xy 145.95 78.2) (xy 145.95 76.2) (xy 129.95 76.2)
			(xy 129.95 78.2) (xy 107.95 78.2)
		)
		(fill no)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_text "Audio Switch rev A\n2025 TPI"
		(at 124.95 114.2 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 162.45 88.7 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 159.95 92.7 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(locked yes)
		(at 116.2 94.2 0)
		(layer "F.SilkS")
	)
	(gr_text "L"
		(at 162.45 92.7 90)
		(layer "F.SilkS")
	)
	(gr_text "MIC+"
		(locked yes)
		(at 116.2 90.2 0)
		(layer "F.SilkS")
	)
	(gr_text "MIC"
		(at 159.95 88.7 90)
		(layer "F.SilkS")
	)
	(gr_text "RIGHT"
		(locked yes)
		(at 116.2 98.2 0)
		(layer "F.SilkS")
	)
	(gr_text "OUT2"
		(at 156.95 104.2 0)
		(layer "F.SilkS")
	)
	(gr_text "IN"
		(locked yes)
		(at 113.95 88.2 0)
		(layer "F.SilkS")
	)
	(gr_text "LEFT"
		(locked yes)
		(at 116.2 102.2 0)
		(layer "F.SilkS")
	)
	(gr_text "OUT1"
		(at 141.95 88.2 90)
		(layer "F.SilkS")
	)
	(gr_text "Strip wires and solder to\nJ1 holes through top side."
		(at 72.95 107.7 0)
		(layer "User.1")
	)
	(gr_text "Cable Wiring\nTensility 10-02145"
		(at 89.95 85.7 0)
		(layer "User.1")
	)
	(table
		(column_count 4)
		(layer "User.1")
		(border
			(external yes)
			(header yes)
		)
		(separators
			(rows yes)
			(cols no)
		)
		(column_widths 12 5 8 8)
		(row_heights 3 3 3 3 3)
		(cells
			(table_cell "Cable"
				(start 72.95 87.2)
				(end 84.95 90.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "Pin"
				(start 84.95 87.2)
				(end 89.95 90.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "Signal"
				(start 89.95 87.2)
				(end 97.95 90.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "Color"
				(start 97.95 87.2)
				(end 105.95 90.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "D-Shield"
				(start 72.95 90.2)
				(end 84.95 93.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "1"
				(start 84.95 90.2)
				(end 89.95 93.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "MIC"
				(start 89.95 90.2)
				(end 97.95 93.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "Black"
				(start 97.95 90.2)
				(end 105.95 93.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "C-Ring2"
				(start 72.95 93.2)
				(end 84.95 96.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "2"
				(start 84.95 93.2)
				(end 89.95 96.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "GND"
				(start 89.95 93.2)
				(end 97.95 96.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "Green"
				(start 97.95 93.2)
				(end 105.95 96.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "B-Ring1"
				(start 72.95 96.2)
				(end 84.95 99.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "3"
				(start 84.95 96.2)
				(end 89.95 99.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "RIGHT"
				(start 89.95 96.2)
				(end 97.95 99.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "White"
				(start 97.95 96.2)
				(end 105.95 99.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "A-Tip"
				(start 72.95 99.2)
				(end 84.95 102.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "4"
				(start 84.95 99.2)
				(end 89.95 102.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "LEFT"
				(start 89.95 99.2)
				(end 97.95 102.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
			(table_cell "Red"
				(start 97.95 99.2)
				(end 105.95 102.2)
				(margins 1.0025 1.0025 1.0025 1.0025)
				(span 1 1)
				(layer "User.1")
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 167.95 116.2) (xy 167.95 78.2)
		)
		(height 4)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "38"
			(at 170.8 97.2 90)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 129.95 76.2) (xy 145.95 76.2)
		)
		(height -5)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "16"
			(at 137.95 70.05 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 107.95 116.2) (xy 167.95 116.2)
		)
		(height 4)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.05)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "60"
			(at 137.95 119.05 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 128.45 80.7) (xy 147.45 80.7)
		)
		(height -15.62)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "19"
			(at 137.95 63.93 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 129.95 76.2) (xy 129.95 78.2)
		)
		(height -6)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction inward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "2"
			(at 122.8 77.2 90)
			(layer "Cmts.User")
		)
	)
	(zone
		(net 7)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 111.45 91.7) (xy 116.45 91.7) (xy 116.45 96.7) (xy 111.45 96.7)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 123.2 93.2) (xy 122.7 92.7) (xy 121.45 92.7) (xy 121.45 94.7) (xy 122.7 94.7) (xy 123.2 94.2)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 135.15 81.2) (xy 135.85 81.2) (xy 136.05 81) (xy 137.95 81) (xy 137.95 83) (xy 136.05 83) (xy 135.85 82.8)
				(xy 135.15 82.8)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 123.2 88.7) (xy 122.7 88.2) (xy 121.45 88.2) (xy 121.45 90.2) (xy 122.7 90.2) (xy 123.2 89.7)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 123.2 97.7) (xy 122.7 97.2) (xy 121.45 97.2) (xy 121.45 99.2) (xy 122.7 99.2) (xy 123.2 98.7)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 162.95 105.2) (xy 164.95 103.2) (xy 164.95 89.2) (xy 162.95 87.2) (xy 144.95 87.2) (xy 142.95 85.2)
				(xy 142.95 78.2) (xy 141.95 77.2) (xy 133.95 77.2) (xy 132.95 78.2) (xy 132.95 85.2) (xy 130.95 87.2)
				(xy 112.95 87.2) (xy 110.95 89.2) (xy 110.95 103.2) (xy 112.95 105.2)
			)
		)
	)
	(embedded_fonts no)
)
