<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="76.2" y2="0" width="0" layer="20"/>
<wire x1="76.2" y1="0" x2="76.2" y2="50.8" width="0" layer="20"/>
<wire x1="76.2" y1="50.8" x2="0" y2="50.8" width="0" layer="20"/>
<wire x1="0" y1="50.8" x2="0" y2="0" width="0" layer="20"/>
<text>d7</text>
<text>aref</text>
<text>GND</text>
<text>a0</text>
<text>a5</text>
<text>Vin</text>
<text>usb</text>
<text>ext</text>
<text>5v</text>
<text>+</text>
<text>-</text>
<text>r</text>
<text>t</text>
<text>blk</text>
<text>+</text>
<text>gnd</text>
<text>rx</text>
<text>tx</text>
<text>d8</text>
<text>d9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>a1</text>
<text>a2</text>
<text>a3</text>
<text>a4</text>
<text>d3</text>
<text>d4</text>
<text>d2</text>
<text>grn</text>
<text>PWR SEL</text>
<text>+5</text>
<text>rx</text>
<text>tx</text>
<text>-</text>
<text>d5</text>
<text>d6</text>
<text>5V</text>
<text>5V</text>
<text>gnd</text>
<text>5V</text>
<text>GND</text>
<text>JSJ BoArduino</text>
<text>V1 July '13</text>
<text>gnd</text>
<text>5V</text>
<text>GND</text>
</plain>
<libraries>
<library name="avr">
<packages>
<package name="DIL28/3">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="minimidi">
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
</packages>
</library>
<library name="digg">
<packages>
<package name="CERM_OSC">
</package>
</packages>
</library>
<library name="switch-omron">
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="v-reg">
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="carduino">
<packages>
<package name="1X06-CLEAN">
</package>
<package name="1X08-CLEANBIG">
</package>
<package name="1X06-CLEANBIG">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2_LOCK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="AVRISP">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="proto">
<description>For making prototype areas on PC boards</description>
<packages>
<package name="PADSTRIP-5V">
<description>Strip of 5 connected pads, .1 inch pitch&lt;br&gt;
Pad 1 top, pad 5 bottom, meant for unconnected proto strip</description>
</package>
<package name="PADSTRIP-2HC">
<description>Strip of 2 connected pads, .1 inch pitch, for continuing at right</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="avr" package="DIL28/3" value="ATMEGA168P">
<attribute name="VALUE"/>
</element>
<element name="X1" library="digg" package="CERM_OSC" value="16.00MHz">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0204V" value="10K">
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-omron" package="B3F-10XX" value="RESET">
<attribute name="VALUE"/>
</element>
<element name="C3" library="minimidi" package="E2,5-6" value="10uF/25V">
<attribute name="VALUE"/>
</element>
<element name="C4" library="minimidi" package="E2,5-6" value="100uF/6V">
<attribute name="VALUE"/>
</element>
<element name="C5" library="minimidi" package="C025-025X050" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="LEDPWR" library="adafruit" package="LED3MM" value="GREEN"/>
<element name="R2" library="adafruit" package="0204V" value="1.0 K">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="v-reg" package="78XXS" value="7805"/>
<element name="D1" library="minimidi" package="DO41-10" value="1N4001"/>
<element name="C1" library="minimidi" package="C025-025X050" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="minimidi" package="C025-025X050" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="PWR_SEL" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JD2" library="carduino" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="carduino" package="1X06-CLEAN" value="">
<attribute name="VALUE"/>
</element>
<element name="JA1" library="carduino" package="1X06-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="C6" library="minimidi" package="C025-025X050" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="JD3" library="carduino" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="MOLEX-1X2_LOCK" value="M02POLAR_LOCK"/>
<element name="U$2" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$3" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="U$4" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="JA2" library="carduino" package="1X06-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JD1" library="carduino" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JD4" library="carduino" package="1X08-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="GNDA1" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW1A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW4A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW2A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW3A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW5A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P7" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P8" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW7A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW8A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW9A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="PR1" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR3" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR5" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR7" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="GNDA2" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="ROW6A" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P10" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P14" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="PR2" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR4" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR6" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR8" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="ROW7B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW6B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW5B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW4B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW3B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW2B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW1B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW9B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW8B" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="5VA1" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="5VA2" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="ROW7C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW6C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW5C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW4C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW3C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW2C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW1C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW9C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW8C" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P1" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="P2" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="PR9" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR10" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR11" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="PR12" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="ROW7D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW6D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW5D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW4D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW3D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW2D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW1D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW9D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="ROW8D" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="GNDE1" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="GNDE2" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="5VE1" library="proto" package="PADSTRIP-5V" value="PADSTRIP5-VA">
<attribute name="BOM" value="no"/>
<attribute name="VALSTAT" value="label"/>
</element>
<element name="5VE2" library="proto" package="PADSTRIP-2HC" value=""/>
<element name="ISP" library="adafruit" package="AVRISP" value="AVRISP-6">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="P$2"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="22"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="2"/>
<contactref element="IC2" pad="GND"/>
<contactref element="C3" pad="-"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="LEDPWR" pad="K"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JD2" pad="8"/>
<contactref element="JD4" pad="8"/>
<contactref element="GNDA1" pad="5"/>
<contactref element="GNDE1" pad="5"/>
<contactref element="ISP" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="9"/>
<contactref element="X1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="10"/>
<contactref element="X1" pad="P$3"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="7"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="PWR_SEL" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="20"/>
<contactref element="5VA1" pad="5"/>
<contactref element="5VE1" pad="5"/>
<contactref element="ISP" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="D1" pad="A"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="17"/>
<contactref element="JD2" pad="4"/>
<contactref element="JD4" pad="4"/>
<contactref element="ISP" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="18"/>
<contactref element="JD2" pad="5"/>
<contactref element="JD4" pad="5"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="19"/>
<contactref element="JD2" pad="6"/>
<contactref element="JD4" pad="6"/>
<contactref element="ISP" pad="3"/>
</signal>
<signal name="RST">
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="USB_5V">
<contactref element="PWR_SEL" pad="3"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="ANALOG0">
<contactref element="IC1" pad="23"/>
<contactref element="JA1" pad="1"/>
<contactref element="JA2" pad="1"/>
</signal>
<signal name="ANALOG1">
<contactref element="IC1" pad="24"/>
<contactref element="JA1" pad="2"/>
<contactref element="JA2" pad="2"/>
</signal>
<signal name="ANALOG2">
<contactref element="IC1" pad="25"/>
<contactref element="JA1" pad="3"/>
<contactref element="JA2" pad="3"/>
</signal>
<signal name="ANALOG3">
<contactref element="IC1" pad="26"/>
<contactref element="JA1" pad="4"/>
<contactref element="JA2" pad="4"/>
</signal>
<signal name="ANALOG4">
<contactref element="IC1" pad="27"/>
<contactref element="JA1" pad="5"/>
<contactref element="JA2" pad="5"/>
</signal>
<signal name="ANALOG5">
<contactref element="IC1" pad="28"/>
<contactref element="JA1" pad="6"/>
<contactref element="JA2" pad="6"/>
</signal>
<signal name="TXD">
<contactref element="IC1" pad="3"/>
<contactref element="JP7" pad="5"/>
<contactref element="JD3" pad="2"/>
<contactref element="JD1" pad="2"/>
</signal>
<signal name="RXD">
<contactref element="IC1" pad="2"/>
<contactref element="JP7" pad="4"/>
<contactref element="JD3" pad="1"/>
<contactref element="JD1" pad="1"/>
</signal>
<signal name="RTS#">
<contactref element="JP7" pad="6"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="IC1" pad="21"/>
<contactref element="JD2" pad="7"/>
<contactref element="JD4" pad="7"/>
</signal>
<signal name="N$22">
<contactref element="PWR_SEL" pad="1"/>
<contactref element="C4" pad="+"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="OUT"/>
</signal>
<signal name="+9V">
<contactref element="IC2" pad="IN"/>
<contactref element="C3" pad="+"/>
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="DIGITAL10">
<contactref element="IC1" pad="16"/>
<contactref element="JD2" pad="3"/>
<contactref element="JD4" pad="3"/>
</signal>
<signal name="DIGITAL9">
<contactref element="IC1" pad="15"/>
<contactref element="JD2" pad="2"/>
<contactref element="JD4" pad="2"/>
</signal>
<signal name="DIGITAL8">
<contactref element="IC1" pad="14"/>
<contactref element="JD2" pad="1"/>
<contactref element="JD4" pad="1"/>
</signal>
<signal name="DIGITAL7">
<contactref element="IC1" pad="13"/>
<contactref element="JD3" pad="8"/>
<contactref element="JD1" pad="8"/>
</signal>
<signal name="DIGITAL6">
<contactref element="IC1" pad="12"/>
<contactref element="JD3" pad="7"/>
<contactref element="JD1" pad="7"/>
</signal>
<signal name="DIGITAL5">
<contactref element="IC1" pad="11"/>
<contactref element="JD3" pad="6"/>
<contactref element="JD1" pad="6"/>
</signal>
<signal name="DIGITAL4">
<contactref element="IC1" pad="6"/>
<contactref element="JD3" pad="5"/>
<contactref element="JD1" pad="5"/>
</signal>
<signal name="DIGITAL3">
<contactref element="IC1" pad="5"/>
<contactref element="JD3" pad="4"/>
<contactref element="JD1" pad="4"/>
</signal>
<signal name="DIGITAL2">
<contactref element="IC1" pad="4"/>
<contactref element="JD3" pad="3"/>
<contactref element="JD1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="LEDPWR" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="P7" pad="5"/>
<contactref element="PR1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="PR1" pad="1"/>
<contactref element="PR3" pad="2"/>
<contactref element="PR3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="P8" pad="5"/>
<contactref element="PR5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="PR5" pad="1"/>
<contactref element="PR7" pad="2"/>
<contactref element="PR7" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="GNDA1" pad="1"/>
<contactref element="GNDA2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="P10" pad="5"/>
<contactref element="PR2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="PR2" pad="1"/>
<contactref element="PR4" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="P14" pad="5"/>
<contactref element="PR6" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="PR6" pad="1"/>
<contactref element="PR8" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="5VA1" pad="1"/>
<contactref element="5VA2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="P1" pad="5"/>
<contactref element="PR9" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="PR9" pad="1"/>
<contactref element="PR10" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="P2" pad="5"/>
<contactref element="PR11" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="PR11" pad="1"/>
<contactref element="PR12" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="GNDE1" pad="1"/>
<contactref element="GNDE2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="5VE1" pad="1"/>
<contactref element="5VE2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
