(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 20)
    (no_connects 0)
    (area 141.224999 98.72412 170.575001 123.17588)
    (thickness 1.6)
    (drawings 26)
    (tracks 46)
    (zones 0)
    (modules 3)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 4.3 4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.3 4.3)
    (pad_drill 4)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J2-Pad20)")
  (net 12 "Net-(J2-Pad18)")
  (net 13 "Net-(J2-Pad16)")
  (net 14 "Net-(J2-Pad14)")
  (net 15 "Net-(J2-Pad12)")
  (net 16 "Net-(J2-Pad19)")
  (net 17 "Net-(J2-Pad17)")
  (net 18 "Net-(J2-Pad15)")
  (net 19 "Net-(J2-Pad13)")
  (net 20 "Net-(J2-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad20)")
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_10pol (layer B.Cu) (tedit 55B5B0C6)
    (at 167.3 117.6 180)
    (descr "10-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J3 (at 11.43 4.50088 180) (layer B.SilkS))
    (fp_text value Screw_Terminal_1x10 (at 11.43 -4.50088 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad14)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad11)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad12)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad13)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad15)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad16)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad17)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad18)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad19)"))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad20)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_10pol.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_10pol (layer B.Cu) (tedit 55B5B0C6)
    (at 144.4 104.2)
    (descr "10-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 11.43 4.50088) (layer B.SilkS))
    (fp_text value Screw_Terminal_1x10 (at 11.43 -4.50088) (layer B.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 22.86 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_10pol.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyConnectors:Harwin_M80-Female-20Pin (layer F.Cu) (tedit 598B6685)
    (at 146.9 110.7)
    (fp_text reference J2 (at 9 0) (layer F.SilkS))
    (fp_text value CONN_01X20 (at 7.7 -5.6) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 21.15 0) (size 4.3 4.3) (drill 4) (layers *.Cu *.Mask))
    (pad 20 smd rect (at 0 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad20)"))
    (pad 19 smd rect (at 2 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad19)"))
    (pad 18 smd rect (at 4 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad18)"))
    (pad 17 smd rect (at 6 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad17)"))
    (pad 16 smd rect (at 8 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad16)"))
    (pad 15 smd rect (at 10 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad15)"))
    (pad 14 smd rect (at 12 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad14)"))
    (pad 13 smd rect (at 14 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad13)"))
    (pad 12 smd rect (at 16 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad12)"))
    (pad 11 smd rect (at 18 3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad11)"))
    (pad 10 smd rect (at 0 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 9 smd rect (at 2 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 8 smd rect (at 4 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 7 smd rect (at 6 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at 8 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 5 smd rect (at 10 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 4 smd rect (at 12 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 3 smd rect (at 14 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 2 smd rect (at 16 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 1 smd rect (at 18 -3.2) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad "" np_thru_hole circle (at -3.15 0) (size 4.3 4.3) (drill 4) (layers *.Cu *.Mask))
  )
  (gr_text 20 (at 144.4 113.9) (layer B.SilkS))
  (gr_text 19 (at 147.1 113.8) (layer B.SilkS))
  (gr_text 18 (at 149.6 113.8) (layer B.SilkS))
  (gr_text 17 (at 152 113.9) (layer B.SilkS))
  (gr_text 16 (at 154.7 114) (layer B.SilkS))
  (gr_text 15 (at 157.1 113.9) (layer B.SilkS))
  (gr_text 14 (at 159.6 114) (layer B.SilkS))
  (gr_text 13 (at 162 114) (layer B.SilkS))
  (gr_text 12 (at 164.6 113.9) (layer B.SilkS))
  (gr_text 11 (at 167.4 113.8) (layer B.SilkS))
  (gr_text 10 (at 144.2 107.9) (layer B.SilkS))
  (gr_text 9 (at 147 107.9) (layer B.SilkS))
  (gr_text 8 (at 149.7 107.9) (layer B.SilkS))
  (gr_text 7 (at 152.1 108) (layer B.SilkS))
  (gr_text 6 (at 154.6 108.1) (layer B.SilkS))
  (gr_text 5 (at 156.8 108) (layer B.SilkS))
  (gr_text 4 (at 159.6 108.1) (layer B.SilkS))
  (gr_text 3 (at 161.9 108.2) (layer B.SilkS))
  (gr_text 2 (at 164.5 108.1) (layer B.SilkS))
  (gr_text 1 (at 167.1 108.1) (layer B.SilkS))
  (gr_text 1 (at 164.9 110) (layer F.SilkS))
  (gr_line (start 141.3 121) (end 141.3 110.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.5 121) (end 141.3 121) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.5 100.8) (end 170.5 121) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.3 100.8) (end 170.5 100.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.3 110.8) (end 141.3 100.8) (angle 90) (layer Edge.Cuts) (width 0.15))
)
