(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 329)
    (no_connects 104)
    (area 29.451299 35.801299 217.436701 315.226701)
    (thickness 1.6)
    (drawings 184)
    (tracks 603)
    (zones 0)
    (modules 171)
    (nets 14)
  )
  (page A4)
  (title_block
    (title "555 Badge")
    (rev v02)
    (comment 2 creativecommons.org/licenses/by/4.0/)
    (comment 3 "License: CC BY 4.0")
    (comment 4 "Author: Shawn Hymel")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.17 2.17)
    (pad_drill 1.17)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 44.704 23.114)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(Q1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 GND)
  (net 4 VCC)
  (net 5 "Net-(BAT1-PadPos)")
  (net 6 "Net-(C1-Pad1)")
  (net 7 "Net-(C2-Pad1)")
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(R1-Pad2)")
  (net 11 "Net-(R3-Pad2)")
  (net 12 "Net-(S1-Pad1)")
  (net 13 "Net-(U1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(BAT1-PadPos)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net VCC)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 43.434 124.46 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 52.07 64.77 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 78.74 64.77 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 65.024 88.9 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 65.532 113.03 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 50.292 124.46 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 82.042 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 78.232 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 82.042 116.84)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 89.662 105.41 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 85.852 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 74.422 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 70.612 105.41 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 76.962 119.38 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 71.374 77.47 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 87.122 121.92 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 76.962 123.19 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 68.072 123.19)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 58.674 77.47 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 117.094 77.47 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 126.492 123.19)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 135.382 123.19 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 145.542 121.92 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 129.794 77.47 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 135.382 119.38 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 129.032 105.41 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 132.842 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 144.272 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 148.082 105.41 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 140.462 116.84)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 136.652 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 140.462 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 108.712 124.46 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 123.952 113.03 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 123.444 88.9 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 137.16 64.77 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 110.49 64.77 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 101.854 124.46 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 175.514 77.47 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 184.912 123.19)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 193.802 123.19 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 203.962 121.92 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 188.214 77.47 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 193.802 119.38 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 187.452 105.41 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 191.262 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 202.692 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 206.502 105.41 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 198.882 116.84)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 195.072 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 198.882 113.03 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 167.132 124.46 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 182.372 113.03 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 181.864 88.9 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 195.58 64.77 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 168.91 64.77 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 160.274 124.46 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 58.674 166.37 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 68.072 212.09)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 76.962 212.09 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 87.122 210.82 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 71.374 166.37 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 76.962 208.28 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 70.612 194.31 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 74.422 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 85.852 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 89.662 194.31 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 82.042 205.74)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 78.232 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 82.042 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 50.292 213.36 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 65.532 201.93 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 65.024 177.8 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 78.74 153.67 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 52.07 153.67 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 43.434 213.36 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 117.094 166.37 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 126.492 212.09)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 135.382 212.09 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 145.542 210.82 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 129.794 166.37 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 135.382 208.28 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 129.032 194.31 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 132.842 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 144.272 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 148.082 194.31 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 140.462 205.74)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 136.652 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 140.462 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 108.712 213.36 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 123.952 201.93 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 123.444 177.8 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 137.16 153.67 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 110.49 153.67 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 101.854 213.36 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 175.514 166.37 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 184.912 212.09)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 193.802 212.09 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 203.962 210.82 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 188.214 166.37 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 193.802 208.28 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 187.452 194.31 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 191.262 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 202.692 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 206.502 194.31 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 198.882 205.74)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 195.072 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 198.882 201.93 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 167.132 213.36 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 182.372 201.93 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 181.864 177.8 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 195.58 153.67 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 168.91 153.67 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 160.274 213.36 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 58.674 255.27 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 68.072 300.99)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 76.962 300.99 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 87.122 299.72 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 71.374 255.27 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 76.962 297.18 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 70.612 283.21 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 74.422 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 85.852 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 89.662 283.21 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 82.042 294.64)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 78.232 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 82.042 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 50.292 302.26 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 65.532 290.83 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 65.024 266.7 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 78.74 242.57 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 52.07 242.57 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 43.434 302.26 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 117.094 255.27 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 126.492 300.99)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 135.382 300.99 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 145.542 299.72 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 129.794 255.27 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 135.382 297.18 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 129.032 283.21 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 132.842 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 144.272 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 148.082 283.21 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 140.462 294.64)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 136.652 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 140.462 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 108.712 302.26 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 123.952 290.83 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 123.444 266.7 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 137.16 242.57 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 110.49 242.57 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 101.854 302.26 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 175.514 255.27 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module 555_badge:ICM7555-PDIP (layer F.Cu) (tedit 5A42EE09)
    (at 184.912 300.99)
    (fp_text reference U1 (at 0 -5.334) (layer F.SilkS))
    (fp_text value 7555 (at -0.254 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 VCC))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A42DBDC)
    (at 193.802 300.99 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.572 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.508 -3.556 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A42DBC2)
    (at 203.962 299.72 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 188.214 255.27 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3 (layer F.Cu) (tedit 5A42ECBF)
    (at 193.802 297.18 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/ff/95/2f/6a/75/70/42/49/CD00000971.pdf/files/CD00000971.pdf/jcr:content/translations/en.CD00000971.pdf)
    (fp_text reference Q1 (at 4.572 0.508 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.22 3.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.794 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE3)
    (at 187.452 283.21 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE7)
    (at 191.262 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 330k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF9)
    (at 202.692 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 22k (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF6)
    (at 206.502 283.21 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 100k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBE0)
    (at 198.882 294.64)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBEA)
    (at 195.072 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A42DBF2)
    (at 198.882 290.83 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:BS-7 (layer F.Cu) (tedit 5AE62383)
    (at 167.132 302.26 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 19.812 -6.35 180) (layer F.SilkS))
    (fp_text value BS-7 (at 7.62 1.778 90) (layer F.Fab) hide)
    (fp_text user %R (at 7.4676 0 90) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad Pos thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module digikey-footprints:EG1218 (layer F.Cu) (tedit 5AE6238A)
    (at 182.372 290.83 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value EG1218 (at 0.254 -3.048 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(BAT1-PadPos)"))
  )
  (module 555_badge:OSHPark-Slide_logo (layer B.Cu) (tedit 5AE615F8)
    (at 181.864 266.7 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:DigiKey_logo (layer B.Cu) (tedit 0)
    (at 195.58 242.57 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:Maker_io_logo (layer B.Cu) (tedit 0)
    (at 168.91 242.57 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module 555_badge:oshw_logo (layer B.Cu) (tedit 0)
    (at 160.274 302.26 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 38.1 129.54) (end 91.948 129.54) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 38.1 129.54) (end 38.1 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 91.948 129.54) (end 91.948 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 38.1 43.942) (end 91.948 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 59.944 46.482) (end 70.104 46.482) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 59.944 50.292) (end 70.104 50.292) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 70.104 48.387) (end 70.104 46.482) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 59.944 48.387) (end 59.944 46.482) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_text "CUT OUT" (at 65.024 48.514) (layer Eco1.User))
  (gr_text "555 Badge" (at 65.024 54.61) (layer B.SilkS))
  (gr_text v02 (at 91.44 128.016) (layer B.Cu))
  (gr_text + (at 56.134 104.394) (layer F.SilkS))
  (gr_text ON (at 61.976 107.95) (layer F.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 65.024 99.06) (layer B.SilkS))
  (gr_text "PCBs by" (at 65.024 85.09) (layer B.SilkS))
  (gr_text + (at 61.214 73.914) (layer B.SilkS))
  (gr_text + (at 73.914 73.914) (layer B.SilkS))
  (gr_text - (at 61.214 78.232) (layer B.SilkS))
  (gr_text - (at 73.914 78.232) (layer B.SilkS))
  (gr_line (start 29.464 315.214) (end 29.464 35.814) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 217.424 315.214) (end 29.464 315.214) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 217.424 35.814) (end 217.424 315.214) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 29.464 35.814) (end 217.424 35.814) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text - (at 132.334 78.232) (layer B.SilkS))
  (gr_text - (at 119.634 78.232) (layer B.SilkS))
  (gr_text + (at 132.334 73.914) (layer B.SilkS))
  (gr_text + (at 119.634 73.914) (layer B.SilkS))
  (gr_text "PCBs by" (at 123.444 85.09) (layer B.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 123.444 99.06) (layer B.SilkS))
  (gr_text ON (at 120.396 107.95) (layer F.SilkS))
  (gr_text + (at 114.554 104.394) (layer F.SilkS))
  (gr_text v02 (at 149.86 128.016) (layer B.Cu))
  (gr_text "555 Badge" (at 123.444 54.61) (layer B.SilkS))
  (gr_text "CUT OUT" (at 123.444 48.514) (layer Eco1.User))
  (gr_arc (start 118.364 48.387) (end 118.364 46.482) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 128.524 48.387) (end 128.524 46.482) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 118.364 50.292) (end 128.524 50.292) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 118.364 46.482) (end 128.524 46.482) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 43.942) (end 150.368 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 150.368 129.54) (end 150.368 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 129.54) (end 96.52 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 129.54) (end 150.368 129.54) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text - (at 190.754 78.232) (layer B.SilkS))
  (gr_text - (at 178.054 78.232) (layer B.SilkS))
  (gr_text + (at 190.754 73.914) (layer B.SilkS))
  (gr_text + (at 178.054 73.914) (layer B.SilkS))
  (gr_text "PCBs by" (at 181.864 85.09) (layer B.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 181.864 99.06) (layer B.SilkS))
  (gr_text ON (at 178.816 107.95) (layer F.SilkS))
  (gr_text + (at 172.974 104.394) (layer F.SilkS))
  (gr_text v02 (at 208.28 128.016) (layer B.Cu))
  (gr_text "555 Badge" (at 181.864 54.61) (layer B.SilkS))
  (gr_text "CUT OUT" (at 181.864 48.514) (layer Eco1.User))
  (gr_arc (start 176.784 48.387) (end 176.784 46.482) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 186.944 48.387) (end 186.944 46.482) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 176.784 50.292) (end 186.944 50.292) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 176.784 46.482) (end 186.944 46.482) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 43.942) (end 208.788 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 208.788 129.54) (end 208.788 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 129.54) (end 154.94 43.942) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 129.54) (end 208.788 129.54) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text - (at 73.914 167.132) (layer B.SilkS))
  (gr_text - (at 61.214 167.132) (layer B.SilkS))
  (gr_text + (at 73.914 162.814) (layer B.SilkS))
  (gr_text + (at 61.214 162.814) (layer B.SilkS))
  (gr_text "PCBs by" (at 65.024 173.99) (layer B.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 65.024 187.96) (layer B.SilkS))
  (gr_text ON (at 61.976 196.85) (layer F.SilkS))
  (gr_text + (at 56.134 193.294) (layer F.SilkS))
  (gr_text v02 (at 91.44 216.916) (layer B.Cu))
  (gr_text "555 Badge" (at 65.024 143.51) (layer B.SilkS))
  (gr_text "CUT OUT" (at 65.024 137.414) (layer Eco1.User))
  (gr_arc (start 59.944 137.287) (end 59.944 135.382) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 70.104 137.287) (end 70.104 135.382) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 59.944 139.192) (end 70.104 139.192) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 59.944 135.382) (end 70.104 135.382) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 38.1 132.842) (end 91.948 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 91.948 218.44) (end 91.948 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 38.1 218.44) (end 38.1 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 38.1 218.44) (end 91.948 218.44) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text - (at 132.334 167.132) (layer B.SilkS))
  (gr_text - (at 119.634 167.132) (layer B.SilkS))
  (gr_text + (at 132.334 162.814) (layer B.SilkS))
  (gr_text + (at 119.634 162.814) (layer B.SilkS))
  (gr_text "PCBs by" (at 123.444 173.99) (layer B.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 123.444 187.96) (layer B.SilkS))
  (gr_text ON (at 120.396 196.85) (layer F.SilkS))
  (gr_text + (at 114.554 193.294) (layer F.SilkS))
  (gr_text v02 (at 149.86 216.916) (layer B.Cu))
  (gr_text "555 Badge" (at 123.444 143.51) (layer B.SilkS))
  (gr_text "CUT OUT" (at 123.444 137.414) (layer Eco1.User))
  (gr_arc (start 118.364 137.287) (end 118.364 135.382) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 128.524 137.287) (end 128.524 135.382) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 118.364 139.192) (end 128.524 139.192) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 118.364 135.382) (end 128.524 135.382) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 132.842) (end 150.368 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 150.368 218.44) (end 150.368 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 218.44) (end 96.52 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 218.44) (end 150.368 218.44) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text - (at 190.754 167.132) (layer B.SilkS))
  (gr_text - (at 178.054 167.132) (layer B.SilkS))
  (gr_text + (at 190.754 162.814) (layer B.SilkS))
  (gr_text + (at 178.054 162.814) (layer B.SilkS))
  (gr_text "PCBs by" (at 181.864 173.99) (layer B.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 181.864 187.96) (layer B.SilkS))
  (gr_text ON (at 178.816 196.85) (layer F.SilkS))
  (gr_text + (at 172.974 193.294) (layer F.SilkS))
  (gr_text v02 (at 208.28 216.916) (layer B.Cu))
  (gr_text "555 Badge" (at 181.864 143.51) (layer B.SilkS))
  (gr_text "CUT OUT" (at 181.864 137.414) (layer Eco1.User))
  (gr_arc (start 176.784 137.287) (end 176.784 135.382) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 186.944 137.287) (end 186.944 135.382) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 176.784 139.192) (end 186.944 139.192) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 176.784 135.382) (end 186.944 135.382) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 132.842) (end 208.788 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 208.788 218.44) (end 208.788 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 218.44) (end 154.94 132.842) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 218.44) (end 208.788 218.44) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text - (at 73.914 256.032) (layer B.SilkS))
  (gr_text - (at 61.214 256.032) (layer B.SilkS))
  (gr_text + (at 73.914 251.714) (layer B.SilkS))
  (gr_text + (at 61.214 251.714) (layer B.SilkS))
  (gr_text "PCBs by" (at 65.024 262.89) (layer B.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 65.024 276.86) (layer B.SilkS))
  (gr_text ON (at 61.976 285.75) (layer F.SilkS))
  (gr_text + (at 56.134 282.194) (layer F.SilkS))
  (gr_text v02 (at 91.44 305.816) (layer B.Cu))
  (gr_text "555 Badge" (at 65.024 232.41) (layer B.SilkS))
  (gr_text "CUT OUT" (at 65.024 226.314) (layer Eco1.User))
  (gr_arc (start 59.944 226.187) (end 59.944 224.282) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 70.104 226.187) (end 70.104 224.282) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 59.944 228.092) (end 70.104 228.092) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 59.944 224.282) (end 70.104 224.282) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 38.1 221.742) (end 91.948 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 91.948 307.34) (end 91.948 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 38.1 307.34) (end 38.1 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 38.1 307.34) (end 91.948 307.34) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text - (at 132.334 256.032) (layer B.SilkS))
  (gr_text - (at 119.634 256.032) (layer B.SilkS))
  (gr_text + (at 132.334 251.714) (layer B.SilkS))
  (gr_text + (at 119.634 251.714) (layer B.SilkS))
  (gr_text "PCBs by" (at 123.444 262.89) (layer B.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 123.444 276.86) (layer B.SilkS))
  (gr_text ON (at 120.396 285.75) (layer F.SilkS))
  (gr_text + (at 114.554 282.194) (layer F.SilkS))
  (gr_text v02 (at 149.86 305.816) (layer B.Cu))
  (gr_text "555 Badge" (at 123.444 232.41) (layer B.SilkS))
  (gr_text "CUT OUT" (at 123.444 226.314) (layer Eco1.User))
  (gr_arc (start 118.364 226.187) (end 118.364 224.282) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 128.524 226.187) (end 128.524 224.282) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 118.364 228.092) (end 128.524 228.092) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 118.364 224.282) (end 128.524 224.282) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 221.742) (end 150.368 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 150.368 307.34) (end 150.368 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 307.34) (end 96.52 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 96.52 307.34) (end 150.368 307.34) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text - (at 190.754 256.032) (layer B.SilkS))
  (gr_text - (at 178.054 256.032) (layer B.SilkS))
  (gr_text + (at 190.754 251.714) (layer B.SilkS))
  (gr_text + (at 178.054 251.714) (layer B.SilkS))
  (gr_text "PCBs by" (at 181.864 262.89) (layer B.SilkS))
  (gr_text "Learn how to make this PCB!\nbit.ly/LearnKiCad" (at 181.864 276.86) (layer B.SilkS))
  (gr_text ON (at 178.816 285.75) (layer F.SilkS))
  (gr_text + (at 172.974 282.194) (layer F.SilkS))
  (gr_text v02 (at 208.28 305.816) (layer B.Cu))
  (gr_text "555 Badge" (at 181.864 232.41) (layer B.SilkS))
  (gr_text "CUT OUT" (at 181.864 226.314) (layer Eco1.User))
  (gr_arc (start 176.784 226.187) (end 176.784 224.282) (angle -180) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 186.944 226.187) (end 186.944 224.282) (angle 180) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 176.784 228.092) (end 186.944 228.092) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 176.784 224.282) (end 186.944 224.282) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 221.742) (end 208.788 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 208.788 307.34) (end 208.788 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 307.34) (end 154.94 221.742) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.94 307.34) (end 208.788 307.34) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.424 101.6) (xy 39.624 101.6) (xy 39.624 50.8) (xy 90.424 50.8)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 129.54) (xy 38.1 129.54) (xy 38.1 43.942) (xy 91.948 43.942)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 129.54) (xy 38.1 129.54) (xy 38.1 43.942) (xy 91.948 43.942)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.844 101.6) (xy 98.044 101.6) (xy 98.044 50.8) (xy 148.844 50.8)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.368 129.54) (xy 96.52 129.54) (xy 96.52 43.942) (xy 150.368 43.942)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.368 129.54) (xy 96.52 129.54) (xy 96.52 43.942) (xy 150.368 43.942)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.264 101.6) (xy 156.464 101.6) (xy 156.464 50.8) (xy 207.264 50.8)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.788 129.54) (xy 154.94 129.54) (xy 154.94 43.942) (xy 208.788 43.942)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.788 129.54) (xy 154.94 129.54) (xy 154.94 43.942) (xy 208.788 43.942)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.424 190.5) (xy 39.624 190.5) (xy 39.624 139.7) (xy 90.424 139.7)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 218.44) (xy 38.1 218.44) (xy 38.1 132.842) (xy 91.948 132.842)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 218.44) (xy 38.1 218.44) (xy 38.1 132.842) (xy 91.948 132.842)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.844 190.5) (xy 98.044 190.5) (xy 98.044 139.7) (xy 148.844 139.7)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.368 218.44) (xy 96.52 218.44) (xy 96.52 132.842) (xy 150.368 132.842)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.368 218.44) (xy 96.52 218.44) (xy 96.52 132.842) (xy 150.368 132.842)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.264 190.5) (xy 156.464 190.5) (xy 156.464 139.7) (xy 207.264 139.7)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.788 218.44) (xy 154.94 218.44) (xy 154.94 132.842) (xy 208.788 132.842)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.788 218.44) (xy 154.94 218.44) (xy 154.94 132.842) (xy 208.788 132.842)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.424 279.4) (xy 39.624 279.4) (xy 39.624 228.6) (xy 90.424 228.6)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 307.34) (xy 38.1 307.34) (xy 38.1 221.742) (xy 91.948 221.742)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 307.34) (xy 38.1 307.34) (xy 38.1 221.742) (xy 91.948 221.742)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.844 279.4) (xy 98.044 279.4) (xy 98.044 228.6) (xy 148.844 228.6)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.368 307.34) (xy 96.52 307.34) (xy 96.52 221.742) (xy 150.368 221.742)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.368 307.34) (xy 96.52 307.34) (xy 96.52 221.742) (xy 150.368 221.742)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.264 279.4) (xy 156.464 279.4) (xy 156.464 228.6) (xy 207.264 228.6)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.788 307.34) (xy 154.94 307.34) (xy 154.94 221.742) (xy 208.788 221.742)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.788 307.34) (xy 154.94 307.34) (xy 154.94 221.742) (xy 208.788 221.742)
      )
    )
  )
)
