(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 78)
    (zones 0)
    (modules 12)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu power)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.6 2.6)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.01)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(Cboot1-Pad2)")
  (net 2 "Net-(Cboot1-Pad1)")
  (net 3 GND)
  (net 4 /Vin)
  (net 5 /Vout)
  (net 6 "Net-(Rfbb1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.25)
    (add_net /Vin)
    (add_net /Vout)
    (add_net GND)
    (add_net "Net-(Cboot1-Pad1)")
    (add_net "Net-(Cboot1-Pad2)")
    (add_net "Net-(Rfbb1-Pad2)")
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 142.8115 101.6635 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module "My Libraries:BE5" locked (layer F.Cu) (tedit 5F4B3643)
    (at 136.9695 87.9475)
    (descr "Imported from BE5.svg")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 8.048) (layer F.SilkS) hide)
  )
  (module "My Libraries:TO-3-withEdgeCuts" (layer F.Cu) (tedit 5F9105FC)
    (at 130.81 92.1385)
    (descr "Transistor TO-3")
    (tags "TR TO-3 TO3 TO-204")
    (fp_text reference J1 (at 1.8 -9.25) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 6.5) (layer F.Fab))
    (fp_line (start -4.3 -6.9) (end -16.2 1.1) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -4.3 17.8) (end -16.276967 9.747694) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.099668 -6.799354) (end 19.9 1.2) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.1 17.7) (end 19.747176 9.803859) (layer Edge.Cuts) (width 0.12))
    (fp_text user %R (at 0 4.25) (layer F.Fab))
    (fp_arc (start 1.8 5.45) (end -4.3 -6.9) (angle 53.5021223) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 1.8 5.45) (end -4.3 17.8) (angle -53.50212705) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start -13.3 5.45) (end -16.2 1.1) (angle -111.6) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 16.9 5.45) (end 19.9 1.2) (angle 111.6000049) (layer Edge.Cuts) (width 0.12))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 /Vin))
    (pad 2 thru_hole circle (at 0 10.92) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 /Vout))
    (pad 3 thru_hole circle (at -13.3 5.45) (size 6.35 6.35) (drill 4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 16.9 5.45) (size 6.35 6.35) (drill 4) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 126.568201 98.0694 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at -2.209799 -2.3876 90) (layer F.SilkS))
    (fp_text value TPS563240DDCR (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 6 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(Cboot1-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Rfbb1-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(Cboot1-Pad1)"))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 121.412 94.488 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference Rfbt1 (at 1.397 -1.2065 90) (layer F.SilkS))
    (fp_text value 73.2k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /Vout))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(Rfbb1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 123.444 94.488 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference Rfbb1 (at -3.2385 -0.0635 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 6 "Net-(Rfbb1-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Bourns_SRP5030T (layer F.Cu) (tedit 5E6F3F9B)
    (at 135.6106 98.298 270)
    (descr "Inductor, Bourns, SRP5030T, 5.7mmx5.2mm (Script generated with StandardBox.py) (https://www.bourns.com/data/global/pdfs/SRP5030T.pdf)")
    (tags "Inductor Bourns_SRP5030T")
    (attr smd)
    (fp_text reference L1 (at -0.4445 -3.4544 90) (layer F.SilkS))
    (fp_text value 1.5u (at 0 3.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.25 0 270) (size 2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /Vout))
    (pad 1 smd roundrect (at -2.25 0 270) (size 2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(Cboot1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_MAPI-4030.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.6 1.3 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 138.684 102.87)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cout2 (at -3.429 0.0635) (layer F.SilkS))
    (fp_text value 22u (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /Vout))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 130.81 100.33 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cout1 (at 0.9525 2.54 90) (layer F.SilkS))
    (fp_text value 22u (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /Vout))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 126.6444 93.5736 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cinx1 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 100n (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /Vin))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 126.6952 90.7034 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cin1 (at 0 1.4224) (layer F.SilkS))
    (fp_text value 22u (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /Vin))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 123.444 100.33 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference Cboot1 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(Cboot1-Pad2)"))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(Cboot1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Vmin 7V" (at 130.8735 85.598) (layer F.SilkS))
  (gr_text "5V  3A" (at 128.651 106.553) (layer F.SilkS))
  (gr_text "Thank you \nFor Your\nHelp, Chat!" (at 135.3185 98.1075) (layer B.SilkS))
  (gr_text "TO3 Switcher\nrev1" (at 144.018 94.107) (layer B.SilkS))
  (gr_text GND (at 151.8285 97.282 90) (layer B.SilkS))
  (gr_text GND (at 151.8285 97.282 90) (layer F.SilkS))
  (gr_text GND (at 113.411 97.409 90) (layer B.SilkS))
  (gr_text GND (at 113.411 97.409 90) (layer F.SilkS))
  (gr_text Vout (at 128.778 105.029) (layer B.SilkS))
  (gr_text Vout (at 128.778 105.029) (layer F.SilkS))
  (gr_text Vin (at 130.81 89.9795) (layer B.SilkS))
  (gr_text Vin (at 130.81 89.9795) (layer F.SilkS))
  (zone (net 4) (net_name /Vin) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 1.27) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 132.842 94.742) (xy 132.08 94.742) (xy 132.08 97.536) (xy 126.746 97.536) (xy 126.746 88.646)
        (xy 132.842 88.646)
      )
    )
  )
  (zone (net 2) (net_name "Net-(Cboot1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 138.684 98.552) (xy 126.746 98.552) (xy 126.746 97.79) (xy 132.334 97.79) (xy 132.334 95.25)
        (xy 133.35 95.25) (xy 133.35 94.488) (xy 138.684 94.488)
      )
    )
  )
  (zone (net 5) (net_name /Vout) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 1.27) (smoothing chamfer) (radius 0.5))
    (polygon
      (pts
        (xy 138.684 104.648) (xy 130.81 104.648) (xy 130.81 103.378) (xy 130.81 101.092) (xy 130.81 98.806)
        (xy 138.684 98.806)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 2.54) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 154.686 112.776) (xy 108.204 112.522) (xy 108.204 81.28) (xy 154.686 81.28)
      )
    )
  )
  (zone (net 6) (net_name "Net-(Rfbb1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 124.714 94.996) (xy 126.238 94.996) (xy 126.238 97.536) (xy 120.65 97.536) (xy 120.65 94.488)
        (xy 124.714 94.488)
      )
    )
  )
  (zone (net 1) (net_name "Net-(Cboot1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 126.238 100.33) (xy 122.428 100.33) (xy 122.428 98.552) (xy 126.238 98.552)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 154.686 112.776) (xy 108.204 112.522) (xy 108.204 81.28) (xy 154.686 81.28)
      )
    )
  )
)
