(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 8)
    (no_connects 1)
    (area 78.473809 92.494999 112.557143 108.075)
    (thickness 1.6)
    (drawings 44)
    (tracks 37)
    (zones 0)
    (modules 5)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.65)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.65)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.3)
    (segment_width 0.01)
    (edge_width 0.01)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 90 92.5)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(J2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
  )
  (net_class newTrack ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module LEDs:LED_WS2812B-PLCC4 (layer F.Cu) (tedit 59A8CB04)
    (at 91.75 100 270)
    (descr http://www.world-semi.com/uploads/soft/150522/1-150522091P5.pdf)
    (tags "LED NeoPixel")
    (attr smd)
    (fp_text reference LED1 (at -4.6 0.05 360) (layer F.SilkS))
    (fp_text value WS2812B (at 0 4 270) (layer F.Fab) hide)
    (pad 3 smd rect (at 2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (pad 4 smd rect (at 2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -2.5 1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -2.5 -1.6 270) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_WS2812B-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59A8DB40)
    (at 92.25 105.5 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value C1 (at 0 1.75 180) (layer F.SilkS) hide)
    (fp_text user %R (at -2.75 -1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINHEAD1-3 (layer F.Cu) (tedit 59BC4502)
    (at 87.1 97.5 270)
    (fp_text reference J2 (at 2.59 -3.8 270) (layer F.SilkS) hide)
    (fp_text value IN (at 7.74 0 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Connectors:PINHEAD1-3 (layer F.Cu) (tedit 59BC4519)
    (at 107.5 102.79 90)
    (fp_text reference J1 (at 2.59 -3.8 90) (layer F.SilkS))
    (fp_text value OUT (at 3.59 -3.3 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)"))
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 92.9 100.1 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_line (start 102 103.8) (end 103.6 105.4) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 104.5 104.5) (end 105.4 103.6) (angle 180) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 105.4 103.6) (end 103.9 102.1) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 103.9 102.1) (end 103.8 102) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 103 103) (end 102 103.8) (angle 168.4653793) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 96.2 102) (end 94.6 103.6) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 95.5 104.5) (end 96.4 105.4) (angle 180) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 96.4 105.4) (end 97.9 103.9) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 97.9 103.9) (end 98 103.8) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 97 103) (end 96.2 102) (angle 168.4653793) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 103.7 94.5) (end 102.1 96.1) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 103 97) (end 103.9 97.9) (angle 180) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 103.9 97.9) (end 105.4 96.4) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 105.4 96.4) (end 105.5 96.3) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 104.5 95.5) (end 103.7 94.5) (angle 168.4653793) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 97 97) (end 98 96.2) (angle 168.4653793) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 96.1 97.9) (end 96.2 98) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 94.6 96.4) (end 96.1 97.9) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 95.5 95.5) (end 94.6 96.4) (angle 180) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 98 96.2) (end 96.4 94.6) (layer Edge.Cuts) (width 0.01))
  (gr_text info@johnty.ca (at 101.5 106.3) (layer B.SilkS))
  (gr_text WS2812B (at 101.3 99.8) (layer B.SilkS))
  (gr_line (start 107.5 92.5) (end 90 92.5) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 90 92.5) (end 87.5 92.5) (layer Edge.Cuts) (width 0.01))
  (gr_text + (at 86.1 94.9) (layer F.SilkS))
  (gr_text + (at 108.7 95.3) (layer F.SilkS))
  (gr_line (start 90 107.5) (end 87.5 107.5) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 107.5 107.5) (end 90 107.5) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 85 95) (end 85 105) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 110 95) (end 110 105) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 87.5 105) (end 87.5 107.5) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 87.5 95) (end 85 95) (angle 89.9) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 107.5 95) (end 107.5 92.5) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_arc (start 107.5 105) (end 110 105) (angle 90) (layer Edge.Cuts) (width 0.01))
)
