(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 35)
    (no_connects 0)
    (area 109.779999 53.264999 142.950001 87.705001)
    (thickness 1.6)
    (drawings 17)
    (tracks 134)
    (zones 0)
    (modules 17)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 103.505 79.375)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory pdf/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +5V)
  (net 5 "Net-(R2-Pad1)")
  (net 6 "Net-(R3-Pad1)")
  (net 7 "Net-(SW1-Pad2)")
  (net 8 "Net-(SW1-Pad1)")
  (net 9 "Net-(SW1-Pad4)")
  (net 10 "Net-(C3-Pad2)")
  (net 11 "Net-(C4-Pad1)")
  (net 12 "Net-(R1-Pad1)")
  (net 13 "Net-(R7-Pad1)")
  (net 14 "Net-(J3-Pad2)")
  (net 15 "Net-(J1-Pad1)")
  (net 16 "Net-(J2-Pad1)")
  (net 17 "Net-(J3-Pad4)")
  (net 18 "Net-(J3-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW1-Pad4)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 1.016)
    (via_dia 1.27)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module lib_fp:EC12PLRGB_Rotary_Encoder (layer F.Cu) (tedit 5A46E4C3)
    (at 132.08 74.295)
    (fp_text reference SW1 (at 8.495 0 90) (layer F.SilkS) hide)
    (fp_text value EC12PLRGB (at -6.858 -4.191 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 -7) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at -2 -7) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(SW1-Pad2)"))
    (pad 1 thru_hole circle (at -4 -7) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(SW1-Pad1)"))
    (pad 4 thru_hole circle (at 2 -7) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(SW1-Pad4)"))
    (pad 5 thru_hole circle (at 4 -7) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad C thru_hole circle (at 0 7.5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad A thru_hole circle (at -2.5 7.5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(R2-Pad1)"))
    (pad B thru_hole circle (at 2.5 7.5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(R3-Pad1)"))
    (pad "" np_thru_hole rect (at -5.6 0) (size 2 2.1) (drill oval 2 2.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole rect (at 5.6 0) (size 2 2.1) (drill oval 2 2.1) (layers *.Cu *.Mask))
  )
  (module lib_fp:C_0805_HandSoldering (layer F.Cu) (tedit 5A28DE31)
    (at 118.11 73.025 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value .1uF (at -0.889 -1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:C_0805_HandSoldering (layer F.Cu) (tedit 5A28DE31)
    (at 118.11 79.375 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value .1uF (at -0.889 -1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:C_0805_HandSoldering (layer F.Cu) (tedit 5A28DE31)
    (at 121.92 59.055 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -1.27 1.905 90) (layer F.SilkS))
    (fp_text value .1uF (at 1.27 1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:C_0805_HandSoldering (layer F.Cu) (tedit 5A28DE31)
    (at 118.11 66.675 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value .1uF (at -0.889 -1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:Pin_Header_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 113.665 75.565)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at -2.54 0) (layer B.SilkS))
    (fp_text value Conn_01x04_Male (at -5.715 -2.54 270) (layer B.Fab))
    (fp_text user %R (at -1.905 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:Pin_Header_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 113.665 62.865)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at -2.54 0) (layer B.SilkS))
    (fp_text value Conn_01x04_Male (at -5.715 -2.54 270) (layer B.Fab))
    (fp_text user %R (at -1.905 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 137.16 55.245 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 -3.175 450) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at -3.175 4.445 360) (layer F.Fab))
    (fp_text user %R (at 0 5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_0805_HandSoldering (layer F.Cu) (tedit 5A28DF52)
    (at 135.89 63.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -1.27 1.905 180) (layer F.SilkS))
    (fp_text value 10K (at 1.27 1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_0805_HandSoldering (layer F.Cu) (tedit 5A28DF52)
    (at 121.92 73.025 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -1.27 1.905 270) (layer F.SilkS))
    (fp_text value 22K (at 1.397 1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_0805_HandSoldering (layer F.Cu) (tedit 5A28DF52)
    (at 121.92 79.375 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -1.27 1.905 270) (layer F.SilkS))
    (fp_text value 22K (at 1.397 1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_0805_HandSoldering (layer F.Cu) (tedit 5A28DF52)
    (at 135.89 84.455 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 1.27 -1.905 360) (layer F.SilkS))
    (fp_text value 10K (at -1.27 -1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_0805_HandSoldering (layer F.Cu) (tedit 5A28DF52)
    (at 128.27 84.455)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -1.27 1.905 180) (layer F.SilkS))
    (fp_text value 10K (at 1.33 1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_0805_HandSoldering (layer F.Cu) (tedit 5A28DF52)
    (at 118.11 59.055 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -1.27 1.905 270) (layer F.SilkS))
    (fp_text value 100 (at 1.397 1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_0805_HandSoldering (layer F.Cu) (tedit 5A28DF52)
    (at 135.89 59.055)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -1.27 1.905 180) (layer F.SilkS))
    (fp_text value 33 (at 1.27 1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_0805_HandSoldering (layer F.Cu) (tedit 5A28DF52)
    (at 121.92 66.675 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -1.27 1.905 270) (layer F.SilkS))
    (fp_text value 22K (at 1.397 1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A349C68)
    (at 128.905 60.96 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 3.81 90) (layer F.SilkS))
    (fp_text value WS2811 (at 0 -3.175 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(SW1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(SW1-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(SW1-Pad4)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J3-Pad3)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R7-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J3-Pad4)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C3-Pad2)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "EC12PLRGB Rotary\nEncoder Breakout\nCarl Raymond Dec. 2017" (at 129.54 60.96) (layer B.SilkS))
  (gr_text "J3: 1=PC3 2=Din 3=Dout. Short 1-2 for Din=PC3\nShort 4-5 for 400KHz / Open for 800KHz" (at 140.97 69.85 90) (layer F.SilkS))
  (gr_arc (start 114.935 78.867) (end 114.935 77.597) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.205 78.867) (end 116.205 87.63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.855 77.597) (end 114.935 77.597) (layer Edge.Cuts) (width 0.15))
  (gr_text PC0 (at 115.824 68.072) (layer F.SilkS))
  (gr_text PC1 (at 115.824 70.612) (layer F.SilkS))
  (gr_text PC2 (at 115.824 73.152) (layer F.SilkS))
  (gr_text 5V (at 115.824 55.245) (layer F.SilkS))
  (gr_text GND (at 115.824 57.785) (layer F.SilkS))
  (gr_text GND (at 115.824 60.325) (layer F.SilkS))
  (gr_text PC3 (at 115.824 75.692) (layer F.SilkS))
  (gr_text Vin (at 115.824 62.865) (layer F.SilkS))
  (gr_line (start 109.855 77.597) (end 109.855 53.34) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.875 87.63) (end 116.205 87.63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.875 53.34) (end 142.875 87.63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.855 53.34) (end 142.875 53.34) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 86.995) (xy 116.84 86.995) (xy 116.84 77.47) (xy 110.49 77.47) (xy 110.49 53.975)
        (xy 142.24 53.975)
      )
    )
  )
)
