(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 86)
    (no_connects 0)
    (area 140.386999 79.426999 182.066001 95.642501)
    (thickness 1.6)
    (drawings 29)
    (tracks 391)
    (zones 0)
    (modules 33)
    (nets 44)
  )
  (page A4)
  (title_block
    (title kyobreak)
    (date 2016-10-06)
    (rev 0.01)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (trace_clearance 0.1)
    (zone_clearance 0.7)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 R0)
  (net 2 R1)
  (net 3 R2)
  (net 4 R3)
  (net 5 R4)
  (net 6 R5)
  (net 7 R6)
  (net 8 R7)
  (net 9 G0)
  (net 10 G1)
  (net 11 G2)
  (net 12 G3)
  (net 13 G4)
  (net 14 G5)
  (net 15 G6)
  (net 16 G7)
  (net 17 B0)
  (net 18 B1)
  (net 19 B2)
  (net 20 B3)
  (net 21 B4)
  (net 22 B5)
  (net 23 B6)
  (net 24 B7)
  (net 25 GND)
  (net 26 VSYNC)
  (net 27 HSYNC)
  (net 28 CLOCK)
  (net 29 BACKL_EN)
  (net 30 V_LED_CATHODE)
  (net 31 V_LED_ANODE)
  (net 32 "Net-(C5-Pad2)")
  (net 33 "Net-(R10-Pad1)")
  (net 34 DISP_ENABLE)
  (net 35 /LED_VIN)
  (net 36 VCC)
  (net 37 TB)
  (net 38 RL)
  (net 39 SPI_SDO)
  (net 40 DISP_RESET)
  (net 41 SPI_CS)
  (net 42 SPI_SCL)
  (net 43 SPI_SDI)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(R10-Pad1)")
  )
  (net_class PWR ""
    (clearance 0.1)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LED_VIN)
  )
  (net_class PWRBIG ""
    (clearance 0.1)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
    (add_net V_LED_ANODE)
    (add_net V_LED_CATHODE)
  )
  (net_class SIG ""
    (clearance 0.1)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net B0)
    (add_net B1)
    (add_net B2)
    (add_net B3)
    (add_net B4)
    (add_net B5)
    (add_net B6)
    (add_net B7)
    (add_net BACKL_EN)
    (add_net CLOCK)
    (add_net DISP_ENABLE)
    (add_net DISP_RESET)
    (add_net G0)
    (add_net G1)
    (add_net G2)
    (add_net G3)
    (add_net G4)
    (add_net G5)
    (add_net G6)
    (add_net G7)
    (add_net HSYNC)
    (add_net R0)
    (add_net R1)
    (add_net R2)
    (add_net R3)
    (add_net R4)
    (add_net R5)
    (add_net R6)
    (add_net R7)
    (add_net RL)
    (add_net SPI_CS)
    (add_net SPI_SCL)
    (add_net SPI_SDI)
    (add_net SPI_SDO)
    (add_net TB)
    (add_net VSYNC)
  )
  (module mylib:pin_header_8x1_1.27mm_pitch (layer F.Cu) (tedit 57F18C09)
    (at 166.1795 80.4545 180)
    (fp_text reference P3 (at 0.635 1.2065 180) (layer F.SilkS) hide)
    (fp_text value CONN_8 (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -4.445 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 17 B0))
    (pad 2 thru_hole circle (at -3.175 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 18 B1))
    (pad 3 thru_hole circle (at -1.905 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 19 B2))
    (pad 4 thru_hole circle (at -0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 20 B3))
    (pad 5 thru_hole circle (at 0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 21 B4))
    (pad 6 thru_hole circle (at 1.905 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 22 B5))
    (pad 7 thru_hole circle (at 3.175 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 23 B6))
    (pad 8 thru_hole circle (at 4.445 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 24 B7))
  )
  (module w_smd_trans:sot23-6 (layer F.Cu) (tedit 57F1D021)
    (at 177.1015 89.408 270)
    (descr SOT23-6)
    (fp_text reference U2 (at 1.9685 1.0795 360) (layer F.SilkS))
    (fp_text value LT1932 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 35 /LED_VIN))
    (pad 3 smd rect (at 0.9525 1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 30 V_LED_CATHODE))
    (pad 2 smd rect (at 0 1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 4 smd rect (at 0.9525 -1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R10-Pad1)"))
    (pad 6 smd rect (at -0.9525 -1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 36 VCC))
    (pad 5 smd rect (at 0 -1.05664 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 29 BACKL_EN))
    (model walter/smd_trans/sot23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_diode:sod323 (layer F.Cu) (tedit 57F1C801)
    (at 173.482 88.265 180)
    (descr SOD323)
    (fp_text reference D1 (at -0.0635 1.2065 180) (layer F.SilkS))
    (fp_text value DIODESCH (at 0 1.19888 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.09982 0 180) (size 1.00076 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 31 V_LED_ANODE))
    (pad 1 smd rect (at -1.09982 0 180) (size 1.00076 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 35 /LED_VIN))
    (model walter/smd_diode/sod323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C89)
    (at 149.6695 81.5975 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R1 (at -0.3175 0.889 180) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 R1))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 R0))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C87)
    (at 148.3995 82.4865 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R2 (at 0 0.9525 180) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 R2))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 R1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C84)
    (at 147.1295 81.5975 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R3 (at 0.9525 0.889 180) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 R3))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 R2))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C7E)
    (at 159.258 82.55 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R4 (at 0.4445 0.889 180) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 G1))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 G0))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C7C)
    (at 158.5595 81.5975 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R5 (at 0.6985 0.889 180) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 G2))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 G1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C10)
    (at 169.9895 81.5975 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R6 (at -0.0635 0.8255 180) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 B1))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 17 B0))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C0D)
    (at 168.5925 82.4865 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R7 (at 0 0.889 180) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 B2))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 B1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F18C0B)
    (at 167.4495 81.5975 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R8 (at 0.762 0.8255 180) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 B3))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 B2))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F5D90C)
    (at 172.4025 93.9165 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R9 (at -0.5715 -0.8255 270) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F30985)
    (at 177.8 91.44)
    (descr "SMT resistor, 0402")
    (fp_text reference R10 (at 0.762 0.8255) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F306C3)
    (at 179.832 89.408 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R11 (at -0.5715 -0.8255 360) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 29 BACKL_EN))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 57F303E5)
    (at 177.1015 81.9785)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at 1.4605 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 36 VCC))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 57F5D8FB)
    (at 173.482 89.9795 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference C3 (at -0.1905 -1.27 360) (layer F.SilkS))
    (fp_text value 1u (at 0 0.9906 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 31 V_LED_ANODE))
    (pad 2 smd rect (at -0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 57F1C397)
    (at 172.4025 91.7575 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C5 (at 0.0508 -0.8255 90) (layer F.SilkS))
    (fp_text value 47n (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 31 V_LED_ANODE))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C5-Pad2)"))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 57F1D034)
    (at 180.213 87.0585 270)
    (descr "SMT capacitor, 0805")
    (fp_text reference C7 (at -0.1905 -1.3335 270) (layer F.SilkS))
    (fp_text value 4u7 (at 0 0.9906 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 270) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 36 VCC))
    (pad 2 smd rect (at -0.9525 0 270) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_8x1_1.27mm_pitch (layer F.Cu) (tedit 57F18C83)
    (at 145.8595 80.4545 180)
    (fp_text reference P1 (at 1.27 1.2065 180) (layer F.SilkS) hide)
    (fp_text value CONN_8 (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -4.445 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 1 R0))
    (pad 2 thru_hole circle (at -3.175 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 2 R1))
    (pad 3 thru_hole circle (at -1.905 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 3 R2))
    (pad 4 thru_hole circle (at -0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 4 R3))
    (pad 5 thru_hole circle (at 0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 5 R4))
    (pad 6 thru_hole circle (at 1.905 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 6 R5))
    (pad 7 thru_hole circle (at 3.175 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 7 R6))
    (pad 8 thru_hole circle (at 4.445 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 8 R7))
  )
  (module mylib:pin_header_8x1_1.27mm_pitch (layer F.Cu) (tedit 57F18C79)
    (at 156.0195 80.4545 180)
    (fp_text reference P2 (at -0.127 1.2065 180) (layer F.SilkS) hide)
    (fp_text value CONN_8 (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -4.445 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 9 G0))
    (pad 2 thru_hole circle (at -3.175 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 10 G1))
    (pad 3 thru_hole circle (at -1.905 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 11 G2))
    (pad 4 thru_hole circle (at -0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 12 G3))
    (pad 5 thru_hole circle (at 0.635 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 13 G4))
    (pad 6 thru_hole circle (at 1.905 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 14 G5))
    (pad 7 thru_hole circle (at 3.175 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 15 G6))
    (pad 8 thru_hole circle (at 4.445 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 16 G7))
  )
  (module mylib:pin_header_2x1_1.27mm_pitch (layer F.Cu) (tedit 57F09BF7)
    (at 177.165 80.391)
    (fp_text reference P4 (at -0.152 -1.4665) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 25 GND))
    (pad 2 thru_hole circle (at 0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 36 VCC))
  )
  (module mylib:l_1210 (layer F.Cu) (tedit 57F303D5)
    (at 176.8475 86.1695 180)
    (descr "SMT resistor, 1210")
    (fp_text reference L2 (at 2.667 1.016 270) (layer F.SilkS))
    (fp_text value 6u8 (at 0 1.7018 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 35 /LED_VIN))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 36 VCC))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 57F1F504)
    (at 177.1015 83.5025)
    (descr "SMT capacitor, 0805")
    (fp_text reference C1 (at 2.159 0 90) (layer F.SilkS))
    (fp_text value 1u (at 0 0.9906) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 36 VCC))
    (pad 2 smd rect (at -0.9525 0) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:62684-401100ALF (layer F.Cu) (tedit 57F5D81A)
    (at 156.5275 91.059)
    (fp_text reference P7 (at -13.843 3.429) (layer F.SilkS))
    (fp_text value T-55343GD035JU-LW-ADN (at 0.9 2.7) (layer F.Fab) hide)
    (fp_text user 40 (at 10.5 -0.7) (layer F.SilkS))
    (fp_text user 1 (at -10.3 -0.7) (layer F.SilkS))
    (pad "" connect rect (at 11.6 2.7 180) (size 1.6 2.4) (layers F.Cu F.Mask))
    (pad "" connect rect (at 12.8 3.1 180) (size 0.8 1.6) (layers F.Cu F.Mask))
    (pad "" connect rect (at -12.8 3.1) (size 0.8 1.6) (layers F.Cu F.Mask))
    (pad 1 smd rect (at -9.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 RL))
    (pad 8 smd rect (at -6.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 R6))
    (pad 9 smd rect (at -5.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 R5))
    (pad 7 smd rect (at -6.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 R7))
    (pad 6 smd rect (at -7.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 DISP_ENABLE))
    (pad 2 smd rect (at -9.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 TB))
    (pad 3 smd rect (at -8.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 CLOCK))
    (pad 5 smd rect (at -7.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 HSYNC))
    (pad 4 smd rect (at -8.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 VSYNC))
    (pad 36 smd rect (at 7.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 DISP_RESET))
    (pad 37 smd rect (at 8.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 SPI_SDO))
    (pad 35 smd rect (at 7.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 SPI_CS))
    (pad 34 smd rect (at 6.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 SPI_SCL))
    (pad 38 smd rect (at 8.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 39 smd rect (at 9.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 VCC))
    (pad 40 smd rect (at 9.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 VCC))
    (pad 32 smd rect (at 5.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 B0))
    (pad 33 smd rect (at 6.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 SPI_SDI))
    (pad 31 smd rect (at 5.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 B1))
    (pad 30 smd rect (at 4.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 B2))
    (pad 26 smd rect (at 2.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 B6))
    (pad 27 smd rect (at 3.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 B5))
    (pad 29 smd rect (at 4.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 B3))
    (pad 28 smd rect (at 3.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 B4))
    (pad 12 smd rect (at -4.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 R2))
    (pad 13 smd rect (at -3.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 R1))
    (pad 11 smd rect (at -4.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 R3))
    (pad 10 smd rect (at -5.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 R4))
    (pad 14 smd rect (at -3.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 R0))
    (pad 15 smd rect (at -2.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 17 smd rect (at -1.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 G6))
    (pad 16 smd rect (at -2.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 G7))
    (pad 24 smd rect (at 1.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 25 smd rect (at 2.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 B7))
    (pad 23 smd rect (at 1.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 G0))
    (pad 22 smd rect (at 0.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 G1))
    (pad 18 smd rect (at -1.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 G5))
    (pad 19 smd rect (at -0.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 G4))
    (pad 21 smd rect (at 0.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 G2))
    (pad 20 smd rect (at -0.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 G3))
    (pad "" connect rect (at -11.6 2.7) (size 1.6 2.4) (layers F.Cu F.Mask))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch_SMD (layer F.Cu) (tedit 57F30978)
    (at 177.4825 93.5355)
    (fp_text reference P8 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 connect circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 30 V_LED_CATHODE))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch_SMD (layer F.Cu) (tedit 57F3097A)
    (at 179.451 93.5355)
    (fp_text reference P9 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 connect circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 31 V_LED_ANODE))
  )
  (module mylib:pin_header_6x1_1.27mm_pitch (layer F.Cu) (tedit 57F6253B)
    (at 170.6245 87.4395 90)
    (fp_text reference P6 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text value CONN_6 (at 0 2.54 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 29 BACKL_EN))
    (pad 2 thru_hole circle (at -1.905 0 90) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 39 SPI_SDO))
    (pad 3 thru_hole circle (at -0.635 0 90) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 40 DISP_RESET))
    (pad 4 thru_hole circle (at 0.635 0 90) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 41 SPI_CS))
    (pad 5 thru_hole circle (at 1.905 0 90) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 42 SPI_SCL))
    (pad 6 thru_hole circle (at 3.175 0 90) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 43 SPI_SDI))
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F5D883)
    (at 172.2755 85.852 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R12 (at 0 0.762 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 40 DISP_RESET))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57F5EF29)
    (at 141.9225 92.964 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R13 (at 0 0.8255 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 DISP_ENABLE))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_4x1_1.27mm_pitch (layer F.Cu) (tedit 57F5EA0C)
    (at 141.351 86.1695 270)
    (fp_text reference P5 (at 0 3.81 270) (layer F.SilkS) hide)
    (fp_text value CONN_4 (at 0 1.905 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.905 0 270) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 34 DISP_ENABLE))
    (pad 2 thru_hole circle (at -0.635 0 270) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 27 HSYNC))
    (pad 3 thru_hole circle (at 0.635 0 270) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 26 VSYNC))
    (pad 4 thru_hole circle (at 1.905 0 270) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 28 CLOCK))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch_SMD (layer F.Cu) (tedit 57F5EEC2)
    (at 142.621 90.2335)
    (fp_text reference P10 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 connect circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 38 RL))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch_SMD (layer F.Cu) (tedit 57F5EEC0)
    (at 141.351 90.2335)
    (fp_text reference P11 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 connect circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 37 TB))
  )
  (module mylib:sot23_mod0 (layer F.Cu) (tedit 57F6252E)
    (at 174.498 92.6465)
    (descr SOT23)
    (fp_text reference Q1 (at 0 1.8415 180) (layer F.SilkS))
    (fp_text value NPN (at 0 0.3302) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C5-Pad2)"))
    (pad 3 smd rect (at 0 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 31 V_LED_ANODE))
    (pad 1 smd rect (at 0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 30 V_LED_CATHODE))
    (model walter/smd_trans/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RL (at 142.3035 89.2175) (layer F.SilkS))
  (gr_text TB (at 140.9065 89.2175) (layer F.SilkS))
  (gr_text "- LED +" (at 180.086 94.361) (layer F.SilkS))
  (gr_text BL_EN (at 169.9895 90.6145) (layer F.SilkS))
  (gr_text SPI_SDO (at 169.9895 89.408) (layer F.SilkS))
  (gr_text DISP_RESET (at 169.9895 88.0745) (layer F.SilkS))
  (gr_text SPI_CS (at 169.926 86.8045) (layer F.SilkS))
  (gr_text SPI_SCL (at 169.926 85.5345) (layer F.SilkS))
  (gr_text SPI_SDI (at 169.926 84.328) (layer F.SilkS))
  (gr_line (start 181.991 79.502) (end 181.991 95.5675) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.462 79.502) (end 140.462 95.5675) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.462 79.502) (end 181.991 79.502) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.991 95.5675) (end 140.462 95.5675) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 0 (at 150.368 82.55) (layer F.SilkS))
  (gr_text 0 (at 160.274 81.534) (layer F.SilkS))
  (gr_text 0 (at 170.6245 82.55) (layer F.SilkS))
  (gr_text BLUE (at 165.735 83.566) (layer F.SilkS))
  (gr_text GREEN (at 159.258 83.566) (layer F.SilkS))
  (gr_text RED (at 149.0345 83.566) (layer F.SilkS))
  (gr_text "CLOCK\n" (at 142.113 88.0745) (layer F.SilkS))
  (gr_text DISP_EN (at 142.113 84.2645) (layer F.SilkS))
  (gr_text HSYNC (at 142.113 85.5345) (layer F.SilkS))
  (gr_text VSYNC (at 142.1765 86.868) (layer F.SilkS))
  (gr_text "kyobreak\nrev0.01\nrel/2016" (at 159.1945 87.0585) (layer F.SilkS))
  (gr_text GND (at 175.8315 80.3275) (layer F.SilkS))
  (gr_text VCC3V3 (at 181.356 80.3275) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.7525 93.7895) (xy 177.546 93.7895) (xy 176.4665 92.71) (xy 176.4665 92.075) (xy 178.7525 92.075)
      )
    )
  )
  (zone (net 25) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.991 95.5675) (xy 140.462 95.5675) (xy 140.462 79.502) (xy 181.991 79.502)
      )
    )
  )
  (zone (net 25) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.991 95.5675) (xy 140.462 95.5675) (xy 140.462 79.502) (xy 181.991 79.502)
      )
    )
  )
)
