<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.1" x2="0" y2="9.4" width="0.1524" layer="20"/>
<wire x1="0" y1="9.4" x2="50.5" y2="9.4" width="0.1524" layer="20"/>
<wire x1="50.5" y1="9.4" x2="50.5" y2="0" width="0.1524" layer="20"/>
<wire x1="50.5" y1="0" x2="0.1" y2="0" width="0.1524" layer="20"/>
<wire x1="0.1" y1="0" x2="0.1" y2="0.4" width="0.1524" layer="20"/>
<text>Pos</text>
<text>D in</text>
<text>Neg</text>
<text>D out</text>
</plain>
<libraries>
<library name="mylibrary">
<packages>
<package name="NEOPIXEL1515">
<description>Adafruit Neopixel 1515</description>
</package>
<package name="PAD-1X1">
<description>PAD - 1 X 2 MM</description>
</package>
</packages>
</library>
<library name="smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Packages&lt;/b&gt;&lt;p&gt;
This is a package-only library, based on the Surface Mount Design and Land Pattern Standard developed by the 
Institute for Interconnecting and Packaging electronic Circuits (IPC).&lt;p&gt;
Source:&lt;p&gt;
IPC-SM-782&lt;br&gt;
Revision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="R0603">
<description>&lt;b&gt;Chip RESISTOR, 0603 EIA (1608 Metric)&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="mylibrary" package="NEOPIXEL1515" value=""/>
<element name="E$2" library="mylibrary" package="NEOPIXEL1515" value=""/>
<element name="E$3" library="mylibrary" package="NEOPIXEL1515" value=""/>
<element name="E$4" library="mylibrary" package="NEOPIXEL1515" value=""/>
<element name="E$5" library="mylibrary" package="NEOPIXEL1515" value=""/>
<element name="E$6" library="mylibrary" package="NEOPIXEL1515" value=""/>
<element name="E$7" library="mylibrary" package="NEOPIXEL1515" value=""/>
<element name="E$8" library="mylibrary" package="PAD-1X1" value=""/>
<element name="E$9" library="mylibrary" package="PAD-1X1" value=""/>
<element name="E$10" library="mylibrary" package="PAD-1X1" value=""/>
<element name="E$11" library="mylibrary" package="PAD-1X1" value=""/>
<element name="E$12" library="smd-ipc" package="R0603" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="E$8" pad="P$1"/>
<contactref element="E$2" pad="2"/>
<contactref element="E$3" pad="2"/>
<contactref element="E$4" pad="2"/>
<contactref element="E$5" pad="2"/>
<contactref element="E$6" pad="2"/>
<contactref element="E$7" pad="2"/>
<contactref element="E$1" pad="2"/>
</signal>
<signal name="S$2">
<contactref element="E$2" pad="1"/>
<contactref element="E$1" pad="3"/>
</signal>
<signal name="S$3">
<contactref element="E$3" pad="1"/>
<contactref element="E$2" pad="3"/>
</signal>
<signal name="S$4">
<contactref element="E$4" pad="1"/>
<contactref element="E$3" pad="3"/>
</signal>
<signal name="S$5">
<contactref element="E$5" pad="1"/>
<contactref element="E$4" pad="3"/>
</signal>
<signal name="S$6">
<contactref element="E$6" pad="1"/>
<contactref element="E$5" pad="3"/>
</signal>
<signal name="S$7">
<contactref element="E$7" pad="1"/>
<contactref element="E$6" pad="3"/>
</signal>
<signal name="S$8">
<contactref element="E$11" pad="P$1"/>
<contactref element="E$7" pad="3"/>
</signal>
<signal name="S$9">
<contactref element="E$1" pad="4"/>
<contactref element="E$10" pad="P$1"/>
<contactref element="E$2" pad="4"/>
<contactref element="E$3" pad="4"/>
<contactref element="E$4" pad="4"/>
<contactref element="E$5" pad="4"/>
<contactref element="E$6" pad="4"/>
<contactref element="E$7" pad="4"/>
</signal>
<signal name="S$11">
<contactref element="E$9" pad="P$1"/>
<contactref element="E$12" pad="1"/>
</signal>
<signal name="S$10">
<contactref element="E$1" pad="1"/>
<contactref element="E$12" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
