<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="124.46" y2="0" width="0.127" layer="20"/>
<wire x1="0" y1="63.5" x2="0" y2="2.54" width="0.127" layer="20"/>
<wire x1="124.46" y1="66.04" x2="127" y2="63.5" width="0.127" layer="20" curve="-82.874984"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0.127" layer="20" curve="-82.874984"/>
<wire x1="127" y1="2.54" x2="124.46" y2="0" width="0.127" layer="20" curve="-82.874984"/>
<wire x1="0" y1="63.5" x2="2.54" y2="66.04" width="0.127" layer="20" curve="-82.874984"/>
<wire x1="127" y1="63.5" x2="127" y2="2.54" width="0.127" layer="20"/>
<wire x1="2.54" y1="66.04" x2="124.46" y2="66.04" width="0.127" layer="20"/>
<text>This is an OSHW project brought to you by
Bifrost Development Group (BDG).

Board dimensions are in mm
unless otherwise indicated.
Board thickness is 1.6mm.
The solder mask color is purple.</text>
<hole x="3.81" y="31.115" drill="3.2512"/>
</plain>
<libraries>
<library name="BeagleBone_Blue_R3">
<description>Generated from &lt;b&gt;BeagleBone_Blue.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="GHI_FIDUCIAL_40MIL">
</package>
</packages>
</library>
<library name="bdg">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="BDG_FRAME_ATTRIBUTES">
</package>
<package name="OSHW_FILLX200_NOTEXT">
</package>
<package name="BDG_FRAME">
</package>
<package name="RESC3216X71N">
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
</packages>
</library>
<library name="halcyonmod_Connectors">
<packages>
<package name="2X05_EUROPWR_SHROUD">
<description>2x05 Shrouded Eurorack Power Header</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="halcyonmod_DiscreteSemi">
<description>NPN Transistor</description>
<packages>
<package name="L0603">
</package>
</packages>
</library>
<library name="halcyonmod_Passives">
<packages>
<package name="ELECTRO-SMD-C-COMBO">
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DBZ_R-PDSO-G3">
<description>&lt;b&gt;DBZ (R-PDSO-G3)&lt;/b&gt; SOT-23&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slcs146e/slcs146e.pdf</description>
</package>
</packages>
</library>
<library name="bdg ADP2370ACPZ-3.3-R7">
<description>&lt;ANALOG DEVICES - ADP2370ACPZ-3.3-R7 - DC/DC CONV, BUCK, 1.2MHZ, LFCSP-8&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SON50P300X300X80-9N">
<description>&lt;b&gt;CP-8-5 (LFCSP_WD)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="bdg GRM32ER7YA106KA12K">
<description>&lt;Multilayer Ceramic Capacitors MLCC - SMD/SMT&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="CAPC3225X270N">
<description>&lt;b&gt;GRM32 L=3.2mm W=2.5mm T=2.5mm&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="bdg XAL4040-103MEC">
<description>&lt;Fixed Inductors 10uH Shld 20% 3.1A 92.4mOhms AECQ2&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="XAL4040103MEC">
<description>&lt;b&gt;XAL4040-103MEC-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="bdg LD1117DT33TR">
<description>&lt;LDO Regulator 3.3V 1.3A DPAK STMicroelectronics LD1117DT33TR, LDO Voltage Regulator, 1.3A, 3.3 V +/-1%, 3-Pin DPAK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="TO228P972X240-3N">
<description>&lt;b&gt;DPAK (TO-252)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="dialog slg46620g">
<packages>
<package name="SOP65P640X120-20N">
</package>
</packages>
</library>
<library name="maxim 6959">
<description>&lt;LED Display Drivers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOP64P602X175-16N">
<description>&lt;b&gt;16 QSOP&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="switch-alps">
<description>ALPS Switch from Markus Faust &amp;lt;mfaust@htwm.de&amp;gt;&lt;p&gt;
Source: EC12E.scr from eagle.support.ger on news.cadsoft.de at 08.10.2007</description>
<packages>
<package name="ALPS_EC12E_SW">
<description>ALPS rotary encoder&lt;br&gt;
EC12E series with push-on switch</description>
</package>
</packages>
</library>
<library name="bdg_ldd_f302nd_2dig_led">
<description>&lt;LED Displays &amp; Accessories LED Display&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="DIP1016W45P254L1550H720Q10N">
<description>&lt;b&gt;LDD-F302NI&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="adafruit-2">
<packages>
<package name="SOD-123">
</package>
</packages>
</library>
<library name="eurorack1">
<packages>
<package name="WQP-PJ301BM">
</package>
</packages>
</library>
<library name="bdg2">
<packages>
<package name="SOT50P170X60-6N">
<description>&lt;b&gt;SOT50P170X60-6N&lt;/b&gt;&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="halcyonmod_AnalogIC">
<packages>
<package name="TSSOP-14">
</package>
</packages>
</library>
<library name="bdg DAC8164IAPW">
<description>&lt;14-Bit, Quad Channel, Ultra-Low Glitch, Voltage Output DAC with 2.5V, 2ppm/C Internal Reference&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOP65P640X120-16N">
<description>&lt;b&gt;PW&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="sparkfun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="bdg_rpi_rp2040">
<description>&lt;ARM Cortex-M0+ - Microcontroller IC 32-Bit Dual-Core 133MHz External Program Memory 56-QFN (7x7)&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SC091413">
<description>&lt;b&gt; QFN-56 77mm&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Memory">
<description>&lt;h3&gt;SparkFun Memory ICs&lt;/h3&gt;
This library contains memory ICs.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOIC-8">
<description>8-Pin SOIC 208-mil</description>
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="bdg_xtal_abracon_12mhz">
<description>&lt;ABRACON - ABLS-12.000MHZ-B4-T - CRYSTAL, 12MHZ, 18PF, HC-49US&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="ABLS">
<description>&lt;b&gt;ABLS&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="wurth">
<packages>
<package name="WE-TVS_SOT23-5L">
<description>TVS Diode Array WE-TVS</description>
</package>
</packages>
</library>
<library name="edison">
<description>Generated from &lt;b&gt;9dof_block.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="bdg molex usbb105164-0001">
<description>&lt;USB - micro B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle; Through Hole&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="1051640001">
<description>&lt;b&gt;105164-0001-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="drilegend">
<packages>
<package name="DRILEGEND">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="CDR" value="1"/>
<attribute name="CPROJECT" value="P01-136"/>
<attribute name="CTITLE" value="Mjölnir"/>
<attribute name="EPOCH" value="2334"/>
<attribute name="INITS" value="jrs"/>
<attribute name="RV" value="F"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FUD1" library="BeagleBone_Blue_R3" package="GHI_FIDUCIAL_40MIL" value="FIDUCIAL"/>
<element name="FUD2" library="BeagleBone_Blue_R3" package="GHI_FIDUCIAL_40MIL" value="FIDUCIAL"/>
<element name="FUD3" library="BeagleBone_Blue_R3" package="GHI_FIDUCIAL_40MIL" value="FIDUCIAL"/>
<element name="FUD4" library="BeagleBone_Blue_R3" package="GHI_FIDUCIAL_40MIL" value="FIDUCIAL"/>
<element name="J1" library="halcyonmod_Connectors" package="2X05_EUROPWR_SHROUD" value="EUROPWR_2X05-SHROUD">
<attribute name="NAME"/>
</element>
<element name="D2" library="diode" package="SOD123" value="MBR0530LT">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
</element>
<element name="D1" library="diode" package="SOD123" value="MBR0530LT">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
</element>
<element name="R1" library="halcyonmod_DiscreteSemi" package="L0603" value="FERRITE BEAD 600">
<attribute name="DESC" value="600R / 100MHz"/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value=" BLM18AG601SN1D"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="81-BLM11A601S"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Ferrite"/>
</element>
<element name="R2" library="halcyonmod_DiscreteSemi" package="L0603" value="FERRITE BEAD 600">
<attribute name="DESC" value="600R / 100MHz"/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MPN" value=" BLM18AG601SN1D"/>
<attribute name="NAME"/>
<attribute name="OC_MOUSER" value="81-BLM11A601S"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value="Ferrite"/>
</element>
<element name="C1" library="halcyonmod_Passives" package="ELECTRO-SMD-C-COMBO" value="22u">
<attribute name="NAME"/>
</element>
<element name="C2" library="halcyonmod_Passives" package="ELECTRO-SMD-C-COMBO" value="22u">
<attribute name="NAME"/>
</element>
<element name="R3" library="bdg" package="R0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="C3" library="bdg" package="C0603" value="470n">
<attribute name="NAME"/>
</element>
<element name="U1" library="texas" package="DBZ_R-PDSO-G3" value="LM4041D10DBZ">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041D12QDBZT"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1755118"/>
<attribute name="OC_NEWARK" value="43K3381"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="U2" library="bdg ADP2370ACPZ-3.3-R7" package="SON50P300X300X80-9N" value="ADP2370ACPZ-5.0-R7">
<attribute name="DESCRIPTION" value="ANALOG DEVICES - ADP2370ACPZ-3.3-R7 - DC/DC CONV, BUCK, 1.2MHZ, LFCSP-8"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Analog Devices"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ADP2370ACPZ-3.3-R7"/>
<attribute name="MOUSER_PART_NUMBER" value="584-ADP2370ACPZ3.3R7"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Analog-Devices/ADP2370ACPZ-33-R7?qs=WIvQP4zGani%2FjYb35ccILQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="bdg GRM32ER7YA106KA12K" package="CAPC3225X270N" value="10u">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM32ER7YA106KA12K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM32ER7YA106KA2K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM32ER7YA106KA12K?qs=hNud%2FORuBR2cWCd9Jqwt3g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="bdg GRM32ER7YA106KA12K" package="CAPC3225X270N" value="10u">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM32ER7YA106KA12K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM32ER7YA106KA2K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM32ER7YA106KA12K?qs=hNud%2FORuBR2cWCd9Jqwt3g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="L1" library="bdg XAL4040-103MEC" package="XAL4040103MEC" value="10uH">
<attribute name="DESCRIPTION" value="Fixed Inductors 10uH Shld 20% 3.1A 92.4mOhms AECQ2"/>
<attribute name="HEIGHT" value="4.1mm"/>
<attribute name="MANUFACTURER_NAME" value="COILCRAFT"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="XAL4040-103MEC"/>
<attribute name="MOUSER_PART_NUMBER" value="994-XAL4040-103MEC"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Coilcraft/XAL4040-103MEC?qs=zCSbvcPd3pYcdvH9kvmQzg%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C7" library="bdg GRM32ER7YA106KA12K" package="CAPC3225X270N" value="10u">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM32ER7YA106KA12K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM32ER7YA106KA2K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM32ER7YA106KA12K?qs=hNud%2FORuBR2cWCd9Jqwt3g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="bdg LD1117DT33TR" package="TO228P972X240-3N" value="LD1117DT33TR">
<attribute name="DESCRIPTION" value="LDO Regulator 3.3V 1.3A DPAK STMicroelectronics LD1117DT33TR, LDO Voltage Regulator, 1.3A, 3.3 V +/-1%, 3-Pin DPAK"/>
<attribute name="HEIGHT" value="2.4mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LD1117DT33TR"/>
<attribute name="MOUSER_PART_NUMBER" value="511-LD1117DT33-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/LD1117DT33TR?qs=4JhUBQGAOSd4P5jVYGxp2g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U4" library="dialog slg46620g" package="SOP65P640X120-20N" value="SLG46620G">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" GreenPAK Programmable Mixed-signal Matrix. 18-GPIO, 6 ACMPs, 3 DCMPs/PWMs, 2 DACs, 26 LUTs (max.), 10 CNT/DLY (max.), 12 DFF/LATCH (max.) and other Macrocells "/>
<attribute name="MF" value="Dialog Semiconductor"/>
<attribute name="MP" value="SLG46620G"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="TSSOP-20 Silego"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SLG46620G/?ref=eda"/>
</element>
<element name="U6" library="maxim 6959" package="SOP64P602X175-16N" value="MAX6959AAEE+">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="LED Display Drivers"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="Maxim Integrated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MAX6959AAEE+"/>
<attribute name="MOUSER_PART_NUMBER" value="700-MAX6959AAEE"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Maxim-Integrated/MAX6959AAEE%2b?qs=p6VZ%252BklCkRSJULIvfQC6xg%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="bdg" package="R0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R6" library="bdg" package="R0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="EN1" library="switch-alps" package="ALPS_EC12E_SW" value="EC12E_SW">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EC12E2424407"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1520813"/>
<attribute name="OC_NEWARK" value="74M1068"/>
<attribute name="POPULARITY" value="3"/>
</element>
<element name="LED1" library="bdg" package="CHIP-LED0603" value="STEP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="bdg" package="CHIP-LED0603" value="DIR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="bdg_ldd_f302nd_2dig_led" package="DIP1016W45P254L1550H720Q10N" value="LDD-F302ND">
<attribute name="DESCRIPTION" value="LED Displays &amp; Accessories LED Display"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Lumex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LDD-F302ND"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="NAME"/>
</element>
<element name="LED4" library="bdg_ldd_f302nd_2dig_led" package="DIP1016W45P254L1550H720Q10N" value="LDD-F302ND">
<attribute name="DESCRIPTION" value="LED Displays &amp; Accessories LED Display"/>
<attribute name="HEIGHT" value="7.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Lumex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LDD-F302ND"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="NAME"/>
</element>
<element name="S1" library="bdg" package="TACTILE-PTH" value="F">
<attribute name="NAME"/>
</element>
<element name="S2" library="bdg" package="TACTILE-PTH" value="E">
<attribute name="NAME"/>
</element>
<element name="S3" library="bdg" package="TACTILE-PTH" value="T">
<attribute name="NAME"/>
</element>
<element name="D3" library="adafruit-2" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D4" library="adafruit-2" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D5" library="adafruit-2" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="R7" library="bdg" package="R0603" value="39K">
<attribute name="NAME"/>
</element>
<element name="C9" library="bdg GRM32ER7YA106KA12K" package="CAPC3225X270N" value="10u">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM32ER7YA106KA12K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM32ER7YA106KA2K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM32ER7YA106KA12K?qs=hNud%2FORuBR2cWCd9Jqwt3g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U7" library="bdg LD1117DT33TR" package="TO228P972X240-3N" value="LD1117DT33TR">
<attribute name="DESCRIPTION" value="LDO Regulator 3.3V 1.3A DPAK STMicroelectronics LD1117DT33TR, LDO Voltage Regulator, 1.3A, 3.3 V +/-1%, 3-Pin DPAK"/>
<attribute name="HEIGHT" value="2.4mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LD1117DT33TR"/>
<attribute name="MOUSER_PART_NUMBER" value="511-LD1117DT33-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/LD1117DT33TR?qs=4JhUBQGAOSd4P5jVYGxp2g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J3" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J4" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J5" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J6" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J7" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J8" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J9" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J12" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="J13" library="eurorack1" package="WQP-PJ301BM" value="WQP-PJ301BM">
<attribute name="NAME"/>
</element>
<element name="R8" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="D6" library="adafruit-2" package="SOD-123" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="Q1" library="bdg2" package="SOT50P170X60-6N" value="2N3906_DUAL">
<attribute name="NAME"/>
</element>
<element name="R9" library="bdg" package="R0603" value="1.5K">
<attribute name="NAME"/>
</element>
<element name="R10" library="bdg" package="R0603" value="100">
<attribute name="NAME"/>
</element>
<element name="R11" library="bdg" package="R0603" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R12" library="bdg" package="R0603" value="3.3K">
<attribute name="NAME"/>
</element>
<element name="R13" library="bdg" package="R0603" value="10K">
<attribute name="NAME"/>
</element>
<element name="C11" library="bdg" package="C0603" value="1n (ESD)">
<attribute name="NAME"/>
</element>
<element name="R14" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R15" library="bdg" package="R0603" value="200K">
<attribute name="NAME"/>
</element>
<element name="R16" library="bdg" package="R0603" value="33K">
<attribute name="NAME"/>
</element>
<element name="C13" library="bdg" package="C0603" value="1n (ESD)">
<attribute name="NAME"/>
</element>
<element name="R17" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R18" library="bdg" package="R0603" value="200K">
<attribute name="NAME"/>
</element>
<element name="R19" library="bdg" package="R0603" value="33K">
<attribute name="NAME"/>
</element>
<element name="C14" library="bdg" package="C0603" value="4.7n">
<attribute name="NAME"/>
</element>
<element name="C15" library="bdg" package="C0603" value="1n (ESD)">
<attribute name="NAME"/>
</element>
<element name="R20" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R21" library="bdg" package="R0603" value="200K">
<attribute name="NAME"/>
</element>
<element name="R22" library="bdg" package="R0603" value="33K">
<attribute name="NAME"/>
</element>
<element name="C16" library="bdg" package="C0603" value="4.7n">
<attribute name="NAME"/>
</element>
<element name="U10" library="bdg DAC8164IAPW" package="SOP65P640X120-16N" value="DAC8164IAPW">
<attribute name="DESCRIPTION" value="14-Bit, Quad Channel, Ultra-Low Glitch, Voltage Output DAC with 2.5V, 2ppm/C Internal Reference"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DAC8164IAPW"/>
<attribute name="MOUSER_PART_NUMBER" value="595-DAC8164IAPW"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/DAC8164IAPW?qs=H5cOD6AgtONDgX3QW2xdOA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C17" library="bdg" package="C0603" value="470n">
<attribute name="NAME"/>
</element>
<element name="C18" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="LED5" library="sparkfun" package="LED3MM" value="F_OUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="sparkfun" package="LED3MM" value="E_OUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="bdg" package="C0603" value="1n (ESD)">
<attribute name="NAME"/>
</element>
<element name="R23" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R24" library="bdg" package="R0603" value="200K">
<attribute name="NAME"/>
</element>
<element name="R25" library="bdg" package="R0603" value="33K">
<attribute name="NAME"/>
</element>
<element name="C21" library="bdg" package="C0603" value="4.7n">
<attribute name="NAME"/>
</element>
<element name="C22" library="bdg" package="C0603" value="1n (ESD)">
<attribute name="NAME"/>
</element>
<element name="R26" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R27" library="bdg" package="R0603" value="200K">
<attribute name="NAME"/>
</element>
<element name="R28" library="bdg" package="R0603" value="33K">
<attribute name="NAME"/>
</element>
<element name="C23" library="bdg" package="C0603" value="4.7n">
<attribute name="NAME"/>
</element>
<element name="C24" library="bdg" package="C0603" value="1n (ESD)">
<attribute name="NAME"/>
</element>
<element name="R29" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R30" library="bdg" package="R0603" value="200K">
<attribute name="NAME"/>
</element>
<element name="R31" library="bdg" package="R0603" value="33K">
<attribute name="NAME"/>
</element>
<element name="C25" library="bdg" package="C0603" value="4.7n">
<attribute name="NAME"/>
</element>
<element name="U8" library="halcyonmod_AnalogIC" package="TSSOP-14" value="MCP6004T-I/STCT">
<attribute name="NAME"/>
</element>
<element name="C26" library="bdg" package="C0603" value="1n (ESD)">
<attribute name="NAME"/>
</element>
<element name="R32" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R33" library="bdg" package="R0603" value="200K">
<attribute name="NAME"/>
</element>
<element name="R34" library="bdg" package="R0603" value="33K">
<attribute name="NAME"/>
</element>
<element name="C27" library="bdg" package="C0603" value="4.7n">
<attribute name="NAME"/>
</element>
<element name="U9" library="halcyonmod_AnalogIC" package="TSSOP-14" value="MCP6004T-I/STCT">
<attribute name="NAME"/>
</element>
<element name="R35" library="bdg" package="R0603" value="150k">
<attribute name="NAME"/>
</element>
<element name="R36" library="bdg" package="R0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="C28" library="bdg" package="C0603" value="470n">
<attribute name="NAME"/>
</element>
<element name="R37" library="bdg" package="R0603" value="23.7K">
<attribute name="NAME"/>
</element>
<element name="R38" library="bdg" package="R0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R39" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="C29" library="bdg" package="C0603" value="470n">
<attribute name="NAME"/>
</element>
<element name="R40" library="bdg" package="R0603" value="680">
<attribute name="NAME"/>
</element>
<element name="R41" library="bdg" package="R0603" value="23.7K">
<attribute name="NAME"/>
</element>
<element name="C30" library="bdg" package="C0603" value="470n">
<attribute name="NAME"/>
</element>
<element name="R42" library="bdg" package="R0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R43" library="bdg" package="R0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="R44" library="bdg" package="R0603" value="680">
<attribute name="NAME"/>
</element>
<element name="C31" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C32" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C33" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C34" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C35" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C36" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C37" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C38" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C39" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C12" library="bdg" package="C0603" value="4.7n">
<attribute name="NAME"/>
</element>
<element name="C19" library="bdg" package="C0603" value="22u">
<attribute name="NAME"/>
</element>
<element name="U$1" library="bdg" package="BDG_FRAME_ATTRIBUTES" value="FRAME_BDG_B_ATTRIBUTES">
<attribute name="CDR" value="1"/>
<attribute name="CPROJECT" value="P01-136"/>
<attribute name="CPROJECT" value="P01-136"/>
<attribute name="CTITLE" value="Mjölnir"/>
<attribute name="CTITLE" value="Mjölnir"/>
<attribute name="DRAWING_NAME"/>
<attribute name="EPOCH" value="2334"/>
<attribute name="EPOCH" value="2334"/>
<attribute name="INITS" value="jrs"/>
<attribute name="INITS" value="jrs"/>
<attribute name="LAST_DATE_TIME"/>
<attribute name="RV" value="F"/>
<attribute name="RV" value="F"/>
</element>
<element name="LOGO1" library="bdg" package="OSHW_FILLX200_NOTEXT" value="OSHW_LOGO_FILLX0200-NT"/>
<element name="U13" library="bdg_rpi_rp2040" package="SC091413" value="RP2040">
<attribute name="DESCRIPTION" value="ARM Cortex-M0+ - Microcontroller IC 32-Bit Dual-Core 133MHz External Program Memory 56-QFN (7x7)"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="RASPBERRY-PI"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SC0914(13)"/>
<attribute name="MOUSER_PART_NUMBER" value="358-SC091413"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Raspberry-Pi/SC091413?qs=T%252BzbugeAwjhr%252BUbBr3TJcw%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="U14" library="SparkFun-IC-Memory" package="SOIC-8" value="W25Q32FV">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-13229"/>
</element>
<element name="C40" library="bdg" package="C0603" value="27p">
<attribute name="NAME"/>
</element>
<element name="C41" library="bdg" package="C0603" value="27p">
<attribute name="NAME"/>
</element>
<element name="R45" library="bdg" package="R0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="R50" library="bdg" package="R0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="U$2" library="bdg" package="BDG_FRAME" value="FRAME_BDG_B_PUB">
<attribute name="CDR" value="1"/>
<attribute name="CPROJECT" value="P01-136"/>
<attribute name="CTITLE" value="Mjölnir"/>
<attribute name="EPOCH" value="2334"/>
<attribute name="INITS" value="jrs"/>
<attribute name="RV" value="F"/>
</element>
<element name="U$3" library="bdg" package="BDG_FRAME" value="FRAME_BDG_B_PUB">
<attribute name="CPROJECT" value="P01-136"/>
<attribute name="CTITLE" value="Mjölnir"/>
<attribute name="EPOCH" value="2334"/>
<attribute name="RV" value="F"/>
</element>
<element name="R4" library="bdg" package="RESC3216X71N" value="0 Ohm">
<attribute name="MPN" value="MC0.125W12061%100K"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9335773"/>
<attribute name="OC_NEWARK" value="39K0873"/>
<attribute name="SUPPLIER" value="Multicomp"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="1/8 W"/>
</element>
<element name="R46" library="bdg" package="R0603" value="27">
<attribute name="NAME"/>
</element>
<element name="R47" library="bdg" package="R0603" value="27">
<attribute name="NAME"/>
</element>
<element name="U5" library="74xx-eu" package="SO16" value="74HC4053PWR">
<attribute name="NAME"/>
</element>
<element name="R51" library="bdg" package="R0603" value="10K">
<attribute name="NAME"/>
</element>
<element name="R52" library="bdg" package="R0603" value="1K">
<attribute name="NAME"/>
</element>
<element name="C8" library="bdg GRM32ER7YA106KA12K" package="CAPC3225X270N" value="10u">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM32ER7YA106KA12K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM32ER7YA106KA2K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM32ER7YA106KA12K?qs=hNud%2FORuBR2cWCd9Jqwt3g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C10" library="bdg GRM32ER7YA106KA12K" package="CAPC3225X270N" value="10u">
<attribute name="DESCRIPTION" value="Multilayer Ceramic Capacitors MLCC - SMD/SMT"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM32ER7YA106KA12K"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM32ER7YA106KA2K"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM32ER7YA106KA12K?qs=hNud%2FORuBR2cWCd9Jqwt3g%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="C42" library="bdg" package="C0603" value="1u">
<attribute name="NAME"/>
</element>
<element name="C43" library="bdg" package="C0603" value="1u">
<attribute name="NAME"/>
</element>
<element name="C44" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C45" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C46" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C47" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C48" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C49" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="C50" library="bdg" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="Y1" library="bdg_xtal_abracon_12mhz" package="ABLS" value="ABLS-12.000MHZ-B4-T">
<attribute name="DESCRIPTION" value="ABRACON - ABLS-12.000MHZ-B4-T - CRYSTAL, 12MHZ, 18PF, HC-49US"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="ABRACON"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ABLS-12.000MHZ-B4-T"/>
<attribute name="MOUSER_PART_NUMBER" value="815-ABLS-12.0M-T"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/ABRACON/ABLS-12.000MHZ-B4-T?qs=yTU0IcKoRlGSQ8ooxPPVnQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="S4" library="bdg" package="TACTILE_SWITCH_SMD" value="RESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S5" library="bdg" package="TACTILE_SWITCH_SMD" value="USBBT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="wurth" package="WE-TVS_SOT23-5L" value="WURTH 824011">
<attribute name="MPN" value="824011"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1748616"/>
<attribute name="OC_NEWARK" value="34R6120"/>
<attribute name="PACKAGE" value="SOT23-5L"/>
<attribute name="SUPPLIER" value="Wuerth Elektronik"/>
</element>
<element name="D8" library="edison" package="SOD-323" value="PMEG4005EJ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-10955"/>
</element>
<element name="U11" library="linear" package="SO08" value="TL082D">
<attribute name="DATA_SHEET" value="&lt;a href=&quot;http://www.ti.com/lit/ds/symlink/tl084a.pdf&quot;&gt; Data sheet &lt;/a&gt;"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
</element>
<element name="U12" library="linear" package="SO08" value="TL072D">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="J10" library="bdg molex usbb105164-0001" package="1051640001" value="105164-0001">
<attribute name="DESCRIPTION" value="USB - micro B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle; Through Hole"/>
<attribute name="HEIGHT" value="2.7mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="105164-0001"/>
<attribute name="MOUSER_PART_NUMBER" value="538-105164-0001"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/105164-0001?qs=JAwGc6FMfvtRY4SkW%2FoGcQ%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="DRILEGEND" library="drilegend" package="DRILEGEND" value=""/>
<element name="C51" library="bdg" package="C0603" value="1n (ESD)">
<attribute name="NAME"/>
</element>
<element name="R48" library="bdg" package="R0603" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="R49" library="bdg" package="R0603" value="2.2K">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U4" pad="11"/>
<contactref element="U6" pad="8"/>
<contactref element="EN1" pad="E"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="EN1" pad="C"/>
<contactref element="EN1" pad="D"/>
<contactref element="J2" pad="SW"/>
<contactref element="J2" pad="SL1"/>
<contactref element="J2" pad="SL2"/>
<contactref element="R9" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="J3" pad="SW"/>
<contactref element="J3" pad="SL2"/>
<contactref element="J3" pad="SL1"/>
<contactref element="C11" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="J4" pad="SL2"/>
<contactref element="J4" pad="SL1"/>
<contactref element="J4" pad="SW"/>
<contactref element="C15" pad="2"/>
<contactref element="J5" pad="SL2"/>
<contactref element="J5" pad="SL1"/>
<contactref element="J5" pad="SW"/>
<contactref element="U10" pad="15"/>
<contactref element="U10" pad="16"/>
<contactref element="U10" pad="14"/>
<contactref element="U10" pad="13"/>
<contactref element="U10" pad="6"/>
<contactref element="U10" pad="5"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="J6" pad="SL2"/>
<contactref element="J6" pad="SL1"/>
<contactref element="J6" pad="SW"/>
<contactref element="C22" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="U8" pad="3"/>
<contactref element="U8" pad="5"/>
<contactref element="U8" pad="10"/>
<contactref element="C26" pad="2"/>
<contactref element="U9" pad="3"/>
<contactref element="U9" pad="5"/>
<contactref element="U9" pad="10"/>
<contactref element="U9" pad="12"/>
<contactref element="J7" pad="SL2"/>
<contactref element="J7" pad="SL1"/>
<contactref element="J7" pad="SW"/>
<contactref element="J8" pad="SL2"/>
<contactref element="J8" pad="SL1"/>
<contactref element="J8" pad="SW"/>
<contactref element="J9" pad="SL2"/>
<contactref element="J9" pad="SL1"/>
<contactref element="J9" pad="SW"/>
<contactref element="U9" pad="11"/>
<contactref element="U8" pad="12"/>
<contactref element="R36" pad="1"/>
<contactref element="C28" pad="2"/>
<contactref element="J12" pad="SW"/>
<contactref element="J12" pad="SL1"/>
<contactref element="J12" pad="SL2"/>
<contactref element="R40" pad="2"/>
<contactref element="J13" pad="SW"/>
<contactref element="R44" pad="2"/>
<contactref element="J13" pad="SL1"/>
<contactref element="J13" pad="SL2"/>
<contactref element="C32" pad="2"/>
<contactref element="C31" pad="1"/>
<contactref element="C34" pad="2"/>
<contactref element="C33" pad="1"/>
<contactref element="C35" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="U8" pad="11"/>
<contactref element="U13" pad="57"/>
<contactref element="U14" pad="4"/>
<contactref element="C40" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U13" pad="19"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="8"/>
<contactref element="C45" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="S5" pad="3"/>
<contactref element="S5" pad="4"/>
<contactref element="S4" pad="3"/>
<contactref element="S4" pad="4"/>
<contactref element="J10" pad="5"/>
<contactref element="D7" pad="2"/>
<contactref element="C51" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="9"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="-12V">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="C1" pad="--"/>
<contactref element="R3" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="U11" pad="4"/>
<contactref element="U12" pad="4"/>
</signal>
<signal name="+12V">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="++"/>
<contactref element="C2" pad="+"/>
<contactref element="U2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="C34" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="U11" pad="8"/>
<contactref element="U12" pad="8"/>
</signal>
<signal name="VREF">
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="C9" pad="2"/>
<contactref element="U7" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="9"/>
<contactref element="U2" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="6"/>
<contactref element="C1" pad="++"/>
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="-"/>
<contactref element="C2" pad="--"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="L1" pad="1"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="+5V">
<contactref element="U2" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="U7" pad="3"/>
<contactref element="C9" pad="1"/>
<contactref element="D8" pad="C"/>
</signal>
<signal name="CTLCS">
<contactref element="U4" pad="9"/>
<contactref element="U13" pad="14"/>
</signal>
<signal name="CTLRDY">
<contactref element="U4" pad="3"/>
<contactref element="U13" pad="13"/>
</signal>
<signal name="ENCA">
<contactref element="EN1" pad="B"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="DIGCLK">
<contactref element="U6" pad="2"/>
<contactref element="U13" pad="5"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="DIGDAT">
<contactref element="U6" pad="1"/>
<contactref element="U13" pad="4"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="DIG2">
<contactref element="LED3" pad="1"/>
<contactref element="LED4" pad="10"/>
<contactref element="U6" pad="6"/>
<contactref element="S3" pad="1"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="SEGA">
<contactref element="LED3" pad="3"/>
<contactref element="LED4" pad="3"/>
<contactref element="U6" pad="15"/>
</signal>
<signal name="DIG3">
<contactref element="LED3" pad="4"/>
<contactref element="LED4" pad="5"/>
<contactref element="U6" pad="7"/>
</signal>
<signal name="DIG1">
<contactref element="LED3" pad="5"/>
<contactref element="LED4" pad="4"/>
<contactref element="U6" pad="5"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="DIG0">
<contactref element="LED4" pad="1"/>
<contactref element="LED3" pad="10"/>
<contactref element="U6" pad="4"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="SEGB">
<contactref element="LED4" pad="9"/>
<contactref element="LED3" pad="9"/>
<contactref element="U6" pad="14"/>
</signal>
<signal name="SEGC">
<contactref element="LED4" pad="8"/>
<contactref element="LED3" pad="8"/>
<contactref element="U6" pad="13"/>
</signal>
<signal name="SEGE">
<contactref element="LED4" pad="7"/>
<contactref element="LED3" pad="7"/>
<contactref element="U6" pad="11"/>
</signal>
<signal name="SEGD">
<contactref element="LED4" pad="6"/>
<contactref element="LED3" pad="6"/>
<contactref element="U6" pad="12"/>
</signal>
<signal name="N$8">
<contactref element="D5" pad="C"/>
<contactref element="S3" pad="3"/>
<contactref element="S3" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="D4" pad="C"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="D3" pad="C"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="R7" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="R7" pad="1"/>
<contactref element="U6" pad="9"/>
</signal>
<signal name="+3V3A">
<contactref element="U7" pad="4"/>
<contactref element="U10" pad="4"/>
<contactref element="C18" pad="1"/>
<contactref element="U8" pad="4"/>
<contactref element="U9" pad="4"/>
<contactref element="C38" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R8" pad="1"/>
<contactref element="J2" pad="TP"/>
<contactref element="C51" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Q1" pad="2"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="N$15">
<contactref element="R9" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="Q1" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="R10" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="Q1" pad="5"/>
</signal>
<signal name="ENV_GATE">
<contactref element="R13" pad="1"/>
<contactref element="U13" pad="11"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="J3" pad="TP"/>
<contactref element="C11" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="U8" pad="2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="FILT_IN">
<contactref element="R16" pad="2"/>
<contactref element="U8" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="U13" pad="38"/>
</signal>
<signal name="N$22">
<contactref element="C13" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="J4" pad="TP"/>
</signal>
<signal name="N$23">
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="U8" pad="6"/>
</signal>
<signal name="FILT_CUT">
<contactref element="C14" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="U8" pad="7"/>
<contactref element="U5" pad="12"/>
</signal>
<signal name="N$24">
<contactref element="C15" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="J5" pad="TP"/>
</signal>
<signal name="N$25">
<contactref element="R20" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="C16" pad="2"/>
<contactref element="U8" pad="9"/>
</signal>
<signal name="FILT_RES">
<contactref element="C16" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="U8" pad="8"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="IOCLK">
<contactref element="U10" pad="10"/>
<contactref element="U4" pad="2"/>
<contactref element="U13" pad="29"/>
</signal>
<signal name="DACCS">
<contactref element="U10" pad="9"/>
<contactref element="U13" pad="15"/>
</signal>
<signal name="VREFH">
<contactref element="U10" pad="3"/>
<contactref element="C17" pad="1"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="ENV_OUT">
<contactref element="U10" pad="2"/>
<contactref element="R41" pad="2"/>
</signal>
<signal name="FILT_OUT">
<contactref element="U10" pad="1"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="C20" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="J6" pad="TP"/>
</signal>
<signal name="N$30">
<contactref element="R23" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="U9" pad="2"/>
</signal>
<signal name="ENV_A">
<contactref element="C21" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="U9" pad="1"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="ENV_D">
<contactref element="C23" pad="1"/>
<contactref element="U9" pad="7"/>
<contactref element="R28" pad="2"/>
<contactref element="U5" pad="13"/>
</signal>
<signal name="ENV_S">
<contactref element="C25" pad="1"/>
<contactref element="U9" pad="8"/>
<contactref element="R31" pad="2"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="ENV_R">
<contactref element="C27" pad="1"/>
<contactref element="U9" pad="14"/>
<contactref element="R34" pad="2"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="DACDAT">
<contactref element="U10" pad="11"/>
<contactref element="U13" pad="31"/>
</signal>
<signal name="CTLDAT">
<contactref element="U4" pad="10"/>
<contactref element="U13" pad="30"/>
</signal>
<signal name="N$32">
<contactref element="C22" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="J7" pad="TP"/>
</signal>
<signal name="N$34">
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="C23" pad="2"/>
<contactref element="U9" pad="6"/>
</signal>
<signal name="N$35">
<contactref element="C24" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="J8" pad="TP"/>
</signal>
<signal name="N$36">
<contactref element="R29" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="C25" pad="2"/>
<contactref element="U9" pad="9"/>
</signal>
<signal name="N$38">
<contactref element="C26" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="J9" pad="TP"/>
</signal>
<signal name="N$39">
<contactref element="R32" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="U9" pad="13"/>
</signal>
<signal name="N$40">
<contactref element="U8" pad="14"/>
<contactref element="U8" pad="13"/>
</signal>
<signal name="BIAS">
<contactref element="R35" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="U11" pad="3"/>
<contactref element="U11" pad="5"/>
</signal>
<signal name="N$41">
<contactref element="R37" pad="1"/>
<contactref element="R39" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="U11" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="C29" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="U11" pad="1"/>
<contactref element="U12" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="R39" pad="1"/>
<contactref element="R38" pad="1"/>
<contactref element="J12" pad="TP"/>
</signal>
<signal name="N$44">
<contactref element="R40" pad="1"/>
<contactref element="LED5" pad="K"/>
<contactref element="U12" pad="3"/>
</signal>
<signal name="N$45">
<contactref element="LED5" pad="A"/>
<contactref element="U12" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="C30" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="R43" pad="2"/>
<contactref element="U11" pad="6"/>
</signal>
<signal name="N$48">
<contactref element="C30" pad="2"/>
<contactref element="R42" pad="2"/>
<contactref element="U11" pad="7"/>
<contactref element="U12" pad="6"/>
</signal>
<signal name="N$49">
<contactref element="R43" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="J13" pad="TP"/>
</signal>
<signal name="N$50">
<contactref element="R44" pad="1"/>
<contactref element="LED6" pad="K"/>
<contactref element="U12" pad="5"/>
</signal>
<signal name="N$47">
<contactref element="LED6" pad="A"/>
<contactref element="U12" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="2"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="ENCB">
<contactref element="EN1" pad="A"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="U3" pad="4"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="U6" pad="16"/>
<contactref element="U10" pad="12"/>
<contactref element="C35" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C36" pad="1"/>
<contactref element="R50" pad="1"/>
<contactref element="U14" pad="8"/>
<contactref element="U4" pad="1"/>
<contactref element="U5" pad="16"/>
<contactref element="R51" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C47" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="U13" pad="44"/>
<contactref element="U13" pad="43"/>
<contactref element="U13" pad="48"/>
<contactref element="U13" pad="49"/>
<contactref element="U13" pad="33"/>
<contactref element="U13" pad="22"/>
<contactref element="R49" pad="2"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="SWSC">
<contactref element="U13" pad="39"/>
<contactref element="U5" pad="9"/>
</signal>
<signal name="QSPISS">
<contactref element="U14" pad="1"/>
<contactref element="R50" pad="2"/>
<contactref element="U13" pad="56"/>
<contactref element="R52" pad="2"/>
</signal>
<signal name="QSPISCLK">
<contactref element="U13" pad="52"/>
<contactref element="U14" pad="6"/>
</signal>
<signal name="QSPISD0">
<contactref element="U14" pad="5"/>
<contactref element="U13" pad="53"/>
</signal>
<signal name="QSPISD1">
<contactref element="U13" pad="55"/>
<contactref element="U14" pad="2"/>
</signal>
<signal name="QSPISD2">
<contactref element="U13" pad="54"/>
<contactref element="U14" pad="3"/>
</signal>
<signal name="QSPISD3">
<contactref element="U14" pad="7"/>
<contactref element="U13" pad="51"/>
</signal>
<signal name="XOUT">
<contactref element="U13" pad="21"/>
<contactref element="R45" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="R45" pad="1"/>
<contactref element="C40" pad="2"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="XIN">
<contactref element="U13" pad="20"/>
<contactref element="C41" pad="2"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="USB_DP">
<contactref element="R46" pad="2"/>
<contactref element="J10" pad="2"/>
<contactref element="D7" pad="4"/>
</signal>
<signal name="USB_P">
<contactref element="R46" pad="1"/>
<contactref element="U13" pad="47"/>
</signal>
<signal name="USB_N">
<contactref element="R47" pad="1"/>
<contactref element="U13" pad="46"/>
</signal>
<signal name="SWSA">
<contactref element="U5" pad="11"/>
<contactref element="U13" pad="41"/>
</signal>
<signal name="SWSB">
<contactref element="U5" pad="10"/>
<contactref element="U13" pad="40"/>
</signal>
<signal name="MXSEL">
<contactref element="U13" pad="37"/>
<contactref element="U5" pad="4"/>
<contactref element="U5" pad="15"/>
<contactref element="U5" pad="14"/>
</signal>
<signal name="RESET">
<contactref element="U13" pad="26"/>
<contactref element="R51" pad="1"/>
<contactref element="S4" pad="2"/>
<contactref element="S4" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="R52" pad="1"/>
<contactref element="S5" pad="2"/>
<contactref element="S5" pad="1"/>
</signal>
<signal name="+1V1">
<contactref element="C45" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="U13" pad="23"/>
<contactref element="U13" pad="45"/>
<contactref element="U13" pad="50"/>
</signal>
<signal name="USB_DN">
<contactref element="R47" pad="2"/>
<contactref element="J10" pad="3"/>
<contactref element="D7" pad="3"/>
</signal>
<signal name="UNGND">
</signal>
<signal name="N$27">
<contactref element="D7" pad="5"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="D6" pad="A"/>
<contactref element="R8" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
