(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 81)
    (no_connects 0)
    (area 99.994999 41.994999 126.005001 100.005001)
    (thickness 1.6)
    (drawings 4)
    (tracks 251)
    (zones 0)
    (modules 32)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.01)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.2 1.2)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.12)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad5)")
  (net 2 "Net-(U1-Pad6)")
  (net 3 "Net-(U1-Pad8)")
  (net 4 "Net-(U1-Pad10)")
  (net 5 "Net-(U1-Pad14)")
  (net 6 "Net-(U1-Pad18)")
  (net 7 "Net-(U1-Pad19)")
  (net 8 "Net-(U1-Pad20)")
  (net 9 "Net-(U1-Pad21)")
  (net 10 "Net-(U1-Pad22)")
  (net 11 "Net-(U1-Pad23)")
  (net 12 "Net-(U1-Pad24)")
  (net 13 "Net-(U1-Pad32)")
  (net 14 GND)
  (net 15 +3V3)
  (net 16 "Net-(D1-Pad2)")
  (net 17 "Net-(D1-Pad1)")
  (net 18 "Net-(R3-Pad1)")
  (net 19 "Net-(C1-Pad2)")
  (net 20 "Net-(C2-Pad2)")
  (net 21 "Net-(C6-Pad2)")
  (net 22 "Net-(U1-Pad16)")
  (net 23 "Net-(R2-Pad1)")
  (net 24 ATM_TXD)
  (net 25 ATM_RXD)
  (net 26 "Net-(C6-Pad1)")
  (net 27 "Net-(R5-Pad1)")
  (net 28 ATM_DTR)
  (net 29 "Net-(C7-Pad2)")
  (net 30 "Net-(C8-Pad1)")
  (net 31 "Net-(IC1-Pad2)")
  (net 32 "Net-(IC1-Pad7)")
  (net 33 "Net-(IC1-Pad8)")
  (net 34 "Net-(IC1-Pad9)")
  (net 35 "Net-(IC1-Pad10)")
  (net 36 "Net-(IC1-Pad11)")
  (net 37 "Net-(IC1-Pad19)")
  (net 38 "Net-(IC1-Pad22)")
  (net 39 ATM_SOFT_RXD)
  (net 40 ATM_SOFT_TXD)
  (net 41 "Net-(IC1-Pad25)")
  (net 42 I2C_SDA)
  (net 43 I2C_SCL)
  (net 44 "Net-(IC1-Pad23)")
  (net 45 "Net-(IC1-Pad24)")
  (net 46 ESP_RXD)
  (net 47 ESP_TXD)
  (net 48 LATCH)
  (net 49 DATA)
  (net 50 "Net-(IC1-Pad16)")
  (net 51 CLOCK)
  (net 52 DISPLAY_RESET)
  (net 53 ENCODER_B)
  (net 54 ENCODER_A)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net ATM_DTR)
    (add_net ATM_RXD)
    (add_net ATM_SOFT_RXD)
    (add_net ATM_SOFT_TXD)
    (add_net ATM_TXD)
    (add_net CLOCK)
    (add_net DATA)
    (add_net DISPLAY_RESET)
    (add_net ENCODER_A)
    (add_net ENCODER_B)
    (add_net ESP_RXD)
    (add_net ESP_TXD)
    (add_net GND)
    (add_net I2C_SCL)
    (add_net I2C_SDA)
    (add_net LATCH)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
  )
  (module micro_switches:ALPS_SKRELHE010 (layer F.Cu) (tedit 58D91429)
    (at 124.5 88.5 90)
    (fp_text reference SW1 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value E_RST (at -0.3 -2.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.9 0 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 1.9 0 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R2-Pad1)"))
  )
  (module micro_switches:ALPS_SKRELHE010 (layer F.Cu) (tedit 58D913D8)
    (at 124.5 81.75 90)
    (fp_text reference SW2 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value E_FL (at 0.8 -2.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.9 0 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 1.9 0 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R5-Pad1)"))
  )
  (module micro_switches:ALPS_SKRELHE010 (layer F.Cu) (tedit 58D91034)
    (at 108.5 43.5)
    (fp_text reference SW3 (at -0.25 0.5) (layer F.SilkS) hide)
    (fp_text value A_RST (at 0 2) (layer F.SilkS))
    (pad 1 smd rect (at -1.9 0) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 1.9 0) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58D90FDA)
    (at 113.5 44.25 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user RS (at -2.4 10.2 180) (layer F.SilkS))
    (fp_text user DA (at -2.4 7.6 180) (layer F.SilkS))
    (fp_text user CL (at -2.4 5.1 180) (layer F.SilkS))
    (fp_text user V (at -2.4 2.6 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 I2C_SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 I2C_SDA))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 DISPLAY_RESET))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58D8DA7E)
    (at 102.5 51.5 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P3 (at -0.25 -2.75 270) (layer F.SilkS) hide)
    (fp_text value ATM_FLASH (at 4 4.6 270) (layer F.SilkS) hide)
    (fp_text user Tx (at -2.3 2.6 270) (layer F.SilkS))
    (fp_text user Rx (at -2.3 5 270) (layer F.SilkS))
    (fp_text user Dtr (at -2.3 7.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 ATM_TXD))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 ATM_RXD))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 ATM_DTR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58D8D620)
    (at 102.5 77.25 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value ESP_FLASH (at 0 7.41 180) (layer F.Fab))
    (fp_text user Tx (at -2.4 2.6 270) (layer F.SilkS))
    (fp_text user Rx (at -2.4 5.1 270) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 ESP_RXD))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 ESP_TXD))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58D8B49D)
    (at 102.5 55)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P7 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 ENCODER_A))
    (pad 2 thru_hole rect (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 ENCODER_B))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MCV-G_04x3.50mm_Vertical (layer F.Cu) (tedit 58BC3FEF)
    (at 120.75 65.25 270)
    (descr "Generic Phoenix Contact connector footprint for series: MCV-G; number of pins: 04; pin pitch: 3.50mm; Vertical || order number: 1843622 8A 160V")
    (tags "phoenix_contact connector MCV_01x04_G_3.5mm")
    (fp_text reference P5 (at 5.25 4.25 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 5.25 4 270) (layer F.Fab))
    (fp_text user LA (at 10.5 -3 270) (layer F.SilkS))
    (fp_text user DA (at 7 -2.9 270) (layer F.SilkS))
    (fp_text user CL (at 3.5 -2.9 270) (layer F.SilkS))
    (fp_text user GND (at 0 -2.9 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 2 thru_hole oval (at 3.5 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 CLOCK))
    (pad 3 thru_hole oval (at 7 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 DATA))
    (pad 4 thru_hole oval (at 10.5 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 48 LATCH))
    (model Connectors_Phoenix.3dshapes/PhoenixContact_MCV-G_04x3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MCV-G_02x3.50mm_Vertical (layer F.Cu) (tedit 58BC38D8)
    (at 120.75 56 270)
    (descr "Generic Phoenix Contact connector footprint for series: MCV-G; number of pins: 02; pin pitch: 3.50mm; Vertical || order number: 1843606 8A 160V")
    (tags "phoenix_contact connector MCV_01x02_G_3.5mm")
    (fp_text reference P4 (at 2 4 270) (layer F.SilkS) hide)
    (fp_text value VCC (at 1.75 4 270) (layer F.Fab))
    (fp_text user GND (at 3.5 -2.9 270) (layer F.SilkS))
    (fp_text user 3V3 (at 0 -2.9 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 2 thru_hole rect (at 3.5 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 GND))
    (model Connectors_Phoenix.3dshapes/PhoenixContact_MCV-G_02x3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58BBECCE)
    (at 111 53)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 58BC0CBC)
    (at 110.5 82.75 90)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 3.5 -2.25 180) (layer F.SilkS) hide)
    (fp_text value ESP8285 (at 0 3.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2.4 -1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at -2.4 -1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C6-Pad2)"))
    (pad 3 smd rect (at -2.4 -0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 4 smd rect (at -2.4 -0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 5 smd rect (at -2.4 0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -2.4 0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -2.4 1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R2-Pad1)"))
    (pad 8 smd rect (at -2.4 1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -1.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (pad 10 smd rect (at -1.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -0.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 12 smd rect (at -0.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 ATM_SOFT_TXD))
    (pad 13 smd rect (at 0.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 ATM_SOFT_RXD))
    (pad 14 smd rect (at 0.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R5-Pad1)"))
    (pad 16 smd rect (at 1.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 2.4 1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 18 smd rect (at 2.4 1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 2.4 0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 2.4 0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 2.4 -0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 2.4 -0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 2.4 -1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 2.4 -1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at 1.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 ESP_TXD))
    (pad 26 smd rect (at 1.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 ESP_RXD))
    (pad 27 smd rect (at 0.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C2-Pad2)"))
    (pad 28 smd rect (at 0.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C1-Pad2)"))
    (pad 29 smd rect (at -0.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 30 smd rect (at -0.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 31 smd rect (at -1.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 32 smd rect (at -1.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad32)"))
    (pad 33 smd rect (at 0.8625 0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 14 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 14 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 14 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 14 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58BC321B)
    (at 116 84.75 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 1.25 1.25 180) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58D91386)
    (at 120 84.75)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.25 1.5 180) (layer F.SilkS))
    (fp_text value 20 (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58BC320D)
    (at 114.75 87.75 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -2 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58B71E11)
    (at 104.25 85.25)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.75 0) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58B71E22)
    (at 104.25 79.75 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.75 0 180) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58BC10B1)
    (at 107.5 89.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.75 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58BC0CCC)
    (at 112.75 89.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58BC10BB)
    (at 111 89.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2.75 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58BC0CE1)
    (at 109.25 89.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 5.6pF (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58BC145D)
    (at 105.5 89.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 2 360) (layer F.SilkS))
    (fp_text value 12k (at 0 1.55 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58BC140A)
    (at 110.75 77.75 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.5 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 ATM_SOFT_RXD))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_2520-4pin_2.5x2.0mm (layer F.Cu) (tedit 58B71E32)
    (at 104.25 82.5 270)
    (descr "SMD Crystal SERIES SMD2520/4 http://www.newxtal.com/UploadFiles/Images/2012-11-12-09-29-09-776.pdf, 2.5x2.0mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference X1 (at 0 2.5 360) (layer F.SilkS))
    (fp_text value "40 MHz" (at 0 2.2 270) (layer F.Fab))
    (pad 1 smd rect (at -0.875 0.7 270) (size 1.15 1) (layers F.Cu F.Mask)
      (net 20 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 0.875 0.7 270) (size 1.15 1) (layers F.Cu F.Mask)
      (net 14 GND))
    (pad 3 smd rect (at 0.875 -0.7 270) (size 1.15 1) (layers F.Cu F.Mask)
      (net 19 "Net-(C1-Pad2)"))
    (pad 4 smd rect (at -0.875 -0.7 270) (size 1.15 1) (layers F.Cu F.Mask)
      (net 14 GND))
    (model Crystals.3dshapes/Crystal_SMD_2520-4pin_2.5x2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58D91394)
    (at 120 83.25 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 1.25 1.5 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module antennas:RFANT8010080A3T (layer F.Cu) (tedit 58BC32EE)
    (at 105.75 95.75 180)
    (fp_text reference P1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value ANT (at 0 -1.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.75 0 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 3.75 0 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58D8B44A)
    (at 107.75 48.25)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 ATM_DTR))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58BC204A)
    (at 116 65.75 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 2.5 0.25 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58D8D659)
    (at 103 64.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 1 -1.75 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 58BC13E7)
    (at 109.75 66.25)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 6.25) (layer F.SilkS) hide)
    (fp_text value ATMEGA328P-A (at 0 6.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 53 ENCODER_B))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 ATM_SOFT_RXD))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 ATM_SOFT_TXD))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 LATCH))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 DATA))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(IC1-Pad16)"))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 CLOCK))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C8-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(IC1-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 52 DISPLAY_RESET))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 I2C_SDA))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 I2C_SCL))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C7-Pad2)"))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 ATM_RXD))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 ATM_TXD))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 54 ENCODER_A))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58BC1413)
    (at 112.25 48.25 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cstce8m00g52a-r0:cstce8m00g52a-r0 (layer F.Cu) (tedit 58D8D64D)
    (at 102.75 68.5 90)
    (fp_text reference X2 (at 2.25 -1.5 180) (layer F.SilkS))
    (fp_text value "8 MHz" (at 0 -0.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1.2 0 90) (size 0.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad7)"))
    (pad 1 smd rect (at -1.2 0 90) (size 0.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad8)"))
    (pad 3 smd rect (at 0 0 90) (size 0.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58BBED97)
    (at 121 95)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 126 100) (end 100 100) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 126 42) (end 126 100) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 100 42) (end 126 42) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 100 100) (end 100 42) (angle 90) (layer Edge.Cuts) (width 0.01))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116 99.75) (xy 100.25 99.75) (xy 100.25 91.75) (xy 116 91.75)
      )
    )
  )
  (zone (net 14) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.125)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 125.75 91.5) (xy 100.25 91.5) (xy 100.25 42.25) (xy 125.75 42.25)
      )
    )
  )
)
