(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 97)
    (no_connects 10)
    (area 19.049999 17.149999 82.650001 51.050001)
    (thickness 1.6)
    (drawings 12)
    (tracks 330)
    (zones 0)
    (modules 42)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.33)
    (user_trace_width 0.25)
    (user_trace_width 0.33)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.203)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.78 1.78)
    (pad_drill 1.78)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFE7FFF)
    (pcbplotparams
      (layerselection 0x01000_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory C:/Users/Dan/Desktop/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 MISO)
  (net 4 SCK)
  (net 5 MOSI)
  (net 6 RST)
  (net 7 +12V)
  (net 8 "Net-(J2-Pad2)")
  (net 9 "Net-(J3-Pad2)")
  (net 10 "Net-(J4-Pad2)")
  (net 11 TACH1)
  (net 12 "Net-(J5-Pad3)")
  (net 13 TACH2)
  (net 14 "Net-(J6-Pad3)")
  (net 15 TACH3)
  (net 16 "Net-(J7-Pad3)")
  (net 17 NTC1)
  (net 18 NTC2)
  (net 19 NTC3)
  (net 20 PSU_V)
  (net 21 "Net-(U2-Pad6)")
  (net 22 TX)
  (net 23 RX)
  (net 24 "Net-(U2-Pad12)")
  (net 25 "Net-(U2-Pad14)")
  (net 26 "Net-(U2-Pad19)")
  (net 27 "Net-(U2-Pad20)")
  (net 28 "Net-(U2-Pad22)")
  (net 29 "Net-(U2-Pad27)")
  (net 30 "Net-(C4-Pad1)")
  (net 31 "Net-(C5-Pad1)")
  (net 32 "Net-(J12-Pad2)")
  (net 33 "Net-(J12-Pad3)")
  (net 34 "Net-(J12-Pad4)")
  (net 35 "Net-(R6-Pad1)")
  (net 36 "Net-(R7-Pad1)")
  (net 37 "Net-(U3-Pad2)")
  (net 38 "Net-(U3-Pad6)")
  (net 39 "Net-(U3-Pad7)")
  (net 40 "Net-(U3-Pad14)")
  (net 41 "Net-(U3-Pad15)")
  (net 42 "Net-(U3-Pad16)")
  (net 43 Qd)
  (net 44 "Net-(D1-Pad1)")
  (net 45 "Net-(D2-Pad1)")
  (net 46 "Net-(D3-Pad1)")
  (net 47 LED1)
  (net 48 LED2)
  (net 49 LED3)
  (net 50 "Net-(R11-Pad2)")
  (net 51 "Net-(Q1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net GND)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net MISO)
    (add_net MOSI)
    (add_net NTC1)
    (add_net NTC2)
    (add_net NTC3)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J12-Pad2)")
    (add_net "Net-(J12-Pad3)")
    (add_net "Net-(J12-Pad4)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net PSU_V)
    (add_net Qd)
    (add_net RST)
    (add_net RX)
    (add_net SCK)
    (add_net TACH1)
    (add_net TACH2)
    (add_net TACH3)
    (add_net TX)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 59.8 44.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.3 90) (layer F.SilkS))
    (fp_text value 0.1uC (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-16_3.9x4.9mm_Pitch0.635mm (layer F.Cu) (tedit 54130A77)
    (at 64.274498 46.755132 180)
    (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot519-1_po.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U3 (at 2.274498 3.555132 180) (layer F.SilkS))
    (fp_text value FT230 (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0.274498 -3.544868 180) (layer F.Fab))
    (pad 1 smd rect (at -2.6 -2.2225 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 RX))
    (pad 2 smd rect (at -2.6 -1.5875 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -2.6 -0.9525 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 4 smd rect (at -2.6 -0.3175 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 TX))
    (pad 5 smd rect (at -2.6 0.3175 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.6 0.9525 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -2.6 1.5875 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -2.6 2.2225 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R6-Pad1)"))
    (pad 9 smd rect (at 2.6 2.2225 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R7-Pad1)"))
    (pad 10 smd rect (at 2.6 1.5875 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 11 smd rect (at 2.6 0.9525 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 12 smd rect (at 2.6 0.3175 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C4-Pad1)"))
    (pad 13 smd rect (at 2.6 -0.3175 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.6 -0.9525 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U3-Pad14)"))
    (pad 15 smd rect (at 2.6 -1.5875 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U3-Pad15)"))
    (pad 16 smd rect (at 2.6 -2.2225 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U3-Pad16)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SSOP-16_3.9x4.9mm_Pitch0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 59.8 48.05 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.15 1.5 270) (layer F.SilkS))
    (fp_text value 0.1uC (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0.05 1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 65.2 43)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 27R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.1) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 70.8 43)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 27R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.1) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J12-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 48.7 33.6 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.9 -0.1 180) (layer F.SilkS))
    (fp_text value 30kR (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at -2.5 0.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 PSU_V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 58.15 41.3)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 3.05 -0.1) (layer F.SilkS))
    (fp_text value 0.1uC (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 2.95 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 37.92 38 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at -0.1 7.68 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 7.88 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 Qd))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 48.7 35.1)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.9 0) (layer F.SilkS))
    (fp_text value 100kR (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 2.5 0.1) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +12V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 PSU_V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 37.92 46.9 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 7.88 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 7.38 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 Qd))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48)
    (at 57.35 34.9 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 4.5 4.95 180) (layer F.SilkS))
    (fp_text value ATTINY88-MU (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 4.6 4.95 180) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 LED1))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 LED2))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 LED3))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 TACH1))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 TACH2))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 TACH3))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 TX))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 RX))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 MOSI))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 MISO))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 SCK))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 NTC1))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 NTC2))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 NTC3))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 PSU_V))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 RST))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad2)"))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J4-Pad2)"))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 57.65 28.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.85 0 180) (layer F.SilkS))
    (fp_text value 0.1uC (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at -2.85 0.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 77 28.12)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 7.5 0.18) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at -2.3 2.58 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 TACH2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 37.92 30.3 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0.7 7.68 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 7.58 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 Qd))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 77 36.86)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 7.2 -0.46) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at -2.2 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 TACH1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 71.6 22.6 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 0.1 4.7 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at -3.3 1.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 NTC1))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 67.5 22.6 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 0.1 4.7 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 4.4 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 NTC2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 71.6 25.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10kR (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0.1 -0.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 NTC1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 67.5 25.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10kR (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 NTC2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 63.4 25.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10kR (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 NTC3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 77 19.32)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0.1 -4.22) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at -5.3 -1.12 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 TACH3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J7-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 63.4 22.6 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J10 (at -0.1 4.7 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at -0.1 4.4 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 NTC3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 48.65 32.1 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.85 -0.1 180) (layer F.SilkS))
    (fp_text value 0.1uC (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at -2.55 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 PSU_V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer F.Cu) (tedit 59650532)
    (at 68.7 32.425 270)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -4.87 270) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 MISO))
    (pad 2 smd rect (at 2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 SCK))
    (pad 4 smd rect (at 2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 MOSI))
    (pad 5 smd rect (at -2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 RST))
    (pad 6 smd rect (at 2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 58CE4E7E)
    (at 41.15 23.5 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0.35 4.7 180) (layer F.SilkS))
    (fp_text value LD1117S33TR_SOT223 (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0.35 -4.2 360) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +12V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_bornier-2_P5.08mm (layer F.Cu) (tedit 59FF03AB)
    (at 59 21.3 180)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J11 (at -1.12 4.8 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.54 5.08 180) (layer F.Fab))
    (fp_text user %R (at -1.32 4.7 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 7 +12V))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 594C50D0)
    (at 73.4 48.2)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference J12 (at 1.1 7.2 180) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 3.4 180) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 1.47 180) (layer Dwgs.User))
    (fp_text user %R (at 6 -0.8) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -2.66) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -0.65 -2.66) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J12-Pad2)"))
    (pad 3 smd rect (at 0 -2.66) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J12-Pad3)"))
    (pad 4 smd rect (at 0.65 -2.66) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J12-Pad4)"))
    (pad 5 smd rect (at 1.3 -2.66) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.4625 -2.3) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.4625 -2.3) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.91 0) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.91 0) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -0.84 0) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.84 0) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 22.9 47.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK1 (at -0.1 -5.4) (layer F.SilkS))
    (fp_text value Mounting_Hole (at 0.5 4.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B4A9B79)
    (at 80.8 19.3)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J13 (at -0.1 -3.7) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 2.7 2.7 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 0 0) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 0 2.54) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 0 5.08) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B4A9BC1)
    (at 80.8 28.12)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J14 (at 6.3 -1.52) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 2.8 2.54 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 0 5.08) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B4A9BEE)
    (at 80.8 36.85)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J15 (at 4.7 -1.75) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 3.4 2.75 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 0 2.54) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 0 5.08) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 29.8 45.4 180)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D1 (at 0.3 4.1 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 29.8 47.3 180)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D2 (at 0.6 5.9 180) (layer F.SilkS))
    (fp_text value LED (at 0 3.2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 29.8 49.2 180)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D3 (at 0.4 7.7 180) (layer F.SilkS))
    (fp_text value LED (at 0 5.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 33.8 45.4)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.3 -3.7) (layer F.SilkS))
    (fp_text value 1.5kR (at 2.3 0.1) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 LED1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 33.8 47.3)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 4.7 5.4) (layer F.SilkS))
    (fp_text value 1.5kR (at 2.3 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 LED2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 33.8 49.2)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 3.1 2.9) (layer F.SilkS))
    (fp_text value 1.5kR (at 2.3 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 LED3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_3x5.3 (layer F.Cu) (tedit 58AA85CF)
    (at 48.7 20 90)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.3")
    (attr smd)
    (fp_text reference C6 (at 1.4 -2.9 90) (layer F.SilkS))
    (fp_text value CP (at -0.03 -2.9 90) (layer F.Fab))
    (fp_text user + (at -0.94 -0.08 90) (layer F.Fab))
    (fp_text user + (at -2.22 1.4 90) (layer F.SilkS))
    (fp_text user %R (at 3.5 -0.1 180) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +12V))
    (model Capacitors_SMD.3dshapes/CP_Elec_3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_3x5.3 (layer F.Cu) (tedit 58AA85CF)
    (at 48.6 27.2 270)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.3")
    (attr smd)
    (fp_text reference C7 (at 0.5 -3 270) (layer F.SilkS))
    (fp_text value CP (at -0.03 -2.9 270) (layer F.Fab))
    (fp_text user + (at -0.94 -0.08 270) (layer F.Fab))
    (fp_text user + (at -2.22 1.4 270) (layer F.SilkS))
    (fp_text user %R (at -3.9 0.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 270) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 0 270) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/CP_Elec_3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 48 38.6 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -1.6 -2.1 180) (layer F.SilkS))
    (fp_text value 100kR (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 49.6 38.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 1.4 -2.3 360) (layer F.SilkS))
    (fp_text value 100R (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R11-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Q1-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:LFPAK33 (layer F.Cu) (tedit 5A710896)
    (at 48.785 44.174 180)
    (descr "LFPAK33 SOT-1210 https://assets.nexperia.com/documents/outline-drawing/SOT1210.pdf")
    (tags "LFPAK33 SOT-1210")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference Q1 (at -3.815 0.174 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDSD (at 0 2.64 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at -0.215 -0.626 180) (size 0.51 0.635) (layers F.Paste))
    (pad "" smd rect (at 0.645 -0.626 180) (size 0.51 0.635) (layers F.Paste))
    (pad "" smd rect (at -0.215 0.626 180) (size 0.51 0.635) (layers F.Paste))
    (pad "" smd rect (at 0.645 0.626 180) (size 0.51 0.635) (layers F.Paste))
    (pad 5 smd rect (at 1.575 -0.975 180) (size 0.75 0.4) (layers F.Cu F.Mask)
      (net 43 Qd))
    (pad 5 smd rect (at 1.575 0.975 180) (size 0.75 0.4) (layers F.Cu F.Mask)
      (net 43 Qd))
    (pad 5 smd rect (at 1.575 -0.325 180) (size 0.75 0.4) (layers F.Cu F.Mask)
      (net 43 Qd))
    (pad 2 smd rect (at -1.535 -0.325 180) (size 0.83 0.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.535 -0.975 180) (size 0.83 0.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.535 0.325 180) (size 0.83 0.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 0.405 0 180) (size 1.85 2.25) (layers F.Cu F.Mask)
      (net 43 Qd))
    (pad "" smd rect (at -1.535 0.975 180) (size 0.83 0.3) (layers F.Paste))
    (pad 5 smd rect (at 1.575 0.325 180) (size 0.75 0.4) (layers F.Cu F.Mask)
      (net 43 Qd))
    (pad 4 smd rect (at -1.535 0.975 180) (size 0.83 0.4) (layers F.Cu F.Mask)
      (net 51 "Net-(Q1-Pad4)"))
    (pad "" smd rect (at -1.535 0.325 180) (size 0.83 0.3) (layers F.Paste))
    (pad "" smd rect (at -1.535 -0.325 180) (size 0.83 0.3) (layers F.Paste))
    (pad "" smd rect (at -1.535 -0.975 180) (size 0.83 0.3) (layers F.Paste))
    (pad "" smd rect (at 1.575 -0.975 180) (size 0.75 0.3) (layers F.Paste))
    (pad "" smd rect (at 1.575 -0.325 180) (size 0.75 0.3) (layers F.Paste))
    (pad "" smd rect (at 1.575 0.325 180) (size 0.75 0.3) (layers F.Paste))
    (pad "" smd rect (at 1.575 0.975 180) (size 0.75 0.3) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/LFPAK33.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text - (at 59.1 26.4) (layer F.SilkS))
  (gr_text + (at 53.9 26.3) (layer F.SilkS))
  (gr_arc (start 20.5 49.6) (end 20.5 51) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 20.5 44.7) (end 19.1 44.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.1 44.7) (end 19.1 49.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 34.9 43.3) (end 20.5 43.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.6 51) (end 82.6 17.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 20.5 51) (end 82.6 51) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 34.9 17.2) (end 34.9 43.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.6 17.2) (end 34.9 17.2) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34 17.2) (xy 82 17.2) (xy 82 51) (xy 34 51)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34 17.2) (xy 82 17.2) (xy 82 51) (xy 34 51)
      )
    )
  )
  (zone (net 43) (net_name Qd) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41.7 47.8) (xy 41.7 29.1) (xy 45.4 29.1) (xy 45.4 42.3) (xy 49.3 42.3)
        (xy 49.3 47.8)
      )
    )
  )
  (zone (net 7) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.6 51) (xy 39.6 34.1) (xy 39.6 23) (xy 56 23) (xy 56 17.2)
        (xy 34 17.2) (xy 34 51)
      )
    )
  )
  (zone (net 43) (net_name Qd) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.203))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 48) (xy 51.5 48) (xy 51.5 40.3) (xy 40.5 40.3)
      )
    )
  )
)
