(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 360)
    (zones 0)
    (modules 32)
    (nets 64)
  )
  (page A4)
  (title_block
    (title "PI Cluster Master Board")
    (date 2018-10-18)
    (rev "rev 2.1")
    (comment 2 creativecommons.org/license/by/4.0)
    (comment 3 "License: CC BY 4.0")
    (comment 4 "Author: Thomas Cate")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.508)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.7 3.7)
    (pad_drill 1.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 /PI_3.3V)
  (net 4 /PI_5V)
  (net 5 /STACK_6)
  (net 6 /STACK_5)
  (net 7 /STACK_4)
  (net 8 "Net-(H1-Pad8)")
  (net 9 "Net-(H1-Pad10)")
  (net 10 /PWR_SW)
  (net 11 /PWR_ON)
  (net 12 /PWR_LED)
  (net 13 /ACT_LED)
  (net 14 /BCAST)
  (net 15 "Net-(H1-Pad17)")
  (net 16 /CLOCK)
  (net 17 /STACK_3)
  (net 18 /STACK_2)
  (net 19 /RESET_SW)
  (net 20 /STACK_1)
  (net 21 "Net-(H1-Pad24)")
  (net 22 "Net-(H1-Pad26)")
  (net 23 "Net-(H1-Pad27)")
  (net 24 "Net-(H1-Pad28)")
  (net 25 "Net-(H1-Pad29)")
  (net 26 "Net-(H1-Pad31)")
  (net 27 "Net-(H1-Pad32)")
  (net 28 "Net-(H1-Pad33)")
  (net 29 "Net-(H1-Pad35)")
  (net 30 "Net-(H1-Pad36)")
  (net 31 "Net-(H1-Pad37)")
  (net 32 "Net-(H1-Pad38)")
  (net 33 "Net-(H1-Pad40)")
  (net 34 "Net-(H2-Pad1)")
  (net 35 "Net-(H2-Pad2)")
  (net 36 "Net-(H2-Pad3)")
  (net 37 "Net-(H2-Pad4)")
  (net 38 "Net-(H2-Pad5)")
  (net 39 "Net-(H2-Pad6)")
  (net 40 "Net-(H2-Pad7)")
  (net 41 "Net-(H2-Pad8)")
  (net 42 "Net-(H3-Pad4)")
  (net 43 "Net-(H3-Pad2)")
  (net 44 /ATX_3.3V)
  (net 45 "Net-(J1-Pad2)")
  (net 46 /5V)
  (net 47 "Net-(J1-Pad8)")
  (net 48 /5V_STB)
  (net 49 /12V)
  (net 50 "Net-(J1-Pad11)")
  (net 51 "Net-(J1-Pad12)")
  (net 52 "Net-(J1-Pad13)")
  (net 53 "Net-(J1-Pad14)")
  (net 54 /PS_ON)
  (net 55 "Net-(J1-Pad20)")
  (net 56 "Net-(R3-Pad1)")
  (net 57 "Net-(R12-Pad1)")
  (net 58 "Net-(R13-Pad1)")
  (net 59 "Net-(R13-Pad2)")
  (net 60 "Net-(R15-Pad1)")
  (net 61 "Net-(SW1-Pad3)")
  (net 62 "Net-(R14-Pad1)")
  (net 63 "Net-(R15-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.508)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /12V)
    (add_net /5V)
    (add_net /5V_STB)
    (add_net /ACT_LED)
    (add_net /ATX_3.3V)
    (add_net /BCAST)
    (add_net /CLOCK)
    (add_net /PI_3.3V)
    (add_net /PI_5V)
    (add_net /PS_ON)
    (add_net /PWR_LED)
    (add_net /PWR_ON)
    (add_net /PWR_SW)
    (add_net /RESET_SW)
    (add_net /STACK_1)
    (add_net /STACK_2)
    (add_net /STACK_3)
    (add_net /STACK_4)
    (add_net /STACK_5)
    (add_net /STACK_6)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(H1-Pad10)")
    (add_net "Net-(H1-Pad17)")
    (add_net "Net-(H1-Pad24)")
    (add_net "Net-(H1-Pad26)")
    (add_net "Net-(H1-Pad27)")
    (add_net "Net-(H1-Pad28)")
    (add_net "Net-(H1-Pad29)")
    (add_net "Net-(H1-Pad31)")
    (add_net "Net-(H1-Pad32)")
    (add_net "Net-(H1-Pad33)")
    (add_net "Net-(H1-Pad35)")
    (add_net "Net-(H1-Pad36)")
    (add_net "Net-(H1-Pad37)")
    (add_net "Net-(H1-Pad38)")
    (add_net "Net-(H1-Pad40)")
    (add_net "Net-(H1-Pad8)")
    (add_net "Net-(H2-Pad1)")
    (add_net "Net-(H2-Pad2)")
    (add_net "Net-(H2-Pad3)")
    (add_net "Net-(H2-Pad4)")
    (add_net "Net-(H2-Pad5)")
    (add_net "Net-(H2-Pad6)")
    (add_net "Net-(H2-Pad7)")
    (add_net "Net-(H2-Pad8)")
    (add_net "Net-(H3-Pad2)")
    (add_net "Net-(H3-Pad4)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(SW1-Pad3)")
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 5BCA1A71)
    (at 101.5 82.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference "" (at 0 -3.7) (layer F.SilkS))
    (fp_text value "" (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 5BCA1A71)
    (at 43.5 82.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference "" (at 0 -3.7) (layer F.SilkS))
    (fp_text value "" (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 5BCA1A71)
    (at 101.5 33.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference "" (at 0 -3.7) (layer F.SilkS))
    (fp_text value "" (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA0918)
    (at 74.46 56.976)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 4.892 -0.072) (layer F.SilkS))
    (fp_text value 270 (at 5.0698 -1.977) (layer F.Fab))
    (fp_text user "" (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R13-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5BCA08F3)
    (at 46.46 44)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer F.Cu) (tedit 5BCA0907)
    (at 48.5 35 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference H1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value "Raspberry_Pi 2X20 2.54mm header" (at -2.8206 31.2052 180) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /PI_3.3V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /PI_5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /STACK_6))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /PI_5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /STACK_5))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /STACK_4))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(H1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /PWR_SW))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /PWR_ON))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /PWR_LED))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ACT_LED))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /BCAST))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(H1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /CLOCK))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /STACK_3))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /STACK_2))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /RESET_SW))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /STACK_1))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(H1-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(H1-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(H1-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(H1-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(H1-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(H1-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(H1-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(H1-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(H1-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(H1-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(H1-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(H1-Pad40)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 5BCA0957)
    (at 65.46 84 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference H2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value "2X4 2.54mm header" (at -2.8934 6.168 180) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(H2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(H2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(H2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(H2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(H2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(H2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(H2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(H2-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 5BCA0952)
    (at 51 84 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference H3 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value "2X4 2.54mm header" (at -2.741 3.0004 180) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /PWR_SW))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /PI_3.3V))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /RESET_SW))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /PI_3.3V))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(H3-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(H3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module conn-pwr_atx:Molex_Micro-Fit_3.0_43045-0800_2x04_P3.00mm_Horizontal (layer F.Cu) (tedit 5BCA0962)
    (at 92.5 76.5 180)
    (descr "Molex Micro-Fit 3.0 Connector System, 43045-0800 (compatible alternatives: 43045-0801, 43045-0802), 4 Pins per row (https://www.molex.com/pdm_docs/sd/430450200_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Micro-Fit_3.0 top entry")
    (fp_text reference J2 (at -2.5 2.5 180) (layer F.SilkS))
    (fp_text value "Molex 43025-0800" (at 4.5 5.7 180) (layer F.Fab))
    (fp_text user %R (at 4.5 -8.22 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.14 -4.32 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.84 -4.32 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask) (roundrect_rratio 0.166667)
      (net 49 /12V))
    (pad 2 thru_hole circle (at 3 0 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 46 /5V))
    (pad 3 thru_hole circle (at 6 0 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 46 /5V))
    (pad 4 thru_hole circle (at 9 0 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 46 /5V))
    (pad 5 thru_hole circle (at 0 3 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 3 3 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 6 3 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 9 3 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Micro-Fit_3.0_43045-0800_2x04_P3.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA08E9)
    (at 46.228 69.342 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 4.73 0 90) (layer F.SilkS))
    (fp_text value 330 (at 6.8326 0.6604 90) (layer F.Fab))
    (fp_text user "" (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(H3-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /ACT_LED))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA08E0)
    (at 52.324 69.34254 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 4.73 0 90) (layer F.SilkS))
    (fp_text value 330 (at 6.78234 0.7112 90) (layer F.Fab))
    (fp_text user "" (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /PWR_LED))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(H3-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA08E4)
    (at 49.276 69.342 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 4.73 0 90) (layer F.SilkS))
    (fp_text value 270 (at 6.9342 0.7112 90) (layer F.Fab))
    (fp_text user "" (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /PWR_ON))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA08FE)
    (at 51.816 54 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.026 -0.102 180) (layer F.SilkS))
    (fp_text value 330 (at 3.302 -0.864 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /5V_STB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA094C)
    (at 54.864 41.656 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -0.086 270) (layer F.SilkS))
    (fp_text value 330 (at 3.2258 -0.6858 270) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA08D1)
    (at 70.358 69.342 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 4.634 -0.046 90) (layer F.SilkS))
    (fp_text value 270 (at 6.8326 0.6096 90) (layer F.Fab))
    (fp_text user "" (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(H2-Pad8)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /STACK_1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA08D7)
    (at 67.31 69.342 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 4.523932 0.106206 90) (layer F.SilkS))
    (fp_text value 270 (at 6.8326 0.762 90) (layer F.Fab))
    (fp_text user "" (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /STACK_2))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(H2-Pad7)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA0966)
    (at 64.262 69.342 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 4.572 0 90) (layer F.SilkS))
    (fp_text value 270 (at 6.9596 0.7112 90) (layer F.Fab))
    (fp_text user "" (at 9.790068 16.705794 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(H2-Pad6)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /STACK_3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA08ED)
    (at 61.214 69.342 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 4.523932 0.006206 90) (layer F.SilkS))
    (fp_text value 270 (at 6.9088 0.7366 90) (layer F.Fab))
    (fp_text user "" (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /STACK_4))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(H2-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BC96863)
    (at 58.166 69.342 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 5.031932 -0.045794 90) (layer F.SilkS))
    (fp_text value 270 (at 6.985 0.889 90) (layer F.Fab))
    (fp_text user "" (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(H2-Pad4)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /STACK_5))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA08DC)
    (at 55.215794 69.342 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 5.031932 -0.097794 90) (layer F.SilkS))
    (fp_text value 270 (at 6.985 0.791206 90) (layer F.Fab))
    (fp_text user "" (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /STACK_6))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(H2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA0901)
    (at 74.46 41.976)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 4.892 -0.058) (layer F.SilkS))
    (fp_text value 270 (at 5.08 2.37) (layer F.Fab))
    (fp_text user "" (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(R12-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /CLOCK))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA090A)
    (at 88.46 41.918)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 5.08 -0.05) (layer F.SilkS))
    (fp_text value 270 (at 5.08 2.37) (layer F.Fab))
    (fp_text user "" (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /BCAST))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R14-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5BCA08F9)
    (at 42.418 42.672)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference SW1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "Adafruit 805" (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /5V_STB))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /PI_5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(SW1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5BCA0926)
    (at 88.496 56.904)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 5.08 0) (layer F.SilkS))
    (fp_text value 270 (at 5.0546 -2.0574) (layer F.Fab))
    (fp_text user "" (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R15-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 5BCA1A71)
    (at 43.5 33.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference "" (at 0 -3.7) (layer F.SilkS))
    (fp_text value "" (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module "conn-pwr_atx:1-1775099-3(fixed)" (layer F.Cu) (tedit 5BCA2F06)
    (at 123.3424 55.9562 90)
    (descr 1-1775099-3)
    (tags Connector)
    (fp_text reference J1 (at -0.444 -5.108 90) (layer F.SilkS))
    (fp_text value "ATX24  TE 1-1775099-3" (at -0.444 -5.108 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -23.1 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 44 /ATX_3.3V))
    (pad 13 thru_hole circle (at -23.1 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(J1-Pad13)"))
    (pad 2 thru_hole circle (at -18.9 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(J1-Pad2)"))
    (pad 14 thru_hole circle (at -18.9 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(J1-Pad14)"))
    (pad 3 thru_hole circle (at -14.7 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole circle (at -14.7 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at -10.5 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 46 /5V))
    (pad 16 thru_hole circle (at -10.5 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 54 /PS_ON))
    (pad 5 thru_hole circle (at -6.3 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole circle (at -6.3 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.1 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 46 /5V))
    (pad 18 thru_hole circle (at -2.1 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole circle (at 2.1 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 19 thru_hole circle (at 2.1 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole circle (at 6.3 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(J1-Pad8)"))
    (pad 20 thru_hole circle (at 6.3 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(J1-Pad20)"))
    (pad 9 thru_hole circle (at 10.5 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 48 /5V_STB))
    (pad 21 thru_hole circle (at 10.5 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 46 /5V))
    (pad 10 thru_hole circle (at 14.7 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 49 /12V))
    (pad 22 thru_hole circle (at 14.7 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 46 /5V))
    (pad 11 thru_hole circle (at 18.9 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(J1-Pad11)"))
    (pad 23 thru_hole circle (at 18.9 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 46 /5V))
    (pad 12 thru_hole circle (at 23.1 -7.55 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(J1-Pad12)"))
    (pad 24 thru_hole circle (at 23.1 -2.05 180) (size 2 2) (drill 1.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 25 thru_hole circle (at -27.8 -2.51 180) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module conn-pwr_atx:TO-92_Inline_NPN (layer F.Cu) (tedit 5BCA2EAA)
    (at 47.752 71.5264 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference T1 (at 2.54 -3.56 270) (layer F.SilkS))
    (fp_text value BC547B (at 2.54 2.79 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(R3-Pad1)"))
    (pad 3 thru_hole circle (at 4.826 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /PS_ON))
    (pad 2 thru_hole circle (at 0.254 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module conn-pwr_atx:TO-92_Inline_NPN (layer F.Cu) (tedit 5BCA2EAA)
    (at 82.1714 49.538 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference T2 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value BC547B (at 2.54 2.79 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(R12-Pad1)"))
    (pad 3 thru_hole circle (at 4.826 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0.254 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module conn-pwr_atx:TO-92_Inline_PNP (layer F.Cu) (tedit 5BCA2E15)
    (at 82.1206 61.5268 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference T3 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value BC557B (at 2.4892 2.4892 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0.254 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /ATX_3.3V))
    (pad 3 thru_hole circle (at 4.826 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module conn-pwr_atx:TO-92_Inline_NPN (layer F.Cu) (tedit 5BCA2EAA)
    (at 96.0652 49.5888 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference T4 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value BC547B (at 2.54 2.79 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0.254 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R15-Pad2)"))
    (pad 3 thru_hole circle (at 4.826 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R14-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module conn-pwr_atx:TO-92_Inline_PNP (layer F.Cu) (tedit 5BCA2E15)
    (at 96.0906 61.5014 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference T5 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value BC557B (at 2.3114 2.4892 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(R15-Pad1)"))
    (pad 3 thru_hole circle (at 4.826 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(H2-Pad2)"))
    (pad 2 thru_hole circle (at 0.254 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /ATX_3.3V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module conn-pwr_atx:BarrelJack_Horizontal_OSHPARK (layer F.Cu) (tedit 5BCA8C62)
    (at 109.00156 43.89374 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J3 (at -8.45 5.75 270) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -6.2 -5.5 270) (layer F.Fab))
    (fp_text user %R (at -3 -2.95 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 49 /12V))
    (pad 2 thru_hole circle (at -6 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3 4.7 270) (size 3.5 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Thomas Cate" (at 40.894 64.6684 270) (layer F.SilkS))
  (gr_text "Pi 2.0 Master Power Rev 2" (at 42.1894 64.8208 270) (layer F.SilkS))
  (gr_line (start 125 30) (end 125 86) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40 86) (end 40 30) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 86) (end 40 86) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40 30) (end 125 30) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40 30) (xy 125 30) (xy 125 86) (xy 40 86)
      )
    )
  )
  (zone (net 46) (net_name /5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80 75) (xy 112 75) (xy 112 35) (xy 124 35) (xy 124 78)
        (xy 80 78)
      )
    )
  )
  (zone (net 46) (net_name /5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80 78) (xy 124 78) (xy 124 81) (xy 80 81)
      )
    )
  )
)
