(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 57)
    (no_connects 0)
    (area 121.844999 93.904999 160.095001 110.565001)
    (thickness 1.6)
    (drawings 15)
    (tracks 210)
    (zones 0)
    (modules 22)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.07)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 PWR_CTRL)
  (net 5 LED_SIG)
  (net 6 RTC_SCL)
  (net 7 RTC_SDA)
  (net 8 BUTTON/RST)
  (net 9 LED_SIG_OUT)
  (net 10 PCELL)
  (net 11 "Net-(R4-Pad2)")
  (net 12 "Net-(R6-Pad2)")
  (net 13 "Net-(U2-Pad1)")
  (net 14 "Net-(U2-Pad3)")
  (net 15 "Net-(U2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net BUTTON/RST)
    (add_net LED_SIG)
    (add_net LED_SIG_OUT)
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net PCELL)
    (add_net RTC_SCL)
    (add_net RTC_SDA)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net PWR_CTRL)
  )
  (module clock-ws2812-schematic-v2:BatteryHolder_3xAAA_Keystone_2479 (layer B.Cu) (tedit 5905A352)
    (at 153.543 108.712 90)
    (descr "3xAAA cell battery holder, Keystone P/N 2479")
    (tags "AAA battery cell holder")
    (fp_text reference BT1 (at -3.81 0 180) (layer B.SilkS) hide)
    (fp_text value Battery (at -1.27 -3.937 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask B.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at -0.0508 -12.7 90) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
  )
  (module Housings_DIP:DIP-8_W7.62mm placed (layer F.Cu) (tedit 59058988)
    (at 138.43 96.52)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 3.81 0.762) (layer F.SilkS))
    (fp_text value ATtiny85 (at 3.81 8.89) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 BUTTON/RST))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 PCELL))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 PWR_CTRL))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 RTC_SDA))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 LED_SIG))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 RTC_SCL))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 590588DB)
    (at 142.414 100.33)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 1.477 -1.27) (layer B.SilkS))
    (fp_text value SCL_PUP (at -1.063 -1.27) (layer B.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 RTC_SCL))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing_Handsoldering placed (layer F.Cu) (tedit 59058FF8)
    (at 156.69514 106.23804 180)
    (descr "SOT89-3, Housing, Handsoldering,")
    (tags "SOT89-3, Housing, Handsoldering,")
    (attr smd)
    (fp_text reference U3 (at -2.18186 -2.60096 450) (layer F.SilkS))
    (fp_text value MCP1700T (at 1.27 -6.858 180) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 2.35204 180) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 2.35204 180) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 1.50114 2.35204 180) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0 -1.6002 180) (size 1.99898 4.0005) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd trapezoid (at 0 0.7493) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16W_7.5x10.3mm_Pitch1.27mm placed (layer B.Cu) (tedit 59055F7D)
    (at 153.748 101.981 180)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -2.794 4.318 180) (layer B.SilkS))
    (fp_text value DS3231 (at -0.049 -4.191 180) (layer B.SilkS))
    (pad 1 smd rect (at -4.65 4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -4.65 3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 PWR_CTRL))
    (pad 3 smd rect (at -4.65 1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -4.65 0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -4.65 -0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.65 -1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -4.65 -3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -4.65 -4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 4.65 -4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 4.65 -3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.65 -1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 4.65 -0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 4.65 0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 4.65 1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at 4.65 3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 RTC_SDA))
    (pad 16 smd rect (at 4.65 4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 RTC_SCL))
    (model Housings_SOIC.3dshapes/SOIC-16_7.5x10.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 placed (layer F.Cu) (tedit 59055CAC)
    (at 147.574 108.458 180)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW3 (at 0.127 0 180) (layer F.SilkS) hide)
    (fp_text value Minute (at -1.016 2.413 180) (layer F.SilkS))
    (pad 2 smd rect (at 2.7 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R6-Pad2)"))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_FSMSM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 placed (layer F.Cu) (tedit 59055CA9)
    (at 135.128 108.458)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at 0.254 2.794) (layer F.SilkS) hide)
    (fp_text value Hour (at 0.254 -2.54) (layer F.SilkS))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R4-Pad2)"))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_FSMSM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer F.Cu) (tedit 5906646C)
    (at 150.542 99.06)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 1.397 -1.27) (layer F.SilkS))
    (fp_text value 5K (at -1.397 -1.27) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 BUTTON/RST))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer F.Cu) (tedit 59066463)
    (at 150.542 96.012 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -1.524 1.27 180) (layer F.SilkS))
    (fp_text value 2K (at 1.524 1.27 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 BUTTON/RST))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer F.Cu) (tedit 590583D7)
    (at 149.86 103.077 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 1.397 1.524 270) (layer F.SilkS))
    (fp_text value 10K (at -1.4605 1.4605 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 BUTTON/RST))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 59055148)
    (at 128.825 104.013)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -1.524 -1.524) (layer B.SilkS))
    (fp_text value R_ADC (at 1.016 -1.524) (layer B.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 PCELL))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Opto-Devices:Resistor_LDR_4.9x4.2_RM2.54 placed (layer F.Cu) (tedit 59055ABD)
    (at 129.54 108.077 180)
    (descr "Resistor, LDR 4.9x4.2mm")
    (tags "Resistor LDR4.9x4.2")
    (fp_text reference R2 (at 1.27 -1.524 180) (layer F.SilkS))
    (fp_text value "PHOTO CELL" (at 1.016 -5.588 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 PWR_CTRL))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 PCELL))
  )
  (module WS2812:WS2812-8mm placed (layer F.Cu) (tedit 5905542C)
    (at 128.524 98.425)
    (fp_text reference LED1 (at 0 3.429) (layer F.SilkS))
    (fp_text value WS2812 (at 0 -3.302) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.905 0) (size 1.016 2.032) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 LED_SIG))
    (pad 2 thru_hole oval (at -0.635 0) (size 1.016 2.032) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 PWR_CTRL))
    (pad 3 thru_hole rect (at 0.635 0) (size 1.016 2.032) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 1.905 0) (size 1.016 2.032) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 LED_SIG_OUT))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 placed (layer F.Cu) (tedit 590555D7)
    (at 134.747 103.378 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value I2C (at 2.159 -0.635 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 RTC_SCL))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 RTC_SDA))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 placed (layer F.Cu) (tedit 59059E41)
    (at 123.698 103.759)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 -2.413) (layer F.SilkS) hide)
    (fp_text value WS2812B_OUT (at 0.635 -2.159) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 LED_SIG_OUT))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 59055AB1)
    (at 157.119 95.504 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.647 0 270) (layer B.SilkS))
    (fp_text value "0.1uF (RTC Vcc)" (at 2.687 -4.318 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 PWR_CTRL))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 59066454)
    (at 151.364 95.504)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -2.667 0.0635 270) (layer B.SilkS))
    (fp_text value "0.1uF (RTC Vbat)" (at -3.663 2.286 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer B.Cu) (tedit 59059B7E)
    (at 123.698 99.969 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -2.941 0 360) (layer B.SilkS))
    (fp_text value "0.1uF (LED)" (at 0.361 -1.397 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 PWR_CTRL))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer F.Cu) (tedit 59066472)
    (at 156.464 100.076)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0.254 -1.397) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering placed (layer F.Cu) (tedit 590589C5)
    (at 152.908 104.628 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.02 1.397 270) (layer F.SilkS))
    (fp_text value 1uF (at -2.647 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer B.Cu) (tedit 590581BE)
    (at 142.414 103.886)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.477 -1.397) (layer B.SilkS))
    (fp_text value SDA_PUP (at -1.063 -1.397) (layer B.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 RTC_SDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5905A404)
    (at 142.387 96.774 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.647 1.397 180) (layer B.SilkS))
    (fp_text value "0.1uF (AT85)" (at 0.655 1.397 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "3V3  DO  GND" (at 125.476 106.68 270) (layer F.SilkS))
  (gr_text https://git.io/vS5e4 (at 128.143 94.869) (layer B.SilkS))
  (dimension 16.51 (width 0.1) (layer Eco2.User)
    (gr_text "0.6500 in" (at 164.195 102.235 270) (layer Eco2.User))
    (feature1 (pts (xy 161.925 110.49) (xy 165.195 110.49)))
    (feature2 (pts (xy 161.925 93.98) (xy 165.195 93.98)))
    (crossbar (pts (xy 163.195 93.98) (xy 163.195 110.49)))
    (arrow1a (pts (xy 163.195 110.49) (xy 162.608579 109.363496)))
    (arrow1b (pts (xy 163.195 110.49) (xy 163.781421 109.363496)))
    (arrow2a (pts (xy 163.195 93.98) (xy 162.608579 95.106504)))
    (arrow2b (pts (xy 163.195 93.98) (xy 163.781421 95.106504)))
  )
  (gr_text "DI  V  G  DO" (at 128.524 96.647) (layer F.SilkS))
  (gr_text "LED Minute Repeater Clock rev 0.5.1\n2017-04-30\n@ryo1kato " (at 134.874 107.696) (layer B.SilkS))
  (gr_text "3V3 SCL SDA GND" (at 136.652 99.187 90) (layer F.SilkS))
  (gr_line (start 121.92 95.25) (end 121.92 109.22) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 109.22) (end 160.02 95.25) (layer Edge.Cuts) (width 0.15))
  (dimension 38.1 (width 0.1) (layer Eco2.User)
    (gr_text "1.5000 in" (at 140.97 89.445994) (layer Eco2.User))
    (feature1 (pts (xy 160.02 91.715994) (xy 160.02 88.445994)))
    (feature2 (pts (xy 121.92 91.715994) (xy 121.92 88.445994)))
    (crossbar (pts (xy 121.92 90.445994) (xy 160.02 90.445994)))
    (arrow1a (pts (xy 160.02 90.445994) (xy 158.893496 91.032415)))
    (arrow1b (pts (xy 160.02 90.445994) (xy 158.893496 89.859573)))
    (arrow2a (pts (xy 121.92 90.445994) (xy 123.046504 91.032415)))
    (arrow2b (pts (xy 121.92 90.445994) (xy 123.046504 89.859573)))
  )
  (gr_line (start 158.75 110.49) (end 123.19 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 93.98) (end 123.19 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.75 109.22) (end 160.02 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.19 109.22) (end 123.19 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.19 95.25) (end 121.92 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.75 95.25) (end 158.75 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 93.98) (xy 160.02 110.49) (xy 121.92 110.49) (xy 121.92 93.98)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 93.98) (xy 160.02 110.49) (xy 121.92 110.49) (xy 121.92 93.98)
      )
    )
  )
)
