<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="4.572" y1="3.937" x2="-4.572" y2="3.937" width="0.254" layer="20"/>
<wire x1="-4.572" y1="3.937" x2="-5.207" y2="3.302" width="0.254" layer="20" curve="90"/>
<wire x1="-5.207" y1="3.302" x2="-5.207" y2="-3.302" width="0.254" layer="20"/>
<wire x1="-5.207" y1="-3.302" x2="-4.572" y2="-3.937" width="0.254" layer="20" curve="90"/>
<wire x1="-4.572" y1="-3.937" x2="4.572" y2="-3.937" width="0.254" layer="20"/>
<wire x1="4.572" y1="-3.937" x2="5.207" y2="-3.302" width="0.254" layer="20" curve="90"/>
<wire x1="5.207" y1="-3.302" x2="5.207" y2="3.302" width="0.254" layer="20"/>
<wire x1="5.207" y1="3.302" x2="4.572" y2="3.937" width="0.254" layer="20" curve="90"/>
<text>SOT-23
TSOT-23</text>
<text>v0</text>
</plain>
<libraries>
<library name="myDevice">
<packages>
<package name="BO_TSOT/SOT-23-6_HS">
<description>SOT23-6 and TSOT23-6 Handsoldering</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC" library="myDevice" package="BO_TSOT/SOT-23-6_HS" value="BREAKOUT_6PIN-TSOT/SOT23-6_HS"/>
</elements>
<signals>
<signal name="2">
<contactref element="IC" pad="2"/>
</signal>
<signal name="1">
<contactref element="IC" pad="1"/>
</signal>
<signal name="3">
<contactref element="IC" pad="3"/>
</signal>
<signal name="4">
<contactref element="IC" pad="4"/>
</signal>
<signal name="5">
<contactref element="IC" pad="5"/>
</signal>
<signal name="6">
<contactref element="IC" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
