(kicad_pcb (version 20171130) (host pcbnew 5.1.2-f72e74a~84~ubuntu14.04.1)
  (general
    (thickness 0.8)
    (drawings 12)
    (tracks 130)
    (zones 0)
    (modules 19)
    (nets 9)
  )
  (page A4)
  (title_block
    (title "RTC and FRAm")
    (date 2017-07-29)
    (rev 1)
    (comment 1 "Copyright © 2017 R Kilvington (eclrpk @ leeds.ac.uk)")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.8)
    (via_min_drill 0.4)
    (uvia_size 0.8)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.1)
    (pcb_text_size 0.8 0.8)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.1)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.1)
    (solder_mask_min_width 0.1)
    (pad_to_paste_clearance -0.1)
    (aux_axis_origin 47 70)
    (grid_origin 46 83.75)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "production/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 SCL-FRAM-RTC)
  (net 4 SDA-FRAM-RTC)
  (net 5 "Net-(BT1-Pad1)")
  (net 6 "Net-(U1-Pad1)")
  (net 7 "Net-(U1-Pad3)")
  (net 8 ~RESET)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net SCL-FRAM-RTC)
    (add_net SDA-FRAM-RTC)
    (add_net ~RESET)
  )
  (net_class 0.5 ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (add_net +3V3)
  )
  (module modules:SO-16-W (layer B.Cu) (tedit 5FFC61F3)
    (at 66.193 76.257 90)
    (descr "Module CMS SOJ 16 pins tres large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value DS3231SN (at 0.107 6.807 90) (layer B.SilkS))
    (fp_text user 1 (at -5.2 -5 90) (layer B.SilkS))
    (pad 1 smd rect (at -4.445 -5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -3.175 -5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 3 smd roundrect (at -1.905 -5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at -0.635 -5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 ~RESET))
    (pad 5 smd roundrect (at 0.635 -5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 1.905 -5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at 3.175 -5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at 4.445 -5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 16 smd roundrect (at -4.445 5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 SCL-FRAM-RTC))
    (pad 15 smd roundrect (at -3.175 5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 SDA-FRAM-RTC))
    (pad 14 smd roundrect (at -1.905 5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(BT1-Pad1)"))
    (pad 13 smd roundrect (at -0.635 5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 smd roundrect (at 0.635 5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at 1.905 5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 3.175 5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at 4.445 5.0165 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model SMD_Packages.3dshapes/SO-16-W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:AVX_Card_Edge_5way_2mmPitch_0.8mmPCB (layer F.Cu) (tedit 5FFC2A91)
    (at 60 84)
    (fp_text reference J1 (at 0 7.2) (layer F.Fab) hide)
    (fp_text value Conn_01x05_Male (at 0 5.75) (layer F.Fab) hide)
    (pad 3 connect rect (at 0 2.9) (size 1 3) (layers F.Cu F.Mask)
      (net 8 ~RESET))
    (pad 2 connect rect (at -2 2.9) (size 1 3) (layers F.Cu F.Mask)
      (net 2 +3V3))
    (pad 1 connect rect (at -4 2.9) (size 1 3) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at 2 2.9) (size 1 3) (layers F.Cu F.Mask)
      (net 4 SDA-FRAM-RTC))
    (pad 5 connect rect (at 4 2.9) (size 1 3) (layers F.Cu F.Mask)
      (net 3 SCL-FRAM-RTC))
  )
  (module modules:R_SM_0805_2012Metric (layer B.Cu) (tedit 5ECAA518)
    (at 53.4 72.55 270)
    (descr "Resistor SMD 0805 (2012 Metric), rounded (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with pain !")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 4K7 (at -2.2 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 0.9 1.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 SDA-FRAM-RTC))
    (pad 1 smd roundrect (at -0.95 0 270) (size 0.9 1.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:R_SM_0805_2012Metric (layer B.Cu) (tedit 5ECAA518)
    (at 50.2 72.55 270)
    (descr "Resistor SMD 0805 (2012 Metric), rounded (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with pain !")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 4K7 (at -2.2 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 0.9 1.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 SCL-FRAM-RTC))
    (pad 1 smd roundrect (at -0.95 0 270) (size 0.9 1.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:C_0603_1608Metric_Pad1.0x1.1mm_HandSolder (layer B.Cu) (tedit 5F91AF13)
    (at 57.4 72.55 270)
    (descr "Capacitor SMD 0603 (1608 Metric), rounded (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 100N (at -2.2 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.95 1.1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.95 1.1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:MPD_BHSD-1225-SM locked (layer F.Cu) (tedit 5FFC5984)
    (at 60 76.35 180)
    (fp_text reference BT1 (at 11.25 5.5 180) (layer F.SilkS) hide)
    (fp_text value 1225 (at -12 4.6 270) (layer F.SilkS))
    (pad 1 smd roundrect (at -10.8 0 180) (size 3.5 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(BT1-Pad1)"))
    (pad 2 smd roundrect (at 10.8 0 180) (size 3.5 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 47.4 82.35)
    (fp_text reference v5 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 63.2 75.75)
    (fp_text reference v4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 69.2 82.15)
    (fp_text reference v3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 72.4 82.15)
    (fp_text reference v2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 56 74.95)
    (fp_text reference v1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 55.8 70.75)
    (fp_text reference v6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 69 70.75)
    (fp_text reference v7 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 48 72.5)
    (fp_text reference v8 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 52.6 75.35)
    (fp_text reference v9 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:GND_PLANE_VIA (layer F.Cu) (tedit 5EA4652C)
    (at 63.6 79.35)
    (fp_text reference v10 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value gnd_via (at 0 -0.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.889 0.889) (drill 0.508) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module modules:SO-8 (layer B.Cu) (tedit 5FFC626F)
    (at 64.0975 78.797 90)
    (fp_text reference U1 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value DS3231MZ (at 0.047 4.7025 90) (layer B.SilkS))
    (fp_text user 1 (at -2.7 -2.9 90) (layer B.SilkS))
    (pad 8 smd roundrect (at -1.905 2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 SCL-FRAM-RTC))
    (pad 7 smd roundrect (at -0.635 2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 SDA-FRAM-RTC))
    (pad 6 smd roundrect (at 0.635 2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(BT1-Pad1)"))
    (pad 5 smd roundrect (at 1.905 2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at 1.905 -2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 ~RESET))
    (pad 3 smd roundrect (at 0.635 -2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad3)"))
    (pad 2 smd roundrect (at -0.635 -2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 1 smd rect (at -1.905 -2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U1-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module modules:SO-8 (layer B.Cu) (tedit 5FFC626F)
    (at 51.715 78.7335 90)
    (fp_text reference U2 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value MB85RC256V (at 0 -0.889 90) (layer B.SilkS) hide)
    (fp_text user 1 (at -2.7 -2.9 90) (layer B.SilkS))
    (pad 8 smd roundrect (at -1.905 2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 7 smd roundrect (at -0.635 2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 0.635 2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 SCL-FRAM-RTC))
    (pad 5 smd roundrect (at 1.905 2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 SDA-FRAM-RTC))
    (pad 4 smd roundrect (at 1.905 -2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0.635 -2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.635 -2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd rect (at -1.905 -2.921 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module modules:EIAJ-SOIC-8 (layer B.Cu) (tedit 5FFC5D45)
    (at 52.731 78.7335 90)
    (fp_text reference U4 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value FM24W256G (at -0.0165 -5.731 90) (layer B.SilkS))
    (fp_text user 1 (at -2.7 -3.9 90) (layer B.SilkS))
    (pad 8 smd roundrect (at -1.905 3.937 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 7 smd roundrect (at -0.635 3.937 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 0.635 3.937 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 SCL-FRAM-RTC))
    (pad 5 smd roundrect (at 1.905 3.937 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 SDA-FRAM-RTC))
    (pad 4 smd roundrect (at 1.905 -3.937 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0.635 -3.937 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.635 -3.937 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd rect (at -1.905 -3.937 90) (size 0.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_line (start 54.55 83.75) (end 46 83.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 65.45 83.75) (end 74 83.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 10.9 (width 0.2) (layer Cmts.User)
    (gr_text "10.900 mm" (at 60 92.55) (layer Cmts.User))
    (feature1 (pts (xy 65.45 88.75) (xy 65.45 93.35)))
    (feature2 (pts (xy 54.55 88.75) (xy 54.55 93.35)))
    (crossbar (pts (xy 54.55 91.75) (xy 65.45 91.75)))
    (arrow1a (pts (xy 65.45 91.75) (xy 64.323496 92.336421)))
    (arrow1b (pts (xy 65.45 91.75) (xy 64.323496 91.163579)))
    (arrow2a (pts (xy 54.55 91.75) (xy 55.676504 92.336421)))
    (arrow2b (pts (xy 54.55 91.75) (xy 55.676504 91.163579)))
  )
  (gr_line (start 54.55 88.75) (end 65.45 88.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 10.8 (width 0.2) (layer Cmts.User)
    (gr_text "10.800 mm" (at 60 82.25) (layer Cmts.User))
    (feature1 (pts (xy 65.4 83.75) (xy 65.4 81.45)))
    (feature2 (pts (xy 54.6 83.75) (xy 54.6 81.45)))
    (crossbar (pts (xy 54.6 83.05) (xy 65.4 83.05)))
    (arrow1a (pts (xy 65.4 83.05) (xy 64.273496 83.636421)))
    (arrow1b (pts (xy 65.4 83.05) (xy 64.273496 82.463579)))
    (arrow2a (pts (xy 54.6 83.05) (xy 55.726504 83.636421)))
    (arrow2b (pts (xy 54.6 83.05) (xy 55.726504 82.463579)))
  )
  (gr_line (start 54.55 83.75) (end 54.55 88.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 65.45 83.75) (end 65.45 88.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 19.75 (width 0.2) (layer Cmts.User)
    (gr_text "19.750 mm" (at 78.8 78.875 270) (layer Cmts.User))
    (feature1 (pts (xy 74.5 88.75) (xy 79.6 88.75)))
    (feature2 (pts (xy 74.5 69) (xy 79.6 69)))
    (crossbar (pts (xy 78 69) (xy 78 88.75)))
    (arrow1a (pts (xy 78 88.75) (xy 77.413579 87.623496)))
    (arrow1b (pts (xy 78 88.75) (xy 78.586421 87.623496)))
    (arrow2a (pts (xy 78 69) (xy 77.413579 70.126504)))
    (arrow2b (pts (xy 78 69) (xy 78.586421 70.126504)))
  )
  (gr_line (start 46 69) (end 46 83.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74 69) (end 74 83.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 46 69) (end 74 69) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "GND 3V3 RSN SDA SCL" (at 59.9 84.35) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.19)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 45.25 69) (xy 74.75 69) (xy 74.75 83.75) (xy 45.25 83.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.19)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 44.75 69) (xy 75.25 69) (xy 75.25 83.75) (xy 44.75 83.75)
      )
    )
  )
)
