(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.2)
    (pcbplotparams
      (layerselection 0x0000030_80000001)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/VTref")
  (net 2 "unconnected-(J1-Pad2)")
  (net 3 "unconnected-(J1-Pad3)")
  (net 4 "/GND")
  (net 5 "/TX (out)")
  (net 6 "/SWDIO")
  (net 7 "/SWCLK")
  (net 8 "unconnected-(J1-Pad11)")
  (net 9 "/SWO")
  (net 10 "unconnected-(J1-Pad14)")
  (net 11 "/nRST")
  (net 12 "unconnected-(J1-Pad16)")
  (net 13 "/Rx (in)")
  (net 14 "unconnected-(J1-Pad18)")
  (net 15 "/5V")
  (net 16 "unconnected-(J1-Pad20)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 139.7 104.145)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "arm-cortex-stm32-adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -3.175 24.125) (layer "F.SilkS"))
    (fp_text value "Conn_01x10" (at -1.27 26.665) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 11.43 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/VTref") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/nRST") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/SWCLK") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/SWDIO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/SWO") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/Rx (in)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/TX (out)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/5V") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pin_Headers:Pin_Header_Straight_2x10_Pitch2.54mm" (layer "B.Cu")
    (tedit 5AA6543C)
    (at 129.54 104.14 180)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (property "Sheetfile" "arm-cortex-stm32-adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 3.81 180) (layer "B.SilkS"))
    (fp_text value "CONN_02X10" (at 1.27 -26.67 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -11.43 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/VTref") (pinfunction "P1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(J1-Pad2)") (pinfunction "P2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval locked (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J1-Pad3)") (pinfunction "P3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval locked (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/GND") (pinfunction "P4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/TX (out)") (pinfunction "P5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/GND") (pinfunction "P6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/SWDIO") (pinfunction "P7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/GND") (pinfunction "P8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/SWCLK") (pinfunction "P9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/GND") (pinfunction "P10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J1-Pad11)") (pinfunction "P11") (pintype "passive+no_connect"))
    (pad "12" thru_hole oval locked (at 2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/GND") (pinfunction "P12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/SWO") (pinfunction "P13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J1-Pad14)") (pinfunction "P14") (pintype "passive+no_connect"))
    (pad "15" thru_hole oval locked (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/nRST") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J1-Pad16)") (pinfunction "P16") (pintype "passive+no_connect"))
    (pad "17" thru_hole oval locked (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/Rx (in)") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at 2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J1-Pad18)") (pinfunction "P18") (pintype "passive+no_connect"))
    (pad "19" thru_hole oval locked (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/5V") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at 2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J1-Pad20)") (pinfunction "P20") (pintype "passive+no_connect"))
    (model "${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x10_Pitch2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 124.46 129.54) (end 124.46 101.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 142.24 129.54) (end 124.46 129.54) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 124.46 101.6) (end 142.24 101.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 142.24 101.6) (end 142.24 129.54) (layer "Edge.Cuts") (width 0.15))
  (gr_text "VTref" (at 134.62 106.68) (layer "F.SilkS"))
  (gr_text "RX(in)" (at 134.62 119.38) (layer "F.SilkS"))
  (gr_text "SWCLK" (at 134.62 111.76) (layer "F.SilkS"))
  (gr_text "TX(out)" (at 134.62 121.92) (layer "F.SilkS"))
  (gr_text "SWDIO" (at 134.62 114.3) (layer "F.SilkS"))
  (gr_text "GND" (at 134.62 104.14) (layer "F.SilkS"))
  (gr_text "GND" (at 134.62 124.46) (layer "F.SilkS"))
  (gr_text "nRST" (at 134.62 109.22) (layer "F.SilkS"))
  (gr_text "5V" (at 134.62 127) (layer "F.SilkS"))
  (gr_text "SWO" (at 134.62 116.84) (layer "F.SilkS"))
  (zone (net 4) (net_name "/GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 129.54)
        (xy 124.46 129.54)
        (xy 124.46 101.6)
        (xy 142.875 101.6)
      )
    )
  )
)
