(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 98)
    (zones 0)
    (modules 7)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 2.5)
    (user_trace_width 2.5)
    (user_trace_width 8.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4 0.3)
    (user_via 4 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "Ceci est la Netclass par défaut."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class fil1 ""
    (clearance 0.2)
    (trace_width 8)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 31.5 34.5)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference pad2 (at 0 -2.148) (layer F.SilkS) hide)
    (fp_text value TestPoint_Pad_2.5x2.5mm (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask))
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 31.5 37.5)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference pad3 (at 0 -2.148) (layer F.SilkS) hide)
    (fp_text value TestPoint_Pad_2.5x2.5mm (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask))
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 63.5 31.5)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference pad11 (at 0 -2.148) (layer F.SilkS) hide)
    (fp_text value TestPoint_Pad_2.5x2.5mm (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask))
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 63.5 34.5)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference pad12 (at 0 -2.148) (layer F.SilkS) hide)
    (fp_text value TestPoint_Pad_2.5x2.5mm (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask))
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 63.5 37.5)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference pad13 (at 0 -2.148) (layer F.SilkS) hide)
    (fp_text value TestPoint_Pad_2.5x2.5mm (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask))
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 31.5 31.5)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference pad1 (at 0 -2.148) (layer F.SilkS) hide)
    (fp_text value TestPoint_Pad_2.5x2.5mm (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask))
  )
  (module Pictures:logo (layer F.Cu) (tedit 0)
    (at 40.5 34.4)
    (fp_text reference G*** (at -1.4 -8.2) (layer F.SilkS) hide)
    (fp_text value "fatoms logo" (at 3.3 -6.1) (layer F.SilkS) hide)
  )
  (gr_text "Fatom's\nRaceWires" (at 52.2 36) (layer F.SilkS))
  (gr_line (start 30 39) (end 30 30) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 65 39) (end 30 39) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 65 30) (end 65 39) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30 30) (end 65 30) (layer Edge.Cuts) (width 0.1))
)
