<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="10.7825" y2="0" width="0" layer="20"/>
<wire x1="10.7825" y1="0" x2="10.7825" y2="10.15" width="0" layer="20"/>
<wire x1="10.7825" y1="10.15" x2="0" y2="10.15" width="0" layer="20"/>
<wire x1="0" y1="10.15" x2="0" y2="0" width="0" layer="20"/>
<text>(c)PDZ</text>
<text>not for resale!</text>
<text>SOT23-6 to DIL8</text>
</plain>
<libraries>
<library name="dummy">
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dummy" package="SOT23-6" value="SOT23-6(DUMMY)">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="ic-package" package="DIL08" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="6"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
