(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 32)
    (no_connects 0)
    (area 129.924999 49.924999 185.075001 60.075001)
    (thickness 1.6)
    (drawings 25)
    (tracks 77)
    (zones 0)
    (modules 18)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.17)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 1.7272)
    (pad_drill 1.00076)
    (pad_to_mask_clearance 0.102)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Batt_-)
  (net 2 +3V3)
  (net 3 "Net-(C2-Pad2)")
  (net 4 Reset)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 SWIM)
  (net 9 Batt_+)
  (net 10 D2)
  (net 11 Batt_Good)
  (net 12 Batt_Meh)
  (net 13 Batt_Low)
  (net 14 A4)
  (net 15 A5)
  (net 16 A6)
  (net 17 A1)
  (net 18 A2)
  (net 19 A3)
  (net 20 B5)
  (net 21 B4)
  (net 22 C3)
  (net 23 C4)
  (net 24 Batt_Read_Out)
  (net_class Default "This is the default net class."
    (clearance 0.17)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net B4)
    (add_net B5)
    (add_net Batt_+)
    (add_net Batt_-)
    (add_net Batt_Good)
    (add_net Batt_Low)
    (add_net Batt_Meh)
    (add_net Batt_Read_Out)
    (add_net C3)
    (add_net C4)
    (add_net D2)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net Reset)
    (add_net SWIM)
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_HandSoldering (layer F.Cu) (tedit 5AF13F68)
    (at 140.335 55.245 270)
    (descr "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (tags "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (attr smd)
    (fp_text reference C1 (at 7.493 -1.397 270) (layer F.SilkS))
    (fp_text value 10u (at 7.493 0 270) (layer F.Fab))
    (fp_text user + (at -4.59994 -1.80086 270) (layer F.SilkS))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.99974 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 Batt_-))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.99974 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AF13FAA)
    (at 149.098 56.261)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -1.905 -7.112) (layer F.SilkS))
    (fp_text value 1u (at 3.048 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 Batt_-))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AF13FB8)
    (at 149.098 58.928 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 100n (at 3.937 -0.381 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 Batt_-))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AF13F96)
    (at 149.098 53.594 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.302 -7.493 180) (layer F.SilkS))
    (fp_text value 100n (at -3.048 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 Reset))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 Batt_-))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5AF13F1B)
    (at 163.195 58.674 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at -3.81 1.905 90) (layer F.SilkS))
    (fp_text value Charged (at -2.794 -1.016 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 2 1.7272) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 Batt_-))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5AF13F22)
    (at 167.386 58.674 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at -3.937 2.286 90) (layer F.SilkS))
    (fp_text value Meh (at -2.794 0.381 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 2 1.7272) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 Batt_-))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5AF13F25)
    (at 171.577 58.674 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value Low (at -2.794 0.762 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 2 1.7272) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 Batt_-))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer B.Cu) (tedit 5AF0B9D9)
    (at 144.78 57.531)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.413 -5.461 90) (layer B.SilkS))
    (fp_text value Boost (at -2.413 0 90) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 Batt_+))
    (pad 2 thru_hole oval (at 0 -2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 Batt_-))
    (pad 3 thru_hole oval (at 0 -5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AF13FB2)
    (at 149.098 51.054)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value RAin (at -3.81 -0.381) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 Batt_+))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 D2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AF13F32)
    (at 164.338 53.848 315)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.334867 -7.184205 315) (layer F.SilkS))
    (fp_text value RLED (at -5.208549 -5.388154 315) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 315) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 Batt_Good))
    (pad 2 smd rect (at 1.35 0 315) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AF13F2E)
    (at 168.529 53.848 315)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.592102 -5.747364 315) (layer F.SilkS))
    (fp_text value RLED (at -5.477956 -5.118746 315) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 315) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 Batt_Meh))
    (pad 2 smd rect (at 1.35 0 315) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AF13F2B)
    (at 172.72 53.848 315)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.053287 -5.926969 315) (layer F.SilkS))
    (fp_text value RLED (at -5.298351 -5.298351 315) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 315) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 Batt_Low))
    (pad 2 smd rect (at 1.35 0 315) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 5AF13F0D)
    (at 156.464 54.102)
    (descr "SSOP20: plastic shrink small outline package; 20 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot266-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0.381 -7.874) (layer F.SilkS))
    (fp_text value STM8S003F (at 0 -6.731 180) (layer F.Fab))
    (pad 1 smd rect (at -2.9 -2.925) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 A4))
    (pad 2 smd rect (at -2.9 -2.275) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 A5))
    (pad 3 smd rect (at -2.9 -1.625) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 A6))
    (pad 4 smd rect (at -2.9 -0.975) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 Reset))
    (pad 5 smd rect (at -2.9 -0.325) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 A1))
    (pad 6 smd rect (at -2.9 0.325) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 A2))
    (pad 7 smd rect (at -2.9 0.975) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 Batt_-))
    (pad 8 smd rect (at -2.9 1.625) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 9 smd rect (at -2.9 2.275) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 10 smd rect (at -2.9 2.925) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 A3))
    (pad 11 smd rect (at 2.9 2.925) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 B5))
    (pad 12 smd rect (at 2.9 2.275) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 B4))
    (pad 13 smd rect (at 2.9 1.625) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 C3))
    (pad 14 smd rect (at 2.9 0.975) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 C4))
    (pad 15 smd rect (at 2.9 0.325) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 Batt_Read_Out))
    (pad 16 smd rect (at 2.9 -0.325) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 Batt_Good))
    (pad 17 smd rect (at 2.9 -0.975) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 Batt_Meh))
    (pad 18 smd rect (at 2.9 -1.625) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 SWIM))
    (pad 19 smd rect (at 2.9 -2.275) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 D2))
    (pad 20 smd rect (at 2.9 -2.925) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 Batt_Low))
    (model Housings_SSOP.3dshapes/SSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5AF13F5D)
    (at 135.255 55.245)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 8.255) (layer F.SilkS))
    (fp_text value B+ (at -3.429 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 Batt_+))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5AF13F40)
    (at 179.705 55.245)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 5.461 -5.461) (layer F.SilkS))
    (fp_text value B- (at 2.921 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 Batt_-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 176.149 58.801 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value Prog (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 Batt_-))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 Reset))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 SWIM))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5AF13F20)
    (at 160.274 58.928 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 3.048 -3.048 270) (layer F.SilkS))
    (fp_text value I2C (at 3.937 0.254 360) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 Batt_-))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 B4))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 B5))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_footprints:1x1_pad (layer B.Cu) (tedit 5AF13F34)
    (at 164.719 52.07)
    (fp_text reference P7 (at 0.635 -4.572) (layer B.SilkS))
    (fp_text value BROut (at -0.254 -3.81) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 24 Batt_Read_Out))
  )
  (gr_text + (at 171.577 54.61) (layer F.SilkS))
  (gr_text + (at 167.386 54.61) (layer F.SilkS))
  (gr_text + (at 163.195 54.61) (layer F.SilkS))
  (gr_text - (at 164.973 59.055) (layer F.SilkS))
  (gr_text - (at 169.164 59.055) (layer F.SilkS))
  (gr_text - (at 173.355 59.055) (layer F.SilkS))
  (gr_text 1 (at 152.273 50.927) (layer F.SilkS))
  (gr_text GND (at 179.451 59.182) (layer B.SilkS))
  (gr_text 3.3V (at 179.578 57.658) (layer B.SilkS))
  (gr_text Reset (at 180.086 52.705) (layer B.SilkS))
  (gr_text SWIM (at 179.705 51.054) (layer B.SilkS))
  (gr_text GND (at 159.893 56.007 90) (layer B.SilkS))
  (gr_text "3.3V\n" (at 157.861 55.88 90) (layer B.SilkS))
  (gr_text SCL (at 155.448 56.134 90) (layer B.SilkS))
  (gr_text SDA (at 152.654 56.134 90) (layer B.SilkS))
  (gr_text Stat (at 167.005 52.07) (layer B.SilkS))
  (gr_text <2Vin (at 149.098 57.404) (layer B.SilkS))
  (gr_text GND (at 148.844 54.864) (layer B.SilkS))
  (gr_text 3.3Vout (at 149.479 52.451) (layer B.SilkS))
  (gr_line (start 180 60) (end 135 60) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135 50) (end 180 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 180 55) (end 180 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 180 55) (end 185 55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 135 55) (end 130 55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 135 55) (end 135 60) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name Batt_-) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 128.905 48.895) (xy 186.055 48.895) (xy 186.055 61.595) (xy 128.905 61.595) (xy 128.905 60.325)
      )
    )
  )
  (zone (net 1) (net_name Batt_-) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 128.27 48.26) (xy 186.69 48.26) (xy 186.69 62.23) (xy 128.27 62.23)
      )
    )
  )
)
