(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 16)
    (no_connects 0)
    (area 108.509999 100.254999 188.035001 112.470001)
    (thickness 1.6)
    (drawings 9)
    (tracks 39)
    (zones 0)
    (modules 5)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.608)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 dt-up)
  (net 3 sck-up)
  (net 4 +3V3)
  (net 5 dt-left)
  (net 6 sck-left)
  (net 7 dt-down)
  (net 8 sck-down)
  (net 9 dt-right)
  (net 10 sck-right)
  (net 11 "Net-(A1-Pad21)")
  (net 12 "Net-(A1-Pad22)")
  (net 13 "Net-(A1-Pad23)")
  (net 14 "Net-(A1-Pad24)")
  (net 15 "Net-(A1-Pad25)")
  (net 16 "Net-(A1-Pad34)")
  (net 17 "Net-(A1-Pad35)")
  (net 18 "Net-(A1-Pad36)")
  (net 19 "Net-(A1-Pad37)")
  (net 20 "Net-(A1-Pad38)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class thic ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.7)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad34)")
    (add_net "Net-(A1-Pad35)")
    (add_net "Net-(A1-Pad36)")
    (add_net "Net-(A1-Pad37)")
    (add_net "Net-(A1-Pad38)")
    (add_net dt-down)
    (add_net dt-left)
    (add_net dt-right)
    (add_net dt-up)
    (add_net sck-down)
    (add_net sck-left)
    (add_net sck-right)
    (add_net sck-up)
  )
  (module module-hx711:conn-hx711-out (layer F.Cu) (tedit 5B08F756)
    (at 179.07 109.22 135)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 135) (layer F.SilkS))
    (fp_text value conn-right (at -3.14309 4.041115 225) (layer F.Fab))
    (fp_text user %R (at 0 3.81 225) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 135) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 135) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 dt-right))
    (pad 3 thru_hole oval (at 0 5.08 135) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 sck-right))
    (pad 4 thru_hole oval (at 0 7.62 135) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module module-hx711:conn-hx711-out (layer F.Cu) (tedit 5B08F762)
    (at 111.76 103.505 45)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 45) (layer F.SilkS))
    (fp_text value conn-up (at -2.694077 4.490128 135) (layer F.Fab))
    (fp_text user %R (at 0 3.81 135) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 45) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 45) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 dt-up))
    (pad 3 thru_hole oval (at 0 5.08 45) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 sck-up))
    (pad 4 thru_hole oval (at 0 7.62 45) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module maple-mini-clone:Pin_Header_Straight_1x20_Pitch2.54mm (layer F.Cu) (tedit 5B08F63B)
    (at 123.825 103.505 90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "" (at 0 50.59 90) (layer F.Fab))
    (fp_text user %R (at 0 24.13 180) (layer F.Fab))
    (pad 21 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad21)"))
    (pad 22 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad22)"))
    (pad 23 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad23)"))
    (pad 24 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad24)"))
    (pad 25 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad25)"))
    (pad 26 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 dt-up))
    (pad 27 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 sck-up))
    (pad 28 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 dt-left))
    (pad 29 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 sck-left))
    (pad 30 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 dt-down))
    (pad 31 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 sck-down))
    (pad 32 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 dt-right))
    (pad 33 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 sck-right))
    (pad 34 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad34)"))
    (pad 35 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad35)"))
    (pad 36 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad36)"))
    (pad 37 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad37)"))
    (pad 38 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad38)"))
    (pad 39 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module module-hx711:conn-hx711-out (layer F.Cu) (tedit 5B08F769)
    (at 132.715 110.49 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value conn-left (at 3.175 3.81 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 dt-left))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 sck-left))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module module-hx711:conn-hx711-out (layer F.Cu) (tedit 5B08F76F)
    (at 156.21 110.49 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value conn-down (at 3.175 3.81 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 dt-down))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 sck-down))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 185.42 102.87) (end 185.42 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 111.125 102.87) (end 108.585 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 111.125 109.855) (end 111.125 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 185.42 109.855) (end 187.96 109.855) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.585 103.505) (end 108.585 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.585 109.855) (end 108.585 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.42 112.395) (end 111.125 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 102.87) (end 187.96 109.855) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.125 100.33) (end 185.42 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.608))
    (min_thickness 0.154)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 108.712 102.87) (xy 108.712 101.854) (xy 110.236 100.584) (xy 111.252 100.33) (xy 185.42 100.33)
        (xy 186.944 100.838) (xy 187.706 102.108) (xy 187.96 102.616) (xy 187.96 109.728) (xy 187.706 111.252)
        (xy 186.944 111.76) (xy 186.182 112.268) (xy 185.42 112.268) (xy 110.998 112.268) (xy 109.728 112.014)
        (xy 109.22 111.252) (xy 108.712 110.236) (xy 108.712 102.616)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.608))
    (min_thickness 0.154)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 100.33) (xy 185.42 100.33) (xy 186.69 100.838) (xy 187.452 101.346) (xy 187.706 101.854)
        (xy 187.96 102.616) (xy 187.96 110.236) (xy 187.706 111.252) (xy 186.944 111.76) (xy 186.69 112.014)
        (xy 186.182 112.268) (xy 185.674 112.268) (xy 110.744 112.268) (xy 110.236 112.014) (xy 109.728 111.76)
        (xy 109.22 111.252) (xy 108.712 110.744) (xy 108.458 109.982) (xy 108.712 102.108) (xy 109.22 101.092)
        (xy 109.982 100.584)
      )
    )
  )
)
