(kicad_pcb (version 4) (host pcbnew no-vcs-found-product)
  (general
    (links 134)
    (no_connects 0)
    (area 102.549999 80.189999 167.650001 110.290001)
    (thickness 1.6)
    (drawings 82)
    (tracks 560)
    (zones 0)
    (modules 40)
    (nets 75)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.01)
    (user_trace_width 0.02)
    (user_trace_width 0.05)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (trace_clearance 0.127)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.0127)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.1)
    (pad_size 2.75 2.75)
    (pad_drill 2.75)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 102.6 80.2)
    (visible_elements 7FFCFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory meta/))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad1)")
  (net 2 "Net-(J2-Pad3)")
  (net 3 "Net-(J2-Pad5)")
  (net 4 "Net-(J2-Pad7)")
  (net 5 "Net-(J2-Pad8)")
  (net 6 "Net-(J2-Pad10)")
  (net 7 "Net-(J2-Pad11)")
  (net 8 "Net-(J2-Pad13)")
  (net 9 "Net-(J2-Pad15)")
  (net 10 "Net-(J2-Pad17)")
  (net 11 "Net-(J2-Pad26)")
  (net 12 "Net-(J2-Pad27)")
  (net 13 "Net-(J2-Pad28)")
  (net 14 "Net-(J2-Pad29)")
  (net 15 "Net-(J2-Pad31)")
  (net 16 "Net-(J2-Pad32)")
  (net 17 "Net-(J2-Pad33)")
  (net 18 "Net-(J2-Pad36)")
  (net 19 "Net-(J2-Pad37)")
  (net 20 +5V)
  (net 21 GND)
  (net 22 +3V3)
  (net 23 +1V2)
  (net 24 "Net-(C403-Pad1)")
  (net 25 "Net-(C405-Pad1)")
  (net 26 GPIO23_CDN)
  (net 27 "Net-(D402-Pad2)")
  (net 28 "Net-(D402-Pad1)")
  (net 29 "Net-(D403-Pad2)")
  (net 30 "Net-(D403-Pad1)")
  (net 31 "Net-(D404-Pad2)")
  (net 32 "Net-(D404-Pad1)")
  (net 33 I2S_BCLK)
  (net 34 GPIO24_CRS)
  (net 35 SPI_MOSI)
  (net 36 SPI_MISO)
  (net 37 GPIO25_SS)
  (net 38 SPI_CLK)
  (net 39 SPI_CE0)
  (net 40 I2S_LRCK)
  (net 41 I2S_DI)
  (net 42 I2S_DO)
  (net 43 "Net-(P401-Pad1)")
  (net 44 "Net-(P401-Pad2)")
  (net 45 "Net-(P401-Pad3)")
  (net 46 "Net-(P401-Pad4)")
  (net 47 "Net-(P401-Pad5)")
  (net 48 "Net-(P401-Pad6)")
  (net 49 "Net-(P401-Pad7)")
  (net 50 "Net-(P401-Pad8)")
  (net 51 "Net-(P401-Pad11)")
  (net 52 "Net-(P403-Pad1)")
  (net 53 "Net-(P403-Pad2)")
  (net 54 "Net-(P403-Pad3)")
  (net 55 "Net-(P403-Pad4)")
  (net 56 "Net-(P403-Pad5)")
  (net 57 "Net-(P403-Pad6)")
  (net 58 "Net-(P403-Pad7)")
  (net 59 "Net-(P403-Pad8)")
  (net 60 "Net-(P403-Pad11)")
  (net 61 "Net-(P404-Pad1)")
  (net 62 "Net-(P404-Pad2)")
  (net 63 "Net-(P404-Pad3)")
  (net 64 "Net-(P404-Pad4)")
  (net 65 "Net-(P404-Pad5)")
  (net 66 "Net-(P404-Pad6)")
  (net 67 "Net-(P404-Pad7)")
  (net 68 "Net-(P404-Pad8)")
  (net 69 "Net-(P404-Pad11)")
  (net 70 "Net-(TP401-Pad1)")
  (net 71 "Net-(TP402-Pad1)")
  (net 72 "Net-(TP403-Pad1)")
  (net 73 "Net-(U301-Pad4)")
  (net 74 "Net-(U302-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GPIO23_CDN)
    (add_net GPIO24_CRS)
    (add_net GPIO25_SS)
    (add_net I2S_BCLK)
    (add_net I2S_DI)
    (add_net I2S_DO)
    (add_net I2S_LRCK)
    (add_net "Net-(C403-Pad1)")
    (add_net "Net-(C405-Pad1)")
    (add_net "Net-(D402-Pad1)")
    (add_net "Net-(D402-Pad2)")
    (add_net "Net-(D403-Pad1)")
    (add_net "Net-(D403-Pad2)")
    (add_net "Net-(D404-Pad1)")
    (add_net "Net-(D404-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad37)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(P401-Pad1)")
    (add_net "Net-(P401-Pad2)")
    (add_net "Net-(P401-Pad3)")
    (add_net "Net-(P401-Pad4)")
    (add_net "Net-(P401-Pad5)")
    (add_net "Net-(P401-Pad6)")
    (add_net "Net-(P401-Pad7)")
    (add_net "Net-(P401-Pad8)")
    (add_net "Net-(P403-Pad1)")
    (add_net "Net-(P403-Pad2)")
    (add_net "Net-(P403-Pad3)")
    (add_net "Net-(P403-Pad4)")
    (add_net "Net-(P403-Pad5)")
    (add_net "Net-(P403-Pad6)")
    (add_net "Net-(P403-Pad7)")
    (add_net "Net-(P403-Pad8)")
    (add_net "Net-(P404-Pad1)")
    (add_net "Net-(P404-Pad2)")
    (add_net "Net-(P404-Pad3)")
    (add_net "Net-(P404-Pad4)")
    (add_net "Net-(P404-Pad5)")
    (add_net "Net-(P404-Pad6)")
    (add_net "Net-(P404-Pad7)")
    (add_net "Net-(P404-Pad8)")
    (add_net "Net-(TP401-Pad1)")
    (add_net "Net-(TP402-Pad1)")
    (add_net "Net-(TP403-Pad1)")
    (add_net "Net-(U301-Pad4)")
    (add_net "Net-(U302-Pad4)")
    (add_net SPI_CE0)
    (add_net SPI_CLK)
    (add_net SPI_MISO)
    (add_net SPI_MOSI)
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V2)
    (add_net +3V3)
    (add_net GND)
  )
  (net_class Supply ""
    (clearance 0.127)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "Net-(P401-Pad11)")
    (add_net "Net-(P403-Pad11)")
    (add_net "Net-(P404-Pad11)")
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 164.1 83.74)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 57F94CD1)
    (at 164.1 106.74)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 57F94D2A)
    (at 106.1 106.74)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CA2)
    (at 106.1 83.74)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9C5E)
    (at 107.807 93.535 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C301 (at 0.0635 1.3335 270) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9C56)
    (at 107.807 89.217 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C302 (at -0.127 1.27 270) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57FA9C4A)
    (at 114.919 88.455)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at -0.0635 1.5875) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57FA9C0A)
    (at 114.919 92.773)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C304 (at 0.0635 -1.4605) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9C92)
    (at 139.684 89.471)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C401 (at 1.2065 -1.143) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9C8C)
    (at 138.033 87.7565)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at -2.2225 -0.8255) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9C74)
    (at 129.9685 98.361 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 1.0795 -1.143 270) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C403-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9C6B)
    (at 128.6985 95.948 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C404 (at 0.127 1.2065 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9CCA)
    (at 133.334 102.806 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C405 (at -0.3175 1.2065 270) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C405-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57FA9C19)
    (at 117.332 94.932)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C406 (at 0.381 1.524) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C405-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9CDE)
    (at 134.731 100.901 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C407 (at -0.381 1.2065 270) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57FA9CF3)
    (at 137.652 100.266)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C408 (at 0.4445 -1.0795) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FA9DCF)
    (at 152.765 90.614)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D401 (at -0.1905 1.3335) (layer F.SilkS))
    (fp_text value LED (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 26 GPIO23_CDN))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FA9DA8)
    (at 152.765 97.091)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D402 (at -0.0635 -2.286) (layer F.SilkS))
    (fp_text value LED (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D402-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D402-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FA9DB1)
    (at 152.765 98.996)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D403 (at -0.127 -3.302) (layer F.SilkS))
    (fp_text value LED (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D403-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D403-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FA9D9F)
    (at 152.765 100.901)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D404 (at -0.1905 1.4605) (layer F.SilkS))
    (fp_text value LED (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D404-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D404-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 574BBA57)
    (at 128.381 98.361 270)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D405 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value D (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C403-Pad1)"))
    (pad 2 smd rect (at 0.85 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
  )
  (module Pin_Headers:Pin_Header_Straight_2x06 (layer B.Cu) (tedit 57FBA9B8)
    (at 165.846 88.7725 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P401 (at 4.6355 -6.731 270) (layer B.SilkS))
    (fp_text value CONN_02X06 (at 0 3.1 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 43 "Net-(P401-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 44 "Net-(P401-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 45 "Net-(P401-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 46 "Net-(P401-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 47 "Net-(P401-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 48 "Net-(P401-Pad6)"))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 49 "Net-(P401-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 50 "Net-(P401-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 GND))
    (pad 10 thru_hole oval (at 2.54 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 GND))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 51 "Net-(P401-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 -12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 51 "Net-(P401-Pad11)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57FA9D2D)
    (at 159 99)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P402 (at -0.139 -2.0995) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(P401-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06 (layer B.Cu) (tedit 57FBA995)
    (at 132.08 108.521 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P403 (at 1.651 2.143 90) (layer B.SilkS))
    (fp_text value CONN_02X06 (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 52 "Net-(P403-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 53 "Net-(P403-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 54 "Net-(P403-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 55 "Net-(P403-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 56 "Net-(P403-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 57 "Net-(P403-Pad6)"))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 58 "Net-(P403-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 59 "Net-(P403-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 GND))
    (pad 10 thru_hole oval (at 2.54 -10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 GND))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 60 "Net-(P403-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 -12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 60 "Net-(P403-Pad11)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06 (layer B.Cu) (tedit 57FBA986)
    (at 154.94 108.521 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P404 (at 1.5875 2.143 90) (layer B.SilkS))
    (fp_text value CONN_02X06 (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 61 "Net-(P404-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 62 "Net-(P404-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 63 "Net-(P404-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 64 "Net-(P404-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 65 "Net-(P404-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 66 "Net-(P404-Pad6)"))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 67 "Net-(P404-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 68 "Net-(P404-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 GND))
    (pad 10 thru_hole oval (at 2.54 -10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 GND))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 69 "Net-(P404-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 -12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 69 "Net-(P404-Pad11)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57FA9CAA)
    (at 114.3 103.378)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P405 (at -0.016 -2.096 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P403-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57FA9CFD)
    (at 137.16 103.378)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P406 (at 0.0475 -2.0325) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P404-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FA9DC1)
    (at 155.94 88.963 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at 0.0635 1.2065 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 GPIO24_CRS))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FA9DC8)
    (at 155.94 90.5505 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R402 (at 0.0635 -1.397 180) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 GPIO23_CDN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FA9D75)
    (at 155.94 97.091 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R403 (at 0.127 2.2225 180) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D402-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FA9D81)
    (at 155.94 98.996 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R404 (at 0.1905 3.2385 180) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D403-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FA9D88)
    (at 155.94 100.901 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R405 (at 0.127 -1.3335 180) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D404-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57FA9C11)
    (at 114.284 94.805 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R406 (at -0.0635 -1.27 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C405-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 57FA9C41)
    (at 110.474 89.344)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U301 (at -0.0635 1.9685) (layer F.SilkS))
    (fp_text value MCP1802-3.3 (at -0.05 2.35) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U301-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 57FA9C36)
    (at 110.474 93.662)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U302 (at -0.0635 2.0955) (layer F.SilkS))
    (fp_text value MCP1802-1.2 (at -0.05 2.35) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U302-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 0)
    (at 120.761 89.09)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP401 (at 0 -1.26746) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(TP401-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 0)
    (at 120.761 92.011)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP402 (at 0 -1.26746) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(TP402-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 0)
    (at 120.761 94.805)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP403 (at 0 -1.26746) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(TP403-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module emeb:Pin_Header_Straight_2x20 locked (layer F.Cu) (tedit 57FA9F68)
    (at 135.1 83.74 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at -2.7465 -26.404 270) (layer F.SilkS))
    (fp_text value RPi_GPIO (at -1.27 -27.23 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 3 thru_hole oval (at -1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 5 thru_hole oval (at -1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GND))
    (pad 7 thru_hole oval (at -1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at -1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GND))
    (pad 10 thru_hole oval (at 1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at -1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 I2S_BCLK))
    (pad 13 thru_hole oval (at -1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GND))
    (pad 15 thru_hole oval (at -1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 GPIO23_CDN))
    (pad 17 thru_hole oval (at -1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 GPIO24_CRS))
    (pad 19 thru_hole oval (at -1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 SPI_MOSI))
    (pad 20 thru_hole oval (at 1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GND))
    (pad 21 thru_hole oval (at -1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 SPI_MISO))
    (pad 22 thru_hole oval (at 1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 GPIO25_SS))
    (pad 23 thru_hole oval (at -1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 SPI_CLK))
    (pad 24 thru_hole oval (at 1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 SPI_CE0))
    (pad 25 thru_hole oval (at -1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GND))
    (pad 26 thru_hole oval (at 1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J2-Pad26)"))
    (pad 27 thru_hole oval (at -1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J2-Pad27)"))
    (pad 28 thru_hole oval (at 1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J2-Pad28)"))
    (pad 29 thru_hole oval (at -1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad29)"))
    (pad 30 thru_hole oval (at 1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GND))
    (pad 31 thru_hole oval (at -1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad31)"))
    (pad 32 thru_hole oval (at 1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J2-Pad32)"))
    (pad 33 thru_hole oval (at -1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J2-Pad33)"))
    (pad 34 thru_hole oval (at 1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GND))
    (pad 35 thru_hole oval (at -1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 I2S_LRCK))
    (pad 36 thru_hole oval (at 1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J2-Pad36)"))
    (pad 37 thru_hole oval (at -1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J2-Pad37)"))
    (pad 38 thru_hole oval (at 1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 I2S_DI))
    (pad 39 thru_hole oval (at -1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GND))
    (pad 40 thru_hole oval (at 1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 I2S_DO))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module emeb:QFN-48-1EP_7x7mm_Pitch0.5mm_DIY_PADS (layer F.Cu) (tedit 57FC3DE6)
    (at 135.4 94.2 270)
    (descr "UK Package; 48-Lead Plastic QFN (7mm x 7mm); (see Linear Technology QFN_48_05-08-1704.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U401 (at 0 -4.75 270) (layer F.SilkS))
    (fp_text value ice5lp4k_sg48 (at 0 4.75 270) (layer F.Fab))
    (pad 1 smd rect (at -3.55 -2.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 2 smd rect (at -3.55 -2.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(P401-Pad2)"))
    (pad 3 smd rect (at -3.55 -1.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P401-Pad1)"))
    (pad 4 smd rect (at -3.55 -1.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(TP401-Pad1)"))
    (pad 5 smd rect (at -3.55 -0.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (pad 6 smd rect (at -3.55 -0.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(TP402-Pad1)"))
    (pad 7 smd rect (at -3.55 0.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GPIO23_CDN))
    (pad 8 smd rect (at -3.55 0.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 GPIO24_CRS))
    (pad 9 smd rect (at -3.55 1.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 I2S_LRCK))
    (pad 10 smd rect (at -3.55 1.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 I2S_BCLK))
    (pad 11 smd rect (at -3.55 2.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 I2S_DI))
    (pad 12 smd rect (at -3.55 2.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 I2S_DO))
    (pad 13 smd rect (at -2.75 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 SPI_CE0))
    (pad 14 smd rect (at -2.25 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 SPI_MISO))
    (pad 15 smd rect (at -1.75 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 SPI_CLK))
    (pad 16 smd rect (at -1.25 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 GPIO25_SS))
    (pad 17 smd rect (at -0.75 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 SPI_MOSI))
    (pad 18 smd rect (at -0.25 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(TP403-Pad1)"))
    (pad 19 smd rect (at 0.25 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(P403-Pad7)"))
    (pad 20 smd rect (at 0.75 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(P403-Pad8)"))
    (pad 21 smd rect (at 1.25 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(P403-Pad5)"))
    (pad 22 smd rect (at 1.75 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 23 smd rect (at 2.25 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(P403-Pad6)"))
    (pad 24 smd rect (at 2.75 3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C403-Pad1)"))
    (pad 25 smd rect (at 3.55 2.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(P403-Pad3)"))
    (pad 26 smd rect (at 3.55 2.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(P403-Pad4)"))
    (pad 27 smd rect (at 3.55 1.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(P403-Pad1)"))
    (pad 28 smd rect (at 3.55 1.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(P403-Pad2)"))
    (pad 29 smd rect (at 3.55 0.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C405-Pad1)"))
    (pad 30 smd rect (at 3.55 0.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 +1V2))
    (pad 31 smd rect (at 3.55 -0.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(P404-Pad7)"))
    (pad 32 smd rect (at 3.55 -0.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(P404-Pad8)"))
    (pad 33 smd rect (at 3.55 -1.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 34 smd rect (at 3.55 -1.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(P404-Pad5)"))
    (pad 35 smd rect (at 3.55 -2.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(P404-Pad6)"))
    (pad 36 smd rect (at 3.55 -2.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(P404-Pad3)"))
    (pad 37 smd rect (at 2.75 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(P404-Pad4)"))
    (pad 38 smd rect (at 2.25 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(P404-Pad1)"))
    (pad 39 smd rect (at 1.75 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D404-Pad1)"))
    (pad 40 smd rect (at 1.25 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D403-Pad1)"))
    (pad 41 smd rect (at 0.75 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D402-Pad1)"))
    (pad 42 smd rect (at 0.25 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(P404-Pad2)"))
    (pad 43 smd rect (at -0.25 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(P401-Pad8)"))
    (pad 44 smd rect (at -0.75 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(P401-Pad7)"))
    (pad 45 smd rect (at -1.25 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(P401-Pad6)"))
    (pad 46 smd rect (at -1.75 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P401-Pad5)"))
    (pad 47 smd rect (at -2.25 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P401-Pad4)"))
    (pad 48 smd rect (at -2.75 -3.55) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(P401-Pad3)"))
    (pad 49 smd rect (at 1.93125 1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -0.64375 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -1.93125 270) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 21 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text p18,31b (at 124.6345 94.805) (layer F.SilkS))
  (gr_text p6,13b (at 124.1265 91.9475) (layer F.SilkS))
  (gr_text p4,8a (at 123.682 89.1535) (layer F.SilkS))
  (gr_text Recept (at 128.9525 103.949) (layer F.SilkS))
  (gr_text Recept (at 153.273 103.949) (layer F.SilkS))
  (gr_text Recept (at 160.1945 89.471) (layer F.SilkS))
  (gr_text P401 (at 160.5755 88.709) (layer F.SilkS))
  (gr_text P403 (at 131.556 103.949) (layer F.SilkS))
  (gr_text P404 (at 155.6225 103.949) (layer F.SilkS))
  (gr_text "1 p27,38b 2 p28,41a\n3 p25,36b 4 p26,39a\n5 p21,23b 6 p23,37a\n7 p19,29b 8 p20,25b" (at 133.334 100.2025) (layer B.SilkS))
  (gr_text "1 p38,50b 2 p42,51a\n3 p36,48b 4 p37,45a\n5 p34,44b 6 p35,46b\n7 p31,42b 8 p32,43a" (at 156.3845 100.2025) (layer B.SilkS))
  (gr_text "1 p3,9b   2 p2,6a\n3 p48,4a  4 p47,2a\n5 p46,0a  6 p45,5a\n7 p44,3b  8 p43,49a" (at 161.02 91.0585) (layer B.SilkS))
  (gr_text 3v3 (at 161.3375 99.758 90) (layer F.SilkS))
  (gr_text 5v0 (at 161.3375 102.933 90) (layer F.SilkS))
  (gr_text 5v0 (at 134.858 107.505 90) (layer F.SilkS))
  (gr_text 3v3 (at 134.858 104.6475 90) (layer F.SilkS))
  (gr_text "icehat v0.1\n(c) 2016 E. Brombaugh" (at 113.522 98.6785) (layer F.SilkS))
  (gr_text 5v0 (at 111.998 107.4415 90) (layer F.SilkS))
  (gr_text 3v3 (at 112.0615 104.3935 90) (layer F.SilkS))
  (gr_text RGB2 (at 148.8915 100.8375) (layer F.SilkS))
  (gr_text RGB1 (at 148.8915 98.996) (layer F.SilkS))
  (gr_text RGB0 (at 148.8915 97.091) (layer F.SilkS))
  (gr_text DONE (at 148.1295 90.5505) (layer F.SilkS))
  (dimension 30.000167 (width 0.15) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 96.202054 95.218493 270.1909852) (layer Dwgs.User))
    (feature1 (pts (xy 101.8 110.2) (xy 94.902062 110.222993)))
    (feature2 (pts (xy 101.7 80.2) (xy 94.802062 80.222993)))
    (crossbar (pts (xy 97.502047 80.213993) (xy 97.602047 110.213993)))
    (arrow1a (pts (xy 97.602047 110.213993) (xy 97.011875 109.08945)))
    (arrow1b (pts (xy 97.602047 110.213993) (xy 98.184709 109.085541)))
    (arrow2a (pts (xy 97.502047 80.213993) (xy 96.919385 81.342445)))
    (arrow2b (pts (xy 97.502047 80.213993) (xy 98.092219 81.338536)))
  )
  (gr_arc (start 164.6 83.24) (end 164.6 80.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.6 80.24) (end 164.6 80.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.6 83.24) (end 102.6 83.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 58 (width 0.15) (layer Dwgs.User)
    (gr_text "58 mm" (at 135.1 74.89) (layer Dwgs.User))
    (feature1 (pts (xy 164.1 78.74) (xy 164.1 73.54)))
    (feature2 (pts (xy 106.1 78.74) (xy 106.1 73.54)))
    (crossbar (pts (xy 106.1 76.24) (xy 164.1 76.24)))
    (arrow1a (pts (xy 164.1 76.24) (xy 162.973496 76.826421)))
    (arrow1b (pts (xy 164.1 76.24) (xy 162.973496 75.653579)))
    (arrow2a (pts (xy 106.1 76.24) (xy 107.226504 76.826421)))
    (arrow2b (pts (xy 106.1 76.24) (xy 107.226504 75.653579)))
  )
  (dimension 65 (width 0.15) (layer Dwgs.User)
    (gr_text "65 mm" (at 135.1 70.39) (layer Dwgs.User))
    (feature1 (pts (xy 167.6 78.74) (xy 167.6 69.04)))
    (feature2 (pts (xy 102.6 78.74) (xy 102.6 69.04)))
    (crossbar (pts (xy 102.6 71.74) (xy 167.6 71.74)))
    (arrow1a (pts (xy 167.6 71.74) (xy 166.473496 72.326421)))
    (arrow1b (pts (xy 167.6 71.74) (xy 166.473496 71.153579)))
    (arrow2a (pts (xy 102.6 71.74) (xy 103.726504 72.326421)))
    (arrow2b (pts (xy 102.6 71.74) (xy 103.726504 71.153579)))
  )
  (gr_arc (start 164.6 107.24) (end 167.6 107.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.6 107.24) (end 105.6 110.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.6 82.74) (end 102.6 107.24) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.6 110.24) (end 164.6 110.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.6 82.74) (end 167.6 107.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 21) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 161.274 86.804) (xy 166.735 86.804) (xy 166.735 103.568) (xy 161.02 103.568) (xy 161.02 109.41)
        (xy 108.95 109.41) (xy 109.077 103.568) (xy 103.616 103.568) (xy 103.616 86.804) (xy 109.204 86.804)
        (xy 109.204 81.216) (xy 161.274 81.216) (xy 161.274 86.804)
      )
    )
  )
  (zone (net 22) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 161.274 104.838) (xy 112.506 104.838) (xy 112.506 86.804) (xy 161.274 86.804)
      )
    )
  )
)
