(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(J1-VDD)")
	(net 3 "Net-(J1-PGC{slash}ICSPCLK)")
	(net 4 "/TONE")
	(net 5 "Net-(J1-~{MCLR}{slash}VPP)")
	(net 6 "Net-(J2-Pin_1)")
	(net 7 "/TO-LS1")
	(net 8 "Net-(Q1-G)")
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 62.64 95.21 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1u"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Fluke 8060 Low Frequency Beep.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 2 "Net-(J1-VDD)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 59.1725 98.56 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2N7002"
			(at 0 2.4 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NDS7002A-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.115A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "Fluke 8060 Low Frequency Beep.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 1.6 1.07 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/TO-LS1")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 59.2725 94.7975 90)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 -2.4 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PIC10F320-IOT"
			(at 7.58 4.8525 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41585A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "256W Flash, 64B SRAM, SOT-23-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT*23*6*")
		(sheetname "Root")
		(sheetfile "Fluke 8060 Low Frequency Beep.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/TONE")
			(pinfunction "RA0")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J1-PGC{slash}ICSPCLK)")
			(pinfunction "RA1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(Q1-G)")
			(pinfunction "RA2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(J1-VDD)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-~{MCLR}{slash}VPP)")
			(pinfunction "RA3")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 67.21 106.59 -90)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J1"
			(at -2.09 -0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_1x05_P2.54mm_Vertical"
			(at 2.98 -0.87 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-~{MCLR}{slash}VPP)")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-VDD)")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/TONE")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-PGC{slash}ICSPCLK)")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 56.03 97.29)
		(descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x01 1.00mm single row")
		(property "Reference" "J2"
			(at 0 -1.56 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 1.56 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Fluke 8060 Low Frequency Beep.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(at 53.04 98.85 90)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q2"
			(at 2.54 -3.56 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2N3904"
			(at 2.54 2.79 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/TONE")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/TO-LS1")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 56.05 94.74 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "470"
			(at 0 1.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Fluke 8060 Low Frequency Beep.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 6 "Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 2 "Net-(J1-VDD)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 56.03 99.12)
		(descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x01 1.00mm single row")
		(property "Reference" "J3"
			(at 0 -1.56 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 1.56 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole exclude_from_bom dnp)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-PGC{slash}ICSPCLK)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 50.26 92.68) (xy 75.46 92.68) (xy 75.46 100.35) (xy 62.67 100.34) (xy 62.67 103.52) (xy 69.11 103.5)
			(xy 69.11 108.51) (xy 54.81 108.52) (xy 54.79 103.54) (xy 61.16 103.54) (xy 61.16 100.34) (xy 50.26 100.33)
		)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "Fluke 8060A Beep\nFrequency Changer\nWise 2024 CC-BY-SA\nReplaces Q6\nRound pad to 40kHz,\nSquare pad to Vdd"
		(at 65.68 98.5 0)
		(layer "F.SilkS")
	)
)