(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 83)
    (no_connects 0)
    (area 101.055714 69.817599 177.616667 136.400001)
    (thickness 1.6)
    (drawings 59)
    (tracks 359)
    (zones 0)
    (modules 34)
    (nets 53)
  )
  (page A4)
  (title_block
    (title "Raspberry Pi Hat Template")
    (date 2015-12-24)
    (rev 1.1)
    (company OpenFet)
    (comment 1 "Author: Julien Jonathan Cohen, Steve Cohen")
    (comment 2 "License: CERN OHL V1.2")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.15)
    (zone_clearance 0.23)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.26)
    (via_min_drill 0.16)
    (user_via 0.4 0.22)
    (user_via 1.5 0.8)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.762)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.50088 4.50088)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 211.1 101.7)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x213f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Version 1.2/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 +5V)
  (net 4 "Net-(JP1-Pad1)")
  (net 5 "Net-(P3-Pad27)")
  (net 6 "Net-(P3-Pad28)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "Net-(J2-Pad2)")
  (net 9 "Net-(J2-Pad3)")
  (net 10 "Net-(J2-Pad4)")
  (net 11 /LDR)
  (net 12 /LS1-O)
  (net 13 /LS2-O)
  (net 14 /LED1-O)
  (net 15 /LED2-O)
  (net 16 /LS1)
  (net 17 /ENABLE)
  (net 18 /STEP)
  (net 19 /DIR)
  (net 20 /LS2)
  (net 21 /LED1)
  (net 22 /LED2)
  (net 23 /M0)
  (net 24 /M1)
  (net 25 /GPIO-R)
  (net 26 /SDA)
  (net 27 /SCL)
  (net 28 /TXD)
  (net 29 /RXD)
  (net 30 /INT)
  (net 31 /5V-in)
  (net 32 /5V-fuse)
  (net 33 "Net-(J8-Pad1)")
  (net 34 "Net-(P3-Pad37)")
  (net 35 "Net-(P3-Pad40)")
  (net 36 "Net-(P3-Pad35)")
  (net 37 "Net-(P3-Pad36)")
  (net 38 "Net-(P3-Pad33)")
  (net 39 "Net-(P3-Pad32)")
  (net 40 "Net-(P3-Pad26)")
  (net 41 "Net-(P3-Pad24)")
  (net 42 "Net-(P3-Pad23)")
  (net 43 "Net-(P3-Pad21)")
  (net 44 "Net-(P3-Pad19)")
  (net 45 "Net-(U7-Pad5)")
  (net 46 "Net-(U7-Pad6)")
  (net 47 "Net-(U7-Pad7)")
  (net 48 "Net-(U7-Pad10)")
  (net 49 "Net-(U7-Pad11)")
  (net 50 "Net-(U7-Pad12)")
  (net 51 "Net-(U8-Pad12)")
  (net 52 "Net-(U8-Pad13)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net +5V)
    (add_net /5V-fuse)
    (add_net /5V-in)
    (add_net /DIR)
    (add_net /ENABLE)
    (add_net /GPIO-R)
    (add_net /INT)
    (add_net /LDR)
    (add_net /LED1)
    (add_net /LED1-O)
    (add_net /LED2)
    (add_net /LED2-O)
    (add_net /LS1)
    (add_net /LS1-O)
    (add_net /LS2)
    (add_net /LS2-O)
    (add_net /M0)
    (add_net /M1)
    (add_net /RXD)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /STEP)
    (add_net /TXD)
    (add_net GND)
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(P3-Pad19)")
    (add_net "Net-(P3-Pad21)")
    (add_net "Net-(P3-Pad23)")
    (add_net "Net-(P3-Pad24)")
    (add_net "Net-(P3-Pad26)")
    (add_net "Net-(P3-Pad27)")
    (add_net "Net-(P3-Pad28)")
    (add_net "Net-(P3-Pad32)")
    (add_net "Net-(P3-Pad33)")
    (add_net "Net-(P3-Pad35)")
    (add_net "Net-(P3-Pad36)")
    (add_net "Net-(P3-Pad37)")
    (add_net "Net-(P3-Pad40)")
    (add_net "Net-(U7-Pad10)")
    (add_net "Net-(U7-Pad11)")
    (add_net "Net-(U7-Pad12)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U7-Pad6)")
    (add_net "Net-(U7-Pad7)")
    (add_net "Net-(U8-Pad12)")
    (add_net "Net-(U8-Pad13)")
  )
  (net_class +3v3 ""
    (clearance 0.15)
    (trace_width 1.016)
    (via_dia 1.651)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class +5V ""
    (clearance 0.15)
    (trace_width 1.524)
    (via_dia 2.159)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 164.586 90.016 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -4.096 0 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0603 (layer F.Cu) (tedit 57FDC40C)
    (at 159.03 90.27 180)
    (descr "SMT resistor, 0603")
    (fp_text reference JP1 (at 0 1.016 180) (layer F.SilkS))
    (fp_text value JUMPER (at 0 0.6096 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_2 (layer F.Cu) (tedit 581A07CE)
    (at 160.3 94.842 90)
    (descr "Pin strip 2pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at -3.556 0.254 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(JP1-Pad1)"))
    (model walter/pin_strip/pin_strip_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_20x2 (layer F.Cu) (tedit 57FDBD8E)
    (at 137.42 74.82)
    (descr "Box header 20x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P3 (at 0 5.798) (layer F.SilkS))
    (fp_text value Raspberry_Pi_+_Conn (at 0 5.7) (layer F.SilkS) hide)
    (pad 37 thru_hole oval (at 21.59 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P3-Pad37)"))
    (pad 38 thru_hole oval (at 21.59 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS))
    (pad 40 thru_hole oval (at 24.13 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P3-Pad40)"))
    (pad 39 thru_hole oval (at 24.13 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 35 thru_hole oval (at 19.05 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P3-Pad35)"))
    (pad 36 thru_hole oval (at 19.05 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P3-Pad36)"))
    (pad 34 thru_hole oval (at 16.51 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 33 thru_hole oval (at 16.51 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P3-Pad33)"))
    (pad 31 thru_hole oval (at 13.97 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LED2))
    (pad 32 thru_hole oval (at 13.97 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P3-Pad32)"))
    (pad 27 thru_hole oval (at 8.89 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P3-Pad27)"))
    (pad 28 thru_hole oval (at 8.89 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P3-Pad28)"))
    (pad 30 thru_hole oval (at 11.43 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 29 thru_hole oval (at 11.43 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LED1))
    (pad 25 thru_hole oval (at 6.35 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 26 thru_hole oval (at 6.35 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P3-Pad26)"))
    (pad 24 thru_hole oval (at 3.81 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P3-Pad24)"))
    (pad 23 thru_hole oval (at 3.81 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P3-Pad23)"))
    (pad 21 thru_hole oval (at 1.27 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P3-Pad21)"))
    (pad 22 thru_hole oval (at 1.27 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 25 /GPIO-R))
    (pad 20 thru_hole oval (at -1.27 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 19 thru_hole oval (at -1.27 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P3-Pad19)"))
    (pad 17 thru_hole oval (at -3.81 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 18 thru_hole oval (at -3.81 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 30 /INT))
    (pad 16 thru_hole oval (at -6.35 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LS2))
    (pad 15 thru_hole oval (at -6.35 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 19 /DIR))
    (pad 13 thru_hole oval (at -8.89 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 18 /STEP))
    (pad 14 thru_hole oval (at -8.89 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 12 thru_hole oval (at -11.43 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 17 /ENABLE))
    (pad 11 thru_hole oval (at -11.43 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 16 /LS1))
    (pad 9 thru_hole oval (at -13.97 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at -13.97 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 29 /RXD))
    (pad 8 thru_hole oval (at -16.51 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 28 /TXD))
    (pad 7 thru_hole oval (at -16.51 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 11 /LDR))
    (pad 1 thru_hole rect (at -24.13 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at -24.13 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 3 thru_hole oval (at -21.59 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 26 /SDA))
    (pad 4 thru_hole oval (at -21.59 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 5 thru_hole oval (at -19.05 1.27) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 27 /SCL))
    (pad 6 thru_hole oval (at -19.05 -1.27) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model walter/conn_strip/vasch_strip_20x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pololu:SWDIP8_.6W (layer F.Cu) (tedit 5BFCBD25)
    (at 128.804 100.938 270)
    (fp_text reference U8 (at 0 2.286 270) (layer F.SilkS))
    (fp_text value DRV8834 (at 1.778 -0.508 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -6.35 6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 3 thru_hole circle (at -3.81 6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J2-Pad1)"))
    (pad 4 thru_hole circle (at -1.27 6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J2-Pad2)"))
    (pad 5 thru_hole circle (at 1.27 6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J2-Pad3)"))
    (pad 6 thru_hole circle (at 3.81 6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J2-Pad4)"))
    (pad 7 thru_hole rect (at 6.35 6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole circle (at 8.89 6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 9 thru_hole circle (at 8.89 -6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /ENABLE))
    (pad 10 thru_hole circle (at 6.35 -6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /M0))
    (pad 11 thru_hole circle (at 3.81 -6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /M1))
    (pad 12 thru_hole circle (at 1.27 -6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U8-Pad12)"))
    (pad 13 thru_hole circle (at -1.27 -6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U8-Pad13)"))
    (pad 14 thru_hole circle (at -3.81 -6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 15 thru_hole circle (at -6.35 -6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /STEP))
    (pad 16 thru_hole circle (at -8.89 -6.35 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /DIR))
  )
  (module w_conn_misc:dc_socket (layer F.Cu) (tedit 58AFB986)
    (at 140.996 119.988)
    (descr "Socket, DC power supply")
    (fp_text reference J8 (at 0 5.08) (layer F.SilkS))
    (fp_text value dc_jack (at 0 -10.16) (layer F.SilkS))
    (pad 1 thru_hole circle (at 5.30098 -3.50012) (size 4.0005 4.0005) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J8-Pad1)"))
    (pad 2 thru_hole circle (at 0 -0.24892) (size 4.0005 4.0005) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at 0 -6.25094) (size 4.50088 4.50088) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 32 /5V-fuse))
    (model walter/conn_misc/dc_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_3pol (layer F.Cu) (tedit 58AFB5D6)
    (at 129.058 123.798)
    (descr "3-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P4 (at 2.286 -5.334) (layer F.SilkS))
    (fp_text value "PWR CONN" (at 2.54 4.50088) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 31 /5V-in))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_3pol.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 581A04F1)
    (at 113.564 124.052)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J11 (at 2.794 -5.08) (layer F.SilkS))
    (fp_text value TSL2591-A (at 2.54 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 11 /LDR))
  )
  (module Connectors_Molex:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 56C6219D)
    (at 154.712 123.544)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J1 (at 1.778 -4.826) (layer F.SilkS))
    (fp_text value LDR (at 2.54 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 30 /INT))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 581A05DA)
    (at 140.742 99.668)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP3 (at 2.794 -6.35 90) (layer F.SilkS))
    (fp_text value M0 (at 0 7.874) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /M0))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D7.5_L11.2_P2.5 (layer F.Cu) (tedit 58AD28F6)
    (at 117.374 111.352 180)
    (descr "Radial Electrolytic Capacitor Diameter 7.5mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C9 (at -3.048 -3.048 180) (layer F.SilkS))
    (fp_text value 47uf (at -3.048 -3.81 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D7.5_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L11.5_P3.5 (layer F.Cu) (tedit 581A1656)
    (at 117.12 83.412)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 11.5mm, Pitch 3.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C10 (at 5.588 4.572) (layer F.SilkS))
    (fp_text value 100uf (at 1.75 5.3) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L11.5_P3.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-04_04x2.54mm_Straight (layer F.Cu) (tedit 581A0E8F)
    (at 115.596 95.858 270)
    (descr "Connector Headers with Friction Lock, 22-27-2041, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2041")
    (fp_text reference J2 (at -2.794 0 270) (layer F.SilkS))
    (fp_text value STEPPER (at 3.81 4.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J2-Pad4)"))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 581A051F)
    (at 108.42 74.82)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 581A0500)
    (at 108.42 123.82)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 581A0508)
    (at 166.42 123.82)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 581A0516)
    (at 166.42 74.82)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 581A1560)
    (at 145.822 85.19)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U7 (at 4.064 -4.318) (layer F.SilkS))
    (fp_text value ULN2003A (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 /LS1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LS2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LED1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LED2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U7-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U7-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U7-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U7-Pad10)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U7-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U7-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /LED2-O))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /LED1-O))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 /LS2-O))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /LS1-O))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 164.586 84.174 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.096 0 180) (layer F.SilkS))
    (fp_text value 3.9k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P3-Pad28)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 164.586 87.222 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -4.096 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JP1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 164.586 81.126 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -4.096 0 180) (layer F.SilkS))
    (fp_text value 3.9k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P3-Pad27)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-04_04x2.54mm_Straight (layer F.Cu) (tedit 58AFB694)
    (at 127.534 85.444)
    (descr "Connector Headers with Friction Lock, 22-27-2041, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2041")
    (fp_text reference J10 (at 3.81 -5.08) (layer F.SilkS))
    (fp_text value SERIAL (at 3.81 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 /TXD))
    (pad 3 thru_hole oval (at 5.08 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 29 /RXD))
    (pad 4 thru_hole oval (at 7.62 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 56C6219C)
    (at 166.396 93.318 270)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J3 (at 1.27 3.918 270) (layer F.SilkS))
    (fp_text value "Laser 1" (at 1.27 4.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 12 /LS1-O))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 581A06FD)
    (at 166.396 100.43 270)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J4 (at 1.524 3.918 270) (layer F.SilkS))
    (fp_text value "Laser 2" (at 1.27 4.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 /LS2-O))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 581A0E37)
    (at 166.396 107.796 270)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J5 (at 1.27 4.064 270) (layer F.SilkS))
    (fp_text value LED1 (at 1.27 4.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 /LED1-O))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 581A0E51)
    (at 166.396 115.162 270)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J6 (at 1.27 4.064 270) (layer F.SilkS))
    (fp_text value LED2 (at 1.27 4.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 15 /LED2-O))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 56C6219C)
    (at 155.728 114.146)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J7 (at 1 -4.5) (layer F.SilkS))
    (fp_text value RESERVED (at 1.27 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 25 /GPIO-R))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 56C6219C)
    (at 122.708 124.052)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J12 (at 1 -5.08) (layer F.SilkS))
    (fp_text value TSL2591-B (at 1.27 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 26 /SDA))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 27 /SCL))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 581A05E7)
    (at 140.742 95.604 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at -2.54 -6.35 270) (layer F.SilkS))
    (fp_text value M1 (at -0.254 -2.032 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /M1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module project_footprints:tssop-8 (layer F.Cu) (tedit 567BA5EA)
    (at 158.08258 84.43308 180)
    (descr TSSOP-8)
    (fp_text reference U2 (at -2.21742 1.27508 270) (layer F.SilkS))
    (fp_text value CAT24C32HU4I-GT3 (at 0 -1.143 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.32258 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.32258 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.97536 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.97536 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.97536 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P3-Pad27)"))
    (pad 6 smd rect (at 0.32258 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P3-Pad28)"))
    (pad 7 smd rect (at -0.32258 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(JP1-Pad1)"))
    (pad 8 smd rect (at -0.97536 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model walter/smd_dil/tssop-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_HandSoldering (layer B.Cu) (tedit 58AE7618)
    (at 134.9 118.26334 90)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann 433 Series, Hand Soldering,")
    (tags "Fuse, Sicherung, SMD1206,  Littlefuse-Wickmann 433 Series, Hand Soldering,")
    (attr smd)
    (fp_text reference "3.5A FUSE" (at -0.0508 2.19964 90) (layer B.SilkS))
    (fp_text value "3.5 FUSE" (at -0.20066 -2.032 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.08534 0) (size 2.02946 2.65176) (layers B.Cu B.Paste B.Mask)
      (net 31 /5V-in))
    (pad 2 smd rect (at 2.08534 0) (size 2.02946 2.65176) (layers B.Cu B.Paste B.Mask)
      (net 32 /5V-fuse))
  )
  (module "3D Scanner 102916:Happy_Mutant" (layer F.Cu) (tedit 0)
    (at 108.738 114.654)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "3D Scanner 102916:PI_logo" (layer F.Cu) (tedit 0)
    (at 110.77 83.158)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "3D Scanner 102816:DC_pin" (layer F.Cu) (tedit 0)
    (at 147.092 111.098 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (gr_text "Happy Mutant" (at 118.898 116.686) (layer F.SilkS))
  (gr_text "CUT OUT" (at 150.14 116.178 90) (layer Dwgs.User))
  (gr_text "CUT OUT" (at 150.14 116.178 90) (layer F.SilkS))
  (gr_text GND (at 135.154 81.888) (layer F.SilkS))
  (gr_text +5V (at 127.28 81.888) (layer F.SilkS))
  (gr_text ULN2003A (at 150.14 94.08 90) (layer F.SilkS))
  (gr_text +5V (at 162.332 92.81) (layer F.SilkS))
  (gr_text +5V (at 162.332 100.176) (layer F.SilkS))
  (gr_text +5V (at 162.332 107.288) (layer F.SilkS))
  (gr_text +5V (at 162.332 114.654) (layer F.SilkS))
  (gr_text GND (at 158.776 110.59) (layer F.SilkS))
  (gr_text GPIO25 (at 154.966 110.59) (layer F.SilkS))
  (gr_text GPIO24 (at 154.204 119.988) (layer F.SilkS))
  (gr_text GND (at 157.252 119.988) (layer F.SilkS))
  (gr_text +5V (at 159.792 119.988) (layer F.SilkS))
  (gr_text RXD (at 132.614 81.888) (layer F.SilkS))
  (gr_text TXD (at 129.82 81.888) (layer F.SilkS))
  (gr_text 3 (at 138.456 104.748) (layer F.SilkS))
  (gr_text 2 (at 138.456 102.208) (layer F.SilkS))
  (gr_text 1 (at 138.456 99.668) (layer F.SilkS))
  (gr_text 1 (at 138.456 95.604) (layer F.SilkS))
  (gr_text 2 (at 138.456 93.064) (layer F.SilkS))
  (gr_text 3 (at 138.456 90.524) (layer F.SilkS))
  (gr_text GPIO4 (at 119.152 120.242) (layer F.SilkS))
  (gr_text GND (at 115.85 120.242) (layer F.SilkS))
  (gr_text 5V-IN (at 134.392 119.988) (layer F.SilkS))
  (gr_text GND (at 131.09 119.988) (layer F.SilkS))
  (gr_text +5V (at 128.296 119.988) (layer F.SilkS))
  (gr_text SCL (at 125.248 120.242) (layer F.SilkS))
  (gr_text SDA (at 122.708 120.242) (layer F.SilkS))
  (gr_text +3.3V (at 112.802 120.242) (layer F.SilkS))
  (gr_text En (at 137.44 111.606) (layer F.SilkS))
  (gr_text 1 (at 145.314 82.904) (layer F.SilkS))
  (gr_text "MADE IN USA" (at 156.744 98.398 90) (layer F.SilkS))
  (gr_text "Scanner\nHAT V2.0" (at 110.77 88.238) (layer F.SilkS))
  (gr_arc (start 149.92 108.57) (end 149.92 107.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.92 108.57) (end 148.92 108.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 137.6 135.05) (layer Dwgs.User))
    (feature1 (pts (xy 105.1 125.2) (xy 105.1 136.4)))
    (feature2 (pts (xy 170.1 125.2) (xy 170.1 136.4)))
    (crossbar (pts (xy 170.1 133.7) (xy 105.1 133.7)))
    (arrow1a (pts (xy 105.1 133.7) (xy 106.226504 133.113579)))
    (arrow1b (pts (xy 105.1 133.7) (xy 106.226504 134.286421)))
    (arrow2a (pts (xy 170.1 133.7) (xy 168.973496 133.113579)))
    (arrow2b (pts (xy 170.1 133.7) (xy 168.973496 134.286421)))
  )
  (dimension 56.5 (width 0.3) (layer Dwgs.User)
    (gr_text "56.500 mm" (at 175.45 99.45 270) (layer Dwgs.User))
    (feature1 (pts (xy 167.1 127.7) (xy 176.8 127.7)))
    (feature2 (pts (xy 167.1 71.2) (xy 176.8 71.2)))
    (crossbar (pts (xy 174.1 71.2) (xy 174.1 127.7)))
    (arrow1a (pts (xy 174.1 127.7) (xy 173.513579 126.573496)))
    (arrow1b (pts (xy 174.1 127.7) (xy 174.686421 126.573496)))
    (arrow2a (pts (xy 174.1 71.2) (xy 173.513579 72.326504)))
    (arrow2b (pts (xy 174.1 71.2) (xy 174.686421 72.326504)))
  )
  (gr_line (start 104.92 109.07) (end 104.92 124.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.92 90.07) (end 104.92 74.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.92 108.07) (end 105.92 108.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.92 92.07) (end 109.92 107.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.92 91.07) (end 108.92 91.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 108.92 107.07) (end 109.92 107.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 108.92 92.07) (end 108.92 91.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.92 109.07) (end 104.92 109.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.92 90.07) (end 105.92 91.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.92 123.57) (end 148.92 108.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150.92 108.57) (end 150.92 123.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.92 123.57) (end 150.92 123.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.92 123.57) (end 149.92 124.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.92 127.57) (end 107.92 127.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.92 74.07) (end 169.92 124.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.92 71.07) (end 166.92 71.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 166.92 124.57) (end 169.92 124.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 107.92 74.07) (end 104.92 74.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 166.92 74.07) (end 166.92 71.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 107.92 124.57) (end 107.92 127.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.23))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.666 71.474) (xy 169.698 73.506) (xy 169.698 125.322) (xy 167.412 127.354) (xy 147.346 127.1)
        (xy 107.214 127.354) (xy 105.182 125.068) (xy 105.182 108.558) (xy 110.516 108.558) (xy 110.516 91.032)
        (xy 105.69 90.524) (xy 105.436 72.744) (xy 106.96 71.474) (xy 118.136 71.474)
      )
    )
  )
)
